&l4_wkup {						/* 0x44c00000 */
	compatible = "ti,am4-l4-wkup", "simple-pm-bus";
	power-domains = <&prm_wkup>;
	clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_L4_WKUP_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x44c00000 0x800>,
	      <0x44c00800 0x800>,
	      <0x44c01000 0x400>,
	      <0x44c01400 0x400>;
	reg-names = "ap", "la", "ia0", "ia1";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x44c00000 0x100000>,	/* segment 0 */
		 <0x00100000 0x44d00000 0x100000>,	/* segment 1 */
		 <0x00200000 0x44e00000 0x100000>;	/* segment 2 */

	segment@0 {					/* 0x44c00000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 1 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 2 */
			 <0x00001400 0x00001400 0x000400>;	/* ap 3 */
	};

	segment@100000 {					/* 0x44d00000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00100000 0x004000>,	/* ap 4 */
			 <0x00004000 0x00104000 0x001000>,	/* ap 5 */
			 <0x00080000 0x00180000 0x002000>,	/* ap 6 */
			 <0x00082000 0x00182000 0x001000>,	/* ap 7 */
			 <0x000f0000 0x001f0000 0x010000>;	/* ap 8 */

		target-module@0 {			/* 0x44d00000, ap 4 28.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x0 0x4>;
			reg-names = "rev";
			clocks = <&l4_wkup_aon_clkctrl AM4_L4_WKUP_AON_WKUP_M3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x00000000 0x00000000 0x4000>,
				 <0x00080000 0x00080000 0x2000>;

			wkup_m3: cpu@0 {
				compatible = "ti,am4372-wkup-m3";
				reg = <0x00000000 0x4000>,
				      <0x00080000 0x2000>;
				reg-names = "umem", "dmem";
				resets = <&prm_wkup 3>;
				reset-names = "rstctrl";
				ti,pm-firmware = "am335x-pm-firmware.elf";
			};
		};

		target-module@f0000 {			/* 0x44df0000, ap 8 58.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xf0000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xf0000 0x10000>;

			prcm: prcm@0 {
				compatible = "ti,am4-prcm", "simple-bus";
				reg = <0x0 0x11000>;
				interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x11000>;

				prcm_clocks: clocks {
					#address-cells = <1>;
					#size-cells = <0>;
				};

				prcm_clockdomains: clockdomains {
				};
			};
		};
	};

	segment@200000 {					/* 0x44e00000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00200000 0x001000>,	/* ap 9 */
			 <0x00003000 0x00203000 0x001000>,	/* ap 10 */
			 <0x00004000 0x00204000 0x001000>,	/* ap 11 */
			 <0x00005000 0x00205000 0x001000>,	/* ap 12 */
			 <0x00006000 0x00206000 0x001000>,	/* ap 13 */
			 <0x00007000 0x00207000 0x001000>,	/* ap 14 */
			 <0x00008000 0x00208000 0x001000>,	/* ap 15 */
			 <0x00009000 0x00209000 0x001000>,	/* ap 16 */
			 <0x0000a000 0x0020a000 0x001000>,	/* ap 17 */
			 <0x0000b000 0x0020b000 0x001000>,	/* ap 18 */
			 <0x0000c000 0x0020c000 0x001000>,	/* ap 19 */
			 <0x0000d000 0x0020d000 0x001000>,	/* ap 20 */
			 <0x0000f000 0x0020f000 0x001000>,	/* ap 21 */
			 <0x00010000 0x00210000 0x010000>,	/* ap 22 */
			 <0x00030000 0x00230000 0x001000>,	/* ap 23 */
			 <0x00031000 0x00231000 0x001000>,	/* ap 24 */
			 <0x00032000 0x00232000 0x001000>,	/* ap 25 */
			 <0x00033000 0x00233000 0x001000>,	/* ap 26 */
			 <0x00034000 0x00234000 0x001000>,	/* ap 27 */
			 <0x00035000 0x00235000 0x001000>,	/* ap 28 */
			 <0x00036000 0x00236000 0x001000>,	/* ap 29 */
			 <0x00037000 0x00237000 0x001000>,	/* ap 30 */
			 <0x00038000 0x00238000 0x001000>,	/* ap 31 */
			 <0x00039000 0x00239000 0x001000>,	/* ap 32 */
			 <0x0003a000 0x0023a000 0x001000>,	/* ap 33 */
			 <0x0003e000 0x0023e000 0x001000>,	/* ap 34 */
			 <0x0003f000 0x0023f000 0x001000>,	/* ap 35 */
			 <0x00040000 0x00240000 0x040000>,	/* ap 36 */
			 <0x00080000 0x00280000 0x001000>,	/* ap 37 */
			 <0x00088000 0x00288000 0x008000>,	/* ap 38 */
			 <0x00092000 0x00292000 0x001000>,	/* ap 39 */
			 <0x00086000 0x00286000 0x001000>,	/* ap 40 */
			 <0x00087000 0x00287000 0x001000>,	/* ap 41 */
			 <0x00090000 0x00290000 0x001000>,	/* ap 42 */
			 <0x00091000 0x00291000 0x001000>;	/* ap 43 */

		target-module@3000 {			/* 0x44e03000, ap 10 0a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3000 0x1000>;
		};

		target-module@5000 {			/* 0x44e05000, ap 12 30.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5000 0x1000>;
		};

		target-module@7000 {			/* 0x44e07000, ap 14 20.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x7000 0x4>,
			      <0x7010 0x4>,
			      <0x7114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_clkdm */
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_GPIO1_CLKCTRL 0>,
				 <&l4_wkup_clkctrl AM4_L4_WKUP_GPIO1_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7000 0x1000>;

			gpio0: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		target-module@9000 {			/* 0x44e09000, ap 16 04.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x9050 0x4>,
			      <0x9054 0x4>,
			      <0x9058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_clkdm */
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_UART1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x9000 0x1000>;

			uart0: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@b000 {			/* 0x44e0b000, ap 18 48.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xb000 0x8>,
			      <0xb010 0x8>,
			      <0xb090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_clkdm */
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_I2C1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xb000 0x1000>;

			i2c0: i2c@0 {
				compatible = "ti,am4372-i2c","ti,omap4-i2c";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@d000 {			/* 0x44e0d000, ap 20 38.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xd000 0x4>,
			      <0xd010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): wkup_pwrdm, l3s_tsc_clkdm */
			clocks = <&l3s_tsc_clkctrl AM4_L3S_TSC_ADC_TSC_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd000 0x1000>;

			tscadc: tscadc@0 {
				compatible = "ti,am3359-tscadc";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&adc_tsc_fck>;
				clock-names = "fck";
				status = "disabled";
				dmas = <&edma 53 0>, <&edma 57 0>;
				dma-names = "fifo0", "fifo1";

				tsc {
					compatible = "ti,am3359-tsc";
				};

				adc {
					#io-channel-cells = <1>;
					compatible = "ti,am3359-adc";
				};

			};
		};

		target-module@10000 {			/* 0x44e10000, ap 22 0c.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x10000 0x4>;
			reg-names = "rev";
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_CONTROL_CLKCTRL 0>;
			clock-names = "fck";
			ti,no-idle;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x10000 0x10000>;

			scm: scm@0 {
				compatible = "ti,am4-scm", "simple-bus";
				reg = <0x0 0x4000>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x4000>;

				am43xx_pinmux: pinmux@800 {
					compatible = "ti,am437-padconf",
						     "pinctrl-single";
					reg = <0x800 0x31c>;
					#address-cells = <1>;
					#size-cells = <0>;
					#pinctrl-cells = <1>;
					#interrupt-cells = <1>;
					interrupt-controller;
					pinctrl-single,register-width = <32>;
					pinctrl-single,function-mask = <0xffffffff>;
				};

				scm_conf: scm_conf@0 {
					compatible = "syscon", "simple-bus";
					reg = <0x0 0x800>;
					#address-cells = <1>;
					#size-cells = <1>;

					phy_gmii_sel: phy-gmii-sel {
						compatible = "ti,am43xx-phy-gmii-sel";
						reg = <0x650 0x4>;
						#phy-cells = <2>;
					};

					scm_clocks: clocks {
						#address-cells = <1>;
						#size-cells = <0>;
					};
				};

				wkup_m3_ipc: wkup_m3_ipc@1324 {
					compatible = "ti,am4372-wkup-m3-ipc";
					reg = <0x1324 0x44>;
					interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
					ti,rproc = <&wkup_m3>;
					mboxes = <&mailbox &mbox_wkupm3>;
				};

				edma_xbar: dma-router@f90 {
					compatible = "ti,am335x-edma-crossbar";
					reg = <0xf90 0x40>;
					#dma-cells = <3>;
					dma-requests = <64>;
					dma-masters = <&edma>;
				};

				scm_clockdomains: clockdomains {
				};
			};
		};

		timer1_target: target-module@31000 {	/* 0x44e31000, ap 24 40.0 */
			compatible = "ti,sysc-omap2-timer", "ti,sysc";
			reg = <0x31000 0x4>,
			      <0x31010 0x4>,
			      <0x31014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_clkdm */
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_TIMER1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x31000 0x1000>;

			timer1: timer@0 {
				compatible = "ti,am4372-timer-1ms","ti,am335x-timer-1ms";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-alwon;
				clocks = <&timer1_fck>;
				clock-names = "fck";
			};
		};

		target-module@33000 {			/* 0x44e33000, ap 26 18.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x33000 0x1000>;
		};

		target-module@35000 {			/* 0x44e35000, ap 28 50.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x35000 0x4>,
			      <0x35010 0x4>,
			      <0x35014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_EMUFREE |
					 SYSC_OMAP2_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_clkdm */
			clocks = <&l4_wkup_clkctrl AM4_L4_WKUP_WD_TIMER2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x35000 0x1000>;

			wdt: wdt@0 {
				compatible = "ti,am4372-wdt","ti,omap3-wdt";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@37000 {			/* 0x44e37000, ap 30 08.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x37000 0x1000>;
		};

		target-module@39000 {			/* 0x44e39000, ap 32 02.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x39000 0x1000>;
		};

		rtc_target: target-module@3e000 {	/* 0x44e3e000, ap 34 60.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x3e074 0x4>,
			      <0x3e078 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): rtc_pwrdm, l4_rtc_clkdm */
			power-domains = <&prm_rtc>;
			clocks = <&l4_rtc_clkctrl AM4_L4_RTC_RTC_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3e000 0x1000>;

			rtc: rtc@0 {
				compatible = "ti,am4372-rtc", "ti,am3352-rtc",
					     "ti,da830-rtc";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&clk_32768_ck>;
				clock-names = "int-clk";
				system-power-controller;
				status = "disabled";
			};
		};

		target-module@40000 {			/* 0x44e40000, ap 36 68.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x40000 0x40000>;
		};

		target-module@86000 {			/* 0x44e86000, ap 40 70.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x86000 0x4>,
			      <0x86004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			/* Domains (P, C): wkup_pwrdm, l4_wkup_aon_clkdm */
			clocks = <&l4_wkup_aon_clkctrl AM4_L4_WKUP_AON_COUNTER_32K_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x86000 0x1000>;

			counter32k: counter@0 {
				compatible = "ti,am4372-counter32k","ti,omap-counter32k";
				reg = <0x0 0x40>;
			};
		};

		target-module@88000 {			/* 0x44e88000, ap 38 12.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x00000000 0x00088000 0x00008000>,
				 <0x00008000 0x00090000 0x00001000>,
				 <0x00009000 0x00091000 0x00001000>;
		};
	};
};

&l4_fast {					/* 0x4a000000 */
	compatible = "ti,am4-l4-fast", "simple-pm-bus";
	power-domains = <&prm_per>;
	clocks = <&l3_clkctrl AM4_L3_L4_HS_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x4a000000 0x800>,
	      <0x4a000800 0x800>,
	      <0x4a001000 0x400>;
	reg-names = "ap", "la", "ia0";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x4a000000 0x1000000>;	/* segment 0 */

	segment@0 {					/* 0x4a000000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 1 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 2 */
			 <0x00100000 0x00100000 0x008000>,	/* ap 3 */
			 <0x00108000 0x00108000 0x001000>,	/* ap 4 */
			 <0x00400000 0x00400000 0x002000>,	/* ap 5 */
			 <0x00402000 0x00402000 0x001000>,	/* ap 6 */
			 <0x00200000 0x00200000 0x080000>,	/* ap 7 */
			 <0x00280000 0x00280000 0x001000>;	/* ap 8 */

		target-module@100000 {			/* 0x4a100000, ap 3 04.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x101200 0x4>,
			      <0x101208 0x4>,
			      <0x101204 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <0>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			ti,syss-mask = <1>;
			clocks = <&cpsw_125mhz_clkctrl AM4_CPSW_125MHZ_CPGMAC0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x100000 0x8000>;

			mac_sw: switch@0 {
				compatible = "ti,am4372-cpsw-switch", "ti,cpsw-switch";
				reg = <0x0 0x4000>;
				ranges = <0 0 0x4000>;
				clocks = <&cpsw_125mhz_gclk>, <&dpll_clksel_mac_clk>;
				clock-names = "fck", "50mclk";
				assigned-clocks = <&dpll_clksel_mac_clk>;
				assigned-clock-rates = <50000000>;
				#address-cells = <1>;
				#size-cells = <1>;
				syscon = <&scm_conf>;
				status = "disabled";

				interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "rx_thresh", "rx", "tx", "misc";

				ethernet-ports {
					#address-cells = <1>;
					#size-cells = <0>;

					cpsw_port1: port@1 {
						reg = <1>;
						label = "port1";
						mac-address = [ 00 00 00 00 00 00 ];
						phys = <&phy_gmii_sel 1 0>;
					};

					cpsw_port2: port@2 {
						reg = <2>;
						label = "port2";
						mac-address = [ 00 00 00 00 00 00 ];
						phys = <&phy_gmii_sel 2 0>;
					};
				};

				davinci_mdio_sw: mdio@1000 {
					compatible = "ti,am4372-mdio", "ti,cpsw-mdio","ti,davinci_mdio";
					clocks = <&cpsw_125mhz_gclk>;
					clock-names = "fck";
					#address-cells = <1>;
					#size-cells = <0>;
					bus_freq = <1000000>;
					reg = <0x1000 0x100>;
				};

				cpts {
					clocks = <&cpsw_cpts_rft_clk>;
					clock-names = "cpts";
				};
			};
		};

		target-module@200000 {			/* 0x4a200000, ap 7 02.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x200000 0x80000>;
		};

		target-module@400000 {			/* 0x4a400000, ap 5 08.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x400000 0x2000>;
		};
	};
};

&l4_per {					/* 0x48000000 */
	compatible = "ti,am4-l4-per", "simple-pm-bus";
	power-domains = <&prm_per>;
	clocks = <&l4ls_clkctrl AM4_L4LS_L4_LS_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x48000000 0x800>,
	      <0x48000800 0x800>,
	      <0x48001000 0x400>,
	      <0x48001400 0x400>,
	      <0x48001800 0x400>,
	      <0x48001c00 0x400>;
	reg-names = "ap", "la", "ia0", "ia1", "ia2", "ia3";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x48000000 0x100000>,	/* segment 0 */
		 <0x00100000 0x48100000 0x100000>,	/* segment 1 */
		 <0x00200000 0x48200000 0x100000>,	/* segment 2 */
		 <0x00300000 0x48300000 0x100000>,	/* segment 3 */
		 <0x46000000 0x46000000 0x400000>,	/* l3 data port */
		 <0x46400000 0x46400000 0x400000>;	/* l3 data port */

	segment@0 {					/* 0x48000000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 1 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 2 */
			 <0x00001400 0x00001400 0x000400>,	/* ap 3 */
			 <0x00001800 0x00001800 0x000400>,	/* ap 4 */
			 <0x00001c00 0x00001c00 0x000400>,	/* ap 5 */
			 <0x00008000 0x00008000 0x001000>,	/* ap 6 */
			 <0x00009000 0x00009000 0x001000>,	/* ap 7 */
			 <0x00022000 0x00022000 0x001000>,	/* ap 8 */
			 <0x00023000 0x00023000 0x001000>,	/* ap 9 */
			 <0x00024000 0x00024000 0x001000>,	/* ap 10 */
			 <0x00025000 0x00025000 0x001000>,	/* ap 11 */
			 <0x0002a000 0x0002a000 0x001000>,	/* ap 12 */
			 <0x0002b000 0x0002b000 0x001000>,	/* ap 13 */
			 <0x00038000 0x00038000 0x002000>,	/* ap 14 */
			 <0x0003a000 0x0003a000 0x001000>,	/* ap 15 */
			 <0x0003c000 0x0003c000 0x002000>,	/* ap 16 */
			 <0x0003e000 0x0003e000 0x001000>,	/* ap 17 */
			 <0x00040000 0x00040000 0x001000>,	/* ap 18 */
			 <0x00041000 0x00041000 0x001000>,	/* ap 19 */
			 <0x00042000 0x00042000 0x001000>,	/* ap 20 */
			 <0x00043000 0x00043000 0x001000>,	/* ap 21 */
			 <0x00044000 0x00044000 0x001000>,	/* ap 22 */
			 <0x00045000 0x00045000 0x001000>,	/* ap 23 */
			 <0x00046000 0x00046000 0x001000>,	/* ap 24 */
			 <0x00047000 0x00047000 0x001000>,	/* ap 25 */
			 <0x00048000 0x00048000 0x001000>,	/* ap 26 */
			 <0x00049000 0x00049000 0x001000>,	/* ap 27 */
			 <0x0004c000 0x0004c000 0x001000>,	/* ap 28 */
			 <0x0004d000 0x0004d000 0x001000>,	/* ap 29 */
			 <0x00060000 0x00060000 0x001000>,	/* ap 30 */
			 <0x00061000 0x00061000 0x001000>,	/* ap 31 */
			 <0x00080000 0x00080000 0x010000>,	/* ap 32 */
			 <0x00090000 0x00090000 0x001000>,	/* ap 33 */
			 <0x00030000 0x00030000 0x001000>,	/* ap 65 */
			 <0x00031000 0x00031000 0x001000>,	/* ap 66 */
			 <0x0004a000 0x0004a000 0x001000>,	/* ap 71 */
			 <0x0004b000 0x0004b000 0x001000>,	/* ap 72 */
			 <0x000c8000 0x000c8000 0x001000>,	/* ap 73 */
			 <0x000c9000 0x000c9000 0x001000>,	/* ap 74 */
			 <0x000ca000 0x000ca000 0x001000>,	/* ap 77 */
			 <0x000cb000 0x000cb000 0x001000>,	/* ap 78 */
			 <0x00034000 0x00034000 0x001000>,	/* ap 80 */
			 <0x00035000 0x00035000 0x001000>,	/* ap 81 */
			 <0x00036000 0x00036000 0x001000>,	/* ap 84 */
			 <0x00037000 0x00037000 0x001000>,	/* ap 85 */
			 <0x46000000 0x46000000 0x400000>,	/* l3 data port */
			 <0x46400000 0x46400000 0x400000>;	/* l3 data port */

		target-module@8000 {			/* 0x48008000, ap 6 10.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8000 0x1000>;
		};

		target-module@22000 {			/* 0x48022000, ap 8 0a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x22050 0x4>,
			      <0x22054 0x4>,
			      <0x22058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_UART2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x22000 0x1000>;

			uart1: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@24000 {			/* 0x48024000, ap 10 1c.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x24050 0x4>,
			      <0x24054 0x4>,
			      <0x24058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_UART3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x24000 0x1000>;

			uart2: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@2a000 {			/* 0x4802a000, ap 12 22.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x2a000 0x8>,
			      <0x2a010 0x8>,
			      <0x2a090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_I2C2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2a000 0x1000>;

			i2c1: i2c@0 {
				compatible = "ti,am4372-i2c","ti,omap4-i2c";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@30000 {			/* 0x48030000, ap 65 08.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x30000 0x4>,
			      <0x30110 0x4>,
			      <0x30114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPI0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x30000 0x1000>;

			spi0: spi@0 {
				compatible = "ti,am4372-mcspi","ti,omap4-mcspi";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@34000 {			/* 0x48034000, ap 80 56.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x34000 0x1000>;
		};

		target-module@36000 {			/* 0x48036000, ap 84 3e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x36000 0x1000>;
		};

		target-module@38000 {			/* 0x48038000, ap 14 04.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x38000 0x4>,
			      <0x38004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_MCASP0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x38000 0x2000>,
				 <0x46000000 0x46000000 0x400000>;

			mcasp0: mcasp@0 {
				compatible = "ti,am33xx-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x46000000 0x400000>;
				reg-names = "mpu", "dat";
				interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				status = "disabled";
				dmas = <&edma 8 2>,
				       <&edma 9 2>;
				dma-names = "tx", "rx";
			};
		};

		target-module@3c000 {			/* 0x4803c000, ap 16 2a.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x3c000 0x4>,
			      <0x3c004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_MCASP1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3c000 0x2000>,
				 <0x46400000 0x46400000 0x400000>;

			mcasp1: mcasp@0 {
				compatible = "ti,am33xx-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x46400000 0x400000>;
				reg-names = "mpu", "dat";
				interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				status = "disabled";
				dmas = <&edma 10 2>,
				       <&edma 11 2>;
				dma-names = "tx", "rx";
			};
		};

		timer2_target: target-module@40000 {	/* 0x48040000, ap 18 1e.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x40000 0x4>,
			      <0x40010 0x4>,
			      <0x40014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x40000 0x1000>;

			timer2: timer@0  {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&timer2_fck>;
				clock-names = "fck";
			};
		};

		target-module@42000 {			/* 0x48042000, ap 20 24.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x42000 0x4>,
			      <0x42010 0x4>,
			      <0x42014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x42000 0x1000>;

			timer3: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@44000 {			/* 0x48044000, ap 22 26.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x44000 0x4>,
			      <0x44010 0x4>,
			      <0x44014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x44000 0x1000>;

			timer4: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
				status = "disabled";
			};
		};

		target-module@46000 {			/* 0x48046000, ap 24 28.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x46000 0x4>,
			      <0x46010 0x4>,
			      <0x46014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x46000 0x1000>;

			timer5: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
				status = "disabled";
			};
		};

		target-module@48000 {			/* 0x48048000, ap 26 1a.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x48000 0x4>,
			      <0x48010 0x4>,
			      <0x48014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER6_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x48000 0x1000>;

			timer6: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
				status = "disabled";
			};
		};

		target-module@4a000 {			/* 0x4804a000, ap 71 48.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x4a000 0x4>,
			      <0x4a010 0x4>,
			      <0x4a014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER7_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4a000 0x1000>;

			timer7: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
				status = "disabled";
			};
		};

		target-module@4c000 {			/* 0x4804c000, ap 28 36.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x4c000 0x4>,
			      <0x4c010 0x4>,
			      <0x4c114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_GPIO2_CLKCTRL 0>,
				 <&l4ls_clkctrl AM4_L4LS_GPIO2_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4c000 0x1000>;

			gpio1: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		target-module@60000 {			/* 0x48060000, ap 30 14.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x602fc 0x4>,
			      <0x60110 0x4>,
			      <0x60114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_MMC1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x60000 0x1000>;

			mmc1: mmc@0 {
				compatible = "ti,am437-sdhci";
				reg = <0x0 0x1000>;
				ti,needs-special-reset;
				dmas = <&edma 24 0>,
					<&edma 25 0>;
				dma-names = "tx", "rx";
				interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@80000 {			/* 0x48080000, ap 32 18.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x80000 0x4>,
			      <0x80010 0x4>,
			      <0x80014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_ELM_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x80000 0x10000>;

			elm: elm@0 {
				compatible = "ti,am3352-elm";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&l4ls_gclk>;
				clock-names = "fck";
				status = "disabled";
			};
		};

		target-module@c8000 {			/* 0x480c8000, ap 73 06.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xc8000 0x4>,
			      <0xc8010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_MAILBOX_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc8000 0x1000>;

			mailbox: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <8>;
				mbox_wkupm3: mbox-wkup-m3 {
					ti,mbox-send-noirq;
					ti,mbox-tx = <0 0 0>;
					ti,mbox-rx = <0 0 3>;
				};
			};
		};

		target-module@ca000 {			/* 0x480ca000, ap 77 38.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xca000 0x4>,
			      <0xca010 0x4>,
			      <0xca014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPINLOCK_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xca000 0x1000>;

			hwspinlock: spinlock@0 {
				compatible = "ti,omap4-hwspinlock";
				reg = <0x0 0x1000>;
				#hwlock-cells = <1>;
			};
		};
	};

	segment@100000 {					/* 0x48100000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x0008c000 0x0018c000 0x001000>,	/* ap 34 */
			 <0x0008d000 0x0018d000 0x001000>,	/* ap 35 */
			 <0x0008e000 0x0018e000 0x001000>,	/* ap 36 */
			 <0x0008f000 0x0018f000 0x001000>,	/* ap 37 */
			 <0x0009c000 0x0019c000 0x001000>,	/* ap 38 */
			 <0x0009d000 0x0019d000 0x001000>,	/* ap 39 */
			 <0x000a6000 0x001a6000 0x001000>,	/* ap 40 */
			 <0x000a7000 0x001a7000 0x001000>,	/* ap 41 */
			 <0x000a8000 0x001a8000 0x001000>,	/* ap 42 */
			 <0x000a9000 0x001a9000 0x001000>,	/* ap 43 */
			 <0x000aa000 0x001aa000 0x001000>,	/* ap 44 */
			 <0x000ab000 0x001ab000 0x001000>,	/* ap 45 */
			 <0x000ac000 0x001ac000 0x001000>,	/* ap 46 */
			 <0x000ad000 0x001ad000 0x001000>,	/* ap 47 */
			 <0x000ae000 0x001ae000 0x001000>,	/* ap 48 */
			 <0x000af000 0x001af000 0x001000>,	/* ap 49 */
			 <0x000cc000 0x001cc000 0x002000>,	/* ap 50 */
			 <0x000ce000 0x001ce000 0x002000>,	/* ap 51 */
			 <0x000d0000 0x001d0000 0x002000>,	/* ap 52 */
			 <0x000d2000 0x001d2000 0x002000>,	/* ap 53 */
			 <0x000d8000 0x001d8000 0x001000>,	/* ap 54 */
			 <0x000d9000 0x001d9000 0x001000>,	/* ap 55 */
			 <0x000a0000 0x001a0000 0x001000>,	/* ap 67 */
			 <0x000a1000 0x001a1000 0x001000>,	/* ap 68 */
			 <0x000a2000 0x001a2000 0x001000>,	/* ap 69 */
			 <0x000a3000 0x001a3000 0x001000>,	/* ap 70 */
			 <0x000a4000 0x001a4000 0x001000>,	/* ap 92 */
			 <0x000a5000 0x001a5000 0x001000>,	/* ap 93 */
			 <0x000c1000 0x001c1000 0x001000>,	/* ap 94 */
			 <0x000c2000 0x001c2000 0x001000>;	/* ap 95 */

		target-module@8c000 {			/* 0x4818c000, ap 34 0c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8c000 0x1000>;
		};

		target-module@8e000 {			/* 0x4818e000, ap 36 02.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8e000 0x1000>;
		};

		target-module@9c000 {			/* 0x4819c000, ap 38 52.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x9c000 0x8>,
			      <0x9c010 0x8>,
			      <0x9c090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_I2C3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x9c000 0x1000>;

			i2c2: i2c@0 {
				compatible = "ti,am4372-i2c","ti,omap4-i2c";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@a0000 {			/* 0x481a0000, ap 67 2c.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa0000 0x4>,
			      <0xa0110 0x4>,
			      <0xa0114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPI1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa0000 0x1000>;

			spi1: spi@0 {
				compatible = "ti,am4372-mcspi","ti,omap4-mcspi";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@a2000 {			/* 0x481a2000, ap 69 2e.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa2000 0x4>,
			      <0xa2110 0x4>,
			      <0xa2114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPI2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa2000 0x1000>;

			spi2: spi@0 {
				compatible = "ti,am4372-mcspi","ti,omap4-mcspi";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@a4000 {			/* 0x481a4000, ap 92 62.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa4000 0x4>,
			      <0xa4110 0x4>,
			      <0xa4114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPI3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa4000 0x1000>;

			spi3: spi@0 {
				compatible = "ti,am4372-mcspi","ti,omap4-mcspi";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@a6000 {			/* 0x481a6000, ap 40 16.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa6050 0x4>,
			      <0xa6054 0x4>,
			      <0xa6058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_UART4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa6000 0x1000>;

			uart3: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@a8000 {			/* 0x481a8000, ap 42 20.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa8050 0x4>,
			      <0xa8054 0x4>,
			      <0xa8058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_UART5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa8000 0x1000>;

			uart4: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@aa000 {			/* 0x481aa000, ap 44 12.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xaa050 0x4>,
			      <0xaa054 0x4>,
			      <0xaa058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_UART6_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xaa000 0x1000>;

			uart5: serial@0 {
				compatible = "ti,am4372-uart";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@ac000 {			/* 0x481ac000, ap 46 30.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xac000 0x4>,
			      <0xac010 0x4>,
			      <0xac114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_GPIO3_CLKCTRL 0>,
				 <&l4ls_clkctrl AM4_L4LS_GPIO3_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xac000 0x1000>;

			gpio2: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		target-module@ae000 {			/* 0x481ae000, ap 48 32.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xae000 0x4>,
			      <0xae010 0x4>,
			      <0xae114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_GPIO4_CLKCTRL 0>,
				 <&l4ls_clkctrl AM4_L4LS_GPIO4_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xae000 0x1000>;

			gpio3: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		target-module@c1000 {			/* 0x481c1000, ap 94 68.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0xc1000 0x4>,
			      <0xc1010 0x4>,
			      <0xc1014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER8_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc1000 0x1000>;

			timer8: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@cc000 {			/* 0x481cc000, ap 50 46.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xcc020 0x4>;
			reg-names = "rev";
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_D_CAN0_CLKCTRL 0>,
			<&dcan0_fck>;
			clock-names = "fck", "osc";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xcc000 0x2000>;

			dcan0: can@0 {
				compatible = "ti,am4372-d_can", "ti,am3352-d_can";
				reg = <0x0 0x2000>;
				clocks = <&dcan0_fck>;
				clock-names = "fck";
				syscon-raminit = <&scm_conf 0x644 0>;
				interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@d0000 {			/* 0x481d0000, ap 52 3a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xd0020 0x4>;
			reg-names = "rev";
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_D_CAN1_CLKCTRL 0>,
			<&dcan1_fck>;
			clock-names = "fck", "osc";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd0000 0x2000>;

			dcan1: can@0 {
				compatible = "ti,am4372-d_can", "ti,am3352-d_can";
				reg = <0x0 0x2000>;
				clocks = <&dcan1_fck>;
				clock-names = "fck";
				syscon-raminit = <&scm_conf 0x644 1>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@d8000 {			/* 0x481d8000, ap 54 5e.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xd82fc 0x4>,
			      <0xd8110 0x4>,
			      <0xd8114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_MMC2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd8000 0x1000>;

			mmc2: mmc@0 {
				compatible = "ti,am437-sdhci";
				reg = <0x0 0x1000>;
				ti,needs-special-reset;
				dmas = <&edma 2 0>,
					<&edma 3 0>;
				dma-names = "tx", "rx";
				interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};
	};

	segment@200000 {					/* 0x48200000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00200000 0x010000>;

		target-module@0 {
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			power-domains = <&prm_mpu>;
			clocks = <&mpu_clkctrl AM4_MPU_MPU_CLKCTRL 0>;
			clock-names = "fck";
			ti,no-idle;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0 0x10000>;

			mpu@0 {
				compatible = "ti,omap4-mpu";
				pm-sram = <&pm_sram_code
					   &pm_sram_data>;
			};
		};
	};

	segment@300000 {					/* 0x48300000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00300000 0x001000>,	/* ap 56 */
			 <0x00001000 0x00301000 0x001000>,	/* ap 57 */
			 <0x00002000 0x00302000 0x001000>,	/* ap 58 */
			 <0x00003000 0x00303000 0x001000>,	/* ap 59 */
			 <0x00004000 0x00304000 0x001000>,	/* ap 60 */
			 <0x00005000 0x00305000 0x001000>,	/* ap 61 */
			 <0x00018000 0x00318000 0x004000>,	/* ap 62 */
			 <0x0001c000 0x0031c000 0x001000>,	/* ap 63 */
			 <0x00010000 0x00310000 0x002000>,	/* ap 64 */
			 <0x00028000 0x00328000 0x001000>,	/* ap 75 */
			 <0x00029000 0x00329000 0x001000>,	/* ap 76 */
			 <0x00012000 0x00312000 0x001000>,	/* ap 79 */
			 <0x00020000 0x00320000 0x001000>,	/* ap 82 */
			 <0x00021000 0x00321000 0x001000>,	/* ap 83 */
			 <0x00026000 0x00326000 0x001000>,	/* ap 86 */
			 <0x00027000 0x00327000 0x001000>,	/* ap 87 */
			 <0x0002a000 0x0032a000 0x000400>,	/* ap 88 */
			 <0x0002c000 0x0032c000 0x001000>,	/* ap 89 */
			 <0x00013000 0x00313000 0x001000>,	/* ap 90 */
			 <0x00014000 0x00314000 0x001000>,	/* ap 91 */
			 <0x00006000 0x00306000 0x001000>,	/* ap 96 */
			 <0x00007000 0x00307000 0x001000>,	/* ap 97 */
			 <0x00008000 0x00308000 0x001000>,	/* ap 98 */
			 <0x00009000 0x00309000 0x001000>,	/* ap 99 */
			 <0x0000a000 0x0030a000 0x001000>,	/* ap 100 */
			 <0x0000b000 0x0030b000 0x001000>,	/* ap 101 */
			 <0x0003d000 0x0033d000 0x001000>,	/* ap 102 */
			 <0x0003e000 0x0033e000 0x001000>,	/* ap 103 */
			 <0x0003f000 0x0033f000 0x001000>,	/* ap 104 */
			 <0x00040000 0x00340000 0x001000>,	/* ap 105 */
			 <0x00041000 0x00341000 0x001000>,	/* ap 106 */
			 <0x00042000 0x00342000 0x001000>,	/* ap 107 */
			 <0x00045000 0x00345000 0x001000>,	/* ap 108 */
			 <0x00046000 0x00346000 0x001000>,	/* ap 109 */
			 <0x00047000 0x00347000 0x001000>,	/* ap 110 */
			 <0x00048000 0x00348000 0x001000>,	/* ap 111 */
			 <0x000f2000 0x003f2000 0x002000>,	/* ap 112 */
			 <0x000f4000 0x003f4000 0x001000>,	/* ap 113 */
			 <0x0004c000 0x0034c000 0x002000>,	/* ap 114 */
			 <0x0004e000 0x0034e000 0x001000>,	/* ap 115 */
			 <0x00022000 0x00322000 0x001000>,	/* ap 116 */
			 <0x00023000 0x00323000 0x001000>,	/* ap 117 */
			 <0x000f0000 0x003f0000 0x001000>,	/* ap 118 */
			 <0x0002a400 0x0032a400 0x000400>,	/* ap 119 */
			 <0x0002a800 0x0032a800 0x000400>,	/* ap 120 */
			 <0x0002ac00 0x0032ac00 0x000400>,	/* ap 121 */
			 <0x0002b000 0x0032b000 0x001000>,	/* ap 122 */
			 <0x00080000 0x00380000 0x020000>,	/* ap 123 */
			 <0x000a0000 0x003a0000 0x001000>,	/* ap 124 */
			 <0x000a8000 0x003a8000 0x008000>,	/* ap 125 */
			 <0x000b0000 0x003b0000 0x001000>,	/* ap 126 */
			 <0x000c0000 0x003c0000 0x020000>,	/* ap 127 */
			 <0x000e0000 0x003e0000 0x001000>,	/* ap 128 */
			 <0x000e8000 0x003e8000 0x008000>;	/* ap 129 */

		target-module@0 {			/* 0x48300000, ap 56 40.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x0 0x4>,
			      <0x4 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1000>;

			epwmss0: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ecap0: pwm@100 {
					compatible = "ti,am4372-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4ls_gclk>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm0: pwm@200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm0_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@2000 {			/* 0x48302000, ap 58 4a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x2000 0x4>,
			      <0x2004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2000 0x1000>;

			epwmss1: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ecap1: pwm@100 {
					compatible = "ti,am4372-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4ls_gclk>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm1: pwm@200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm1_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@4000 {			/* 0x48304000, ap 60 44.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x4000 0x4>,
			      <0x4004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4000 0x1000>;

			epwmss2: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ecap2: pwm@100 {
					compatible = "ti,am4372-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4ls_gclk>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm2: pwm@200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm2_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@6000 {			/* 0x48306000, ap 96 58.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x6000 0x4>,
			      <0x6004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6000 0x1000>;

			epwmss3: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ehrpwm3: pwm@200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm3_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@8000 {			/* 0x48308000, ap 98 54.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x8000 0x4>,
			      <0x8004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8000 0x1000>;

			epwmss4: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ehrpwm4: pwm@48308200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm4_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@a000 {			/* 0x4830a000, ap 100 60.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xa000 0x4>,
			      <0xa004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_EPWMSS5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa000 0x1000>;

			epwmss5: epwmss@0 {
				compatible = "ti,am4372-pwmss","ti,am33xx-pwmss";
				reg = <0x0 0x10>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x1000>;
				status = "disabled";

				ehrpwm5: pwm@200 {
					compatible = "ti,am4372-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm5_tbclk>, <&l4ls_gclk>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@10000 {			/* 0x48310000, ap 64 4e.1 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x11fe0 0x4>,
			      <0x11fe4 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP2_AUTOIDLE>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_RNG_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x10000 0x2000>;

			rng: rng@0 {
				compatible = "ti,omap4-rng";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@13000 {			/* 0x48313000, ap 90 50.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x13000 0x1000>;
		};

		target-module@18000 {			/* 0x48318000, ap 62 4c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x18000 0x4000>;
		};

		target-module@20000 {			/* 0x48320000, ap 82 34.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x20000 0x4>,
			      <0x20010 0x4>,
			      <0x20114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_GPIO5_CLKCTRL 0>,
				 <&l4ls_clkctrl AM4_L4LS_GPIO5_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x20000 0x1000>;

			gpio4: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		gpio5_target: target-module@22000 {		/* 0x48322000, ap 116 64.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x22000 0x4>,
			      <0x22010 0x4>,
			      <0x22114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_GPIO6_CLKCTRL 0>,
				 <&l4ls_clkctrl AM4_L4LS_GPIO6_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x22000 0x1000>;

			gpio5: gpio@0 {
				compatible = "ti,am4372-gpio","ti,omap4-gpio";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
				status = "disabled";
			};
		};

		target-module@26000 {			/* 0x48326000, ap 86 66.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x26000 0x4>,
			      <0x26104 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_VPFE0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x26000 0x1000>;

			vpfe0: vpfe@0 {
				compatible = "ti,am437x-vpfe";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@28000 {			/* 0x48328000, ap 75 0e.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x28000 0x4>,
			      <0x28104 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_VPFE1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x28000 0x1000>;

			vpfe1: vpfe@0 {
				compatible = "ti,am437x-vpfe";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@2a000 {			/* 0x4832a000, ap 88 3c.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x2a000 0x4>,
			      <0x2a010 0x4>,
			      <0x2a014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, dss_clkdm */
			clocks = <&dss_clkctrl AM4_DSS_DSS_CORE_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x00000000 0x0002a000 0x00000400>,
				 <0x00000400 0x0002a400 0x00000400>,
				 <0x00000800 0x0002a800 0x00000400>,
				 <0x00000c00 0x0002ac00 0x00000400>,
				 <0x00001000 0x0002b000 0x00001000>;

			dss: dss@0 {
				compatible = "ti,omap3-dss";
				reg = <0 0x200>;
				status = "disabled";
				clocks = <&disp_clk>;
				clock-names = "fck";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0x00000000 0x00000000 0x00000400>,
					 <0x00000400 0x00000400 0x00000400>,
					 <0x00000800 0x00000800 0x00000400>,
					 <0x00000c00 0x00000c00 0x00000400>,
					 <0x00001000 0x00001000 0x00001000>;

				target-module@400 {
					compatible = "ti,sysc-omap2", "ti,sysc";
					reg = <0x400 0x4>,
					      <0x410 0x4>,
					      <0x414 0x4>;
					reg-names = "rev", "sysc", "syss";
					ti,sysc-sidle = <SYSC_IDLE_FORCE>,
							<SYSC_IDLE_NO>,
							<SYSC_IDLE_SMART>;
					ti,sysc-midle = <SYSC_IDLE_FORCE>,
							<SYSC_IDLE_NO>,
							<SYSC_IDLE_SMART>;
					ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
							 SYSC_OMAP2_ENAWAKEUP |
							 SYSC_OMAP2_SOFTRESET |
							 SYSC_OMAP2_AUTOIDLE)>;
					ti,syss-mask = <1>;
					clocks = <&dss_clkctrl AM4_DSS_DSS_CORE_CLKCTRL 0>;
					clock-names = "fck";
					#address-cells = <1>;
					#size-cells = <1>;
					ranges = <0 0x400 0x400>;

					dispc: dispc@0 {
						compatible = "ti,omap3-dispc";
						reg = <0 0x400>;
						interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
						clocks = <&disp_clk>;
						clock-names = "fck";

						max-memory-bandwidth = <230000000>;
					};
				};

				target-module@800 {
					compatible = "ti,sysc-omap2", "ti,sysc";
					reg = <0x800 0x4>,
					      <0x810 0x4>,
					      <0x814 0x4>;
					reg-names = "rev", "sysc", "syss";
					ti,sysc-sidle = <SYSC_IDLE_FORCE>,
							<SYSC_IDLE_NO>,
							<SYSC_IDLE_SMART>;
					ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
							 SYSC_OMAP2_AUTOIDLE)>;
					ti,syss-mask = <1>;
					clocks = <&dss_clkctrl AM4_DSS_DSS_CORE_CLKCTRL 0>;
					clock-names = "fck";
					#address-cells = <1>;
					#size-cells = <1>;
					ranges = <0 0x800 0x400>;

					rfbi: rfbi@0 {
						compatible = "ti,omap3-rfbi";
						reg = <0 0x100>;
						clocks = <&dss_clkctrl AM4_DSS_DSS_CORE_CLKCTRL 0>;
						clock-names = "fck";
						status = "disabled";
					};
				};
			};
		};

		target-module@3d000 {			/* 0x4833d000, ap 102 6e.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x3d000 0x4>,
			      <0x3d010 0x4>,
			      <0x3d014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER9_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3d000 0x1000>;

			timer9: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@3f000 {			/* 0x4833f000, ap 104 5c.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x3f000 0x4>,
			      <0x3f010 0x4>,
			      <0x3f014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER10_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3f000 0x1000>;

			timer10: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@41000 {			/* 0x48341000, ap 106 76.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x41000 0x4>,
			      <0x41010 0x4>,
			      <0x41014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_TIMER11_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x41000 0x1000>;

			timer11: timer@0 {
				compatible = "ti,am4372-timer","ti,am335x-timer";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@45000 {			/* 0x48345000, ap 108 6a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x45000 0x4>,
			      <0x45110 0x4>,
			      <0x45114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_SPI4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x45000 0x1000>;

			spi4: spi@0 {
				compatible = "ti,am4372-mcspi","ti,omap4-mcspi";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@47000 {			/* 0x48347000, ap 110 70.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x47000 0x4>,
			      <0x47014 0x4>,
			      <0x47018 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_HDQ1W_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x47000 0x1000>;

			hdq: hdq@0 {
				compatible = "ti,am4372-hdq";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&func_12m_clk>;
				clock-names = "fck";
				status = "disabled";
			};
		};

		target-module@4c000 {			/* 0x4834c000, ap 114 72.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x4c000 0x4>,
			      <0x4c010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			clocks = <&l3s_clkctrl AM4_L3S_ADC1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4c000 0x2000>;

			magadc: magadc@0 {
				compatible = "ti,am4372-magadc";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&adc_mag_fck>;
				clock-names = "fck";
				dmas = <&edma 54 0>, <&edma 55 0>;
				dma-names = "fifo0", "fifo1";
				status = "disabled";

				mag {
					compatible = "ti,am4372-mag";
				};

				adc {
					#io-channel-cells = <1>;
					compatible = "ti,am4372-adc";
				};
			};
		};

		target-module@80000 {			/* 0x48380000, ap 123 42.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x80000 0x4>,
			      <0x80010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_DMADISABLE>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_USB_OTG_SS0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x80000 0x20000>;

			dwc3_1: omap_dwc3@0 {
				compatible = "ti,am437x-dwc3";
				reg = <0x0 0x10000>;
				interrupts = <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				utmi-mode = <1>;
				ranges = <0 0 0x20000>;

				usb1: usb@10000 {
					compatible = "snps,dwc3";
					reg = <0x10000 0x10000>;
					interrupts = <GIC_SPI 168 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 168 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "peripheral",
							  "host",
							  "otg";
					phys = <&usb2_phy1>;
					phy-names = "usb2-phy";
					maximum-speed = "high-speed";
					dr_mode = "otg";
					status = "disabled";
					snps,dis_u3_susphy_quirk;
					snps,dis_u2_susphy_quirk;
				};
			};
		};

		target-module@a8000 {			/* 0x483a8000, ap 125 6c.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xa8000 0x4>;
			reg-names = "rev";
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_OCP2SCP0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa8000 0x8000>;

			ocp2scp0: ocp2scp@0 {
				compatible = "ti,am437x-ocp2scp", "ti,omap-ocp2scp";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x8000>;

				usb2_phy1: phy@8000 {
					compatible = "ti,am437x-usb2";
					reg = <0x0 0x8000>;
					syscon-phy-power = <&scm_conf 0x620>;
					clocks = <&usb_phy0_always_on_clk32k>,
						 <&l3s_clkctrl AM4_L3S_USB_OTG_SS0_CLKCTRL 8>;
					clock-names = "wkupclk", "refclk";
					#phy-cells = <0>;
					status = "disabled";
				};
			};
		};

		target-module@c0000 {			/* 0x483c0000, ap 127 7a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xc0000 0x4>,
			      <0xc0010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_DMADISABLE>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): per_pwrdm, l3s_clkdm */
			clocks = <&l3s_clkctrl AM4_L3S_USB_OTG_SS1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc0000 0x20000>;

			dwc3_2: omap_dwc3@0 {
				compatible = "ti,am437x-dwc3";
				reg = <0x0 0x10000>;
				interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				utmi-mode = <1>;
				ranges = <0 0 0x20000>;

				usb2: usb@10000 {
					compatible = "snps,dwc3";
					reg = <0x10000 0x10000>;
					interrupts = <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "peripheral",
							  "host",
							  "otg";
					phys = <&usb2_phy2>;
					phy-names = "usb2-phy";
					maximum-speed = "high-speed";
					dr_mode = "otg";
					status = "disabled";
					snps,dis_u3_susphy_quirk;
					snps,dis_u2_susphy_quirk;
				};
			};
		};

		target-module@e8000 {			/* 0x483e8000, ap 129 78.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xe8000 0x4>;
			reg-names = "rev";
			/* Domains (P, C): per_pwrdm, l4ls_clkdm */
			clocks = <&l4ls_clkctrl AM4_L4LS_OCP2SCP1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe8000 0x8000>;

			ocp2scp1: ocp2scp@0 {
				compatible = "ti,am437x-ocp2scp", "ti,omap-ocp2scp";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x8000>;

				usb2_phy2: phy@8000 {
					compatible = "ti,am437x-usb2";
					reg = <0x0 0x8000>;
					syscon-phy-power = <&scm_conf 0x628>;
					clocks = <&usb_phy1_always_on_clk32k>,
						 <&l3s_clkctrl AM4_L3S_USB_OTG_SS1_CLKCTRL 8>;
					clock-names = "wkupclk", "refclk";
					#phy-cells = <0>;
					status = "disabled";
				};
			};
		};

		target-module@f2000 {			/* 0x483f2000, ap 112 5a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xf2000 0x2000>;
		};
	};
};

