/*
 * Copyright 2016 Grinn
 *
 * Author: Marcin Niestroj <m.niestroj@grinn-global.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License
 *     version 2 as published by the Free Software Foundation.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;

#include "imx6ul-litesom.dtsi"

/ {
	model = "Grinn i.MX6UL liteBoard";
	compatible = "grinn,imx6ul-liteboard", "grinn,imx6ul-litesom",
		     "fsl,imx6ul";

	chosen {
		stdout-path = &uart1;
	};

	reg_usb_otg1_vbus: regulator-usb-otg1-vbus {
		compatible = "regulator-fixed";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_usb_otg1_vbus>;
		regulator-name = "usb_otg1_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio2 8 GPIO_ACTIVE_LOW>;
	};
};

&iomuxc {
	pinctrl_enet1: enet1grp {
		fsl,pins = <
			MX6UL_PAD_GPIO1_IO07__ENET1_MDC		0x1b0b0
			MX6UL_PAD_GPIO1_IO06__ENET1_MDIO	0x1b0b0
			MX6UL_PAD_ENET1_RX_EN__ENET1_RX_EN	0x1b0b0
			MX6UL_PAD_ENET1_RX_ER__ENET1_RX_ER	0x1b0b0
			MX6UL_PAD_ENET1_RX_DATA0__ENET1_RDATA00 0x1b0b0
			MX6UL_PAD_ENET1_RX_DATA1__ENET1_RDATA01 0x1b0b0
			MX6UL_PAD_ENET1_TX_EN__ENET1_TX_EN	0x1b0b0
			MX6UL_PAD_ENET1_TX_DATA0__ENET1_TDATA00 0x1b0b0
			MX6UL_PAD_ENET1_TX_DATA1__ENET1_TDATA01 0x1b0b0
			MX6UL_PAD_ENET1_TX_CLK__ENET1_REF_CLK1	0x4001b031
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX6UL_PAD_UART1_TX_DATA__UART1_DCE_TX	0x1b0b1
			MX6UL_PAD_UART1_RX_DATA__UART1_DCE_RX	0x1b0b1
		>;
	};

	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <
			MX6UL_PAD_UART1_RTS_B__GPIO1_IO19	0x17059
			MX6UL_PAD_SD1_CMD__USDHC1_CMD		0x17059
			MX6UL_PAD_SD1_CLK__USDHC1_CLK		0x10071
			MX6UL_PAD_SD1_DATA0__USDHC1_DATA0	0x17059
			MX6UL_PAD_SD1_DATA1__USDHC1_DATA1	0x17059
			MX6UL_PAD_SD1_DATA2__USDHC1_DATA2	0x17059
			MX6UL_PAD_SD1_DATA3__USDHC1_DATA3	0x17059
		>;
	};

	pinctrl_usb_otg1_vbus: usb-otg1-vbus-grp {
		fsl,pins = <
			MX6UL_PAD_ENET2_RX_DATA0__GPIO2_IO08	0x79
		>;
	};
};

&fec1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet1>;
	phy-mode = "rmii";
	phy-handle = <&ethphy0>;
	status = "okay";

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;

		ethphy0: ethernet-phy@0 {
			reg = <0>;
		};
	};
};

&snvs_poweroff {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	status = "okay";
};

&usbotg1 {
	vbus-supply = <&reg_usb_otg1_vbus>;
	dr_mode = "host";
	status = "okay";
};

&usdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc1>;
	cd-gpios = <&gpio1 19 GPIO_ACTIVE_LOW>;
	no-1-8-v;
	keep-power-in-suspend;
	wakeup-source;
	status = "okay";
};
