// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2014-2016 Texas Instruments Incorporated - https://www.ti.com/
 */
/dts-v1/;

#include "dra72x.dtsi"
#include "dra7-ipu-dsp-common.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/clock/ti-dra7-atl.h>

/ {
	compatible = "ti,dra72-evm", "ti,dra722", "ti,dra72", "ti,dra7";

	aliases {
		display0 = &hdmi0;
	};

	chosen {
		stdout-path = &uart1;
	};

	evm_12v0: fixedregulator-evm12v0 {
		/* main supply */
		compatible = "regulator-fixed";
		regulator-name = "evm_12v0";
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	evm_5v0: fixedregulator-evm5v0 {
		/* Output 1 of TPS43351QDAPRQ1 on dra72-evm */
		/* Output 1 of LM5140QRWGTQ1 on dra71-evm */
		compatible = "regulator-fixed";
		regulator-name = "evm_5v0";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&evm_12v0>;
		regulator-always-on;
		regulator-boot-on;
	};

	evm_3v6: fixedregulator-evm_3v6 {
		compatible = "regulator-fixed";
		regulator-name = "evm_3v6";
		regulator-min-microvolt = <3600000>;
		regulator-max-microvolt = <3600000>;
		vin-supply = <&evm_5v0>;
		regulator-always-on;
		regulator-boot-on;
	};

	vsys_3v3: fixedregulator-vsys3v3 {
		/* Output 2 of TPS43351QDAPRQ1 on dra72-evm */
		/* Output 2 of LM5140QRWGTQ1 on dra71-evm */
		compatible = "regulator-fixed";
		regulator-name = "vsys_3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&evm_12v0>;
		regulator-always-on;
		regulator-boot-on;
	};

	evm_3v3_sw: fixedregulator-evm_3v3 {
		/* TPS22965DSG */
		compatible = "regulator-fixed";
		regulator-name = "evm_3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vsys_3v3>;
		regulator-always-on;
		regulator-boot-on;
	};

	aic_dvdd: fixedregulator-aic_dvdd {
		/* TPS77018DBVT */
		compatible = "regulator-fixed";
		regulator-name = "aic_dvdd";
		vin-supply = <&evm_3v3_sw>;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	evm_3v3_sd: fixedregulator-sd {
		compatible = "regulator-fixed";
		regulator-name = "evm_3v3_sd";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&evm_3v3_sw>;
		enable-active-high;
		gpio = <&pcf_gpio_21 5 GPIO_ACTIVE_HIGH>;
	};

	extcon_usb1: extcon_usb1 {
		compatible = "linux,extcon-usb-gpio";
		id-gpios = <&pcf_gpio_21 1 GPIO_ACTIVE_HIGH>;
	};

	extcon_usb2: extcon_usb2 {
		compatible = "linux,extcon-usb-gpio";
		id-gpios = <&pcf_gpio_21 2 GPIO_ACTIVE_HIGH>;
	};

	hdmi0: connector {
		compatible = "hdmi-connector";
		label = "hdmi";

		type = "a";

		port {
			hdmi_connector_in: endpoint {
				remote-endpoint = <&tpd12s015_out>;
			};
		};
	};

	tpd12s015: encoder {
		compatible = "ti,tpd12s015";

		gpios = <&pcf_hdmi 4 GPIO_ACTIVE_HIGH>,	/* P4, CT CP HPD */
			<&pcf_hdmi 5 GPIO_ACTIVE_HIGH>,	/* P5, LS OE */
			<&gpio7 12 GPIO_ACTIVE_HIGH>;	/* gpio7_12/sp1_cs2, HPD */

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				tpd12s015_in: endpoint {
					remote-endpoint = <&hdmi_out>;
				};
			};

			port@1 {
				reg = <1>;

				tpd12s015_out: endpoint {
					remote-endpoint = <&hdmi_connector_in>;
				};
			};
		};
	};

	sound0: sound0 {
		compatible = "simple-audio-card";
		simple-audio-card,name = "DRA7xx-EVM";
		simple-audio-card,widgets =
			"Headphone", "Headphone Jack",
			"Line", "Line Out",
			"Microphone", "Mic Jack",
			"Line", "Line In";
		simple-audio-card,routing =
			"Headphone Jack",       "HPLOUT",
			"Headphone Jack",       "HPROUT",
			"Line Out",		"LLOUT",
			"Line Out",		"RLOUT",
			"MIC3L",		"Mic Jack",
			"MIC3R",		"Mic Jack",
			"Mic Jack",		"Mic Bias",
			"LINE1L",               "Line In",
			"LINE1R",               "Line In";
		simple-audio-card,format = "dsp_b";
		simple-audio-card,bitclock-master = <&sound0_master>;
		simple-audio-card,frame-master = <&sound0_master>;
		simple-audio-card,bitclock-inversion;

		sound0_master: simple-audio-card,cpu {
			sound-dai = <&mcasp3>;
			system-clock-frequency = <5644800>;
		};

		simple-audio-card,codec {
			sound-dai = <&tlv320aic3106>;
			clocks = <&atl_clkin2_ck>;
		};
	};

	vmmcwl_fixed: fixedregulator-mmcwl {
		compatible = "regulator-fixed";
		regulator-name = "vmmcwl_fixed";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		gpio = <&gpio5 8 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	clk_ov5640_fixed: clock {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
	};
};

&dra7_pmx_core {
	dcan1_pins_default: dcan1-default-pins {
		pinctrl-single,pins = <
			DRA7XX_CORE_IOPAD(0x37d0, PIN_OUTPUT_PULLUP | MUX_MODE0) /* dcan1_tx */
			DRA7XX_CORE_IOPAD(0x3818, PULL_UP | MUX_MODE1)	/* wakeup0.dcan1_rx */
		>;
	};

	dcan1_pins_sleep: dcan1-sleep-pins {
		pinctrl-single,pins = <
			DRA7XX_CORE_IOPAD(0x37d0, MUX_MODE15 | PULL_UP)	/* dcan1_tx.off */
			DRA7XX_CORE_IOPAD(0x3818, MUX_MODE15 | PULL_UP)	/* wakeup0.off */
		>;
	};
};

&i2c1 {
	status = "okay";
	clock-frequency = <400000>;

	pcf_lcd: gpio@20 {
		compatible = "nxp,pcf8575";
		reg = <0x20>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	pcf_gpio_21: gpio@21 {
		compatible = "nxp,pcf8575";
		reg = <0x21>;
		lines-initial-states = <0x1408>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	tlv320aic3106: tlv320aic3106@19 {
		#sound-dai-cells = <0>;
		compatible = "ti,tlv320aic3106";
		reg = <0x19>;
		adc-settle-ms = <40>;
		ai3x-micbias-vg = <1>;		/* 2.0V */
		status = "okay";

		/* Regulators */
		AVDD-supply = <&evm_3v3_sw>;
		IOVDD-supply = <&evm_3v3_sw>;
		DRVDD-supply = <&evm_3v3_sw>;
		DVDD-supply = <&aic_dvdd>;
	};
};

&i2c5 {
	status = "okay";
	clock-frequency = <400000>;

	pcf_hdmi: pcf8575@26 {
		compatible = "nxp,pcf8575";
		reg = <0x26>;
		gpio-controller;
		#gpio-cells = <2>;
		/*
		 * initial state is used here to keep the mdio interface
		 * selected on RU89 through SEL_VIN4_MUX_S0, VIN2_S1 and
		 * VIN2_S0 driven high otherwise Ethernet stops working
		 * VIN6_SEL_S0 is low, thus selecting McASP3 over VIN6
		 */
		lines-initial-states = <0x0f2b>;

		hdmi-audio-hog {
			/* vin6_sel_s0: high: VIN6, low: audio */
			gpio-hog;
			gpios = <1 GPIO_ACTIVE_HIGH>;
			output-low;
			line-name = "vin6_sel_s0";
		};
	};

	ov5640@3c {
		compatible = "ovti,ov5640";
		reg = <0x3c>;

		clocks = <&clk_ov5640_fixed>;
		clock-names = "xclk";

		port {
			csi2_cam0: endpoint {
				remote-endpoint = <&csi2_phy0>;
				clock-lanes = <0>;
				data-lanes = <1 2>;
			};
		};
	};

};

&uart1 {
	status = "okay";
	interrupts-extended = <&crossbar_mpu GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>,
			      <&dra7_pmx_core 0x3e0>;
};

&elm {
	status = "okay";
};

&gpmc {
	/*
	 * For the existing IOdelay configuration via U-Boot we don't
	 * support NAND on dra72-evm. Keep it disabled. Enabling it
	 * requires a different configuration by U-Boot.
	 */
	status = "disabled";
	ranges = <0 0 0x08000000 0x01000000>;	/* minimum GPMC partition = 16MB */
	nand@0,0 {
		/* To use NAND, DIP switch SW5 must be set like so:
		 * SW5.1 (NAND_SELn) = ON (LOW)
		 * SW5.9 (GPMC_WPN) = OFF (HIGH)
		 */
		compatible = "ti,omap2-nand";
		reg = <0 0 4>;		/* device IO registers */
		interrupt-parent = <&gpmc>;
		interrupts = <0 IRQ_TYPE_NONE>, /* fifoevent */
			     <1 IRQ_TYPE_NONE>;	/* termcount */
		rb-gpios = <&gpmc 0 GPIO_ACTIVE_HIGH>; /* gpmc_wait0 pin */
		ti,nand-xfer-type = "prefetch-dma";
		ti,nand-ecc-opt = "bch8";
		ti,elm-id = <&elm>;
		nand-bus-width = <16>;
		gpmc,device-width = <2>;
		gpmc,sync-clk-ps = <0>;
		gpmc,cs-on-ns = <0>;
		gpmc,cs-rd-off-ns = <80>;
		gpmc,cs-wr-off-ns = <80>;
		gpmc,adv-on-ns = <0>;
		gpmc,adv-rd-off-ns = <60>;
		gpmc,adv-wr-off-ns = <60>;
		gpmc,we-on-ns = <10>;
		gpmc,we-off-ns = <50>;
		gpmc,oe-on-ns = <4>;
		gpmc,oe-off-ns = <40>;
		gpmc,access-ns = <40>;
		gpmc,wr-access-ns = <80>;
		gpmc,rd-cycle-ns = <80>;
		gpmc,wr-cycle-ns = <80>;
		gpmc,bus-turnaround-ns = <0>;
		gpmc,cycle2cycle-delay-ns = <0>;
		gpmc,clk-activation-ns = <0>;
		gpmc,wr-data-mux-bus-ns = <0>;
		/* MTD partition table */
		/* All SPL-* partitions are sized to minimal length
		 * which can be independently programmable. For
		 * NAND flash this is equal to size of erase-block */
		#address-cells = <1>;
		#size-cells = <1>;
		partition@0 {
			label = "NAND.SPL";
			reg = <0x00000000 0x00020000>;
		};
		partition@1 {
			label = "NAND.SPL.backup1";
			reg = <0x00020000 0x00020000>;
		};
		partition@2 {
			label = "NAND.SPL.backup2";
			reg = <0x00040000 0x00020000>;
		};
		partition@3 {
			label = "NAND.SPL.backup3";
			reg = <0x00060000 0x00020000>;
		};
		partition@4 {
			label = "NAND.u-boot-spl-os";
			reg = <0x00080000 0x00040000>;
		};
		partition@5 {
			label = "NAND.u-boot";
			reg = <0x000c0000 0x00100000>;
		};
		partition@6 {
			label = "NAND.u-boot-env";
			reg = <0x001c0000 0x00020000>;
		};
		partition@7 {
			label = "NAND.u-boot-env.backup1";
			reg = <0x001e0000 0x00020000>;
		};
		partition@8 {
			label = "NAND.kernel";
			reg = <0x00200000 0x00800000>;
		};
		partition@9 {
			label = "NAND.file-system";
			reg = <0x00a00000 0x0f600000>;
		};
	};
};

&omap_dwc3_1 {
	extcon = <&extcon_usb1>;
};

&omap_dwc3_2 {
	extcon = <&extcon_usb2>;
};

&usb1 {
	dr_mode = "otg";
	extcon = <&extcon_usb1>;
};

&usb2 {
	dr_mode = "host";
	extcon = <&extcon_usb2>;
};

&mmc1 {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins_default>;
	vmmc-supply = <&evm_3v3_sd>;
	bus-width = <4>;
	/*
	 * SDCD signal is not being used here - using the fact that GPIO mode
	 * is a viable alternative
	 */
	cd-gpios = <&gpio6 27 GPIO_ACTIVE_LOW>;
	max-frequency = <192000000>;
};

&mmc2 {
	/* SW5-3 in ON position */
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&mmc2_pins_default>;
	bus-width = <8>;
	non-removable;
	max-frequency = <192000000>;
};

&mmc4 {
	status = "okay";
	vmmc-supply = <&evm_3v6>;
	vqmmc-supply = <&vmmcwl_fixed>;
	bus-width = <4>;
	cap-power-off-card;
	keep-power-in-suspend;
	non-removable;
	pinctrl-names = "default", "hs", "sdr12", "sdr25";
	pinctrl-0 = <&mmc4_pins_default>;
	pinctrl-1 = <&mmc4_pins_default>;
	pinctrl-2 = <&mmc4_pins_default>;
	pinctrl-3 = <&mmc4_pins_default>;
	#address-cells = <1>;
	#size-cells = <0>;
	wifi@2 {
		compatible = "ti,wl1835";
		reg = <2>;
		interrupt-parent = <&gpio5>;
		interrupts = <7 IRQ_TYPE_EDGE_RISING>;
	};
};

&dcan1 {
	status = "okay";
	pinctrl-names = "default", "sleep", "active";
	pinctrl-0 = <&dcan1_pins_sleep>;
	pinctrl-1 = <&dcan1_pins_sleep>;
	pinctrl-2 = <&dcan1_pins_default>;
};

&qspi {
	status = "okay";

	spi-max-frequency = <76800000>;
	flash@0 {
		compatible = "s25fl256s1";
		spi-max-frequency = <76800000>;
		reg = <0>;
		spi-tx-bus-width = <1>;
		spi-rx-bus-width = <4>;
		#address-cells = <1>;
		#size-cells = <1>;

		/* MTD partition table.
		 * The ROM checks the first four physical blocks
		 * for a valid file to boot and the flash here is
		 * 64KiB block size.
		 */
		partition@0 {
			label = "QSPI.SPL";
			reg = <0x00000000 0x00010000>;
		};
		partition@1 {
			label = "QSPI.SPL.backup1";
			reg = <0x00010000 0x00010000>;
		};
		partition@2 {
			label = "QSPI.SPL.backup2";
			reg = <0x00020000 0x00010000>;
		};
		partition@3 {
			label = "QSPI.SPL.backup3";
			reg = <0x00030000 0x00010000>;
		};
		partition@4 {
			label = "QSPI.u-boot";
			reg = <0x00040000 0x00100000>;
		};
		partition@5 {
			label = "QSPI.u-boot-spl-os";
			reg = <0x00140000 0x00080000>;
		};
		partition@6 {
			label = "QSPI.u-boot-env";
			reg = <0x001c0000 0x00010000>;
		};
		partition@7 {
			label = "QSPI.u-boot-env.backup1";
			reg = <0x001d0000 0x0010000>;
		};
		partition@8 {
			label = "QSPI.kernel";
			reg = <0x001e0000 0x0800000>;
		};
		partition@9 {
			label = "QSPI.file-system";
			reg = <0x009e0000 0x01620000>;
		};
	};
};

&dss {
	status = "okay";
};

&hdmi {
	status = "okay";

	port {
		hdmi_out: endpoint {
			remote-endpoint = <&tpd12s015_in>;
		};
	};
};

&atl {
	assigned-clocks = <&abe_dpll_sys_clk_mux>,
			  <&atl_clkctrl DRA7_ATL_ATL_CLKCTRL 26>,
			  <&dpll_abe_ck>,
			  <&dpll_abe_m2x2_ck>,
			  <&atl_clkin2_ck>;
	assigned-clock-parents = <&sys_clkin2>, <&dpll_abe_m2_ck>;
	assigned-clock-rates = <0>, <0>, <180633600>, <361267200>, <5644800>;

	status = "okay";

	atl2 {
		bws = <DRA7_ATL_WS_MCASP2_FSX>;
		aws = <DRA7_ATL_WS_MCASP3_FSX>;
	};
};

&mcasp3 {
	#sound-dai-cells = <0>;

	assigned-clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP3_CLKCTRL 24>;
	assigned-clock-parents = <&atl_clkin2_ck>;

	status = "okay";

	op-mode = <0>;          /* MCASP_IIS_MODE */
	tdm-slots = <2>;
	/* 4 serializer */
	serial-dir = <  /* 0: INACTIVE, 1: TX, 2: RX */
		1 2 0 0
	>;
	tx-num-evt = <32>;
	rx-num-evt = <32>;
};

&pcie1_rc {
	status = "okay";
};

&csi2_0 {
	csi2_phy0: endpoint {
		remote-endpoint = <&csi2_cam0>;
		clock-lanes = <0>;
		data-lanes = <1 2>;
	};
};
