// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (c) 2013-2014 Linaro Ltd.
 * Copyright (c) 2013-2014 HiSilicon Limited.
 */

/dts-v1/;
#include "hisi-x5hd2.dtsi"

/ {
	model = "Hisilicon HIX5HD2 Development Board";
	compatible = "hisilicon,hix5hd2";

	chosen {
		stdout-path = "serial0:115200n8";
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "hisilicon,hix5hd2-smp";

		cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&l2>;
		};

		cpu@1 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&l2>;
		};
	};

	memory@0 {
		device_type = "memory";
		reg = <0x00000000 0x80000000>;
	};
};

&timer0 {
	status = "okay";
};

&uart0 {
	status = "okay";
};

&gmac0 {
	#address-cells = <1>;
	#size-cells = <0>;
	phy-handle = <&phy2>;
	phy-mode = "mii";
	/* Placeholder, overwritten by bootloader */
	mac-address = [00 00 00 00 00 00];
	status = "okay";

	phy2: ethernet-phy@2 {
		reg = <2>;
	};
};

&gmac1 {
	#address-cells = <1>;
	#size-cells = <0>;
	phy-handle = <&phy1>;
	phy-mode = "rgmii";
	/* Placeholder, overwritten by bootloader */
	mac-address = [00 00 00 00 00 00];
	status = "okay";

	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&ahci {
	phys = <&sata_phy>;
	phy-names = "sata-phy";
};
