// SPDX-License-Identifier: (GPL-2.0+ OR BSD-3-Clause)
/*
 * Copyright (C) Geanix ApS 2023 - All Rights Reserved
 * Author: Sean Nyekjaer <sean@geanix.com>
 */

/dts-v1/;

#include "stm32mp157.dtsi"
#include "stm32mp15xc.dtsi"
#include "stm32mp15xx-osd32.dtsi"
#include "stm32mp15xxac-pinctrl.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pinctrl/stm32-pinfunc.h>

/ {
	model = "Octavo OSD32MP1 RED board";
	compatible = "oct,stm32mp157c-osd32-red", "oct,stm32mp15xx-osd32", "st,stm32mp157";

	aliases {
		serial0 = &uart4;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	led-controller-0 {
		compatible = "gpio-leds";

		led-0 {
			label = "heartbeat";
			gpios = <&gpiod 11 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};
};

&crc1 {
	status = "okay";
};

&dts {
	status = "okay";
};

&ethernet0 {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&ethernet0_rgmii_pins_a>;
	pinctrl-1 = <&ethernet0_rgmii_sleep_pins_a>;
	phy-mode = "rgmii-id";
	max-speed = <1000>;
	phy-handle = <&phy0>;
	st,eth-clk-sel;
	status = "okay";

	mdio {
		compatible = "snps,dwmac-mdio";
		#address-cells = <1>;
		#size-cells = <0>;

		phy0: ethernet-phy@3 {
			reg = <3>;
		};
	};
};

&iwdg2 {
	timeout-sec = <32>;
	status = "okay";
};

&i2c1 {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&i2c1_pins_a>;
	pinctrl-1 = <&i2c1_sleep_pins_a>;
	status = "okay";
	i2c-scl-rising-time-ns = <100>;
	i2c-scl-falling-time-ns = <7>;
	/* spare dmas for other usage */
	/delete-property/dmas;
	/delete-property/dma-names;

	hdmi-transmitter@39 {
		compatible = "sil,sii9022";
		reg = <0x39>;
		reset-gpios = <&gpiog 0 GPIO_ACTIVE_LOW>;
		interrupts = <1 IRQ_TYPE_EDGE_FALLING>;
		interrupt-parent = <&gpiog>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&ltdc_pins_e>;
		pinctrl-1 = <&ltdc_sleep_pins_e>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				sii9022_in: endpoint {
					remote-endpoint = <&ltdc_ep0_out>;
				};
			};

			port@3 {
				reg = <3>;
				sii9022_tx_endpoint: endpoint {
					remote-endpoint = <&i2s2_endpoint>;
				};
			};
		};
	};
};

&i2s2 {
	clocks = <&rcc SPI2>, <&rcc SPI2_K>, <&rcc CK_PER>, <&rcc PLL3_R>;
	clock-names = "pclk", "i2sclk", "x8k", "x11k";
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&i2s2_pins_b>;
	pinctrl-1 = <&i2s2_sleep_pins_b>;
	status = "okay";

	i2s2_port: port {
		i2s2_endpoint: endpoint {
			remote-endpoint = <&sii9022_tx_endpoint>;
			dai-format = "i2s";
			mclk-fs = <256>;
		};
	};
};

&ltdc {
	status = "okay";

	port {
		ltdc_ep0_out: endpoint {
			remote-endpoint = <&sii9022_in>;
		};
	};
};

&m_can1 {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&m_can1_pins_d>;
	pinctrl-1 = <&m_can1_sleep_pins_d>;
	status = "okay";
};

&rtc {
	status = "okay";
};

&sdmmc1 {
	pinctrl-names = "default", "opendrain", "sleep";
	pinctrl-0 = <&sdmmc1_b4_pins_a>;
	pinctrl-1 = <&sdmmc1_b4_od_pins_a>;
	pinctrl-2 = <&sdmmc1_b4_sleep_pins_a>;
	cd-gpios = <&gpioe 7 (GPIO_ACTIVE_LOW | GPIO_PULL_UP)>;
	disable-wp;
	st,neg-edge;
	bus-width = <4>;
	vmmc-supply = <&v3v3>;
	status = "okay";
};

&sdmmc2 {
	pinctrl-names = "default", "opendrain", "sleep";
	pinctrl-0 = <&sdmmc2_b4_pins_a &sdmmc2_d47_pins_d>;
	pinctrl-1 = <&sdmmc2_b4_od_pins_a>;
	pinctrl-2 = <&sdmmc2_b4_sleep_pins_a &sdmmc2_d47_sleep_pins_d>;
	non-removable;
	no-sd;
	no-sdio;
	st,neg-edge;
	bus-width = <8>;
	vmmc-supply = <&v3v3>;
	vqmmc-supply = <&vdd>;
	mmc-ddr-3_3v;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default", "sleep", "idle";
	pinctrl-0 = <&uart4_pins_a>;
	pinctrl-1 = <&uart4_sleep_pins_a>;
	pinctrl-2 = <&uart4_idle_pins_a>;
	/* spare dmas for other usage */
	/delete-property/dmas;
	/delete-property/dma-names;
	status = "okay";
};

&usbh_ehci {
	status = "okay";
};

&usbh_ohci {
	status = "okay";
};

&usbotg_hs {
	vbus-supply = <&vbus_otg>;
};

&usbphyc {
	status = "okay";
};
