// SPDX-License-Identifier: GPL-2.0
/*
 * Hardkernel Odroid XU/XU3 LED device tree source
 *
 * Copyright (c) 2015,2016 Krzysztof Kozlowski
 * Copyright (c) 2014 Collabora Ltd.
 * Copyright (c) 2013 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 */

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/leds/common.h>

/ {
	led-controller-1 {
		compatible = "pwm-leds";

		led-1 {
			label = "green:mmc0";
			function = LED_FUNCTION_DISK_ACTIVITY;
			color = <LED_COLOR_ID_GREEN>;
			pwms = <&pwm 1 2000000 0>;
			pwm-names = "pwm1";
			/*
			 * Green LED is much brighter than the others
			 * so limit its max brightness
			 */
			max-brightness = <127>;
			linux,default-trigger = "mmc0";
		};

		led-2 {
			function = LED_FUNCTION_HEARTBEAT;
			color = <LED_COLOR_ID_BLUE>;
			pwms = <&pwm 2 2000000 0>;
			pwm-names = "pwm2";
			max-brightness = <255>;
			linux,default-trigger = "heartbeat";
		};
	};

	led-controller-2 {
		compatible = "gpio-leds";

		led-3 {
			label = "red:microSD";
			function = LED_FUNCTION_DISK_ACTIVITY;
			color = <LED_COLOR_ID_RED>;
			gpios = <&gpx2 3 GPIO_ACTIVE_HIGH>;
			default-state = "off";
			linux,default-trigger = "mmc1";
		};
	};
};
