/*
 * Copyright 2014 Hans de Goede <hdegoede@redhat.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun7i-a20.dtsi"
#include "sunxi-common-regulators.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	model = "I12 / Q5 / QT840A A20 tvbox";
	compatible = "allwinner,i12-tvbox", "allwinner,sun7i-a20";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "i12_tvbox:red:usr";
			gpios = <&pio 7 9 GPIO_ACTIVE_LOW>;
		};

		led-1 {
			label = "i12_tvbox:blue:usr";
			gpios = <&pio 7 20 GPIO_ACTIVE_HIGH>;
		};
	};

	reg_vmmc3: vmmc3 {
		compatible = "regulator-fixed";
		regulator-name = "vmmc3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		enable-active-high;
		gpio = <&pio 7 2 GPIO_ACTIVE_HIGH>;
	};

	reg_vmmc3_io: vmmc3-io {
		compatible = "regulator-fixed";
		regulator-name = "vmmc3-io";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		/* This controls VCC-PI, must be always on! */
		regulator-always-on;
		enable-active-high;
		gpio = <&pio 7 12 GPIO_ACTIVE_HIGH>;
	};

	reg_gmac_3v3: gmac-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "gmac-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <50000>;
		enable-active-high;
		gpio = <&pio 7 21 GPIO_ACTIVE_HIGH>;
	};
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&gmac {
	pinctrl-names = "default";
	pinctrl-0 = <&gmac_mii_pins>;
	phy-handle = <&phy1>;
	phy-mode = "mii";
	phy-supply = <&reg_gmac_3v3>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	axp209: pmic@34 {
		compatible = "x-powers,axp209";
		reg = <0x34>;
		interrupt-parent = <&nmi_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;

		interrupt-controller;
		#interrupt-cells = <1>;
	};
};

&ir0 {
	pinctrl-names = "default";
	pinctrl-0 = <&ir0_rx_pin>;
	status = "okay";
};

&gmac_mdio {
	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 7 1 GPIO_ACTIVE_LOW>; /* PH1 */
	status = "okay";
};

&mmc3 {
	vmmc-supply = <&reg_vmmc3>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	brcmf: wifi@1 {
		reg = <1>;
		compatible = "brcm,bcm4329-fmac";
		interrupt-parent = <&pio>;
		interrupts = <7 10 IRQ_TYPE_LEVEL_LOW>; /* PH10 / EINT10 */
		interrupt-names = "host-wake";
	};
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&reg_usb1_vbus {
	status = "okay";
};

&reg_usb2_vbus {
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pb_pins>;
	status = "okay";
};

&usbphy {
	usb1_vbus-supply = <&reg_usb1_vbus>;
	usb2_vbus-supply = <&reg_usb2_vbus>;
	status = "okay";
};
