// SPDX-License-Identifier: GPL-2.0
/dts-v1/;
#include "exynos4412-midas.dtsi"

/ {
	compatible = "samsung,n710x", "samsung,midas", "samsung,exynos4412", "samsung,exynos4";
	model = "Samsung Galaxy Note 2 (GT-N7100, GT-N7105) based on Exynos4412";
	chassis-type = "handset";

	memory@40000000 {
		device_type = "memory";
		reg = <0x40000000 0x7fc00000>;
	};

	/* bootargs are passed in by bootloader */

	cam_vdda_reg: voltage-regulator-10 {
		compatible = "regulator-fixed";
		regulator-name = "CAM_SENSOR_CORE_1.2V";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <1200000>;
		gpio = <&gpm4 1 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&buck9_reg {
	maxim,ena-gpios = <&gpm1 0 GPIO_ACTIVE_HIGH>;
};

&cam_af_reg {
	gpio = <&gpm1 1 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&cam_io_reg {
	gpio = <&gpm0 7 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&i2c_3 {
	samsung,i2c-sda-delay = <100>;
	samsung,i2c-slave-addr = <0x10>;
	samsung,i2c-max-bus-freq = <400000>;
	pinctrl-0 = <&i2c3_bus>;
	pinctrl-names = "default";
	status = "okay";

	touchscreen@48 {
		compatible = "melfas,mms152";
		reg = <0x48>;
		interrupt-parent = <&gpm2>;
		interrupts = <3 IRQ_TYPE_EDGE_FALLING>;
		touchscreen-size-x = <720>;
		touchscreen-size-y = <1280>;
		avdd-supply = <&ldo23_reg>;
		vdd-supply = <&ldo24_reg>;
	};
};

&ldo13_reg {
	regulator-name = "VCC_1.8V_LCD";
	regulator-always-on;
};

&ldo25_reg {
	regulator-name = "VCI_3.0V_LCD";
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
};

&s5c73m3 {
	standby-gpios = <&gpm0 6 GPIO_ACTIVE_LOW>;   /* ISP_STANDBY */
	vdda-supply = <&cam_vdda_reg>;
	status = "okay";
};

&sound {
	audio-routing = "HP", "HPOUT1L",
			"HP", "HPOUT1R",

			"SPK", "SPKOUTLN",
			"SPK", "SPKOUTLP",

			"RCV", "HPOUT2N",
			"RCV", "HPOUT2P",

			"HDMI", "LINEOUT1N",
			"HDMI", "LINEOUT1P",

			"LINE", "LINEOUT2N",
			"LINE", "LINEOUT2P",

			"IN1LP", "MICBIAS2",
			"IN1LN", "MICBIAS2",
			"Headset Mic", "MICBIAS2",

			"IN1RP", "Sub Mic",
			"IN1RN", "Sub Mic",

			"IN2LP:VXRN", "Main Mic",
			"IN2LN", "Main Mic",

			"IN2RN", "FM In",
			"IN2RP:VXRP", "FM In";
};

&submic_bias_reg {
	regulator-always-on;
};

&touchkey_reg {
	gpio = <&gpm0 5 GPIO_ACTIVE_HIGH>;
	status = "okay";
};
