// SPDX-License-Identifier: GPL-2.0

/dts-v1/;

/*
 * There are two types of 4.3" LCD, Type 15 and Type 28.
 * By default, type 15 was used.  This device tree file
 * uses the timing for the type 28 LCD
 */

#include "logicpd-torpedo-37xx-devkit.dts"

&lcd0 {
	compatible = "logicpd,type28";
};
