// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2015-2016 Texas Instruments Incorporated - https://www.ti.com/
 */

#include "am57xx-industrial-grade.dtsi"

/ {
	aliases {
		rtc0 = &tps659038_rtc;
		rtc1 = &rtc;
		display0 = &hdmi0;
	};

	chosen {
		stdout-path = &uart3;
	};

	vmain: fixedregulator-vmain {
		compatible = "regulator-fixed";
		regulator-name = "VMAIN";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	v3_3d: fixedregulator-v3_3d {
		compatible = "regulator-fixed";
		regulator-name = "V3_3D";
		vin-supply = <&smps9_reg>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	v1_2d: fixedregulator-v1_2d {
		compatible = "regulator-fixed";
		regulator-name = "V1_2D";
		vin-supply = <&vmain>;
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <1200000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vtt_fixed: fixedregulator-vtt {
		/* TPS51200 */
		compatible = "regulator-fixed";
		regulator-name = "vtt_fixed";
		vin-supply = <&v3_3d>;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	leds-iio {
		status = "disabled";
		compatible = "gpio-leds";
		led-out0 {
			label = "out0";
			gpios = <&tpic2810 0 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out1 {
			label = "out1";
			gpios = <&tpic2810 1 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out2 {
			label = "out2";
			gpios = <&tpic2810 2 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out3 {
			label = "out3";
			gpios = <&tpic2810 3 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out4 {
			label = "out4";
			gpios = <&tpic2810 4 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out5 {
			label = "out5";
			gpios = <&tpic2810 5 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out6 {
			label = "out6";
			gpios = <&tpic2810 6 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led-out7 {
			label = "out7";
			gpios = <&tpic2810 7 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};
	};

	hdmi0: connector@0 {
		compatible = "hdmi-connector";
		label = "hdmi";

		type = "a";

		port {
			hdmi_connector_in: endpoint {
				remote-endpoint = <&tpd12s015_out>;
			};
		};
	};

	tpd12s015: encoder@0 {
		compatible = "ti,tpd12s016", "ti,tpd12s015";

		gpios = <0>, /* optional CT_CP_HPD */
			<0>, /* optional LS_OE */
			<&gpio7 12 GPIO_ACTIVE_HIGH>;	/* HPD */

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				tpd12s015_in: endpoint@0 {
					remote-endpoint = <&hdmi_out>;
				};
			};

			port@1 {
				reg = <1>;

				tpd12s015_out: endpoint@0 {
					remote-endpoint = <&hdmi_connector_in>;
				};
			};
		};
	};

	src_clk_x1: src_clk_x1 {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <20000000>;
	};
};

&dra7_pmx_core {
	dcan1_pins_default: dcan1-default-pins {
		pinctrl-single,pins = <
			DRA7XX_CORE_IOPAD(0x37d0, PIN_OUTPUT_PULLUP | MUX_MODE0)	/* dcan1_tx */
			DRA7XX_CORE_IOPAD(0x37d4, PIN_INPUT_PULLUP | MUX_MODE0)		/* dcan1_rx */
		>;
	};

	dcan1_pins_sleep: dcan1-sleep-pins {
		pinctrl-single,pins = <
			DRA7XX_CORE_IOPAD(0x37d0, MUX_MODE15 | PULL_UP)	/* dcan1_tx.off */
			DRA7XX_CORE_IOPAD(0x37d4, MUX_MODE15 | PULL_UP)	/* dcan1_rx.off */
		>;
	};
};

&i2c1 {
	status = "okay";
	clock-frequency = <400000>;

	tps659038: tps659038@58 {
		compatible = "ti,tps659038";
		reg = <0x58>;
		interrupts-extended = <&gpio6 16 IRQ_TYPE_LEVEL_HIGH
			       &dra7_pmx_core 0x418>;
		#interrupt-cells = <2>;
		interrupt-controller;
		ti,system-power-controller;
		ti,palmas-override-powerhold;

		tps659038_pmic {
			compatible = "ti,tps659038-pmic";

			smps12-in-supply = <&vmain>;
			smps3-in-supply = <&vmain>;
			smps45-in-supply = <&vmain>;
			smps6-in-supply = <&vmain>;
			smps7-in-supply = <&vmain>;
			smps8-in-supply = <&vmain>;
			smps9-in-supply = <&vmain>;
			ldo1-in-supply = <&vmain>;
			ldo2-in-supply = <&vmain>;
			ldo3-in-supply = <&vmain>;
			ldo4-in-supply = <&vmain>;
			ldo9-in-supply = <&vmain>;
			ldoln-in-supply = <&vmain>;
			ldousb-in-supply = <&vmain>;
			ldortc-in-supply = <&vmain>;

			regulators {
				smps12_reg: smps12 {
					/* VDD_MPU */
					regulator-name = "smps12";
					regulator-min-microvolt = <850000>;
					regulator-max-microvolt = <1250000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps3_reg: smps3 {
					/* VDD_DDR EMIF1 EMIF2 */
					regulator-name = "smps3";
					regulator-min-microvolt = <1350000>;
					regulator-max-microvolt = <1350000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps45_reg: smps45 {
					/* VDD_DSPEVE on AM572 */
					/* VDD_IVA + VDD_DSP on AM571 */
					regulator-name = "smps45";
					regulator-min-microvolt = <850000>;
					regulator-max-microvolt = <1250000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps6_reg: smps6 {
					/* VDD_GPU */
					regulator-name = "smps6";
					regulator-min-microvolt = <850000>;
					regulator-max-microvolt = <1250000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps7_reg: smps7 {
					/* VDD_CORE */
					regulator-name = "smps7";
					regulator-min-microvolt = <850000>;
					regulator-max-microvolt = <1150000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps8_reg: smps8 {
					/* 5728 - VDD_IVAHD */
					/* 5718 - N.C. test point */
					regulator-name = "smps8";
				};

				smps9_reg: smps9 {
					/* VDD_3_3D */
					regulator-name = "smps9";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldo1_reg: ldo1 {
					/* VDDSHV8 - VSDMMC  */
					/* NOTE: on rev 1.3a, data supply */
					regulator-name = "ldo1";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <3300000>;
					regulator-boot-on;
					regulator-always-on;
				};

				ldo2_reg: ldo2 {
					/* VDDSH18V */
					regulator-name = "ldo2";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldo3_reg: ldo3 {
					/* R1.3a 572x V1_8PHY_LDO3: USB, SATA */
					regulator-name = "ldo3";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldo4_reg: ldo4 {
					/* R1.3a 572x V1_8PHY_LDO4: PCIE, HDMI*/
					regulator-name = "ldo4";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				/* LDO5-8 unused */

				ldo9_reg: ldo9 {
					/* VDD_RTC  */
					regulator-name = "ldo9";
					regulator-min-microvolt = <840000>;
					regulator-max-microvolt = <1160000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldoln_reg: ldoln {
					/* VDDA_1V8_PLL */
					regulator-name = "ldoln";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldousb_reg: ldousb {
					/* VDDA_3V_USB: VDDA_USBHS33 */
					regulator-name = "ldousb";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldortc_reg: ldortc {
					/* VDDA_RTC  */
					regulator-name = "ldortc";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				regen1: regen1 {
					/* VDD_3V3_ON */
					regulator-name = "regen1";
					regulator-boot-on;
					regulator-always-on;
				};

				regen2: regen2 {
					/* Needed for PMIC internal resource */
					regulator-name = "regen2";
					regulator-boot-on;
					regulator-always-on;
				};
			};
		};

		tps659038_rtc: tps659038_rtc {
			compatible = "ti,palmas-rtc";
			interrupt-parent = <&tps659038>;
			interrupts = <8 IRQ_TYPE_EDGE_FALLING>;
			wakeup-source;
		};

		tps659038_pwr_button: tps659038_pwr_button {
			compatible = "ti,palmas-pwrbutton";
			interrupt-parent = <&tps659038>;
			interrupts = <1 IRQ_TYPE_EDGE_FALLING>;
			wakeup-source;
			ti,palmas-long-press-seconds = <12>;
		};

		tps659038_gpio: tps659038_gpio {
			compatible = "ti,palmas-gpio";
			gpio-controller;
			#gpio-cells = <2>;
		};

		extcon_usb2: tps659038_usb {
			compatible = "ti,palmas-usb-vid";
			ti,enable-vbus-detection;
			ti,enable-id-detection;
			/* ID & VBUS GPIOs provided in board dts */
		};
	};

	tpic2810: tpic2810@60 {
		compatible = "ti,tpic2810";
		reg = <0x60>;
		gpio-controller;
		#gpio-cells = <2>;
	};

	dsi_bridge: tc358778@e {
		compatible = "toshiba,tc358778", "toshiba,tc358768";
		reg = <0xe>;
		status = "disabled";

		clocks = <&src_clk_x1>;
		clock-names = "refclk";

		vddc-supply = <&v1_2d>;
		vddmipi-supply = <&v1_2d>;
		vddio-supply = <&v3_3d>;

		dsi_bridge_ports: ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				rgb_in: endpoint {
					remote-endpoint = <&dpi_out>;
					data-lines = <24>;
				};
			};
		};
	};
};

&mcspi3 {
	status = "okay";
	ti,pindir-d0-out-d1-in;

	sn65hvs882: sn65hvs882@0 {
		compatible = "pisosr-gpio";
		gpio-controller;
		#gpio-cells = <2>;

		reg = <0>;
		spi-max-frequency = <1000000>;
		spi-cpol;
	};
};

&uart3 {
	status = "okay";
	interrupts-extended = <&crossbar_mpu GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH
			       &dra7_pmx_core 0x248>;
};

&rtc {
	status = "okay";
	ext-clk-src;
};

&mac_sw {
	status = "okay";
};

&cpsw_port1 {
	phy-handle = <&ethphy0>;
	phy-mode = "rgmii-rxid";
	ti,dual-emac-pvid = <1>;
};

&cpsw_port2 {
	phy-handle = <&ethphy1>;
	phy-mode = "rgmii-rxid";
	ti,dual-emac-pvid = <2>;
};

&davinci_mdio_sw {
	ethphy0: ethernet-phy@0 {
		reg = <0>;
	};

	ethphy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&usb2_phy1 {
	phy-supply = <&ldousb_reg>;
};

&usb2_phy2 {
	phy-supply = <&ldousb_reg>;
};

&usb1 {
	dr_mode = "host";
};

&omap_dwc3_2 {
	extcon = <&extcon_usb2>;
};

&usb2 {
	extcon = <&extcon_usb2>;
	dr_mode = "otg";
};

&mmc1 {
	status = "okay";
	vmmc-supply = <&v3_3d>;
	vqmmc-supply = <&ldo1_reg>;
	bus-width = <4>;
	cd-gpios = <&gpio6 27 GPIO_ACTIVE_LOW>; /* gpio 219 */
	no-1-8-v;
};

&mmc2 {
	status = "okay";
	vmmc-supply = <&v3_3d>;
	vqmmc-supply = <&v3_3d>;
	bus-width = <8>;
	non-removable;
	max-frequency = <96000000>;
	no-1-8-v;
};

&dcan1 {
	status = "okay";
	pinctrl-names = "default", "sleep", "active";
	pinctrl-0 = <&dcan1_pins_sleep>;
	pinctrl-1 = <&dcan1_pins_sleep>;
	pinctrl-2 = <&dcan1_pins_default>;
};

&qspi {
	status = "okay";

	spi-max-frequency = <76800000>;
	flash@0 {
		compatible = "s25fl256s1", "jedec,spi-nor";
		spi-max-frequency = <76800000>;
		reg = <0>;
		spi-tx-bus-width = <1>;
		spi-rx-bus-width = <4>;
		#address-cells = <1>;
		#size-cells = <1>;

		/* MTD partition table.
		 * The ROM checks the first four physical blocks
		 * for a valid file to boot and the flash here is
		 * 64KiB block size.
		 */
		partition@0 {
			label = "QSPI.SPL";
			reg = <0x00000000 0x00040000>;
		};
		partition@1 {
			label = "QSPI.u-boot";
			reg = <0x00040000 0x00100000>;
		};
		partition@2 {
			label = "QSPI.u-boot-spl-os";
			reg = <0x00140000 0x00080000>;
		};
		partition@3 {
			label = "QSPI.u-boot-env";
			reg = <0x001c0000 0x00010000>;
		};
		partition@4 {
			label = "QSPI.u-boot-env.backup1";
			reg = <0x001d0000 0x0010000>;
		};
		partition@5 {
			label = "QSPI.kernel";
			reg = <0x001e0000 0x0800000>;
		};
		partition@6 {
			label = "QSPI.file-system";
			reg = <0x009e0000 0x01620000>;
		};
	};
};

&cpu0 {
	vdd-supply = <&smps12_reg>;
};

&hdmi {
	status = "okay";

	vdda-supply = <&ldo4_reg>;

	port {
		hdmi_out: endpoint {
			remote-endpoint = <&tpd12s015_in>;
		};
	};
};

&dss {
	status = "okay";

	vdda_video-supply = <&ldoln_reg>;

	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;

			dpi_out: endpoint {
				remote-endpoint = <&rgb_in>;
				data-lines = <24>;
			};
		};
	};
};
