// SPDX-License-Identifier: GPL-2.0-or-later
/*
 * at91sam9n12ek.dts - Device Tree file for AT91SAM9N12-EK board
 *
 *  Copyright (C) 2012 Atmel,
 *                2012 Hong Xu <hong.xu@atmel.com>
 */
/dts-v1/;
#include "at91sam9n12.dtsi"

/ {
	model = "Atmel AT91SAM9N12-EK";
	compatible = "atmel,at91sam9n12ek", "atmel,at91sam9n12", "atmel,at91sam9";

	chosen {
		bootargs = "root=/dev/mtdblock1 rw rootfstype=jffs2";
		stdout-path = "serial0:115200n8";
	};

	memory@20000000 {
		reg = <0x20000000 0x8000000>;
	};

	clocks {
		slow_xtal {
			clock-frequency = <32768>;
		};

		main_xtal {
			clock-frequency = <16000000>;
		};
	};

	ahb {
		apb {
			dbgu: serial@fffff200 {
				status = "okay";
			};

			ssc0: ssc@f0010000 {
				status = "okay";
			};

			tcb0: timer@f8008000 {
				timer@0 {
					compatible = "atmel,tcb-timer";
					reg = <0>;
				};

				timer@1 {
					compatible = "atmel,tcb-timer";
					reg = <1>;
				};
			};

			i2c0: i2c@f8010000 {
				status = "okay";

				wm8904: codec@1a {
					compatible = "wlf,wm8904";
					reg = <0x1a>;
					clocks = <&pmc PMC_TYPE_SYSTEM 8>;
					clock-names = "mclk";
				};

				qt1070: keyboard@1b {
					compatible = "qt1070";
					reg = <0x1b>;
					interrupt-parent = <&pioA>;
					interrupts = <2 IRQ_TYPE_EDGE_FALLING>;
					pinctrl-names = "default";
					pinctrl-0 = <&pinctrl_qt1070_irq>;
				};
			};

			mmc0: mmc@f0008000 {
				pinctrl-0 = <
					&pinctrl_board_mmc0
					&pinctrl_mmc0_slot0_clk_cmd_dat0
					&pinctrl_mmc0_slot0_dat1_3>;
				status = "okay";
				slot@0 {
					reg = <0>;
					bus-width = <4>;
					cd-gpios = <&pioA 7 GPIO_ACTIVE_HIGH>;
				};
			};

			pinctrl@fffff400 {
				mmc0 {
					pinctrl_board_mmc0: mmc0-board {
						atmel,pins =
							<AT91_PIOA 7 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;	/* PA7 gpio CD pin pull up and deglitch */
					};
				};

				qt1070 {
					pinctrl_qt1070_irq: qt1070_irq {
						atmel,pins =
							<AT91_PIOA 2 AT91_PERIPH_GPIO AT91_PINCTRL_PULL_UP_DEGLITCH>;
					};
				};

				sound {
					pinctrl_pck0_as_audio_mck: pck0_as_audio_mck {
						atmel,pins =
							<AT91_PIOB 10 AT91_PERIPH_B AT91_PINCTRL_NONE>;
					};
				};

				usb1 {
					pinctrl_usb1_vbus_sense: usb1_vbus_sense {
						atmel,pins =
							<AT91_PIOB 16 AT91_PERIPH_GPIO AT91_PINCTRL_DEGLITCH>;	/* PB16 gpio usb vbus sense, no pull up and deglitch */
					};
				};
			};

			spi0: spi@f0000000 {
				status = "okay";
				cs-gpios = <&pioA 14 0>, <0>, <0>, <0>;
				flash@0 {
					compatible = "atmel,at25df321a";
					spi-max-frequency = <50000000>;
					reg = <0>;
				};
			};

			hlcdc: hlcdc@f8038000 {
				status = "okay";

				hlcdc-display-controller {
					pinctrl-names = "default";
					pinctrl-0 = <&pinctrl_lcd_base &pinctrl_lcd_rgb888>;

					port@0 {
						hlcdc_panel_output: endpoint@0 {
							reg = <0>;
							remote-endpoint = <&panel_input>;
						};
					};
				};
			};

			usb1: gadget@f803c000 {
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_usb1_vbus_sense>;
				atmel,vbus-gpio = <&pioB 16 GPIO_ACTIVE_HIGH>;
				status = "okay";
			};

			watchdog@fffffe40 {
				status = "okay";
			};

			rtc@fffffeb0 {
				status = "okay";
			};
		};

		ebi: ebi@10000000 {
			status = "okay";

			nand_controller: nand-controller {
				status = "okay";
				pinctrl-0 = <&pinctrl_nand_cs &pinctrl_nand_rb>;
				pinctrl-names = "default";

				nand@3 {
					reg = <0x3 0x0 0x800000>;
					rb-gpios = <&pioD 5 GPIO_ACTIVE_HIGH>;
					cs-gpios = <&pioD 4 GPIO_ACTIVE_HIGH>;
					nand-bus-width = <8>;
					nand-ecc-mode = "soft";
					nand-ecc-strength = <2>;
					nand-ecc-step-size = <512>;
					nand-on-flash-bbt;
					label = "atmel_nand";
				};
			};
		};

		usb0: ohci@500000 {
			num-ports = <1>;
			atmel,vbus-gpio = <&pioB 7 GPIO_ACTIVE_LOW>;
			status = "okay";
		};
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&hlcdc_pwm 0 50000 0>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <6>;
		power-supply = <&bl_reg>;
		status = "okay";
	};

	bl_reg: backlight_regulator {
		compatible = "regulator-fixed";
		regulator-name = "backlight-power-supply";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		status = "okay";
	};

	leds {
		compatible = "gpio-leds";

		led-d8 {
			label = "d8";
			gpios = <&pioB 4 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "mmc0";
		};

		led-d9 {
			label = "d9";
			gpios = <&pioB 5 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "nand-disk";
		};

		led-d10 {
			label = "d10";
			gpios = <&pioB 6 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		button-enter {
			label = "Enter";
			gpios = <&pioB 3 GPIO_ACTIVE_LOW>;
			linux,code = <28>;
			wakeup-source;
		};
	};

	panel: panel {
		compatible = "qiaodian,qd43003c0-40";
		backlight = <&backlight>;
		power-supply = <&panel_reg>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "okay";

		port@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			panel_input: endpoint@0 {
				reg = <0>;
				remote-endpoint = <&hlcdc_panel_output>;
			};
		};
	};

	panel_reg: panel_regulator {
		compatible = "regulator-fixed";
		regulator-name = "panel-power-supply";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		status = "okay";
	};

	sound {
		compatible = "atmel,asoc-wm8904";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_pck0_as_audio_mck>;

		atmel,model = "wm8904 @ AT91SAM9N12";
		atmel,audio-routing =
			"Headphone Jack", "HPOUTL",
			"Headphone Jack", "HPOUTR",
			"IN2L", "Line In Jack",
			"IN2R", "Line In Jack",
			"Mic", "MICBIAS",
			"IN1L", "Mic";

		atmel,ssc-controller = <&ssc0>;
		atmel,audio-codec = <&wm8904>;
	};
};
