// SPDX-License-Identifier: GPL-2.0
/*
 * Google Peach Pi Rev 10+ board device tree source
 *
 * Copyright (c) 2014 Google, Inc
 */

/dts-v1/;
#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/clock/maxim,max77802.h>
#include <dt-bindings/regulator/maxim,max77802.h>
#include <dt-bindings/sound/samsung-i2s.h>
#include "exynos5800.dtsi"
#include "exynos5420-cpus.dtsi"

/ {
	model = "Google Peach Pi Rev 10+";

	compatible = "google,pi-rev16",
		"google,pi-rev15", "google,pi-rev14",
		"google,pi-rev13", "google,pi-rev12",
		"google,pi-rev11", "google,pi-rev10",
		"google,pi", "google,peach", "samsung,exynos5800",
		"samsung,exynos5";
	chassis-type = "laptop";

	aliases {
		/* Assign 20 so we don't get confused w/ builtin ones */
		i2c20 = &i2c_tunnel;
		mmc0 = &mmc_0; /* eMMC */
		mmc1 = &mmc_2; /* SD */
		mmc2 = &mmc_1; /* WiFi */
	};

	backlight: backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm 0 1000000 0>;
		brightness-levels = <0 100 500 1000 1500 2000 2500 2800>;
		default-brightness-level = <7>;
		enable-gpios = <&gpx2 2 GPIO_ACTIVE_HIGH>;
		power-supply = <&tps65090_fet1>;
		pinctrl-0 = <&pwm0_out>;
		pinctrl-names = "default";
	};

	chosen {
		stdout-path = "serial3:115200n8";
	};

	fixed-rate-clocks {
		oscclk {
			compatible = "samsung,exynos5420-oscclk";
			clock-frequency = <24000000>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&power_key_irq &lid_irq>;

		power-key {
			label = "Power";
			gpios = <&gpx1 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			wakeup-source;
		};

		lid-switch {
			label = "Lid";
			gpios = <&gpx3 4 GPIO_ACTIVE_LOW>;
			linux,input-type = <5>; /* EV_SW */
			linux,code = <0>; /* SW_LID */
			debounce-interval = <1>;
			wakeup-source;
		};

	};

	memory@20000000 {
		device_type = "memory";
		reg = <0x20000000 0x80000000>;
	};

	sound {
		compatible = "google,snow-audio-max98091";

		samsung,model = "Peach-Pi-I2S-MAX98091";
		samsung,i2s-controller = <&i2s0>;
		samsung,audio-codec = <&max98091>;

		cpu {
			sound-dai = <&i2s0 0>;
		};

		codec {
			sound-dai = <&max98091>, <&hdmi>;
		};
	};

	usb300_vbus_reg: regulator-usb300 {
		compatible = "regulator-fixed";
		regulator-name = "P5.0V_USB3CON0";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gph0 0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&usb300_vbus_en>;
		enable-active-high;
	};

	usb301_vbus_reg: regulator-usb301 {
		compatible = "regulator-fixed";
		regulator-name = "P5.0V_USB3CON1";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gph0 1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&usb301_vbus_en>;
		enable-active-high;
	};

	vbat: fixed-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vbat-supply";
		regulator-boot-on;
		regulator-always-on;
	};

	panel: panel {
		compatible = "auo,b133htn01";
		power-supply = <&tps65090_fet6>;
		backlight = <&backlight>;

		port {
			panel_in: endpoint {
				remote-endpoint = <&dp_out>;
			};
		};
	};

	mmc1_pwrseq: mmc1-pwrseq {
		compatible = "mmc-pwrseq-simple";
		reset-gpios = <&gpx0 0 GPIO_ACTIVE_LOW>; /* WIFI_EN */
		clocks = <&max77802 MAX77802_CLK_32K_CP>;
		clock-names = "ext_clock";
	};
};

&adc {
	status = "okay";
	vdd-supply = <&ldo9_reg>;
};

&clock_audss {
	assigned-clocks = <&clock_audss EXYNOS_MOUT_AUDSS>;
	assigned-clock-parents = <&clock CLK_MAU_EPLL>;
};

/*
 * Peach Pi board uses SoC revision with lower maximum frequency for A7 cores
 * (1.3 GHz instead of 1.4 GHz) than Odroid XU3/XU4 boards.  Thus we need to
 * update A7 OPPs table accordingly.
 */
&cluster_a7_opp_table {
	/delete-node/opp-1400000000;
};

&cpu0 {
	cpu-supply = <&buck2_reg>;
};

&cpu4 {
	cpu-supply = <&buck6_reg>;
};

&dp {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&dp_hpd_gpio>;
	samsung,color-space = <0>;
	samsung,color-depth = <1>;
	samsung,link-rate = <0x0a>;
	samsung,lane-count = <2>;
	hpd-gpios = <&gpx2 6 GPIO_ACTIVE_HIGH>;

	ports {
		port {
			dp_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};

&fimd {
	status = "okay";
	samsung,invert-vclk;
};

&hdmi {
	status = "okay";
	hpd-gpios = <&gpx3 7 GPIO_ACTIVE_HIGH>;
	pinctrl-names = "default";
	pinctrl-0 = <&hdmi_hpd_irq>;
	ddc = <&i2c_2>;

	hdmi-en-supply = <&tps65090_fet7>;
	vdd-supply = <&ldo8_reg>;
	vdd_osc-supply = <&ldo10_reg>;
	vdd_pll-supply = <&ldo8_reg>;
};

&hsi2c_4 {
	status = "okay";
	clock-frequency = <400000>;

	max77802: pmic@9 {
		compatible = "maxim,max77802";
		interrupt-parent = <&gpx3>;
		interrupts = <1 IRQ_TYPE_NONE>;
		pinctrl-names = "default";
		pinctrl-0 = <&max77802_irq>, <&pmic_selb>,
			    <&pmic_dvs_1>, <&pmic_dvs_2>;
		wakeup-source;
		reg = <0x9>;
		#clock-cells = <1>;

		inb1-supply = <&tps65090_dcdc2>;
		inb2-supply = <&tps65090_dcdc1>;
		inb3-supply = <&tps65090_dcdc2>;
		inb4-supply = <&tps65090_dcdc2>;
		inb5-supply = <&tps65090_dcdc1>;
		inb6-supply = <&tps65090_dcdc2>;
		inb7-supply = <&tps65090_dcdc1>;
		inb8-supply = <&tps65090_dcdc1>;
		inb9-supply = <&tps65090_dcdc1>;
		inb10-supply = <&tps65090_dcdc1>;

		inl1-supply = <&buck5_reg>;
		inl2-supply = <&buck7_reg>;
		inl3-supply = <&buck9_reg>;
		inl4-supply = <&buck9_reg>;
		inl5-supply = <&buck9_reg>;
		inl6-supply = <&tps65090_dcdc2>;
		inl7-supply = <&buck9_reg>;
		inl9-supply = <&tps65090_dcdc2>;
		inl10-supply = <&buck7_reg>;

		regulators {
			buck1_reg: BUCK1 {
				regulator-name = "vdd_mif";
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1300000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-ramp-delay = <12500>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck2_reg: BUCK2 {
				regulator-name = "vdd_arm";
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1500000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-ramp-delay = <12500>;
				regulator-coupled-with = <&buck3_reg>;
				regulator-coupled-max-spread = <300000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck3_reg: BUCK3 {
				regulator-name = "vdd_int";
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1400000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-ramp-delay = <12500>;
				regulator-coupled-with = <&buck2_reg>;
				regulator-coupled-max-spread = <300000>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck4_reg: BUCK4 {
				regulator-name = "vdd_g3d";
				regulator-min-microvolt = <700000>;
				regulator-max-microvolt = <1400000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-ramp-delay = <12500>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck5_reg: BUCK5 {
				regulator-name = "vdd_1v2";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck6_reg: BUCK6 {
				regulator-name = "vdd_kfc";
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1500000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-ramp-delay = <12500>;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck7_reg: BUCK7 {
				regulator-name = "vdd_1v35";
				regulator-min-microvolt = <1350000>;
				regulator-max-microvolt = <1350000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			buck8_reg: BUCK8 {
				regulator-name = "vdd_emmc";
				regulator-min-microvolt = <2850000>;
				regulator-max-microvolt = <2850000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			buck9_reg: BUCK9 {
				regulator-name = "vdd_2v";
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			buck10_reg: BUCK10 {
				regulator-name = "vdd_1v8";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			ldo1_reg: LDO1 {
				regulator-name = "vdd_1v0";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-mode = <MAX77802_OPMODE_LP>;
				};
			};

			ldo2_reg: LDO2 {
				regulator-name = "vdd_1v2_2";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
			};

			ldo3_reg: LDO3 {
				regulator-name = "vdd_1v8_3";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-mode = <MAX77802_OPMODE_LP>;
				};
			};

			vqmmc_sdcard: ldo4_reg: LDO4 {
				regulator-name = "vdd_sd";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo5_reg: LDO5 {
				regulator-name = "vdd_1v8_5";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo6_reg: LDO6 {
				regulator-name = "vdd_1v8_6";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo7_reg: LDO7 {
				regulator-name = "vdd_1v8_7";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo8_reg: LDO8 {
				regulator-name = "vdd_ldo8";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo9_reg: LDO9 {
				regulator-name = "vdd_ldo9";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-mode = <MAX77802_OPMODE_LP>;
				};
			};

			ldo10_reg: LDO10 {
				regulator-name = "vdd_ldo10";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo11_reg: LDO11 {
				regulator-name = "vdd_ldo11";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-mode = <MAX77802_OPMODE_LP>;
				};
			};

			ldo12_reg: LDO12 {
				regulator-name = "vdd_ldo12";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo13_reg: LDO13 {
				regulator-name = "vdd_ldo13";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-mode = <MAX77802_OPMODE_LP>;
				};
			};

			ldo14_reg: LDO14 {
				regulator-name = "vdd_ldo14";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo15_reg: LDO15 {
				regulator-name = "vdd_ldo15";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo17_reg: LDO17 {
				regulator-name = "vdd_g3ds";
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1400000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo18_reg: LDO18 {
				regulator-name = "ldo_18";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo19_reg: LDO19 {
				regulator-name = "ldo_19";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo20_reg: LDO20 {
				regulator-name = "ldo_20";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
			};

			ldo21_reg: LDO21 {
				regulator-name = "ldo_21";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
			};

			ldo23_reg: LDO23 {
				regulator-name = "ldo_23";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
			};
			ldo24_reg: LDO24 {
				regulator-name = "ldo_24";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
			};

			ldo25_reg: LDO25 {
				regulator-name = "ldo_25";
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
			};

			ldo26_reg: LDO26 {
				regulator-name = "ldo_26";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
			};

			ldo27_reg: LDO27 {
				regulator-name = "ldo_27";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
			};

			ldo28_reg: LDO28 {
				regulator-name = "ldo_28";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo29_reg: LDO29 {
				regulator-name = "ldo_29";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo30_reg: LDO30 {
				regulator-name = "vdd_mifs";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			ldo32_reg: LDO32 {
				regulator-name = "ldo_32";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
			};

			ldo33_reg: LDO33 {
				regulator-name = "ldo_33";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
			};

			ldo34_reg: LDO34 {
				regulator-name = "ldo_34";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
			};

			ldo35_reg: LDO35 {
				regulator-name = "ldo_35";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
			};
		};
	};
};

&hsi2c_7 {
	status = "okay";
	clock-frequency = <400000>;

	max98091: codec@10 {
		compatible = "maxim,max98091";
		reg = <0x10>;
		interrupts = <2 IRQ_TYPE_NONE>;
		interrupt-parent = <&gpx0>;
		pinctrl-names = "default";
		pinctrl-0 = <&max98091_irq>;
		clocks = <&pmu_system_controller 0>;
		clock-names = "mclk";
		#sound-dai-cells = <0>;
	};

	light-sensor@44 {
		compatible = "isil,isl29018";
		reg = <0x44>;
		vcc-supply = <&tps65090_fet5>;
	};
};

&hsi2c_8 {
	status = "okay";
	clock-frequency = <333000>;
	/* Atmel mXT540S */
	trackpad@4b {
		compatible = "atmel,maxtouch";
		reg = <0x4b>;
		interrupt-parent = <&gpx1>;
		interrupts = <1 IRQ_TYPE_EDGE_FALLING>;
		wakeup-source;
		pinctrl-names = "default";
		pinctrl-0 = <&trackpad_irq>;
		linux,gpio-keymap = <KEY_RESERVED
				     KEY_RESERVED
				     KEY_RESERVED	/* GPIO 0 */
				     KEY_RESERVED	/* GPIO 1 */
				     BTN_LEFT		/* GPIO 2 */
				     KEY_RESERVED>;	/* GPIO 3 */
	};
};

&hsi2c_9 {
	status = "okay";
	clock-frequency = <400000>;

	tpm@20 {
		compatible = "infineon,slb9645tt";
		reg = <0x20>;

		/* Unused irq; but still need to configure the pins */
		pinctrl-names = "default";
		pinctrl-0 = <&tpm_irq>;
	};
};

&i2c_2 {
	status = "okay";
	samsung,i2c-sda-delay = <100>;
	samsung,i2c-max-bus-freq = <66000>;
	samsung,i2c-slave-addr = <0x50>;
};

&i2s0 {
	assigned-clocks = <&i2s0 CLK_I2S_RCLK_SRC>;
	assigned-clock-parents = <&clock_audss EXYNOS_I2S_BUS>;
	status = "okay";
};

&mixer {
	status = "okay";
};

/* eMMC flash */
&mmc_0 {
	status = "okay";
	mmc-ddr-1_8v;
	mmc-hs200-1_8v;
	mmc-hs400-1_8v;
	cap-mmc-highspeed;
	non-removable;
	clock-frequency = <800000000>;
	samsung,dw-mshc-ciu-div = <3>;
	samsung,dw-mshc-sdr-timing = <0 4>;
	samsung,dw-mshc-ddr-timing = <0 2>;
	samsung,dw-mshc-hs400-timing = <0 2>;
	samsung,read-strobe-delay = <90>;
	pinctrl-names = "default";
	pinctrl-0 = <&sd0_clk &sd0_cmd &sd0_bus1 &sd0_bus4 &sd0_bus8 &sd0_rclk>;
	bus-width = <8>;
};

/* WiFi SDIO module */
&mmc_1 {
	status = "okay";
	non-removable;
	cap-sdio-irq;
	keep-power-in-suspend;
	clock-frequency = <400000000>;
	samsung,dw-mshc-ciu-div = <1>;
	samsung,dw-mshc-sdr-timing = <0 1>;
	samsung,dw-mshc-ddr-timing = <0 2>;
	pinctrl-names = "default";
	pinctrl-0 = <&sd1_clk>, <&sd1_cmd>, <&sd1_int>, <&sd1_bus1>,
		    <&sd1_bus4>, <&sd1_bus8>, <&wifi_en>;
	bus-width = <4>;
	cap-sd-highspeed;
	mmc-pwrseq = <&mmc1_pwrseq>;
	vqmmc-supply = <&buck10_reg>;
};

/* uSD card */
&mmc_2 {
	status = "okay";
	cap-sd-highspeed;
	card-detect-delay = <200>;
	clock-frequency = <400000000>;
	samsung,dw-mshc-ciu-div = <3>;
	samsung,dw-mshc-sdr-timing = <2 3>;
	samsung,dw-mshc-ddr-timing = <1 2>;
	pinctrl-names = "default";
	pinctrl-0 = <&sd2_clk &sd2_cmd &sd2_cd &sd2_bus1 &sd2_bus4>;
	bus-width = <4>;
};


&pinctrl_0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mask_tpm_reset>;

	wifi_en: wifi-en-pins {
		samsung,pins = "gpx0-0";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	max98091_irq: max98091-irq-pins {
		samsung,pins = "gpx0-2";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	/* We need GPX0_6 to be low at sleep time; just keep it low always */
	mask_tpm_reset: mask-tpm-reset-pins {
		samsung,pins = "gpx0-6";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
		samsung,pin-val = <0>;
	};

	tpm_irq: tpm-irq-pins {
		samsung,pins = "gpx1-0";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	trackpad_irq: trackpad-irq-pins {
		samsung,pins = "gpx1-1";
		samsung,pin-function = <EXYNOS_PIN_FUNC_F>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	power_key_irq: power-key-irq-pins {
		samsung,pins = "gpx1-2";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	ec_irq: ec-irq-pins {
		samsung,pins = "gpx1-5";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	tps65090_irq: tps65090-irq-pins {
		samsung,pins = "gpx2-5";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	dp_hpd_gpio: dp-hpd-gpio-pins {
		samsung,pins = "gpx2-6";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_UP>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	max77802_irq: max77802-irq-pins {
		samsung,pins = "gpx3-1";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	lid_irq: lid-irq-pins {
		samsung,pins = "gpx3-4";
		samsung,pin-function = <EXYNOS_PIN_FUNC_F>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	hdmi_hpd_irq: hdmi-hpd-irq-pins {
		samsung,pins = "gpx3-7";
		samsung,pin-function = <EXYNOS_PIN_FUNC_INPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_DOWN>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	pmic_dvs_1: pmic-dvs-1-pins {
		samsung,pins = "gpy7-6";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};
};

/* pinctrl_1 */
/* Adjust WiFi drive strengths lower for EMI */
&sd1_bus1 {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&sd1_bus4 {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&sd1_bus8 {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&sd1_clk {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&sd1_cmd {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&pinctrl_2 {
	pmic_dvs_2: pmic-dvs-2-pins {
		samsung,pins = "gpj4-2", "gpj4-3";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};
};

/* pinctrl_3*/
/* Drive SPI lines at x2 for better integrity */
&spi2_bus {
	samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
};

&pinctrl_3 {
	/* Drive SPI chip select at x2 for better integrity */
	ec_spi_cs: ec-spi-cs-pins {
		samsung,pins = "gpb1-2";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV3>;
	};

	usb300_vbus_en: usb300-vbus-en-pins {
		samsung,pins = "gph0-0";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	usb301_vbus_en: usb301-vbus-en-pins {
		samsung,pins = "gph0-1";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};

	pmic_selb: pmic-selb-pins {
		samsung,pins = "gph0-2", "gph0-3", "gph0-4", "gph0-5",
			       "gph0-6";
		samsung,pin-function = <EXYNOS_PIN_FUNC_OUTPUT>;
		samsung,pin-pud = <EXYNOS_PIN_PULL_NONE>;
		samsung,pin-drv = <EXYNOS5420_PIN_DRV_LV1>;
	};
};

&pmu_system_controller {
	assigned-clocks = <&pmu_system_controller 0>;
	assigned-clock-parents = <&clock CLK_FIN_PLL>;
};

&rtc {
	status = "okay";
	clocks = <&clock CLK_RTC>, <&max77802 MAX77802_CLK_32K_AP>;
	clock-names = "rtc", "rtc_src";
};

&spi_2 {
	status = "okay";
	num-cs = <1>;
	samsung,spi-src-clk = <0>;
	cs-gpios = <&gpb1 2 GPIO_ACTIVE_HIGH>;

	cros_ec: cros-ec@0 {
		compatible = "google,cros-ec-spi";
		interrupt-parent = <&gpx1>;
		interrupts = <5 IRQ_TYPE_NONE>;
		pinctrl-names = "default";
		pinctrl-0 = <&ec_spi_cs &ec_irq>;
		reg = <0>;
		spi-max-frequency = <3125000>;
		google,has-vbc-nvram;
		wakeup-source;

		controller-data {
			samsung,spi-feedback-delay = <1>;
		};

		i2c_tunnel: i2c-tunnel {
			compatible = "google,cros-ec-i2c-tunnel";
			#address-cells = <1>;
			#size-cells = <0>;
			google,remote-bus = <0>;

			battery: sbs-battery@b {
				compatible = "sbs,sbs-battery";
				reg = <0xb>;
				sbs,poll-retry-count = <1>;
				sbs,i2c-retry-count = <2>;
			};

			power-regulator@48 {
				compatible = "ti,tps65090";
				reg = <0x48>;

				/*
				 * Config irq to disable internal pulls
				 * even though we run in polling mode.
				 */
				pinctrl-names = "default";
				pinctrl-0 = <&tps65090_irq>;

				vsys1-supply = <&vbat>;
				vsys2-supply = <&vbat>;
				vsys3-supply = <&vbat>;
				infet1-supply = <&vbat>;
				infet2-supply = <&tps65090_dcdc1>;
				infet3-supply = <&tps65090_dcdc2>;
				infet4-supply = <&tps65090_dcdc2>;
				infet5-supply = <&tps65090_dcdc2>;
				infet6-supply = <&tps65090_dcdc2>;
				infet7-supply = <&tps65090_dcdc1>;
				vsys-l1-supply = <&vbat>;
				vsys-l2-supply = <&vbat>;

				regulators {
					tps65090_dcdc1: dcdc1 {
						ti,enable-ext-control;
					};
					tps65090_dcdc2: dcdc2 {
						ti,enable-ext-control;
					};
					tps65090_dcdc3: dcdc3 {
						ti,enable-ext-control;
					};
					tps65090_fet1: fet1 {
						regulator-name = "vcd_led";
					};
					tps65090_fet2: fet2 {
						regulator-name = "video_mid";
						regulator-always-on;
					};
					tps65090_fet3: fet3 {
						regulator-name = "wwan_r";
						regulator-always-on;
					};
					tps65090_fet4: fet4 {
						regulator-name = "sdcard";
						regulator-always-on;
					};
					tps65090_fet5: fet5 {
						regulator-name = "camout";
						regulator-always-on;
					};
					tps65090_fet6: fet6 {
						regulator-name = "lcd_vdd";
					};
					tps65090_fet7: fet7 {
						regulator-name = "video_mid_1a";
						regulator-always-on;
					};
					tps65090_ldo1: ldo1 {
					};
					tps65090_ldo2: ldo2 {
					};
				};

				charger {
					compatible = "ti,tps65090-charger";
				};
			};
		};
	};
};

&serial_3 {
	status = "okay";
};

&timer {
	arm,cpu-registers-not-fw-configured;
};

&tmu_cpu0 {
	vtmu-supply = <&ldo10_reg>;
};

&tmu_cpu1 {
	vtmu-supply = <&ldo10_reg>;
};

&tmu_cpu2 {
	vtmu-supply = <&ldo10_reg>;
};

&tmu_cpu3 {
	vtmu-supply = <&ldo10_reg>;
};

&tmu_gpu {
	vtmu-supply = <&ldo10_reg>;
};

&usbdrd3_0 {
	vdd10-supply = <&ldo15_reg>;
	vdd33-supply = <&ldo12_reg>;
};

&usbdrd3_1 {
	vdd10-supply = <&ldo15_reg>;
	vdd33-supply = <&ldo12_reg>;
};

&usbdrd_dwc3_0 {
	dr_mode = "host";
};

&usbdrd_dwc3_1 {
	dr_mode = "host";
};

&usbdrd_phy0 {
	vbus-supply = <&usb300_vbus_reg>;
};

&usbdrd_phy1 {
	vbus-supply = <&usb301_vbus_reg>;
};

/*
 * Use longest HW watchdog in SoC (32 seconds) since the hardware
 * watchdog provides no debugging information (compared to soft/hard
 * lockup detectors) and so should be last resort.
 */
&watchdog {
	timeout-sec = <32>;
};

#include "../cros-ec-keyboard.dtsi"
#include "../cros-adc-thermistors.dtsi"
