// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/input/gpio-keys.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/thermal/thermal.h>

#include "tegra30.dtsi"
#include "tegra30-cpu-opp.dtsi"
#include "tegra30-cpu-opp-microvolt.dtsi"
#include "tegra30-asus-lvds-display.dtsi"

/ {
	model = "Pegatron Chagall";
	compatible = "pegatron,chagall", "nvidia,tegra30";
	chassis-type = "tablet";

	aliases {
		mmc0 = &sdmmc4; /* eMMC */
		mmc1 = &sdmmc1; /* uSD slot */
		mmc2 = &sdmmc3; /* WiFi */

		rtc0 = &pmic;
		rtc1 = "/rtc@7000e000";

		display0 = &lcd;
		display1 = &hdmi;

		serial1 = &uartc; /* Bluetooth */
		serial2 = &uartb; /* GPS */
	};

	/*
	 * The decompressor and also some bootloaders rely on a
	 * pre-existing /chosen node to be available to insert the
	 * command line and merge other ATAGS info.
	 */
	chosen {};

	firmware {
		trusted-foundations {
			compatible = "tlm,trusted-foundations";
			tlm,version-major = <2>;
			tlm,version-minor = <8>;
		};
	};

	memory@80000000 {
		reg = <0x80000000 0x40000000>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		linux,cma@80000000 {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x80000000 0x30000000>;
			size = <0x10000000>; /* 256MiB */
			linux,cma-default;
			reusable;
		};

		ramoops@beb00000 {
			compatible = "ramoops";
			reg = <0xbeb00000 0x10000>; /* 64kB */
			console-size = <0x8000>; /* 32kB */
			record-size = <0x400>; /* 1kB */
			ecc-size = <16>;
		};

		trustzone@bfe00000 {
			reg = <0xbfe00000 0x200000>; /* 2MB */
			no-map;
		};
	};

	host1x@50000000 {
		hdmi: hdmi@54280000 {
			status = "okay";

			hdmi-supply = <&hdmi_5v0_sys>;
			pll-supply = <&vdd_1v8_vio>;
			vdd-supply = <&vdd_3v3_sys>;

			nvidia,hpd-gpio = <&gpio TEGRA_GPIO(N, 7) GPIO_ACTIVE_HIGH>;
			nvidia,ddc-i2c-bus = <&hdmi_ddc>;
		};
	};

	vde@6001a000 {
		assigned-clocks = <&tegra_car TEGRA30_CLK_VDE>;
		assigned-clock-parents = <&tegra_car TEGRA30_CLK_PLL_P>;
		assigned-clock-rates = <408000000>;
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			/* SDMMC1 pinmux */
			sdmmc1_clk_pz0 {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc1_dat3_py4 {
				nvidia,pins = "sdmmc1_dat3_py4",
						"sdmmc1_dat2_py5",
						"sdmmc1_dat1_py6",
						"sdmmc1_dat0_py7",
						"sdmmc1_cmd_pz1";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* SDMMC2 pinmux */
			vi_d1_pd5 {
				nvidia,pins = "vi_d1_pd5",
						"vi_d2_pl0",
						"vi_d3_pl1",
						"vi_d5_pl3",
						"vi_d7_pl5";
				nvidia,function = "sdmmc2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			vi_d8_pl6 {
				nvidia,pins = "vi_d8_pl6",
						"vi_d9_pl7";
				nvidia,function = "sdmmc2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
				nvidia,io-reset = <0>;
			};

			/* SDMMC3 pinmux */
			sdmmc3_clk_pa6 {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc3_cmd_pa7 {
				nvidia,pins = "sdmmc3_cmd_pa7",
						"sdmmc3_dat3_pb4",
						"sdmmc3_dat2_pb5",
						"sdmmc3_dat1_pb6",
						"sdmmc3_dat0_pb7",
						"sdmmc3_dat5_pd0",
						"sdmmc3_dat4_pd1",
						"sdmmc3_dat6_pd3",
						"sdmmc3_dat7_pd4";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* SDMMC4 pinmux */
			sdmmc4_clk_pcc4 {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc4_cmd_pt7 {
				nvidia,pins = "sdmmc4_cmd_pt7",
						"sdmmc4_dat0_paa0",
						"sdmmc4_dat1_paa1",
						"sdmmc4_dat2_paa2",
						"sdmmc4_dat3_paa3",
						"sdmmc4_dat4_paa4",
						"sdmmc4_dat5_paa5",
						"sdmmc4_dat6_paa6",
						"sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* I2C pinmux */
			gen1_i2c_scl_pc4 {
				nvidia,pins = "gen1_i2c_scl_pc4",
						"gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			gen2_i2c_scl_pt5 {
				nvidia,pins = "gen2_i2c_scl_pt5",
						"gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			cam_i2c_scl_pbb1 {
				nvidia,pins = "cam_i2c_scl_pbb1",
						"cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			ddc_scl_pv4 {
				nvidia,pins = "ddc_scl_pv4",
						"ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			pwr_i2c_scl_pz6 {
				nvidia,pins = "pwr_i2c_scl_pz6",
						"pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			/* HDMI-CEC pinmux */
			hdmi_cec_pee3 {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
			};

			/* UART-A */
			ulpi_data0_po1 {
				nvidia,pins = "ulpi_data0_po1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			ulpi_data1_po2 {
				nvidia,pins = "ulpi_data1_po2",
						"ulpi_data2_po3",
						"ulpi_data3_po4",
						"ulpi_data4_po5",
						"ulpi_data5_po6",
						"ulpi_data6_po7";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ulpi_data7_po0 {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* UART-B */
			uart2_txd_pc2 {
				nvidia,pins = "uart2_txd_pc2",
						"uart2_rts_n_pj6";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			uart2_rxd_pc3 {
				nvidia,pins = "uart2_rxd_pc3",
						"uart2_cts_n_pj5";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* UART-C */
			uart3_cts_n_pa1 {
				nvidia,pins = "uart3_cts_n_pa1",
						"uart3_rxd_pw7";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uart3_rts_n_pc0 {
				nvidia,pins = "uart3_rts_n_pc0",
						"uart3_txd_pw6";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* UART-D */
			ulpi_clk_py0 {
				nvidia,pins = "ulpi_clk_py0",
						"ulpi_stp_py3";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			ulpi_dir_py1 {
				nvidia,pins = "ulpi_dir_py1",
						"ulpi_nxt_py2";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* I2S pinmux */
			dap1_fs_pn0 {
				nvidia,pins = "dap1_fs_pn0",
						"dap1_din_pn1",
						"dap1_dout_pn2",
						"dap1_sclk_pn3";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap2_fs_pa2 {
				nvidia,pins = "dap2_fs_pa2",
						"dap2_sclk_pa3",
						"dap2_din_pa4",
						"dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap3_fs_pp0 {
				nvidia,pins = "dap3_fs_pp0",
						"dap3_din_pp1",
						"dap3_dout_pp2",
						"dap3_sclk_pp3";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap4_fs_pp4 {
				nvidia,pins = "dap4_fs_pp4",
						"dap4_din_pp5",
						"dap4_dout_pp6",
						"dap4_sclk_pp7";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pcc2 {
				nvidia,pins = "pcc2";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PCI-e pinmux */
			pex_l2_rst_n_pcc6 {
				nvidia,pins = "pex_l2_rst_n_pcc6",
						"pex_l0_rst_n_pdd1",
						"pex_l1_rst_n_pdd5";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pex_l2_clkreq_n_pcc7 {
				nvidia,pins = "pex_l2_clkreq_n_pcc7",
						"pex_l0_prsnt_n_pdd0",
						"pex_l0_clkreq_n_pdd2",
						"pex_l2_prsnt_n_pdd7";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pex_wake_n_pdd3 {
				nvidia,pins = "pex_wake_n_pdd3";
				nvidia,function = "pcie";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* SPI pinmux */
			spi1_mosi_px4 {
				nvidia,pins = "spi1_mosi_px4",
						"spi1_sck_px5",
						"spi1_cs0_n_px6",
						"spi1_miso_px7";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			spi2_cs1_n_pw2 {
				nvidia,pins = "spi2_cs1_n_pw2",
						"spi2_cs2_n_pw3";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			spi2_sck_px2 {
				nvidia,pins = "spi2_sck_px2";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_a16_pj7 {
				nvidia,pins = "gmi_a16_pj7",
						"gmi_a19_pk7";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_a17_pb0 {
				nvidia,pins = "gmi_a17_pb0",
						"gmi_a18_pb1";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spi2_mosi_px0 {
				nvidia,pins = "spi2_mosi_px0";
				nvidia,function = "spi6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spdif_out_pk5 {
				nvidia,pins = "spdif_out_pk5";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spdif_in_pk6 {
				nvidia,pins = "spdif_in_pk6";
				nvidia,function = "spdif";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Display A pinmux */
			lcd_pwr0_pb2 {
				nvidia,pins = "lcd_pwr0_pb2",
						"lcd_pclk_pb3",
						"lcd_pwr1_pc1",
						"lcd_pwr2_pc6",
						"lcd_d0_pe0",
						"lcd_d1_pe1",
						"lcd_d2_pe2",
						"lcd_d3_pe3",
						"lcd_d4_pe4",
						"lcd_d5_pe5",
						"lcd_d6_pe6",
						"lcd_d7_pe7",
						"lcd_d8_pf0",
						"lcd_d9_pf1",
						"lcd_d10_pf2",
						"lcd_d11_pf3",
						"lcd_d12_pf4",
						"lcd_d13_pf5",
						"lcd_d14_pf6",
						"lcd_d15_pf7",
						"lcd_de_pj1",
						"lcd_hsync_pj3",
						"lcd_vsync_pj4",
						"lcd_d16_pm0",
						"lcd_d17_pm1",
						"lcd_d18_pm2",
						"lcd_d19_pm3",
						"lcd_d20_pm4",
						"lcd_d21_pm5",
						"lcd_d22_pm6",
						"lcd_d23_pm7",
						"lcd_cs0_n_pn4",
						"lcd_sdout_pn5",
						"lcd_dc0_pn6",
						"lcd_sdin_pz2",
						"lcd_wr_n_pz3",
						"lcd_sck_pz4",
						"lcd_cs1_n_pw0",
						"lcd_m1_pw1";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			lcd_dc1_pd2 {
				nvidia,pins = "lcd_dc1_pd2";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk_32k_out_pa0 {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,function = "blink";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* KBC keys */
			kb_row0_pr0 {
				nvidia,pins = "kb_row0_pr0",
						"kb_row1_pr1",
						"kb_row2_pr2",
						"kb_row3_pr3",
						"kb_row8_ps0",
						"kb_col0_pq0",
						"kb_col1_pq1",
						"kb_col2_pq2",
						"kb_col3_pq3",
						"kb_col4_pq4",
						"kb_col5_pq5",
						"kb_col7_pq7";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb_row4_pr4 {
				nvidia,pins = "kb_row4_pr4",
						"kb_row7_pr7",
						"kb_row10_ps2",
						"kb_row13_ps5";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb_row11_ps3 {
				nvidia,pins = "kb_row11_ps3",
						"kb_row12_ps4",
						"kb_row15_ps7";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb_row14_ps6 {
				nvidia,pins = "kb_row14_ps6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_iordy_pi5 {
				nvidia,pins = "gmi_iordy_pi5";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			vi_pclk_pt0 {
				nvidia,pins = "vi_pclk_pt0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
				nvidia,io-reset = <0>;
			};

			pu1 {
				nvidia,pins = "pu1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pu2 {
				nvidia,pins = "pu2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pv0 {
				nvidia,pins = "pv0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pv1 {
				nvidia,pins = "pv1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pcc1 {
				nvidia,pins = "pcc1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc4_rst_n_pcc3 {
				nvidia,pins = "sdmmc4_rst_n_pcc3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pv3 {
				nvidia,pins = "pv3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			vi_vsync_pd6 {
				nvidia,pins = "vi_vsync_pd6",
						"vi_hsync_pd7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <0>;
				nvidia,io-reset = <0>;
			};

			vi_d10_pt2 {
				nvidia,pins = "vi_d10_pt2",
						"vi_d0_pt4", "pbb0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			vi_d11_pt3 {
				nvidia,pins = "vi_d11_pt3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pu0 {
				nvidia,pins = "pu0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pu3 {
				nvidia,pins = "pu3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pu6 {
				nvidia,pins = "pu6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pex_l1_prsnt_n_pdd4 {
				nvidia,pins = "pex_l1_prsnt_n_pdd4",
						"pex_l1_clkreq_n_pdd6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_wait_pi7 {
				nvidia,pins = "gmi_wait_pi7",
						"gmi_cs0_n_pj0",
						"gmi_cs1_n_pj2",
						"gmi_cs4_n_pk2";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_ad0_pg0 {
				nvidia,pins = "gmi_ad0_pg0",
						"gmi_ad1_pg1",
						"gmi_ad2_pg2",
						"gmi_ad3_pg3",
						"gmi_ad4_pg4",
						"gmi_ad5_pg5",
						"gmi_ad6_pg6",
						"gmi_ad7_pg7",
						"gmi_wr_n_pi0",
						"gmi_oe_n_pi1",
						"gmi_dqs_pi2",
						"gmi_adv_n_pk0",
						"gmi_clk_pk1";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_cs2_n_pk3 {
				nvidia,pins = "gmi_cs2_n_pk3";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_cs3_n_pk4 {
				nvidia,pins = "gmi_cs3_n_pk4";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_ad10_ph2 {
				nvidia,pins = "gmi_ad10_ph2",
						"gmi_ad11_ph3",
						"gmi_ad14_ph6";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_ad13_ph5 {
				nvidia,pins = "gmi_ad13_ph5",
						"gmi_ad12_ph4",
						"gmi_cs7_n_pi6";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_rst_n_pi4 {
				nvidia,pins = "gmi_rst_n_pi4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_ad8_ph0 {
				nvidia,pins = "gmi_ad8_ph0";
				nvidia,function = "pwm0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_ad9_ph1 {
				nvidia,pins = "gmi_ad9_ph1";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi_wp_n_pc7 {
				nvidia,pins = "gmi_wp_n_pc7";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi_cs6_n_pi3 {
				nvidia,pins = "gmi_cs6_n_pi3";
				nvidia,function = "sata";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			vi_d4_pl2 {
				nvidia,pins = "vi_d4_pl2";
				nvidia,function = "vi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			vi_d6_pl4 {
				nvidia,pins = "vi_d6_pl4";
				nvidia,function = "vi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
				nvidia,lock = <0>;
				nvidia,io-reset = <0>;
			};

			vi_mclk_pt1 {
				nvidia,pins = "vi_mclk_pt1";
				nvidia,function = "vi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* HDMI hot-plug-detect */
			hdmi_int_pn7 {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,function = "hdmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pu4 {
				nvidia,pins = "pu4";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pu5 {
				nvidia,pins = "pu5";
				nvidia,function = "pwm2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			jtag_rtck_pu7 {
				nvidia,pins = "jtag_rtck_pu7";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			crt_hsync_pv6 {
				nvidia,pins = "crt_hsync_pv6",
						"crt_vsync_pv7";
				nvidia,function = "crt";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk1_out_pw4 {
				nvidia,pins = "clk1_out_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			clk2_out_pw5 {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "extperiph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk3_out_pee0 {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			sys_clk_req_pz5 {
				nvidia,pins = "sys_clk_req_pz5";
				nvidia,function = "sysclk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pbb4 {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pbb5 {
				nvidia,pins = "pbb5";
				nvidia,function = "vgp5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pbb6 {
				nvidia,pins = "pbb6";
				nvidia,function = "vgp6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			clk1_req_pee2 {
				nvidia,pins = "clk1_req_pee2";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk2_req_pcc5 {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk3_req_pee1 {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "dev3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			owr {
				nvidia,pins = "owr";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pv2 {
				nvidia,pins = "pv2",
						"kb_row5_pr5";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pbb3 {
				nvidia,pins = "pbb3";
				nvidia,function = "vgp3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pbb7 {
				nvidia,pins = "pbb7";
				nvidia,function = "i2s4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			cam_mclk_pcc0 {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GPIO power/drive control */
			drive_dap1 {
				nvidia,pins = "drive_dap1",
						"drive_dap2",
						"drive_dbg",
						"drive_at5",
						"drive_gme",
						"drive_ddc",
						"drive_ao1",
						"drive_uart3";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};

			drive_sdio1 {
				nvidia,pins = "drive_sdio1";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <5>;
				nvidia,pull-up-strength = <5>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FAST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FAST>;
			};

			drive_sdio3 {
				nvidia,pins = "drive_sdio3";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <46>;
				nvidia,pull-up-strength = <42>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FAST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FAST>;
			};

			drive_gma {
				nvidia,pins = "drive_gma",
						"drive_gmb",
						"drive_gmc",
						"drive_gmd";
				nvidia,pull-down-strength = <9>;
				nvidia,pull-up-strength = <9>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
			};

			drive_lcd2 {
				nvidia,pins = "drive_lcd2";
				nvidia,high-speed-mode = <0>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_4>;
				nvidia,pull-down-strength = <20>;
				nvidia,pull-up-strength = <20>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};
		};
	};

	uartb: serial@70006040 {
		compatible = "nvidia,tegra30-hsuart";
		reset-names = "serial";
		/delete-property/ reg-shift;
		status = "okay";

		/* Broadcom GPS BCM47511 */
	};

	uartc: serial@70006200 {
		compatible = "nvidia,tegra30-hsuart";
		reset-names = "serial";
		/delete-property/ reg-shift;
		status = "okay";

		nvidia,adjust-baud-rates = <0 9600 100>,
					   <9600 115200 200>,
					   <1000000 4000000 136>;

		/* Azurewave AW-AH663 BCM4330B1 */
		bluetooth {
			compatible = "brcm,bcm4330-bt";
			max-speed = <4000000>;

			clocks = <&tegra_pmc TEGRA_PMC_CLK_BLINK>;
			clock-names = "txco";

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(U, 6) IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "host-wakeup";

			device-wakeup-gpios = <&gpio TEGRA_GPIO(U, 1) GPIO_ACTIVE_HIGH>;
			shutdown-gpios = <&gpio TEGRA_GPIO(U, 0) GPIO_ACTIVE_HIGH>;

			vbat-supply  = <&vdd_3v3_sys>;
			vddio-supply = <&vdd_1v8_vio>;
		};
	};

	pwm: pwm@7000a000 {
		status = "okay";
	};

	lcd_ddc: i2c@7000c000 {
		status = "okay";
		clock-frequency = <400000>;

		/* Wolfson Microelectronics WM8903 audio codec */
		wm8903: audio-codec@1a {
			compatible = "wlf,wm8903";
			reg = <0x1a>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(W, 3) IRQ_TYPE_EDGE_BOTH>;

			gpio-controller;
			#gpio-cells = <2>;

			micdet-cfg = <0>;
			micdet-delay = <100>;

			gpio-cfg = <0xffffffff 0xffffffff 0 0xffffffff 0xffffffff>;

			AVDD-supply  = <&vdd_1v8_vio>;
			CPVDD-supply = <&vdd_1v8_vio>;
			DBVDD-supply = <&vdd_1v8_vio>;
			DCVDD-supply = <&vdd_1v8_vio>;
		};
	};

	i2c2: i2c@7000c400 {
		status = "okay";
		clock-frequency = <400000>;

		/* Atmel touchscreen */
		touchscreen@4d {
			compatible = "atmel,maxtouch";
			reg = <0x4d>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(H, 4) IRQ_TYPE_EDGE_FALLING>;
			reset-gpios = <&gpio TEGRA_GPIO(H, 6) GPIO_ACTIVE_LOW>;

			vdda-supply = <&vdd_3v3_sys>;
			vdd-supply  = <&vdd_3v3_sys>;
		};
	};

	i2c3: i2c@7000c500 {
		status = "okay";
		clock-frequency = <400000>;

		/* AsahiKASEI AK8975 magnetometer sensor */
		magnetometer@c {
			compatible = "asahi-kasei,ak8975";
			reg = <0x0c>;

			vdd-supply = <&vdd_3v3_sen>;
			vid-supply = <&vdd_1v8_vio>;

			mount-matrix =   "0",  "1",  "0",
					 "1",  "0",  "0",
					 "0",  "0", "-1";
		};

		light-sensor@44 {
			compatible = "isil,isl29023";
			reg = <0x44>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(Q, 3) IRQ_TYPE_LEVEL_HIGH>;

			vcc-supply = <&vdd_3v3_sen>;
		};

		gyroscope@68 {
			compatible = "invensense,mpu3050";
			reg = <0x68>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(X, 1) IRQ_TYPE_EDGE_RISING>;

			vdd-supply = <&vdd_3v3_sen>;
			vlogic-supply = <&vdd_1v8_vio>;

			mount-matrix =   "0",  "1",  "0",
					 "1",  "0",  "0",
					 "0",  "0", "-1";

			/* External I2C interface */
			i2c-gate {
				#address-cells = <1>;
				#size-cells = <0>;

				accelerometer@f {
					compatible = "kionix,kxtf9";
					reg = <0x0f>;

					interrupt-parent = <&gpio>;
					interrupts = <TEGRA_GPIO(L, 1) IRQ_TYPE_EDGE_RISING>;

					vdd-supply = <&vdd_1v8_vio>;
					vddio-supply = <&vdd_1v8_vio>;

					mount-matrix =  "-1",  "0",  "0",
							 "0",  "1",  "0",
							 "0",  "0",  "1";
				};
			};
		};
	};

	hdmi_ddc: i2c@7000c700 {
		status = "okay";
		clock-frequency = <93750>;
	};

	i2c5: i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		/* Texas Instruments TPS659110 PMIC */
		pmic: pmic@2d {
			compatible = "ti,tps65911";
			reg = <0x2d>;

			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			#interrupt-cells = <2>;
			interrupt-controller;
			wakeup-source;

			ti,en-gpio-sleep = <0 0 1 0 0 0 0 0 0>;
			ti,system-power-controller;
			ti,sleep-keep-ck32k;
			ti,sleep-enable;

			#gpio-cells = <2>;
			gpio-controller;

			vcc1-supply = <&vdd_5v0_sys>;
			vcc2-supply = <&vdd_5v0_sys>;
			vcc3-supply = <&vdd_1v8_vio>;
			vcc4-supply = <&vdd_1v8_vio>;
			vcc5-supply = <&vdd_5v0_sys>;
			vcc6-supply = <&vddio_1v2_ddr>;
			vcc7-supply = <&vdd_5v0_sys>;
			vccio-supply = <&vdd_5v0_sys>;

			pmic-sleep-hog {
				gpio-hog;
				gpios = <0 GPIO_ACTIVE_HIGH>,
					<2 GPIO_ACTIVE_HIGH>,
					<6 GPIO_ACTIVE_HIGH>,
					<8 GPIO_ACTIVE_HIGH>;
				output-high;
			};

			regulators {
				/* VDD1 is not used by Chagall */

				vddio_1v2_ddr: vdd2 {
					regulator-name = "vddio_1v2_ddr";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vdd_cpu: vddctrl {
					regulator-name = "vdd_cpu,vdd_sys";
					regulator-min-microvolt = <600000>;
					regulator-max-microvolt = <1400000>;
					regulator-coupled-with = <&vdd_core>;
					regulator-coupled-max-spread = <300000>;
					regulator-max-step-microvolt = <100000>;
					regulator-always-on;
					regulator-boot-on;
					ti,regulator-ext-sleep-control = <1>;

					nvidia,tegra-cpu-regulator;
				};

				vdd_1v8_vio: vio {
					regulator-name = "vdd_1v8_gen";
					/* FIXME: eMMC won't work, if set to 1.8 V */
					regulator-min-microvolt = <1500000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
					regulator-boot-on;
				};

				/* eMMC VDD */
				vcore_emmc: ldo1 {
					regulator-name = "vdd_emmc_core";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};

				/* uSD slot VDD */
				vdd_usd: ldo2 {
					regulator-name = "vdd_usd";
					regulator-min-microvolt = <3200000>;
					regulator-max-microvolt = <3200000>;
				};

				/* uSD slot VDDIO */
				vddio_usd: ldo3 {
					regulator-name = "vddio_usd";
					regulator-min-microvolt = <1900000>;
					regulator-max-microvolt = <3200000>;
				};

				ldo4 {
					regulator-name = "vdd_rtc";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo5 {
					regulator-name = "vdd_1v3_cam_isp";
					regulator-min-microvolt = <1300000>;
					regulator-max-microvolt = <1300000>;
				};

				ldo6 {
					regulator-name = "avdd_dsi_csi,pwrdet_mipi";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo7 {
					regulator-name = "vdd_pllm,x,u,a_p_c_s";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
					regulator-boot-on;
					ti,regulator-ext-sleep-control = <8>;
				};

				ldo8 {
					regulator-name = "vdd_ddr_hs";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
					ti,regulator-ext-sleep-control = <8>;
				};
			};
		};

		nct72: temperature-sensor@4c {
			compatible = "onnn,nct1008";
			reg = <0x4c>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(U, 5) IRQ_TYPE_EDGE_FALLING>;

			vcc-supply = <&vdd_3v3_sys>;
			#thermal-sensor-cells = <1>;
		};

		vdd_core: core-regulator@60 {
			compatible = "ti,tps62361";
			reg = <0x60>;

			regulator-name = "tps62361-vout";
			regulator-min-microvolt = <500000>;
			regulator-max-microvolt = <1770000>;
			regulator-coupled-with = <&vdd_cpu>;
			regulator-coupled-max-spread = <300000>;
			regulator-max-step-microvolt = <100000>;
			regulator-boot-on;
			regulator-always-on;
			ti,enable-vout-discharge;
			ti,vsel0-state-high;
			ti,vsel1-state-high;

			nvidia,tegra-core-regulator;
		};
	};

	vdd_5v0_sys: regulator-5v {
		compatible = "regulator-fixed";
		regulator-name = "vdd_5v0_sys";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_3v3_sys: regulator-3v {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v3_sys";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_pnl: regulator-panel {
		compatible = "regulator-fixed";
		regulator-name = "vdd_panel";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-enable-ramp-delay = <300000>;
		gpio = <&gpio TEGRA_GPIO(W, 1) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_3v3_sen: regulator-sensors {
		compatible = "regulator-fixed";
		regulator-name = "sen_3v3_en";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio TEGRA_GPIO(K, 5) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_5v0_bl: regulator-bl {
		compatible = "regulator-fixed";
		regulator-name = "vdd_5v0_bl";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(C, 6) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	hdmi_5v0_sys: regulator-hdmi {
		compatible = "regulator-fixed";
		regulator-name = "hdmi_5v0_sys";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(P, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	vdd_vbus_usb1: regulator-usb1 {
		compatible = "regulator-fixed";
		regulator-name = "vdd_vbus_micro_usb";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(DD, 3) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	vdd_vbus_usb3: regulator-usb3 {
		compatible = "regulator-fixed";
		regulator-name = "vdd_vbus_typea_usb";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio TEGRA_GPIO(CC, 6) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	pmc@7000e400 {
		status = "okay";
		nvidia,invert-interrupt;
		nvidia,suspend-mode = <2>;
		nvidia,cpu-pwr-good-time = <2000>;
		nvidia,cpu-pwr-off-time = <200>;
		nvidia,core-pwr-good-time = <3845 3845>;
		nvidia,core-pwr-off-time = <0>;
		nvidia,core-power-req-active-high;
		nvidia,sys-clock-req-active-high;
		core-supply = <&vdd_core>;

		/* Set DEV_OFF + PWR_OFF_SET bit in DCDC control register of TPS65911 PMIC  */
		i2c-thermtrip {
			nvidia,i2c-controller-id = <4>;
			nvidia,bus-addr = <0x2d>;
			nvidia,reg-addr = <0x3f>;
			nvidia,reg-data = <0x81>;
		};
	};

	memory-controller@7000f000 {
		emc-timings-0 {
			/* SAMSUNG K4P8G304EB FGC1 */
			nvidia,ram-code = <0>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emem-configuration = < 0x00020001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x73e30303 0x001f0000 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emem-configuration = < 0x00010001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x72c30303 0x001f0000 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emem-configuration = < 0x00000001 0xc0000018
					0x00000001 0x00000001 0x00000003 0x00000001
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060403 0x72430504 0x001f0000 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emem-configuration = < 0x00000003 0xc0000025
					0x00000001 0x00000001 0x00000006 0x00000003
					0x00000005 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000003 0x00000002
					0x02030001 0x00070506 0x71e40a07 0x001f0000 >;
			};

			timing-400000000 {
				clock-frequency = <400000000>;

				nvidia,emem-configuration = < 0x00000006 0xc0000048
					0x00000002 0x00000003 0x0000000c 0x00000007
					0x00000009 0x00000001 0x00000002 0x00000006
					0x00000001 0x00000000 0x00000004 0x00000004
					0x04040001 0x000d090c 0x7026120d 0x001f0000 >;
			};
		};

		emc-timings-1 {
			/* ELPIDA EDB8132B2MA 8D_F */
			nvidia,ram-code = <1>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emem-configuration = < 0x00020001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x73e30303 0x001f0000 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emem-configuration = < 0x00010001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x72c30303 0x001f0000 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emem-configuration = < 0x00000001 0xc0000018
					0x00000001 0x00000001 0x00000003 0x00000001
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060403 0x72430504 0x001f0000 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emem-configuration = < 0x00000003 0xc0000025
					0x00000001 0x00000001 0x00000006 0x00000003
					0x00000005 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000003 0x00000002
					0x02030001 0x00070506 0x71e40a07 0x001f0000 >;
			};

			timing-400000000 {
				clock-frequency = <400000000>;

				nvidia,emem-configuration = < 0x00000006 0xc0000048
					0x00000002 0x00000003 0x0000000c 0x00000007
					0x00000009 0x00000001 0x00000002 0x00000006
					0x00000001 0x00000000 0x00000004 0x00000004
					0x04040001 0x000d090c 0x7026120d 0x001f0000 >;
			};
		};

		emc-timings-2 {
			/* SAMSUNG K4P8G304EB FGC2 */
			nvidia,ram-code = <2>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emem-configuration = < 0x00020001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x73e30303 0x001f0000 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emem-configuration = < 0x00010001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x72c30303 0x001f0000 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emem-configuration = < 0x00000001 0xc0000018
					0x00000001 0x00000001 0x00000003 0x00000001
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060403 0x72430504 0x001f0000 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emem-configuration = < 0x00000003 0xc0000025
					0x00000001 0x00000001 0x00000006 0x00000003
					0x00000005 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000003 0x00000002
					0x02030001 0x00070506 0x71e40a07 0x001f0000 >;
			};

			timing-533000000 {
				clock-frequency = <533000000>;

				nvidia,emem-configuration = < 0x00000008 0xc0000060
					0x00000003 0x00000004 0x00000010 0x0000000a
					0x0000000d 0x00000002 0x00000002 0x00000008
					0x00000002 0x00000000 0x00000004 0x00000005
					0x05040002 0x00110b10 0x70281811 0x001f0000 >;
			};
		};

		emc-timings-3 {
			/* HYNIX H9TCNNN8JDMMPR NGM */
			nvidia,ram-code = <3>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emem-configuration = < 0x00020001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x73e30303 0x001f0000 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emem-configuration = < 0x00010001 0xc0000010
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060402 0x72c30303 0x001f0000 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emem-configuration = < 0x00000001 0xc0000018
					0x00000001 0x00000001 0x00000003 0x00000001
					0x00000003 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000002 0x00000002
					0x02020001 0x00060403 0x72430504 0x001f0000 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emem-configuration = < 0x00000003 0xc0000025
					0x00000001 0x00000001 0x00000006 0x00000003
					0x00000005 0x00000001 0x00000002 0x00000004
					0x00000001 0x00000000 0x00000003 0x00000002
					0x02030001 0x00070506 0x71e40a07 0x001f0000 >;
			};

			timing-533000000 {
				clock-frequency = <533000000>;

				nvidia,emem-configuration = < 0x00000008 0xc0000060
					0x00000003 0x00000004 0x00000010 0x0000000a
					0x0000000d 0x00000002 0x00000002 0x00000008
					0x00000002 0x00000000 0x00000004 0x00000005
					0x05040002 0x00110b10 0x70281811 0x001f0000 >;
			};
		};
	};

	memory-controller@7000f400 {
		emc-timings-0 {
			/* SAMSUNG K4P8G304EB FGC1 */
			nvidia,ram-code = <0>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000001
					0x00000003 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x00000009 0x00000060 0x00000000 0x00000018
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000004 0x00000004
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x0000006b 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000000a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x800001c5 0xe0000000 0xff00ff00 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000003
					0x00000006 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x00000009 0x000000c0 0x00000000 0x00000030
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000008 0x00000008
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000000d5 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000013 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000287 0xe0000000 0xff00ff00 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x0000000a>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000006
					0x0000000d 0x00000004 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x00000009 0x00000181 0x00000000 0x00000060
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x0000000f 0x0000000f
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000001a9 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000025 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x8000040b 0xe0000000 0xff00ff00 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010042>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000013>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000000c
					0x0000001a 0x00000008 0x00000003 0x00000005
					0x00000004 0x00000001 0x00000006 0x00000003
					0x00000003 0x00000002 0x00000002 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000c
					0x0000000a 0x00000303 0x00000000 0x000000c0
					0x00000001 0x00000001 0x00000003 0x00000000
					0x00000001 0x00000007 0x0000001d 0x0000001d
					0x00000004 0x0000000b 0x00000005 0x00000004
					0x00000002 0x00000351 0x00000004 0x00000006
					0x00000000 0x00000000 0x00004282 0x004400a4
					0x00008000 0x00080000 0x00080000 0x00080000
					0x00080000 0x00080000 0x00080000 0x00080000
					0x00080000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00080000 0x00080000 0x00080000
					0x00080000 0x000e0220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000004a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000713 0xe0000000 0xff00ff00 >;
			};

			timing-400000000 {
				clock-frequency = <400000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010082>;
				nvidia,emc-mode-2 = <0x00020004>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000024>;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000017
					0x00000033 0x00000010 0x00000007 0x00000007
					0x00000007 0x00000002 0x0000000a 0x00000007
					0x00000007 0x00000003 0x00000002 0x00000000
					0x00000003 0x00000007 0x00000004 0x0000000d
					0x0000000e 0x000005e9 0x00000000 0x0000017a
					0x00000002 0x00000002 0x00000007 0x00000000
					0x00000001 0x0000000c 0x00000038 0x00000038
					0x00000006 0x00000014 0x00000009 0x00000004
					0x00000002 0x00000680 0x00000000 0x00000006
					0x00000000 0x00000000 0x00006282 0x001d0084
					0x00008000 0x00034000 0x00034000 0x00034000
					0x00034000 0x00034000 0x00034000 0x00034000
					0x00034000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00038000 0x00038000 0x00038000
					0x00038000 0x00080220 0x0800003d 0x00000000
					0x77ffc004 0x01f1f408 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000090 0x000c000c 0xa0f10404 0x00000000
					0x00000000 0x80000ce6 0xe0000000 0xff00ff88 >;
			};
		};

		emc-timings-1 {
			/* ELPIDA EDB8132B2MA 8D_F */
			nvidia,ram-code = <1>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000001
					0x00000003 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x00000060 0x00000000 0x00000018
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000004 0x00000004
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x0000006b 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000000a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x800001c5 0xe0000000 0xff00ff00 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000003
					0x00000006 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x000000c0 0x00000000 0x00000030
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000008 0x00000008
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000000d5 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000013 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000287 0xe0000000 0xff00ff00 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x0000000a>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000006
					0x0000000d 0x00000004 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x00000181 0x00000000 0x00000060
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x0000000f 0x0000000f
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000001a9 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000025 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x8000040b 0xe0000000 0xff00ff00 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010042>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000013>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000000c
					0x0000001a 0x00000008 0x00000003 0x00000005
					0x00000004 0x00000001 0x00000006 0x00000003
					0x00000003 0x00000002 0x00000002 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000c
					0x0000000a 0x00000303 0x00000000 0x000000c0
					0x00000001 0x00000001 0x00000003 0x00000000
					0x00000001 0x00000007 0x0000001d 0x0000001d
					0x00000004 0x0000000b 0x00000005 0x00000004
					0x00000002 0x00000351 0x00000004 0x00000006
					0x00000000 0x00000000 0x00004282 0x004400a4
					0x00008000 0x00070000 0x00070000 0x00070000
					0x00070000 0x00070000 0x00070000 0x00070000
					0x00070000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00080000 0x00080000 0x00080000
					0x00080000 0x000e0220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000004a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000713 0xe0000000 0xff00ff00 >;
			};

			timing-400000000 {
				clock-frequency = <400000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010082>;
				nvidia,emc-mode-2 = <0x00020004>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000024>;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000017
					0x00000033 0x00000010 0x00000007 0x00000007
					0x00000007 0x00000002 0x0000000a 0x00000007
					0x00000007 0x00000003 0x00000002 0x00000000
					0x00000003 0x00000007 0x00000004 0x0000000d
					0x0000000e 0x000005e9 0x00000000 0x0000017a
					0x00000002 0x00000002 0x00000007 0x00000000
					0x00000001 0x0000000c 0x00000038 0x00000038
					0x00000006 0x00000014 0x00000009 0x00000004
					0x00000002 0x00000680 0x00000000 0x00000004
					0x00000000 0x00000000 0x00006282 0x001d0084
					0x00008000 0x00034000 0x00034000 0x00034000
					0x00034000 0x00034000 0x00034000 0x00034000
					0x00034000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00048000 0x00048000 0x00048000
					0x00048000 0x00060220 0x0800003d 0x00000000
					0x77ffc004 0x01f1f408 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000090 0x000c000c 0xa0f10000 0x00000000
					0x00000000 0x80000ce6 0xe0000000 0xff00ff88 >;
			};
		};

		emc-timings-2 {
			/* SAMSUNG K4P8G304EB FGC2 */
			nvidia,ram-code = <2>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000001
					0x00000003 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x00000060 0x00000000 0x00000018
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000004 0x00000004
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x0000006b 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000000a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x800001c5 0xe0000000 0xff00ff00 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000003
					0x00000006 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x000000c0 0x00000000 0x00000030
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000008 0x00000008
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000000d5 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000013 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000287 0xe0000000 0xff00ff00 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x0000000a>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000006
					0x0000000d 0x00000004 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x00000009 0x00000181 0x00000000 0x00000060
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x0000000f 0x0000000f
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000001a9 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000025 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x8000040b 0xe0000000 0xff00ff00 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010042>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000013>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000000c
					0x0000001a 0x00000008 0x00000003 0x00000005
					0x00000004 0x00000001 0x00000006 0x00000003
					0x00000003 0x00000002 0x00000002 0x00000000
					0x00000001 0x00000004 0x00000001 0x0000000c
					0x0000000a 0x00000303 0x00000000 0x000000c0
					0x00000001 0x00000001 0x00000003 0x00000000
					0x00000001 0x00000007 0x0000001d 0x0000001d
					0x00000004 0x0000000b 0x00000005 0x00000004
					0x00000002 0x00000351 0x00000005 0x00000004
					0x00000000 0x00000000 0x00004282 0x004400a4
					0x00008000 0x00080000 0x00080000 0x00080000
					0x00080000 0x00080000 0x00080000 0x00080000
					0x00080000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00080000 0x00080000 0x00080000
					0x00080000 0x000e0220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000004a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000713 0xe0000000 0xff00ff00 >;
			};

			timing-533000000 {
				clock-frequency = <533000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x000100c2>;
				nvidia,emc-mode-2 = <0x00020006>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000030>;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000001f
					0x00000045 0x00000016 0x00000009 0x00000008
					0x00000009 0x00000003 0x0000000d 0x00000009
					0x00000009 0x00000005 0x00000003 0x00000000
					0x00000004 0x0000000a 0x00000006 0x0000000d
					0x00000010 0x000007df 0x00000000 0x000001f7
					0x00000003 0x00000003 0x00000009 0x00000000
					0x00000001 0x0000000f 0x0000004b 0x0000004b
					0x00000008 0x0000001b 0x0000000c 0x00000004
					0x00000002 0x000008aa 0x00000000 0x00000004
					0x00000000 0x00000000 0x00006282 0xf0120091
					0x00008000 0x007f8008 0x007f8008 0x007f8008
					0x007f8008 0x007f8008 0x007f8008 0x007f8008
					0x007f8008 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x0000000c 0x0000000c 0x0000000c
					0x0000000c 0x00080220 0x0200003d 0x00000000
					0x77ffc004 0x01f1f408 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x000000c0 0x000e000e 0xa0f10000 0x00000000
					0x00000000 0x800010d9 0xf0000000 0xff00ff88 >;
			};
		};

		emc-timings-3 {
			/* HYNIX H9TCNNN8JDMMPR NGM */
			nvidia,ram-code = <3>;

			timing-25500000 {
				clock-frequency = <25500000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000001
					0x00000003 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x00000060 0x00000000 0x00000018
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000004 0x00000004
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x0000006b 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000000a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x800001c5 0xe0000000 0xff00ff00 >;
			};

			timing-51000000 {
				clock-frequency = <51000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000009>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000003
					0x00000006 0x00000002 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x000000c0 0x00000000 0x00000030
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x00000008 0x00000008
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000000d5 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000013 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000287 0xe0000000 0xff00ff00 >;
			};

			timing-102000000 {
				clock-frequency = <102000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010022>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x0000000a>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x00000006
					0x0000000d 0x00000004 0x00000002 0x00000004
					0x00000004 0x00000001 0x00000005 0x00000002
					0x00000002 0x00000001 0x00000001 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000b
					0x0000000a 0x00000181 0x00000000 0x00000060
					0x00000001 0x00000001 0x00000002 0x00000000
					0x00000001 0x00000007 0x0000000f 0x0000000f
					0x00000003 0x00000008 0x00000004 0x00000004
					0x00000002 0x000001a9 0x00000004 0x00000004
					0x00000000 0x00000000 0x00004282 0x007800a4
					0x00008000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x000fc000 0x000fc000 0x000fc000
					0x000fc000 0x00100220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x00000025 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x8000040b 0xe0000000 0xff00ff00 >;
			};

			timing-204000000 {
				clock-frequency = <204000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x00010042>;
				nvidia,emc-mode-2 = <0x00020001>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000013>;
				nvidia,emc-cfg-dyn-self-ref;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000000c
					0x0000001a 0x00000008 0x00000003 0x00000005
					0x00000004 0x00000001 0x00000006 0x00000003
					0x00000003 0x00000002 0x00000002 0x00000000
					0x00000001 0x00000003 0x00000001 0x0000000c
					0x0000000b 0x00000303 0x00000000 0x000000c0
					0x00000001 0x00000001 0x00000003 0x00000000
					0x00000001 0x00000007 0x0000001d 0x0000001d
					0x00000004 0x0000000b 0x00000005 0x00000004
					0x00000002 0x00000351 0x00000004 0x00000006
					0x00000000 0x00000000 0x00004282 0x004400a4
					0x00008000 0x00072000 0x00072000 0x00072000
					0x00072000 0x00072000 0x00072000 0x00072000
					0x00072000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00080000 0x00080000 0x00080000
					0x00080000 0x000e0220 0x0800201c 0x00000000
					0x77ffc004 0x01f1f008 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x0000004a 0x00090009 0xa0f10000 0x00000000
					0x00000000 0x80000713 0xd0000000 0xff00ff00 >;
			};

			timing-533000000 {
				clock-frequency = <533000000>;

				nvidia,emc-auto-cal-interval = <0x001fffff>;
				nvidia,emc-mode-1 = <0x000100c2>;
				nvidia,emc-mode-2 = <0x00020006>;
				nvidia,emc-mode-reset = <0x00000000>;
				nvidia,emc-zcal-cnt-long = <0x00000030>;
				nvidia,emc-cfg-periodic-qrst;

				nvidia,emc-configuration =  < 0x0000001f
					0x00000045 0x00000016 0x00000009 0x00000008
					0x00000009 0x00000003 0x0000000d 0x00000009
					0x00000009 0x00000005 0x00000003 0x00000000
					0x00000004 0x00000009 0x00000006 0x0000000d
					0x00000010 0x000007df 0x00000000 0x000001f7
					0x00000003 0x00000003 0x00000009 0x00000000
					0x00000001 0x0000000f 0x0000004b 0x0000004b
					0x00000008 0x0000001b 0x0000000c 0x00000004
					0x00000002 0x000008aa 0x00000000 0x00000006
					0x00000000 0x00000000 0x00006282 0xf0120091
					0x00008000 0x0000000a 0x0000000a 0x0000000a
					0x0000000a 0x0000000a 0x0000000a 0x0000000a
					0x0000000a 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x00000000 0x00000000 0x00000000
					0x00000000 0x0000000c 0x0000000c 0x0000000c
					0x0000000c 0x000a0220 0x0800003d 0x00000000
					0x77ffc004 0x01f1f408 0x00000000 0x00000007
					0x08000068 0x08000000 0x00000802 0x00064000
					0x000000c0 0x000e000e 0xa0f10000 0x00000000
					0x00000000 0x800010d9 0xe0000000 0xff00ff88 >;
			};
		};
	};

	hda@70030000 {
		status = "okay";
	};

	ahub@70080000 {
		i2s@70080400 { /* i2s1 */
			status = "okay";
		};

		/* BT SCO */
		i2s@70080600 { /* i2s3 */
			status = "okay";
		};
	};

	sdmmc1: mmc@78000000 {
		status = "okay";

		cd-gpios = <&gpio TEGRA_GPIO(I, 5) GPIO_ACTIVE_LOW>;
		bus-width = <4>;

		vmmc-supply = <&vdd_usd>; /* ldo2 */
		vqmmc-supply = <&vddio_usd>; /* ldo3 */
	};

	sdmmc3: mmc@78000400 {
		status = "okay";

		#address-cells = <1>;
		#size-cells = <0>;

		assigned-clocks = <&tegra_car TEGRA30_CLK_SDMMC3>;
		assigned-clock-parents = <&tegra_car TEGRA30_CLK_PLL_C>;
		assigned-clock-rates = <50000000>;

		max-frequency = <50000000>;
		keep-power-in-suspend;
		bus-width = <4>;
		non-removable;

		mmc-pwrseq = <&brcm_wifi_pwrseq>;
		vmmc-supply = <&vdd_3v3_sys>;
		vqmmc-supply = <&vdd_1v8_vio>;

		/* Azurewave AW-AH663 BCM4330B1 */
		wifi@1 {
			compatible = "brcm,bcm4329-fmac";
			reg = <1>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(O, 4) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "host-wake";
		};
	};

	sdmmc4: mmc@78000600 {
		status = "okay";
		bus-width = <8>;
		vmmc-supply = <&vcore_emmc>;
		vqmmc-supply = <&vdd_1v8_vio>;
		non-removable;
	};

	usb@7d000000 {
		compatible = "nvidia,tegra30-udc";
		status = "okay";
		dr_mode = "otg";
		vbus-supply = <&vdd_vbus_usb1>;
	};

	usb-phy@7d000000 {
		status = "okay";
		dr_mode = "otg";
		nvidia,hssync-start-delay = <0>;
		nvidia,xcvr-lsfslew = <2>;
		nvidia,xcvr-lsrslew = <2>;
	};

	usb@7d008000 {
		status = "okay";
	};

	usb-phy@7d008000 {
		status = "okay";
		vbus-supply = <&vdd_vbus_usb3>;
	};

	mains: ac-adapter-detect {
		compatible = "gpio-charger";
		charger-type = "mains";
		gpios = <&gpio TEGRA_GPIO(V, 1) GPIO_ACTIVE_HIGH>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";

		enable-gpios = <&gpio TEGRA_GPIO(H, 2) GPIO_ACTIVE_HIGH>;
		power-supply = <&vdd_5v0_bl>;
		pwms = <&pwm 0 5000000>;

		brightness-levels = <1 255>;
		num-interpolated-steps = <254>;
		default-brightness-level = <15>;
	};

	/* PMIC has a built-in 32KHz oscillator which is used by PMC */
	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "pmic-oscillator";
	};

	cpus {
		cpu0: cpu@0 {
			cpu-supply = <&vdd_cpu>;
			operating-points-v2 = <&cpu0_opp_table>;
			#cooling-cells = <2>;
		};
		cpu1: cpu@1 {
			cpu-supply = <&vdd_cpu>;
			operating-points-v2 = <&cpu0_opp_table>;
			#cooling-cells = <2>;
		};
		cpu2: cpu@2 {
			cpu-supply = <&vdd_cpu>;
			operating-points-v2 = <&cpu0_opp_table>;
			#cooling-cells = <2>;
		};
		cpu3: cpu@3 {
			cpu-supply = <&vdd_cpu>;
			operating-points-v2 = <&cpu0_opp_table>;
			#cooling-cells = <2>;
		};
	};

	display-panel {
		compatible = "hannstar,hsd101pww2", "panel-lvds";

		width-mm = <217>;
		height-mm = <136>;

		data-mapping = "jeida-24";

		panel-timing {
			/* 1280x800@60Hz */
			clock-frequency = <68000000>;
			hactive = <1280>;
			vactive = <800>;
			hfront-porch = <48>;
			hback-porch = <18>;
			hsync-len = <30>;
			vsync-len = <5>;
			vfront-porch = <3>;
			vback-porch = <12>;
		};
	};

	extcon-keys {
		compatible = "gpio-keys";

		switch-dock-insert {
			label = "Chagall Dock";
			gpios = <&gpio TEGRA_GPIO(S, 4) GPIO_ACTIVE_LOW>;
			linux,input-type = <EV_SW>;
			linux,code = <SW_DOCK>;
			debounce-interval = <10>;
			wakeup-event-action = <EV_ACT_ASSERTED>;
			wakeup-source;
		};

		switch-lineout-detect {
			label = "Audio dock line-out detect";
			gpios = <&gpio TEGRA_GPIO(S, 3) GPIO_ACTIVE_LOW>;
			linux,input-type = <EV_SW>;
			linux,code = <SW_LINEOUT_INSERT>;
			debounce-interval = <10>;
			wakeup-event-action = <EV_ACT_ASSERTED>;
			wakeup-source;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(V, 0) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			debounce-interval = <10>;
			wakeup-event-action = <EV_ACT_ASSERTED>;
			wakeup-source;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio TEGRA_GPIO(Q, 1) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEDOWN>;
			debounce-interval = <10>;
			wakeup-event-action = <EV_ACT_ASSERTED>;
			wakeup-source;
		};

		key-volume-up {
			label = "Volume Up";
			gpios = <&gpio TEGRA_GPIO(Q, 0) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEUP>;
			debounce-interval = <10>;
			wakeup-event-action = <EV_ACT_ASSERTED>;
			wakeup-source;
		};
	};

	haptic-feedback {
		compatible = "gpio-vibrator";
		enable-gpios = <&gpio TEGRA_GPIO(U, 4) GPIO_ACTIVE_HIGH>;
		vcc-supply = <&vdd_3v3_sys>;
	};

	opp-table-actmon {
		/delete-node/ opp-625000000;
		/delete-node/ opp-667000000;
		/delete-node/ opp-750000000;
		/delete-node/ opp-800000000;
		/delete-node/ opp-900000000;
	};

	opp-table-emc {
		/delete-node/ opp-625000000-1200;
		/delete-node/ opp-625000000-1250;
		/delete-node/ opp-667000000-1200;
		/delete-node/ opp-750000000-1300;
		/delete-node/ opp-800000000-1300;
		/delete-node/ opp-900000000-1350;
	};

	brcm_wifi_pwrseq: pwrseq-wifi {
		compatible = "mmc-pwrseq-simple";

		clocks = <&tegra_pmc TEGRA_PMC_CLK_BLINK>;
		clock-names = "ext_clock";

		reset-gpios = <&gpio TEGRA_GPIO(D, 3) GPIO_ACTIVE_LOW>;
		post-power-on-delay-ms = <300>;
		power-off-delay-us = <300>;
	};

	sound {
		compatible = "pegatron,tegra-audio-wm8903-chagall",
			     "nvidia,tegra-audio-wm8903";
		nvidia,model = "Pegatron Chagall WM8903";

		nvidia,audio-routing =
			"Headphone Jack", "HPOUTR",
			"Headphone Jack", "HPOUTL",
			"Int Spk", "ROP",
			"Int Spk", "RON",
			"Int Spk", "LOP",
			"Int Spk", "LON",
			"IN1R", "Mic Jack",
			"DMICDAT", "Int Mic";

		nvidia,i2s-controller = <&tegra_i2s1>;
		nvidia,audio-codec = <&wm8903>;

		nvidia,spkr-en-gpios = <&wm8903 2 GPIO_ACTIVE_HIGH>;
		nvidia,hp-det-gpios = <&gpio TEGRA_GPIO(W, 2) GPIO_ACTIVE_LOW>;
		nvidia,headset;

		clocks = <&tegra_car TEGRA30_CLK_PLL_A>,
			 <&tegra_car TEGRA30_CLK_PLL_A_OUT0>,
			 <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;
		clock-names = "pll_a", "pll_a_out0", "mclk";

		assigned-clocks = <&tegra_car TEGRA30_CLK_EXTERN1>,
				  <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;

		assigned-clock-parents = <&tegra_car TEGRA30_CLK_PLL_A_OUT0>,
					 <&tegra_car TEGRA30_CLK_EXTERN1>;
	};

	thermal-zones {
		/*
		 * NCT72 has two sensors:
		 *
		 *	0: internal that monitors ambient/skin temperature
		 *	1: external that is connected to the CPU's diode
		 *
		 * Ideally we should use userspace thermal governor,
		 * but it's a much more complex solution.  The "skin"
		 * zone exists as a simpler solution which prevents
		 * Chagall from getting too hot from a user's tactile
		 * perspective. The CPU zone is intended to protect
		 * silicon from damage.
		 */

		skin-thermal {
			polling-delay-passive = <1000>; /* milliseconds */
			polling-delay = <5000>; /* milliseconds */

			thermal-sensors = <&nct72 0>;

			trips {
				trip0: skin-alert {
					/* throttle at 57C until temperature drops to 56.8C */
					temperature = <57000>;
					hysteresis = <200>;
					type = "passive";
				};

				trip1: skin-crit {
					/* shut down at 65C */
					temperature = <65000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&trip0>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&actmon THERMAL_NO_LIMIT
								  THERMAL_NO_LIMIT>;
				};
			};
		};

		cpu-thermal {
			polling-delay-passive = <1000>; /* milliseconds */
			polling-delay = <5000>; /* milliseconds */

			thermal-sensors = <&nct72 1>;

			trips {
				trip2: cpu-alert {
					/* throttle at 85C until temperature drops to 84.8C */
					temperature = <85000>;
					hysteresis = <200>;
					type = "passive";
				};

				trip3: cpu-crit {
					/* shut down at 90C */
					temperature = <90000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map1 {
					trip = <&trip2>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&actmon THERMAL_NO_LIMIT
								  THERMAL_NO_LIMIT>;
				};
			};
		};
	};
};
