// SPDX-License-Identifier: GPL-2.0
#include <dt-bindings/clock/tegra124-car.h>
#include <dt-bindings/gpio/tegra-gpio.h>
#include <dt-bindings/memory/tegra124-mc.h>
#include <dt-bindings/pinctrl/pinctrl-tegra.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/reset/tegra124-car.h>
#include <dt-bindings/thermal/tegra124-soctherm.h>
#include <dt-bindings/soc/tegra-pmc.h>

#include "tegra124-peripherals-opp.dtsi"

/ {
	compatible = "nvidia,tegra124";
	interrupt-parent = <&lic>;
	#address-cells = <2>;
	#size-cells = <2>;

	memory@80000000 {
		device_type = "memory";
		reg = <0x0 0x80000000 0x0 0x0>;
	};

	pcie@1003000 {
		compatible = "nvidia,tegra124-pcie";
		device_type = "pci";
		reg = <0x0 0x01003000 0x0 0x00000800>, /* PADS registers */
		      <0x0 0x01003800 0x0 0x00000800>, /* AFI registers */
		      <0x0 0x02000000 0x0 0x10000000>; /* configuration space */
		reg-names = "pads", "afi", "cs";
		interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>, /* controller interrupt */
			     <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>; /* MSI interrupt */
		interrupt-names = "intr", "msi";

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 0 0>;
		interrupt-map = <0 0 0 0 &gic GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;

		bus-range = <0x00 0xff>;
		#address-cells = <3>;
		#size-cells = <2>;

		ranges = <0x02000000 0 0x01000000 0x0 0x01000000 0 0x00001000>, /* port 0 configuration space */
			 <0x02000000 0 0x01001000 0x0 0x01001000 0 0x00001000>, /* port 1 configuration space */
			 <0x01000000 0 0x0        0x0 0x12000000 0 0x00010000>, /* downstream I/O (64 KiB) */
			 <0x02000000 0 0x13000000 0x0 0x13000000 0 0x0d000000>, /* non-prefetchable memory (208 MiB) */
			 <0x42000000 0 0x20000000 0x0 0x20000000 0 0x20000000>; /* prefetchable memory (512 MiB) */

		clocks = <&tegra_car TEGRA124_CLK_PCIE>,
			 <&tegra_car TEGRA124_CLK_AFI>,
			 <&tegra_car TEGRA124_CLK_PLL_E>,
			 <&tegra_car TEGRA124_CLK_CML0>;
		clock-names = "pex", "afi", "pll_e", "cml";
		resets = <&tegra_car 70>,
			 <&tegra_car 72>,
			 <&tegra_car 74>;
		reset-names = "pex", "afi", "pcie_x";
		status = "disabled";

		pci@1,0 {
			device_type = "pci";
			assigned-addresses = <0x82000800 0 0x01000000 0 0x1000>;
			reg = <0x000800 0 0 0 0>;
			bus-range = <0x00 0xff>;
			status = "disabled";

			#address-cells = <3>;
			#size-cells = <2>;
			ranges;

			nvidia,num-lanes = <2>;
		};

		pci@2,0 {
			device_type = "pci";
			assigned-addresses = <0x82001000 0 0x01001000 0 0x1000>;
			reg = <0x001000 0 0 0 0>;
			bus-range = <0x00 0xff>;
			status = "disabled";

			#address-cells = <3>;
			#size-cells = <2>;
			ranges;

			nvidia,num-lanes = <1>;
		};
	};

	host1x@50000000 {
		compatible = "nvidia,tegra124-host1x";
		reg = <0x0 0x50000000 0x0 0x00034000>;
		interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>, /* syncpt */
			     <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>; /* general */
		interrupt-names = "syncpt", "host1x";
		clocks = <&tegra_car TEGRA124_CLK_HOST1X>;
		clock-names = "host1x";
		resets = <&tegra_car 28>, <&mc TEGRA124_MC_RESET_HC>;
		reset-names = "host1x", "mc";
		iommus = <&mc TEGRA_SWGROUP_HC>;

		#address-cells = <2>;
		#size-cells = <2>;

		ranges = <0 0x54000000 0 0x54000000 0 0x01000000>;

		dc@54200000 {
			compatible = "nvidia,tegra124-dc";
			reg = <0x0 0x54200000 0x0 0x00040000>;
			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_DISP1>;
			clock-names = "dc";
			resets = <&tegra_car 27>;
			reset-names = "dc";

			iommus = <&mc TEGRA_SWGROUP_DC>;

			nvidia,head = <0>;

			interconnects = <&mc TEGRA124_MC_DISPLAY0A &emc>,
					<&mc TEGRA124_MC_DISPLAY0B &emc>,
					<&mc TEGRA124_MC_DISPLAY0C &emc>,
					<&mc TEGRA124_MC_DISPLAYHC &emc>,
					<&mc TEGRA124_MC_DISPLAYD &emc>,
					<&mc TEGRA124_MC_DISPLAYT &emc>;
			interconnect-names = "wina",
					     "winb",
					     "winc",
					     "cursor",
					     "wind",
					     "wint";
		};

		dc@54240000 {
			compatible = "nvidia,tegra124-dc";
			reg = <0x0 0x54240000 0x0 0x00040000>;
			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_DISP2>;
			clock-names = "dc";
			resets = <&tegra_car 26>;
			reset-names = "dc";

			iommus = <&mc TEGRA_SWGROUP_DCB>;

			nvidia,head = <1>;

			interconnects = <&mc TEGRA124_MC_DISPLAY0AB &emc>,
					<&mc TEGRA124_MC_DISPLAY0BB &emc>,
					<&mc TEGRA124_MC_DISPLAY0CB &emc>,
					<&mc TEGRA124_MC_DISPLAYHCB &emc>;
			interconnect-names = "wina",
					     "winb",
					     "winc",
					     "cursor";
		};

		hdmi: hdmi@54280000 {
			compatible = "nvidia,tegra124-hdmi";
			reg = <0x0 0x54280000 0x0 0x00040000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_HDMI>,
				 <&tegra_car TEGRA124_CLK_PLL_D2_OUT0>;
			clock-names = "hdmi", "parent";
			resets = <&tegra_car 51>;
			reset-names = "hdmi";
			status = "disabled";
		};

		vic@54340000 {
			compatible = "nvidia,tegra124-vic";
			reg = <0x0 0x54340000 0x0 0x00040000>;
			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_VIC03>;
			clock-names = "vic";
			resets = <&tegra_car 178>;
			reset-names = "vic";

			iommus = <&mc TEGRA_SWGROUP_VIC>;
		};

		sor@54540000 {
			compatible = "nvidia,tegra124-sor";
			reg = <0x0 0x54540000 0x0 0x00040000>;
			interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_SOR0>,
				 <&tegra_car TEGRA124_CLK_SOR0_OUT>,
				 <&tegra_car TEGRA124_CLK_PLL_D_OUT0>,
				 <&tegra_car TEGRA124_CLK_PLL_DP>,
				 <&tegra_car TEGRA124_CLK_CLK_M>;
			clock-names = "sor", "out", "parent", "dp", "safe";
			resets = <&tegra_car 182>;
			reset-names = "sor";
			status = "disabled";
		};

		dpaux: dpaux@545c0000 {
			compatible = "nvidia,tegra124-dpaux";
			reg = <0x0 0x545c0000 0x0 0x00040000>;
			interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&tegra_car TEGRA124_CLK_DPAUX>,
				 <&tegra_car TEGRA124_CLK_PLL_DP>;
			clock-names = "dpaux", "parent";
			resets = <&tegra_car 181>;
			reset-names = "dpaux";
			status = "disabled";

			i2c-bus {
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};
	};

	gic: interrupt-controller@50041000 {
		compatible = "arm,cortex-a15-gic";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0x0 0x50041000 0x0 0x1000>,
		      <0x0 0x50042000 0x0 0x1000>,
		      <0x0 0x50044000 0x0 0x2000>,
		      <0x0 0x50046000 0x0 0x2000>;
		interrupts = <GIC_PPI 9
			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
		interrupt-parent = <&gic>;
	};

	gpu@57000000 {
		compatible = "nvidia,gk20a";
		reg = <0x0 0x57000000 0x0 0x01000000>,
		      <0x0 0x58000000 0x0 0x01000000>;
		interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "stall", "nonstall";
		clocks = <&tegra_car TEGRA124_CLK_GPU>,
			 <&tegra_car TEGRA124_CLK_PLL_P_OUT5>;
		clock-names = "gpu", "pwr";
		resets = <&tegra_car 184>;
		reset-names = "gpu";

		iommus = <&mc TEGRA_SWGROUP_GPU>;

		status = "disabled";
	};

	lic: interrupt-controller@60004000 {
		compatible = "nvidia,tegra124-ictlr", "nvidia,tegra30-ictlr";
		reg = <0x0 0x60004000 0x0 0x100>,
		      <0x0 0x60004100 0x0 0x100>,
		      <0x0 0x60004200 0x0 0x100>,
		      <0x0 0x60004300 0x0 0x100>,
		      <0x0 0x60004400 0x0 0x100>;
		interrupt-controller;
		#interrupt-cells = <3>;
		interrupt-parent = <&gic>;
	};

	timer@60005000 {
		compatible = "nvidia,tegra124-timer", "nvidia,tegra30-timer";
		reg = <0x0 0x60005000 0x0 0x400>;
		interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_TIMER>;
	};

	tegra_car: clock@60006000 {
		compatible = "nvidia,tegra124-car";
		reg = <0x0 0x60006000 0x0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
		nvidia,external-memory-controller = <&emc>;
	};

	flow-controller@60007000 {
		compatible = "nvidia,tegra124-flowctrl";
		reg = <0x0 0x60007000 0x0 0x1000>;
	};

	actmon: actmon@6000c800 {
		compatible = "nvidia,tegra124-actmon";
		reg = <0x0 0x6000c800 0x0 0x400>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_ACTMON>,
			 <&tegra_car TEGRA124_CLK_EMC>;
		clock-names = "actmon", "emc";
		resets = <&tegra_car 119>;
		reset-names = "actmon";
		operating-points-v2 = <&emc_bw_dfs_opp_table>;
		interconnects = <&mc TEGRA124_MC_MPCORER &emc>;
		interconnect-names = "cpu-read";
		#cooling-cells = <2>;
	};

	gpio: gpio@6000d000 {
		compatible = "nvidia,tegra124-gpio", "nvidia,tegra30-gpio";
		reg = <0x0 0x6000d000 0x0 0x1000>;
		interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
		#gpio-cells = <2>;
		gpio-controller;
		#interrupt-cells = <2>;
		interrupt-controller;
		gpio-ranges = <&pinmux 0 0 251>;
	};

	apbdma: dma@60020000 {
		compatible = "nvidia,tegra124-apbdma", "nvidia,tegra148-apbdma";
		reg = <0x0 0x60020000 0x0 0x1400>;
		interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_APBDMA>;
		resets = <&tegra_car 34>;
		reset-names = "dma";
		#dma-cells = <1>;
	};

	apbmisc@70000800 {
		compatible = "nvidia,tegra124-apbmisc", "nvidia,tegra20-apbmisc";
		reg = <0x0 0x70000800 0x0 0x64>,   /* Chip revision */
		      <0x0 0x7000e864 0x0 0x04>;   /* Strapping options */
	};

	pinmux: pinmux@70000868 {
		compatible = "nvidia,tegra124-pinmux";
		reg = <0x0 0x70000868 0x0 0x164>, /* Pad control registers */
		      <0x0 0x70003000 0x0 0x434>, /* Mux registers */
		      <0x0 0x70000820 0x0 0x008>; /* MIPI pad control */
	};

	/*
	 * There are two serial driver i.e. 8250 based simple serial
	 * driver and APB DMA based serial driver for higher baudrate
	 * and performace. To enable the 8250 based driver, the compatible
	 * is "nvidia,tegra124-uart", "nvidia,tegra20-uart" and to enable
	 * the APB DMA based serial driver, the compatible is
	 * "nvidia,tegra124-hsuart", "nvidia,tegra30-hsuart".
	 */
	uarta: serial@70006000 {
		compatible = "nvidia,tegra124-uart", "nvidia,tegra20-uart";
		reg = <0x0 0x70006000 0x0 0x40>;
		reg-shift = <2>;
		interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_UARTA>;
		resets = <&tegra_car 6>;
		dmas = <&apbdma 8>, <&apbdma 8>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	uartb: serial@70006040 {
		compatible = "nvidia,tegra124-uart", "nvidia,tegra20-uart";
		reg = <0x0 0x70006040 0x0 0x40>;
		reg-shift = <2>;
		interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_UARTB>;
		resets = <&tegra_car 7>;
		dmas = <&apbdma 9>, <&apbdma 9>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	uartc: serial@70006200 {
		compatible = "nvidia,tegra124-uart", "nvidia,tegra20-uart";
		reg = <0x0 0x70006200 0x0 0x40>;
		reg-shift = <2>;
		interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_UARTC>;
		resets = <&tegra_car 55>;
		dmas = <&apbdma 10>, <&apbdma 10>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	uartd: serial@70006300 {
		compatible = "nvidia,tegra124-uart", "nvidia,tegra20-uart";
		reg = <0x0 0x70006300 0x0 0x40>;
		reg-shift = <2>;
		interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_UARTD>;
		resets = <&tegra_car 65>;
		dmas = <&apbdma 19>, <&apbdma 19>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	pwm: pwm@7000a000 {
		compatible = "nvidia,tegra124-pwm", "nvidia,tegra20-pwm";
		reg = <0x0 0x7000a000 0x0 0x100>;
		#pwm-cells = <2>;
		clocks = <&tegra_car TEGRA124_CLK_PWM>;
		resets = <&tegra_car 17>;
		reset-names = "pwm";
		status = "disabled";
	};

	i2c@7000c000 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000c000 0x0 0x100>;
		interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C1>;
		clock-names = "div-clk";
		resets = <&tegra_car 12>;
		reset-names = "i2c";
		dmas = <&apbdma 21>, <&apbdma 21>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	i2c@7000c400 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000c400 0x0 0x100>;
		interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C2>;
		clock-names = "div-clk";
		resets = <&tegra_car 54>;
		reset-names = "i2c";
		dmas = <&apbdma 22>, <&apbdma 22>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	i2c@7000c500 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000c500 0x0 0x100>;
		interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C3>;
		clock-names = "div-clk";
		resets = <&tegra_car 67>;
		reset-names = "i2c";
		dmas = <&apbdma 23>, <&apbdma 23>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	i2c@7000c700 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000c700 0x0 0x100>;
		interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C4>;
		clock-names = "div-clk";
		resets = <&tegra_car 103>;
		reset-names = "i2c";
		dmas = <&apbdma 26>, <&apbdma 26>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	i2c@7000d000 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000d000 0x0 0x100>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C5>;
		clock-names = "div-clk";
		resets = <&tegra_car 47>;
		reset-names = "i2c";
		dmas = <&apbdma 24>, <&apbdma 24>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	i2c@7000d100 {
		compatible = "nvidia,tegra124-i2c";
		reg = <0x0 0x7000d100 0x0 0x100>;
		interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_I2C6>;
		clock-names = "div-clk";
		resets = <&tegra_car 166>;
		reset-names = "i2c";
		dmas = <&apbdma 30>, <&apbdma 30>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000d400 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000d400 0x0 0x200>;
		interrupts = <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC1>;
		clock-names = "spi";
		resets = <&tegra_car 41>;
		reset-names = "spi";
		dmas = <&apbdma 15>, <&apbdma 15>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000d600 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000d600 0x0 0x200>;
		interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC2>;
		clock-names = "spi";
		resets = <&tegra_car 44>;
		reset-names = "spi";
		dmas = <&apbdma 16>, <&apbdma 16>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000d800 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000d800 0x0 0x200>;
		interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC3>;
		clock-names = "spi";
		resets = <&tegra_car 46>;
		reset-names = "spi";
		dmas = <&apbdma 17>, <&apbdma 17>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000da00 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000da00 0x0 0x200>;
		interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC4>;
		clock-names = "spi";
		resets = <&tegra_car 68>;
		reset-names = "spi";
		dmas = <&apbdma 18>, <&apbdma 18>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000dc00 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000dc00 0x0 0x200>;
		interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC5>;
		clock-names = "spi";
		resets = <&tegra_car 104>;
		reset-names = "spi";
		dmas = <&apbdma 27>, <&apbdma 27>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	spi@7000de00 {
		compatible = "nvidia,tegra124-spi", "nvidia,tegra114-spi";
		reg = <0x0 0x7000de00 0x0 0x200>;
		interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car TEGRA124_CLK_SBC6>;
		clock-names = "spi";
		resets = <&tegra_car 105>;
		reset-names = "spi";
		dmas = <&apbdma 28>, <&apbdma 28>;
		dma-names = "rx", "tx";
		status = "disabled";
	};

	rtc@7000e000 {
		compatible = "nvidia,tegra124-rtc", "nvidia,tegra20-rtc";
		reg = <0x0 0x7000e000 0x0 0x100>;
		interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_RTC>;
	};

	tegra_pmc: pmc@7000e400 {
		compatible = "nvidia,tegra124-pmc";
		reg = <0x0 0x7000e400 0x0 0x400>;
		clocks = <&tegra_car TEGRA124_CLK_PCLK>, <&clk32k_in>;
		clock-names = "pclk", "clk32k_in";
		#clock-cells = <1>;
	};

	fuse@7000f800 {
		compatible = "nvidia,tegra124-efuse";
		reg = <0x0 0x7000f800 0x0 0x400>;
		clocks = <&tegra_car TEGRA124_CLK_FUSE>;
		clock-names = "fuse";
		resets = <&tegra_car 39>;
		reset-names = "fuse";
	};

	cec@70015000 {
		compatible = "nvidia,tegra124-cec";
		reg = <0x0 0x70015000 0x0 0x00001000>;
		interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_CEC>;
		clock-names = "cec";
		status = "disabled";
		hdmi-phandle = <&hdmi>;
	};

	mc: memory-controller@70019000 {
		compatible = "nvidia,tegra124-mc";
		reg = <0x0 0x70019000 0x0 0x1000>;
		clocks = <&tegra_car TEGRA124_CLK_MC>;
		clock-names = "mc";

		interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;

		#iommu-cells = <1>;
		#reset-cells = <1>;
		#interconnect-cells = <1>;
	};

	emc: external-memory-controller@7001b000 {
		compatible = "nvidia,tegra124-emc";
		reg = <0x0 0x7001b000 0x0 0x1000>;
		clocks = <&tegra_car TEGRA124_CLK_EMC>;
		clock-names = "emc";

		nvidia,memory-controller = <&mc>;
		operating-points-v2 = <&emc_icc_dvfs_opp_table>;

		#interconnect-cells = <0>;
	};

	sata@70020000 {
		compatible = "nvidia,tegra124-ahci";
		reg = <0x0 0x70027000 0x0 0x2000>, /* AHCI */
		      <0x0 0x70020000 0x0 0x7000>; /* SATA */
		interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_SATA>,
			 <&tegra_car TEGRA124_CLK_SATA_OOB>;
		clock-names = "sata", "sata-oob";
		resets = <&tegra_car 124>,
			 <&tegra_car 129>,
			 <&tegra_car 123>;
		reset-names = "sata", "sata-cold", "sata-oob";
		status = "disabled";
	};

	hda@70030000 {
		compatible = "nvidia,tegra124-hda", "nvidia,tegra30-hda";
		reg = <0x0 0x70030000 0x0 0x10000>;
		interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_HDA>,
			 <&tegra_car TEGRA124_CLK_HDA2HDMI>,
			 <&tegra_car TEGRA124_CLK_HDA2CODEC_2X>;
		clock-names = "hda", "hda2hdmi", "hda2codec_2x";
		resets = <&tegra_car 125>, /* hda */
			 <&tegra_car 128>, /* hda2hdmi */
			 <&tegra_car 111>; /* hda2codec_2x */
		reset-names = "hda", "hda2hdmi", "hda2codec_2x";
		status = "disabled";
	};

	usb@70090000 {
		compatible = "nvidia,tegra124-xusb";
		reg = <0x0 0x70090000 0x0 0x8000>,
		      <0x0 0x70098000 0x0 0x1000>,
		      <0x0 0x70099000 0x0 0x1000>;
		reg-names = "hcd", "fpci", "ipfs";

		interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;

		clocks = <&tegra_car TEGRA124_CLK_XUSB_HOST>,
			 <&tegra_car TEGRA124_CLK_XUSB_HOST_SRC>,
			 <&tegra_car TEGRA124_CLK_XUSB_FALCON_SRC>,
			 <&tegra_car TEGRA124_CLK_XUSB_SS>,
			 <&tegra_car TEGRA124_CLK_XUSB_SS_DIV2>,
			 <&tegra_car TEGRA124_CLK_XUSB_SS_SRC>,
			 <&tegra_car TEGRA124_CLK_XUSB_HS_SRC>,
			 <&tegra_car TEGRA124_CLK_XUSB_FS_SRC>,
			 <&tegra_car TEGRA124_CLK_PLL_U_480M>,
			 <&tegra_car TEGRA124_CLK_CLK_M>,
			 <&tegra_car TEGRA124_CLK_PLL_E>;
		clock-names = "xusb_host", "xusb_host_src",
			      "xusb_falcon_src", "xusb_ss",
			      "xusb_ss_div2", "xusb_ss_src",
			      "xusb_hs_src", "xusb_fs_src",
			      "pll_u_480m", "clk_m", "pll_e";
		resets = <&tegra_car 89>, <&tegra_car 156>,
			 <&tegra_car 143>;
		reset-names = "xusb_host", "xusb_ss", "xusb_src";

		nvidia,xusb-padctl = <&padctl>;

		status = "disabled";
	};

	padctl: padctl@7009f000 {
		compatible = "nvidia,tegra124-xusb-padctl";
		reg = <0x0 0x7009f000 0x0 0x1000>;
		resets = <&tegra_car 142>;
		reset-names = "padctl";

		pads {
			usb2 {
				status = "disabled";

				lanes {
					usb2-0 {
						status = "disabled";
						#phy-cells = <0>;
					};

					usb2-1 {
						status = "disabled";
						#phy-cells = <0>;
					};

					usb2-2 {
						status = "disabled";
						#phy-cells = <0>;
					};
				};
			};

			ulpi {
				status = "disabled";

				lanes {
					ulpi-0 {
						status = "disabled";
						#phy-cells = <0>;
					};
				};
			};

			hsic {
				status = "disabled";

				lanes {
					hsic-0 {
						status = "disabled";
						#phy-cells = <0>;
					};

					hsic-1 {
						status = "disabled";
						#phy-cells = <0>;
					};
				};
			};

			pcie {
				status = "disabled";

				lanes {
					pcie-0 {
						status = "disabled";
						#phy-cells = <0>;
					};

					pcie-1 {
						status = "disabled";
						#phy-cells = <0>;
					};

					pcie-2 {
						status = "disabled";
						#phy-cells = <0>;
					};

					pcie-3 {
						status = "disabled";
						#phy-cells = <0>;
					};

					pcie-4 {
						status = "disabled";
						#phy-cells = <0>;
					};
				};
			};

			sata {
				status = "disabled";

				lanes {
					sata-0 {
						status = "disabled";
						#phy-cells = <0>;
					};
				};
			};
		};

		ports {
			usb2-0 {
				status = "disabled";
			};

			usb2-1 {
				status = "disabled";
			};

			usb2-2 {
				status = "disabled";
			};

			ulpi-0 {
				status = "disabled";
			};

			hsic-0 {
				status = "disabled";
			};

			hsic-1 {
				status = "disabled";
			};

			usb3-0 {
				status = "disabled";
			};

			usb3-1 {
				status = "disabled";
			};
		};
	};

	mmc@700b0000 {
		compatible = "nvidia,tegra124-sdhci";
		reg = <0x0 0x700b0000 0x0 0x200>;
		interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_SDMMC1>;
		clock-names = "sdhci";
		resets = <&tegra_car 14>;
		reset-names = "sdhci";
		status = "disabled";
	};

	mmc@700b0200 {
		compatible = "nvidia,tegra124-sdhci";
		reg = <0x0 0x700b0200 0x0 0x200>;
		interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_SDMMC2>;
		clock-names = "sdhci";
		resets = <&tegra_car 9>;
		reset-names = "sdhci";
		status = "disabled";
	};

	mmc@700b0400 {
		compatible = "nvidia,tegra124-sdhci";
		reg = <0x0 0x700b0400 0x0 0x200>;
		interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_SDMMC3>;
		clock-names = "sdhci";
		resets = <&tegra_car 69>;
		reset-names = "sdhci";
		status = "disabled";
	};

	mmc@700b0600 {
		compatible = "nvidia,tegra124-sdhci";
		reg = <0x0 0x700b0600 0x0 0x200>;
		interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_SDMMC4>;
		clock-names = "sdhci";
		resets = <&tegra_car 15>;
		reset-names = "sdhci";
		status = "disabled";
	};

	soctherm: thermal-sensor@700e2000 {
		compatible = "nvidia,tegra124-soctherm";
		reg = <0x0 0x700e2000 0x0 0x600>, /* SOC_THERM reg_base */
		      <0x0 0x60006000 0x0 0x400>; /* CAR reg_base */
		reg-names = "soctherm-reg", "car-reg";
		interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "thermal", "edp";
		clocks = <&tegra_car TEGRA124_CLK_TSENSOR>,
			 <&tegra_car TEGRA124_CLK_SOC_THERM>;
		clock-names = "tsensor", "soctherm";
		resets = <&tegra_car 78>;
		reset-names = "soctherm";
		#thermal-sensor-cells = <1>;

		throttle-cfgs {
			throttle_heavy: heavy {
				nvidia,priority = <100>;
				nvidia,cpu-throt-percent = <85>;
				nvidia,gpu-throt-level = <TEGRA_SOCTHERM_THROT_LEVEL_HIGH>;

				#cooling-cells = <2>;
			};
		};
	};

	dfll: clock@70110000 {
		compatible = "nvidia,tegra124-dfll";
		reg = <0 0x70110000 0 0x100>, /* DFLL control */
		      <0 0x70110000 0 0x100>, /* I2C output control */
		      <0 0x70110100 0 0x100>, /* Integrated I2C controller */
		      <0 0x70110200 0 0x100>; /* Look-up table RAM */
		interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_DFLL_SOC>,
			 <&tegra_car TEGRA124_CLK_DFLL_REF>,
			 <&tegra_car TEGRA124_CLK_I2C5>;
		clock-names = "soc", "ref", "i2c";
		resets = <&tegra_car TEGRA124_RST_DFLL_DVCO>;
		reset-names = "dvco";
		#clock-cells = <0>;
		clock-output-names = "dfllCPU_out";
		nvidia,sample-rate = <12500>;
		nvidia,droop-ctrl = <0x00000f00>;
		nvidia,force-mode = <1>;
		nvidia,cf = <10>;
		nvidia,ci = <0>;
		nvidia,cg = <2>;
		status = "disabled";
	};

	ahub@70300000 {
		compatible = "nvidia,tegra124-ahub";
		reg = <0x0 0x70300000 0x0 0x200>,
		      <0x0 0x70300800 0x0 0x800>,
		      <0x0 0x70300200 0x0 0x600>;
		interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&tegra_car TEGRA124_CLK_D_AUDIO>,
			 <&tegra_car TEGRA124_CLK_APBIF>;
		clock-names = "d_audio", "apbif";
		resets = <&tegra_car 106>, /* d_audio */
			 <&tegra_car 107>, /* apbif */
			 <&tegra_car 30>,  /* i2s0 */
			 <&tegra_car 11>,  /* i2s1 */
			 <&tegra_car 18>,  /* i2s2 */
			 <&tegra_car 101>, /* i2s3 */
			 <&tegra_car 102>, /* i2s4 */
			 <&tegra_car 108>, /* dam0 */
			 <&tegra_car 109>, /* dam1 */
			 <&tegra_car 110>, /* dam2 */
			 <&tegra_car 10>,  /* spdif */
			 <&tegra_car 153>, /* amx */
			 <&tegra_car 185>, /* amx1 */
			 <&tegra_car 154>, /* adx */
			 <&tegra_car 180>, /* adx1 */
			 <&tegra_car 186>, /* afc0 */
			 <&tegra_car 187>, /* afc1 */
			 <&tegra_car 188>, /* afc2 */
			 <&tegra_car 189>, /* afc3 */
			 <&tegra_car 190>, /* afc4 */
			 <&tegra_car 191>; /* afc5 */
		reset-names = "d_audio", "apbif", "i2s0", "i2s1", "i2s2",
			      "i2s3", "i2s4", "dam0", "dam1", "dam2",
			      "spdif", "amx", "amx1", "adx", "adx1",
			      "afc0", "afc1", "afc2", "afc3", "afc4", "afc5";
		dmas = <&apbdma 1>, <&apbdma 1>,
		       <&apbdma 2>, <&apbdma 2>,
		       <&apbdma 3>, <&apbdma 3>,
		       <&apbdma 4>, <&apbdma 4>,
		       <&apbdma 6>, <&apbdma 6>,
		       <&apbdma 7>, <&apbdma 7>,
		       <&apbdma 12>, <&apbdma 12>,
		       <&apbdma 13>, <&apbdma 13>,
		       <&apbdma 14>, <&apbdma 14>,
		       <&apbdma 29>, <&apbdma 29>;
		dma-names = "rx0", "tx0", "rx1", "tx1", "rx2", "tx2",
			    "rx3", "tx3", "rx4", "tx4", "rx5", "tx5",
			    "rx6", "tx6", "rx7", "tx7", "rx8", "tx8",
			    "rx9", "tx9";
		ranges;
		#address-cells = <2>;
		#size-cells = <2>;

		tegra_i2s0: i2s@70301000 {
			compatible = "nvidia,tegra124-i2s";
			reg = <0x0 0x70301000 0x0 0x100>;
			nvidia,ahub-cif-ids = <4 4>;
			clocks = <&tegra_car TEGRA124_CLK_I2S0>;
			resets = <&tegra_car 30>;
			reset-names = "i2s";
			status = "disabled";
		};

		tegra_i2s1: i2s@70301100 {
			compatible = "nvidia,tegra124-i2s";
			reg = <0x0 0x70301100 0x0 0x100>;
			nvidia,ahub-cif-ids = <5 5>;
			clocks = <&tegra_car TEGRA124_CLK_I2S1>;
			resets = <&tegra_car 11>;
			reset-names = "i2s";
			status = "disabled";
		};

		tegra_i2s2: i2s@70301200 {
			compatible = "nvidia,tegra124-i2s";
			reg = <0x0 0x70301200 0x0 0x100>;
			nvidia,ahub-cif-ids = <6 6>;
			clocks = <&tegra_car TEGRA124_CLK_I2S2>;
			resets = <&tegra_car 18>;
			reset-names = "i2s";
			status = "disabled";
		};

		tegra_i2s3: i2s@70301300 {
			compatible = "nvidia,tegra124-i2s";
			reg = <0x0 0x70301300 0x0 0x100>;
			nvidia,ahub-cif-ids = <7 7>;
			clocks = <&tegra_car TEGRA124_CLK_I2S3>;
			resets = <&tegra_car 101>;
			reset-names = "i2s";
			status = "disabled";
		};

		tegra_i2s4: i2s@70301400 {
			compatible = "nvidia,tegra124-i2s";
			reg = <0x0 0x70301400 0x0 0x100>;
			nvidia,ahub-cif-ids = <8 8>;
			clocks = <&tegra_car TEGRA124_CLK_I2S4>;
			resets = <&tegra_car 102>;
			reset-names = "i2s";
			status = "disabled";
		};
	};

	usb@7d000000 {
		compatible = "nvidia,tegra124-ehci", "nvidia,tegra30-ehci";
		reg = <0x0 0x7d000000 0x0 0x4000>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USBD>;
		resets = <&tegra_car 22>;
		reset-names = "usb";
		nvidia,phy = <&phy1>;
		status = "disabled";
	};

	phy1: usb-phy@7d000000 {
		compatible = "nvidia,tegra124-usb-phy", "nvidia,tegra30-usb-phy";
		reg = <0x0 0x7d000000 0x0 0x4000>,
		      <0x0 0x7d000000 0x0 0x4000>;
		interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USBD>,
			 <&tegra_car TEGRA124_CLK_PLL_U>,
			 <&tegra_car TEGRA124_CLK_USBD>;
		clock-names = "reg", "pll_u", "utmi-pads";
		resets = <&tegra_car 22>, <&tegra_car 22>;
		reset-names = "usb", "utmi-pads";
		#phy-cells = <0>;
		nvidia,hssync-start-delay = <0>;
		nvidia,idle-wait-delay = <17>;
		nvidia,elastic-limit = <16>;
		nvidia,term-range-adj = <6>;
		nvidia,xcvr-setup = <9>;
		nvidia,xcvr-lsfslew = <0>;
		nvidia,xcvr-lsrslew = <3>;
		nvidia,hssquelch-level = <2>;
		nvidia,hsdiscon-level = <5>;
		nvidia,xcvr-hsslew = <12>;
		nvidia,has-utmi-pad-registers;
		nvidia,pmc = <&tegra_pmc 0>;
		status = "disabled";
	};

	usb@7d004000 {
		compatible = "nvidia,tegra124-ehci", "nvidia,tegra30-ehci";
		reg = <0x0 0x7d004000 0x0 0x4000>;
		interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USB2>;
		resets = <&tegra_car 58>;
		reset-names = "usb";
		nvidia,phy = <&phy2>;
		status = "disabled";
	};

	phy2: usb-phy@7d004000 {
		compatible = "nvidia,tegra124-usb-phy", "nvidia,tegra30-usb-phy";
		reg = <0x0 0x7d004000 0x0 0x4000>,
		      <0x0 0x7d000000 0x0 0x4000>;
		interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USB2>,
			 <&tegra_car TEGRA124_CLK_PLL_U>,
			 <&tegra_car TEGRA124_CLK_USBD>;
		clock-names = "reg", "pll_u", "utmi-pads";
		resets = <&tegra_car 58>, <&tegra_car 22>;
		reset-names = "usb", "utmi-pads";
		#phy-cells = <0>;
		nvidia,hssync-start-delay = <0>;
		nvidia,idle-wait-delay = <17>;
		nvidia,elastic-limit = <16>;
		nvidia,term-range-adj = <6>;
		nvidia,xcvr-setup = <9>;
		nvidia,xcvr-lsfslew = <0>;
		nvidia,xcvr-lsrslew = <3>;
		nvidia,hssquelch-level = <2>;
		nvidia,hsdiscon-level = <5>;
		nvidia,xcvr-hsslew = <12>;
		nvidia,pmc = <&tegra_pmc 1>;
		status = "disabled";
	};

	usb@7d008000 {
		compatible = "nvidia,tegra124-ehci", "nvidia,tegra30-ehci";
		reg = <0x0 0x7d008000 0x0 0x4000>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USB3>;
		resets = <&tegra_car 59>;
		reset-names = "usb";
		nvidia,phy = <&phy3>;
		status = "disabled";
	};

	phy3: usb-phy@7d008000 {
		compatible = "nvidia,tegra124-usb-phy", "nvidia,tegra30-usb-phy";
		reg = <0x0 0x7d008000 0x0 0x4000>,
		      <0x0 0x7d000000 0x0 0x4000>;
		interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
		phy_type = "utmi";
		clocks = <&tegra_car TEGRA124_CLK_USB3>,
			 <&tegra_car TEGRA124_CLK_PLL_U>,
			 <&tegra_car TEGRA124_CLK_USBD>;
		clock-names = "reg", "pll_u", "utmi-pads";
		resets = <&tegra_car 59>, <&tegra_car 22>;
		reset-names = "usb", "utmi-pads";
		#phy-cells = <0>;
		nvidia,hssync-start-delay = <0>;
		nvidia,idle-wait-delay = <17>;
		nvidia,elastic-limit = <16>;
		nvidia,term-range-adj = <6>;
		nvidia,xcvr-setup = <9>;
		nvidia,xcvr-lsfslew = <0>;
		nvidia,xcvr-lsrslew = <3>;
		nvidia,hssquelch-level = <2>;
		nvidia,hsdiscon-level = <5>;
		nvidia,xcvr-hsslew = <12>;
		nvidia,pmc = <&tegra_pmc 2>;
		status = "disabled";
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;

			clocks = <&tegra_car TEGRA124_CLK_CCLK_G>,
				 <&tegra_car TEGRA124_CLK_CCLK_LP>,
				 <&tegra_car TEGRA124_CLK_PLL_X>,
				 <&tegra_car TEGRA124_CLK_PLL_P>,
				 <&dfll>;
			clock-names = "cpu_g", "cpu_lp", "pll_x", "pll_p", "dfll";
			/* FIXME: what's the actual transition time? */
			clock-latency = <300000>;
		};

		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <1>;
		};

		cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <2>;
		};

		cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <3>;
		};
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&{/cpus/cpu@0}>,
				     <&{/cpus/cpu@1}>,
				     <&{/cpus/cpu@2}>,
				     <&{/cpus/cpu@3}>;
	};

	thermal-zones {
		cpu-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <1000>;

			thermal-sensors =
				<&soctherm TEGRA124_SOCTHERM_SENSOR_CPU>;

			trips {
				cpu-shutdown-trip {
					temperature = <103000>;
					hysteresis = <0>;
					type = "critical";
				};
				cpu_throttle_trip: throttle-trip {
					temperature = <100000>;
					hysteresis = <1000>;
					type = "hot";
				};
			};

			cooling-maps {
				map0 {
					trip = <&cpu_throttle_trip>;
					cooling-device = <&throttle_heavy 1 1>;
				};
			};
		};

		mem-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <1000>;

			thermal-sensors =
				<&soctherm TEGRA124_SOCTHERM_SENSOR_MEM>;

			trips {
				mem-shutdown-trip {
					temperature = <103000>;
					hysteresis = <0>;
					type = "critical";
				};
				mem-throttle-trip {
					temperature = <99000>;
					hysteresis = <1000>;
					type = "hot";
				};
			};

			cooling-maps {
				/*
				 * There are currently no cooling maps,
				 * because there are no cooling devices.
				 */
			};
		};

		gpu-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <1000>;

			thermal-sensors =
				<&soctherm TEGRA124_SOCTHERM_SENSOR_GPU>;

			trips {
				gpu-shutdown-trip {
					temperature = <101000>;
					hysteresis = <0>;
					type = "critical";
				};
				gpu_throttle_trip: throttle-trip {
					temperature = <99000>;
					hysteresis = <1000>;
					type = "hot";
				};
			};

			cooling-maps {
				map0 {
					trip = <&gpu_throttle_trip>;
					cooling-device = <&throttle_heavy 1 1>;
				};
			};
		};

		pllx-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <1000>;

			thermal-sensors =
				<&soctherm TEGRA124_SOCTHERM_SENSOR_PLLX>;

			trips {
				pllx-shutdown-trip {
					temperature = <103000>;
					hysteresis = <0>;
					type = "critical";
				};
				pllx-throttle-trip {
					temperature = <99000>;
					hysteresis = <1000>;
					type = "hot";
				};
			};

			cooling-maps {
				/*
				 * There are currently no cooling maps,
				 * because there are no cooling devices.
				 */
			};
		};
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <GIC_PPI 13
				(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14
				(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11
				(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10
				(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
		interrupt-parent = <&gic>;
	};
};
