// SPDX-License-Identifier: GPL-2.0
// Copyright (c) 2019 Nuvoton Technology <kwliu@nuvoton.com>
// Copyright (c) 2019 Quanta Computer Inc. <Samuel.Jiang@quantatw.com>

/dts-v1/;
#include "nuvoton-npcm750.dtsi"
#include "nuvoton-npcm750-runbmc-olympus-pincfg.dtsi"

#include <dt-bindings/i2c/i2c.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	model = "Nuvoton npcm750 RunBMC Olympus";
	compatible = "nuvoton,npcm750";

	aliases {
		ethernet1 = &gmac0;
		serial0 = &serial0;
		serial1 = &serial1;
		serial2 = &serial2;
		serial3 = &serial3;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &i2c6;
		i2c7 = &i2c7;
		i2c8 = &i2c8;
		i2c9 = &i2c9;
		i2c10 = &i2c10;
		i2c11 = &i2c11;
		i2c12 = &i2c12;
		i2c13 = &i2c13;
		spi0 = &spi0;
		spi1 = &spi1;
		fiu0 = &fiu0;
		fiu1 = &fiu3;
	};

	chosen {
		stdout-path = &serial3;
	};

	memory {
		reg = <0 0x40000000>;
	};

	iio-hwmon {
		compatible = "iio-hwmon";
		io-channels = <&adc 0>, <&adc 1>, <&adc 2>, <&adc 3>,
			<&adc 4>, <&adc 5>, <&adc 6>, <&adc 7>;
	};

	leds {
		compatible = "gpio-leds";
		heartbeat {
		label = "heartbeat";
			gpios = <&gpio3 14 1>;
		};

		identify {
			label = "identify";
			gpios = <&gpio3 15 1>;
		};
	};

	jtag {
		compatible = "nuvoton,npcm750-jtag";
		enable_pspi_jtag = <1>;
		pspi-index = <2>;
		tck {
			label = "tck";
			gpios = <&gpio0 19 0>; /* gpio19 */
			regbase = <0xf0010000 0x1000>;
		};

		tdi {
			label = "tdi";
			gpios = <&gpio0 18 0>; /* gpio18 */
			regbase = <0xf0010000 0x1000>;
		};

		tdo {
			label = "tdo";
			gpios = <&gpio0 17 0>; /* gpio17 */
			regbase = <0xf0010000 0x1000>;
		};
		tms {
			label = "tms";
			gpios = <&gpio0 16 0>; /* gpio16 */
			regbase = <0xf0010000 0x1000>;
		};
	};
};

&fiu0 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi0cs1_pins>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		spi-rx-bus-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
			bmc@0 {
				label = "bmc";
				reg = <0x000000 0x2000000>;
			};
			u-boot@0 {
				label = "u-boot";
				reg = <0x0000000 0x80000>;
				read-only;
			};
			u-boot-env@100000 {
				label = "u-boot-env";
				reg = <0x00100000 0x40000>;
			};
			kernel@200000 {
				label = "kernel";
				reg = <0x0200000 0x600000>;
			};
			rofs@800000 {
				label = "rofs";
				reg = <0x800000 0x1500000>;
			};
			rwfs@1d00000 {
				label = "rwfs";
				reg = <0x1d00000 0x300000>;
			};
		};
	};

	flash@1 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <1>;
		npcm,fiu-rx-bus-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
			spare1@0 {
				label = "spi0-cs1-spare1";
				reg = <0x0 0x800000>;
			};
			spare2@800000 {
				label = "spi0-cs1-spare2";
				reg = <0x800000 0x0>;
			};
		};
	};
};

&fiu3 {
	pinctrl-0 = <&spi3_pins>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		spi-rx-bus-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
			system1@0 {
				label = "spi3-system1";
				reg = <0x0 0x800000>;
			};
			system2@800000 {
				label = "spi3-system2";
				reg = <0x800000 0x0>;
			};
		};
	};
};

&gcr {
	mux-controller {
		compatible = "mmio-mux";
		#mux-control-cells = <1>;

		mux-reg-masks = <0x38 0x07>;
		idle-states = <6>;
	};
};

&gmac0 {
	phy-mode = "rgmii-id";
	snps,eee-force-disable;
	status = "okay";
};

&i2c1 {
	status = "okay";

	i2c-mux@70 {
		compatible = "nxp,pca9548";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x70>;
		i2c-mux-idle-disconnect;

		i2c_slot1a: i2c@0 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0>;
		};

		i2c_slot1b: i2c@1 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <1>;
		};

		i2c_slot2a: i2c@2 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <2>;
		};

		i2c_slot2b: i2c@3 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <3>;
		};

		i2c_slot3: i2c@4 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <4>;
		};

		i2c_slot4: i2c@5 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <5>;
		};

		i2c_slot5: i2c@6 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <6>;
		};
	};

	i2c-mux@71 {
		compatible = "nxp,pca9546";
		reg = <0x71>;
		#address-cells = <1>;
		#size-cells = <0>;
		i2c-mux-idle-disconnect;

		i2c_m2_s1: i2c@0 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0>;
		};

		i2c_m2_s2: i2c@1 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <1>;
		};
		i2c_m2_s3: i2c@2 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <2>;
		};

		i2c_m2_s4: i2c@3 {
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <3>;
		};
	};
};

&i2c2 {
	status = "okay";

	tmp421@4c {
		compatible = "ti,tmp421";
		reg = <0x4c>;
	};

	power-supply@58 {
		compatible = "delta,dps800";
		reg = <0x58>;
	};
};

&i2c3 {
	status = "okay";
};

&i2c4 {
	status = "okay";

	eeprom@54 {
		compatible = "atmel,24c64";
		reg = <0x54>;
	};
};

&i2c5 {
	status = "okay";

	i2c-slave-mqueue@10 {
		compatible = "i2c-slave-mqueue";
		reg = <(I2C_OWN_SLAVE_ADDRESS | 0x10)>;
	};
};

&i2c6 {
	status = "okay";

	ina219@40 {
		compatible = "ti,ina219";
		reg = <0x40>;
	};
	ina219@41 {
		compatible = "ti,ina219";
		reg = <0x41>;
	};
	ina219@44 {
		compatible = "ti,ina219";
		reg = <0x44>;
	};
	ina219@45 {
		compatible = "ti,ina219";
		reg = <0x45>;
	};
	tps53679@60 {
		compatible = "ti,tps53679";
		reg = <0x60>;
	};
	tps53659@62 {
		compatible = "ti,tps53659";
		reg = <0x62>;
	};
	tps53659@64 {
		compatible = "ti,tps53659";
		reg = <0x64>;
	};
	tps53622@67 {
		compatible = "ti,tps53622";
		reg = <0x67>;
	};
	tps53622@69 {
		compatible = "ti,tps53622";
		reg = <0x69>;
	};
	tps53679@70 {
		compatible = "ti,tps53679";
		reg = <0x70>;
	};
	tps53659@72 {
		compatible = "ti,tps53659";
		reg = <0x72>;
	};
	tps53659@74 {
		compatible = "ti,tps53659";
		reg = <0x74>;
	};
	tps53622@77 {
		compatible = "ti,tps53622";
		reg = <0x77>;
	};
};

&i2c7 {
	status = "okay";

	tmp421@4c {
		compatible = "ti,tmp421";
		reg = <0x4c>;
	};
};

&i2c8 {
	status = "okay";

	adm1278@11 {
		compatible = "adm1278";
		reg = <0x11>;
		Rsense = <500>;
	};
};

&i2c9 {
	status = "okay";
};

&i2c10 {
	status = "okay";

	gpio: pca9555@27 {
		compatible = "nxp,pca9555";
		reg = <0x27>;

		gpio-controller;
		#gpio-cells = <2>;
	};
};

&i2c11 {
	status = "okay";

	pca9539_g1a: pca9539-g1a@74 {
		compatible = "nxp,pca9539";
		reg = <0x74>;
		gpio-controller;
		#gpio-cells = <2>;
		reset-gpios = <&gpio7 4 GPIO_ACTIVE_LOW>;
		G1A_P0_0 {
			gpio-hog;
			gpios = <0 0>;
			output-high;
			line-name = "TPM_BMC_ALERT_N";
		};
		G1A_P0_1 {
			gpio-hog;
			gpios = <1 0>;
			input;
			line-name = "FM_BIOS_TOP_SWAP";
		};
		G1A_P0_2 {
			gpio-hog;
			gpios = <2 0>;
			input;
			line-name = "FM_BIOS_PREFRB2_GOOD";
		};
		G1A_P0_3 {
			gpio-hog;
			gpios = <3 0>;
			input;
			line-name = "BMC_SATAXPCIE_0TO3_SEL";
		};
		G1A_P0_4 {
			gpio-hog;
			gpios = <4 0>;
			input;
			line-name = "BMC_SATAXPCIE_4TO7_SEL";
		};
		G1A_P0_5 {
			gpio-hog;
			gpios = <5 0>;
			output-low;
			line-name = "FM_UV_ADR_TRIGGER_EN_N";
		};
		G1A_P0_6 {
			gpio-hog;
			gpios = <6 0>;
			input;
			line-name = "RM_THROTTLE_EN_N";
		};
		G1A_P1_0 {
			gpio-hog;
			gpios = <8 0>;
			input;
			line-name = "FM_BMC_TPM_PRES_N";
		};
		G1A_P1_1 {
			gpio-hog;
			gpios = <9 0>;
			input;
			line-name = "FM_CPU0_SKTOCC_LVT3_N";
		};
		G1A_P1_2 {
			gpio-hog;
			gpios = <10 0>;
			input;
			line-name = "FM_CPU1_SKTOCC_LVT3_N";
		};
		G1A_P1_3 {
			gpio-hog;
			gpios = <11 0>;
			input;
			line-name = "PSU1_ALERT_N";
		};
		G1A_P1_4 {
			gpio-hog;
			gpios = <12 0>;
			input;
			line-name = "PSU2_ALERT_N";
		};
		G1A_P1_5 {
			gpio-hog;
			gpios = <13 0>;
			input;
			line-name = "H_CPU0_FAST_WAKE_LVT3_N";
		};
		G1A_P1_6 {
			gpio-hog;
			gpios = <14 0>;
			output-high;
			line-name = "I2C_MUX1_RESET_N";
		};
		G1A_P1_7 {
			gpio-hog;
			gpios = <15 0>;
			input;
			line-name = "FM_CPU_CATERR_LVT3_N";
		};
	};

	pca9539_g1b: pca9539-g1b@75 {
		compatible = "nxp,pca9539";
		reg = <0x75>;
		gpio-controller;
		#gpio-cells = <2>;
		G1B_P0_0 {
			gpio-hog;
			gpios = <0 0>;
			input;
			line-name = "PVDDQ_ABC_PINALERT_N";
		};
		G1B_P0_1 {
			gpio-hog;
			gpios = <1 0>;
			input;
			line-name = "PVDDQ_DEF_PINALERT_N";
		};
		G1B_P0_2 {
			gpio-hog;
			gpios = <2 0>;
			input;
			line-name = "PVDDQ_GHJ_PINALERT_N";
		};
		G1B_P0_3 {
			gpio-hog;
			gpios = <3 0>;
			input;
			line-name = "PVDDQ_KLM_PINALERT_N";
		};
		G1B_P0_5 {
			gpio-hog;
			gpios = <5 0>;
			input;
			line-name = "FM_BOARD_REV_ID0";
		};
		G1B_P0_6 {
			gpio-hog;
			gpios = <6 0>;
			input;
			line-name = "FM_BOARD_REV_ID1";
		};
		G1B_P0_7 {
			gpio-hog;
			gpios = <7 0>;
			input;
			line-name = "FM_BOARD_REV_ID2";
		};
		G1B_P1_0 {
			gpio-hog;
			gpios = <8 0>;
			input;
			line-name = "FM_OC_DETECT_EN_N";
		};
		G1B_P1_1 {
			gpio-hog;
			gpios = <9 0>;
			input;
			line-name = "FM_FLASH_DESC_OVERRIDE";
		};
		G1B_P1_2 {
			gpio-hog;
			gpios = <10 0>;
			output-low;
			line-name = "FP_PWR_ID_LED_N";
		};
		G1B_P1_3 {
			gpio-hog;
			gpios = <11 0>;
			output-low;
			line-name = "BMC_LED_PWR_GRN";
		};
		G1B_P1_4 {
			gpio-hog;
			gpios = <12 0>;
			output-low;
			line-name = "BMC_LED_PWR_AMBER";
		};
		G1B_P1_5 {
			gpio-hog;
			gpios = <13 0>;
			output-high;
			line-name = "FM_BMC_FAULT_LED_N";
		};
		G1B_P1_6 {
			gpio-hog;
			gpios = <14 0>;
			output-high;
			line-name = "FM_CPLD_BMC_PWRDN_N";
		};
		G1B_P1_7 {
			gpio-hog;
			gpios = <15 0>;
			output-high;
			line-name = "BMC_LED_CATERR_N";
		};
	};
};

&i2c12 {
	status = "okay";

	pca9539_g2a: pca9539-g2a@74 {
		compatible = "nxp,pca9539";
		reg = <0x74>;
		gpio-controller;
		#gpio-cells = <2>;
		reset-gpios = <&gpio5 28 GPIO_ACTIVE_LOW>;
		G2A_P0_0 {
			gpio-hog;
			gpios = <0 0>;
			output-high;
			line-name = "BMC_PON_RST_REQ_N";
		};
		G2A_P0_1 {
			gpio-hog;
			gpios = <1 0>;
			output-high;
			line-name = "BMC_RST_IND_REQ_N";
		};
		G2A_P0_2 {
			gpio-hog;
			gpios = <2 0>;
			input;
			line-name = "RST_BMC_RTCRST";
		};
		G2A_P0_3 {
			gpio-hog;
			gpios = <3 0>;
			output-high;
			line-name = "FM_BMC_PWRBTN_OUT_N";
		};
		G2A_P0_4 {
			gpio-hog;
			gpios = <4 0>;
			output-high;
			line-name = "RST_BMC_SYSRST_BTN_OUT_N";
		};
		G2A_P0_5 {
			gpio-hog;
			gpios = <5 0>;
			output-high;
			line-name = "FM_BATTERY_SENSE_EN_N";
		};
		G2A_P0_6 {
			gpio-hog;
			gpios = <6 0>;
			output-high;
			line-name = "FM_BMC_READY_N";
		};
		G2A_P0_7 {
			gpio-hog;
			gpios = <7 0>;
			input;
			line-name = "IRQ_BMC_PCH_SMI_LPC_N";
		};
		G2A_P1_0 {
			gpio-hog;
			gpios = <8 0>;
			input;
			line-name = "FM_SLOT4_CFG0";
		};
		G2A_P1_1 {
			gpio-hog;
			gpios = <9 0>;
			input;
			line-name = "FM_SLOT4_CFG1";
		};
		G2A_P1_2 {
			gpio-hog;
			gpios = <10 0>;
			input;
			line-name = "FM_NVDIMM_EVENT_N";
		};
		G2A_P1_3 {
			gpio-hog;
			gpios = <11 0>;
			input;
			line-name = "PSU1_BLADE_EN_N";
		};
		G2A_P1_4 {
			gpio-hog;
			gpios = <12 0>;
			input;
			line-name = "BMC_PCH_FNM";
		};
		G2A_P1_5 {
			gpio-hog;
			gpios = <13 0>;
			input;
			line-name = "FM_SOL_UART_CH_SEL";
		};
		G2A_P1_6 {
			gpio-hog;
			gpios = <14 0>;
			input;
			line-name = "FM_BIOS_POST_CMPLT_N";
		};
	};

	pca9539_g2b: pca9539-g2b@75 {
		compatible = "nxp,pca9539";
		reg = <0x75>;
		gpio-controller;
		#gpio-cells = <2>;
		G2B_P0_0 {
			gpio-hog;
			gpios = <0 0>;
			input;
			line-name = "FM_CPU_MSMI_LVT3_N";
		};
		G2B_P0_1 {
			gpio-hog;
			gpios = <1 0>;
			input;
			line-name = "FM_BIOS_MRC_DEBUG_MSG_DIS";
		};
		G2B_P0_2 {
			gpio-hog;
			gpios = <2 0>;
			input;
			line-name = "FM_CPU1_DISABLE_BMC_N";
		};
		G2B_P0_3 {
			gpio-hog;
			gpios = <3 0>;
			output-low;
			line-name = "BMC_JTAG_SELECT";
		};
		G2B_P0_4 {
			gpio-hog;
			gpios = <4 0>;
			output-high;
			line-name = "PECI_MUX_SELECT";
		};
		G2B_P0_5 {
			gpio-hog;
			gpios = <5 0>;
			output-high;
			line-name = "I2C_MUX2_RESET_N";
		};
		G2B_P0_6 {
			gpio-hog;
			gpios = <6 0>;
			input;
			line-name = "FM_BMC_CPLD_PSU2_ON";
		};
		G2B_P0_7 {
			gpio-hog;
			gpios = <7 0>;
			output-high;
			line-name = "PSU2_ALERT_EN_N";
		};
		G2B_P1_0 {
			gpio-hog;
			gpios = <8 0>;
			output-high;
			line-name = "FM_CPU_BMC_INIT";
		};
		G2B_P1_1 {
			gpio-hog;
			gpios = <9 0>;
			output-high;
			line-name = "IRQ_BMC_PCH_SCI_LPC_N";
		};
		G2B_P1_2 {
			gpio-hog;
			gpios = <10 0>;
			output-low;
			line-name = "PMB_ALERT_EN_N";
		};
		G2B_P1_3 {
			gpio-hog;
			gpios = <11 0>;
			output-high;
			line-name = "FM_FAST_PROCHOT_EN_N";
		};
		G2B_P1_4 {
			gpio-hog;
			gpios = <12 0>;
			output-high;
			line-name = "BMC_NVDIMM_PRSNT_N";
		};
		G2B_P1_5 {
			gpio-hog;
			gpios = <13 0>;
			output-low;
			line-name = "FM_BACKUP_BIOS_SEL_H_BMC";
		};
		G2B_P1_6 {
			gpio-hog;
			gpios = <14 0>;
			output-high;
			line-name = "FM_PWRBRK_N";
		};
	};
};

&i2c13 {
	status = "okay";

	tmp75@4a {
		compatible = "ti,tmp75";
		reg = <0x4a>;
		status = "okay";
	};
	m24128_fru@51 {
		compatible = "atmel,24c128";
		reg = <0x51>;
		pagesize = <64>;
		status = "okay";
	};
};

&pwm_fan {
	pinctrl-names = "default";
	pinctrl-0 = <   &pwm0_pins &pwm1_pins
			&fanin0_pins &fanin1_pins
			&fanin2_pins &fanin3_pins
			&fanin4_pins &fanin5_pins
			&fanin6_pins &fanin7_pins
			&fanin8_pins &fanin9_pins
			&fanin10_pins &fanin11_pins>;
	status = "okay";

	fan@0 {
		reg = <0x00>;
		fan-tach-ch = /bits/ 8 <0x00 0x01>;
		cooling-levels = <127 255>;
	};
	fan@1 {
		reg = <0x01>;
		fan-tach-ch = /bits/ 8 <0x02 0x03>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@2 {
		reg = <0x02>;
		fan-tach-ch = /bits/ 8 <0x04 0x05>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@3 {
		reg = <0x03>;
		fan-tach-ch = /bits/ 8 <0x06 0x07>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@4 {
		reg = <0x04>;
		fan-tach-ch = /bits/ 8 <0x08 0x09>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@5 {
		reg = <0x05>;
		fan-tach-ch = /bits/ 8 <0x0A 0x0B>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@6 {
		reg = <0x06>;
		fan-tach-ch = /bits/ 8 <0x0C 0x0D>;
		cooling-levels = /bits/ 8 <127 255>;
	};
	fan@7 {
		reg = <0x07>;
		fan-tach-ch = /bits/ 8 <0x0E 0x0F>;
		cooling-levels = /bits/ 8 <127 255>;
	};
};

&ehci1 {
	status = "okay";
};

&watchdog1 {
	status = "okay";
};

&rng {
	status = "okay";
};

&serial0 {
	status = "okay";
};

&serial1 {
	status = "okay";
};

&serial2 {
	status = "okay";
};

&serial3 {
	status = "okay";
};

&adc {
	#io-channel-cells = <1>;
	status = "okay";
};

&kcs1 {
	status = "okay";
};

&kcs2 {
	status = "okay";
};

&kcs3 {
	status = "okay";
};

&spi0 {
	cs-gpios = <&gpio6 11 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&spi1 {
	status = "okay";
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <
			/******* RunBMC inside Module pins *******/
			&gpio0ol_pins
			&gpio1ol_pins
			&gpio2ol_pins
			&gpio3ol_pins
			&gpio8o_pins
			&gpio9ol_pins
			&gpio12ol_pins
			&gpio13ol_pins
			&gpio14ol_pins
			&gpio15ol_pins
			&gpio37o_pins
			&gpio38_pins
			&gpio39_pins
			&gpio94ol_pins
			&gpio108ol_pins
			&gpio109ol_pins
			&gpio111ol_pins
			&gpio112ol_pins
			&gpio113ol_pins
			&gpio208_pins
			&gpio209ol_pins
			&gpio210ol_pins
			&gpio211ol_pins
			&gpio212ol_pins
			&gpio213ol_pins
			&gpio214ol_pins
			&gpio215ol_pins
			&gpio216ol_pins
			&gpio217ol_pins
			/******* RunBMC outside Connector pins *******/
			&gpio5_pins
			&gpio6_pins
			&gpio7_pins
			&gpio10_pins
			&gpio11_pins
			&gpio20_pins
			&gpio21_pins
			&gpio22o_pins
			&gpio23_pins
			&gpio24_pins
			&gpio25_pins
			&gpio30_pins
			&gpio31_pins
			&gpio40o_pins
			&gpio59_pins
			&gpio76_pins
			&gpio77_pins
			&gpio78o_pins
			&gpio79_pins
			&gpio82_pins
			&gpio83_pins
			&gpio84_pins
			&gpio85o_pins
			&gpio86ol_pins
			&gpio87_pins
			&gpio88_pins
			&gpio89_pins
			&gpio90_pins
			&gpio93_pins
			&gpio114o_pins
			&gpio115_pins
			&gpio120_pins
			&gpio121_pins
			&gpio122_pins
			&gpio123_pins
			&gpio124_pins
			&gpio125_pins
			&gpio126_pins
			&gpio127o_pins
			&gpio136_pins
			&gpio137_pins
			&gpio138_pins
			&gpio139_pins
			&gpio140_pins
			&gpio141_pins
			&gpio142_pins
			&gpio143_pins
			&gpio144_pins
			&gpio146_pins
			&gpio145_pins
			&gpio147_pins
			&gpio153o_pins
			&gpio155_pins
			&gpio160o_pins
			&gpio169o_pins
			&gpio188o_pins
			&gpio189_pins
			&gpio196_pins
			&gpio197_pins
			&gpio198o_pins
			&gpio199o_pins
			&gpio200_pins
			&gpio202_pins
			&gpio203o_pins
			&gpio224_pins
			&gpio225ol_pins
			&gpio226ol_pins
			&gpio227ol_pins
			&gpio228o_pins
			&gpio229o_pins
			&gpio230_pins
			&gpio231o_pins
			&ddc_pins
			&wdog1_pins
			&wdog2_pins
			>;
};
