// SPDX-License-Identifier: BSD-3-Clause
/*
 * SDX55 SoC device tree source
 *
 * Copyright (c) 2018, The Linux Foundation. All rights reserved.
 * Copyright (c) 2020, Linaro Ltd.
 */

#include <dt-bindings/clock/qcom,gcc-sdx55.h>
#include <dt-bindings/clock/qcom,rpmh.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interconnect/qcom,sdx55.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/power/qcom-rpmpd.h>
#include <dt-bindings/soc/qcom,rpmh-rsc.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	qcom,msm-id = <357 0x10000>, <368 0x10000>, <418 0x10000>;
	interrupt-parent = <&intc>;

	memory {
		device_type = "memory";
		reg = <0 0>;
	};

	clocks {
		xo_board: xo-board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <38400000>;
			clock-output-names = "xo_board";
		};

		sleep_clk: sleep-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32000>;
		};

		nand_clk_dummy: nand-clk-dummy {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32000>;
		};
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x0>;
			enable-method = "psci";
			clocks = <&apcs>;
			power-domains = <&rpmhpd SDX55_CX>;
			power-domain-names = "rpmhpd";
			operating-points-v2 = <&cpu_opp_table>;
		};
	};

	firmware {
		scm {
			compatible = "qcom,scm-sdx55", "qcom,scm";
		};
	};

	cpu_opp_table: opp-table-cpu {
		compatible = "operating-points-v2";
		opp-shared;

		opp-345600000 {
			opp-hz = /bits/ 64 <345600000>;
			required-opps = <&rpmhpd_opp_low_svs>;
		};

		opp-576000000 {
			opp-hz = /bits/ 64 <576000000>;
			required-opps = <&rpmhpd_opp_svs>;
		};

		opp-1094400000 {
			opp-hz = /bits/ 64 <1094400000>;
			required-opps = <&rpmhpd_opp_nom>;
		};

		opp-1555200000 {
			opp-hz = /bits/ 64 <1555200000>;
			required-opps = <&rpmhpd_opp_turbo>;
		};
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		hyp_mem: memory@8fc00000 {
			no-map;
			reg = <0x8fc00000 0x80000>;
		};

		ac_db_mem: memory@8fc80000 {
			no-map;
			reg = <0x8fc80000 0x40000>;
		};

		secdata_mem: memory@8fcfd000 {
			no-map;
			reg = <0x8fcfd000 0x1000>;
		};

		sbl_mem: memory@8fd00000 {
			no-map;
			reg = <0x8fd00000 0x100000>;
		};

		aop_image: memory@8fe00000 {
			no-map;
			reg = <0x8fe00000 0x20000>;
		};

		aop_cmd_db: memory@8fe20000 {
			compatible = "qcom,cmd-db";
			reg = <0x8fe20000 0x20000>;
			no-map;
		};

		smem_mem: memory@8fe40000 {
			no-map;
			reg = <0x8fe40000 0xc0000>;
		};

		tz_mem: memory@8ff00000 {
			no-map;
			reg = <0x8ff00000 0x100000>;
		};

		tz_apps_mem: memory@90000000 {
			no-map;
			reg = <0x90000000 0x500000>;
		};
	};

	smem {
		compatible = "qcom,smem";
		memory-region = <&smem_mem>;
		hwlocks = <&tcsr_mutex 3>;
	};

	smp2p-mpss {
		compatible = "qcom,smp2p";
		qcom,smem = <435>, <428>;
		interrupts = <GIC_SPI 113 IRQ_TYPE_EDGE_RISING>;
		mboxes = <&apcs 14>;
		qcom,local-pid = <0>;
		qcom,remote-pid = <1>;

		modem_smp2p_out: master-kernel {
			qcom,entry-name = "master-kernel";
			#qcom,smem-state-cells = <1>;
		};

		modem_smp2p_in: slave-kernel {
			qcom,entry-name = "slave-kernel";
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		ipa_smp2p_out: ipa-ap-to-modem {
			qcom,entry-name = "ipa";
			#qcom,smem-state-cells = <1>;
		};

		ipa_smp2p_in: ipa-modem-to-ap {
			qcom,entry-name = "ipa";
			interrupt-controller;
			#interrupt-cells = <2>;
		};
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		gcc: clock-controller@100000 {
			compatible = "qcom,gcc-sdx55";
			reg = <0x100000 0x1f0000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
			#power-domain-cells = <1>;
			clock-names = "bi_tcxo", "sleep_clk";
			clocks = <&rpmhcc RPMH_CXO_CLK>, <&sleep_clk>;
		};

		blsp1_uart3: serial@831000 {
			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
			reg = <0x00831000 0x200>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc 30>,
				 <&gcc 9>;
			clock-names = "core", "iface";
			status = "disabled";
		};

		usb_hsphy: phy@ff4000 {
			compatible = "qcom,sdx55-usb-hs-phy",
				     "qcom,usb-snps-hs-7nm-phy";
			reg = <0x00ff4000 0x114>;
			status = "disabled";
			#phy-cells = <0>;

			clocks = <&rpmhcc RPMH_CXO_CLK>;
			clock-names = "ref";

			resets = <&gcc GCC_QUSB2PHY_BCR>;
		};

		usb_qmpphy: phy@ff6000 {
			compatible = "qcom,sdx55-qmp-usb3-uni-phy";
			reg = <0x00ff6000 0x1000>;

			clocks = <&gcc GCC_USB3_PHY_AUX_CLK>,
				 <&gcc GCC_USB3_PRIM_CLKREF_CLK>,
				 <&gcc GCC_USB_PHY_CFG_AHB2PHY_CLK>,
				 <&gcc GCC_USB3_PHY_PIPE_CLK>;
			clock-names = "aux",
				      "ref",
				      "cfg_ahb",
				      "pipe";
			clock-output-names = "usb3_uni_phy_pipe_clk_src";
			#clock-cells = <0>;
			#phy-cells = <0>;

			resets = <&gcc GCC_USB3_PHY_BCR>,
				 <&gcc GCC_USB3PHY_PHY_BCR>;
			reset-names = "phy",
				      "phy_phy";

			status = "disabled";
		};

		mc_virt: interconnect@1100000 {
			compatible = "qcom,sdx55-mc-virt";
			reg = <0x01100000 0x400000>;
			#interconnect-cells = <1>;
			qcom,bcm-voters = <&apps_bcm_voter>;
		};

		mem_noc: interconnect@9680000 {
			compatible = "qcom,sdx55-mem-noc";
			reg = <0x09680000 0x40000>;
			#interconnect-cells = <1>;
			qcom,bcm-voters = <&apps_bcm_voter>;
		};

		system_noc: interconnect@162c000 {
			compatible = "qcom,sdx55-system-noc";
			reg = <0x0162c000 0x31200>;
			#interconnect-cells = <1>;
			qcom,bcm-voters = <&apps_bcm_voter>;
		};

		qpic_bam: dma-controller@1b04000 {
			compatible = "qcom,bam-v1.7.0";
			reg = <0x01b04000 0x1c000>;
			interrupts = <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&rpmhcc RPMH_QPIC_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
			qcom,controlled-remotely;
			status = "disabled";
		};

		qpic_nand: nand-controller@1b30000 {
			compatible = "qcom,sdx55-nand";
			reg = <0x01b30000 0x10000>;
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&rpmhcc RPMH_QPIC_CLK>,
				 <&nand_clk_dummy>;
			clock-names = "core", "aon";

			dmas = <&qpic_bam 0>,
			       <&qpic_bam 1>,
			       <&qpic_bam 2>;
			dma-names = "tx", "rx", "cmd";
			status = "disabled";
		};

		pcie_rc: pcie@1c00000 {
			compatible = "qcom,pcie-sdx55";
			reg = <0x01c00000 0x3000>,
			      <0x40000000 0xf1d>,
			      <0x40000f20 0xc8>,
			      <0x40001000 0x1000>,
			      <0x40100000 0x100000>;
			reg-names = "parf",
				    "dbi",
				    "elbi",
				    "atu",
				    "config";
			device_type = "pci";
			linux,pci-domain = <0>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;

			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x01000000 0x0 0x00000000 0x40200000 0x0 0x100000>,
				 <0x02000000 0x0 0x40300000 0x40300000 0x0 0x3fd00000>;

			interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi",
					  "msi2",
					  "msi3",
					  "msi4",
					  "msi5",
					  "msi6",
					  "msi7",
					  "msi8";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 141 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 142 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 143 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 144 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc GCC_PCIE_PIPE_CLK>,
				 <&gcc GCC_PCIE_AUX_CLK>,
				 <&gcc GCC_PCIE_CFG_AHB_CLK>,
				 <&gcc GCC_PCIE_MSTR_AXI_CLK>,
				 <&gcc GCC_PCIE_SLV_AXI_CLK>,
				 <&gcc GCC_PCIE_SLV_Q2A_AXI_CLK>,
				 <&gcc GCC_PCIE_SLEEP_CLK>;
			clock-names = "pipe",
				      "aux",
				      "cfg",
				      "bus_master",
				      "bus_slave",
				      "slave_q2a",
				      "sleep";

			assigned-clocks = <&gcc GCC_PCIE_AUX_CLK>;
			assigned-clock-rates = <19200000>;

			iommu-map = <0x0   &apps_smmu 0x0200 0x1>,
				    <0x100 &apps_smmu 0x0201 0x1>,
				    <0x200 &apps_smmu 0x0202 0x1>,
				    <0x300 &apps_smmu 0x0203 0x1>,
				    <0x400 &apps_smmu 0x0204 0x1>;

			resets = <&gcc GCC_PCIE_BCR>;
			reset-names = "pci";

			power-domains = <&gcc PCIE_GDSC>;

			phys = <&pcie_phy>;
			phy-names = "pciephy";

			status = "disabled";

			pcie@0 {
				device_type = "pci";
				reg = <0x0 0x0 0x0 0x0 0x0>;
				bus-range = <0x01 0xff>;

				#address-cells = <3>;
				#size-cells = <2>;
				ranges;
			};
		};

		pcie_ep: pcie-ep@1c00000 {
			compatible = "qcom,sdx55-pcie-ep";
			reg = <0x01c00000 0x3000>,
			      <0x40000000 0xf1d>,
			      <0x40000f20 0xc8>,
			      <0x40001000 0x1000>,
			      <0x40200000 0x100000>,
			      <0x01c03000 0x3000>;
			reg-names = "parf",
				    "dbi",
				    "elbi",
				    "atu",
				    "addr_space",
				    "mmio";

			qcom,perst-regs = <&tcsr 0xb258 0xb270>;

			clocks = <&gcc GCC_PCIE_AUX_CLK>,
				 <&gcc GCC_PCIE_CFG_AHB_CLK>,
				 <&gcc GCC_PCIE_MSTR_AXI_CLK>,
				 <&gcc GCC_PCIE_SLV_AXI_CLK>,
				 <&gcc GCC_PCIE_SLV_Q2A_AXI_CLK>,
				 <&gcc GCC_PCIE_SLEEP_CLK>,
				 <&gcc GCC_PCIE_0_CLKREF_CLK>;
			clock-names = "aux",
				      "cfg",
				      "bus_master",
				      "bus_slave",
				      "slave_q2a",
				      "sleep",
				      "ref";

			interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "global",
					  "doorbell";

			interconnects = <&system_noc MASTER_PCIE &mc_virt SLAVE_EBI_CH0>;
			interconnect-names = "pcie-mem";

			resets = <&gcc GCC_PCIE_BCR>;
			reset-names = "core";
			power-domains = <&gcc PCIE_GDSC>;
			phys = <&pcie_phy>;
			phy-names = "pciephy";
			max-link-speed = <3>;
			num-lanes = <2>;

			status = "disabled";
		};

		pcie_phy: phy@1c06000 {
			compatible = "qcom,sdx55-qmp-pcie-phy";
			reg = <0x01c06000 0x2000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			clocks = <&gcc GCC_PCIE_AUX_PHY_CLK_SRC>,
				 <&gcc GCC_PCIE_CFG_AHB_CLK>,
				 <&gcc GCC_PCIE_0_CLKREF_CLK>,
				 <&gcc GCC_PCIE_RCHNG_PHY_CLK>,
				 <&gcc GCC_PCIE_PIPE_CLK>;
			clock-names = "aux",
				      "cfg_ahb",
				      "ref",
				      "refgen",
				      "pipe";

			clock-output-names = "pcie_pipe_clk";
			#clock-cells = <0>;

			#phy-cells = <0>;

			resets = <&gcc GCC_PCIE_PHY_BCR>;
			reset-names = "phy";

			assigned-clocks = <&gcc GCC_PCIE_RCHNG_PHY_CLK>;
			assigned-clock-rates = <100000000>;

			status = "disabled";
		};

		ipa: ipa@1e40000 {
			compatible = "qcom,sdx55-ipa";

			iommus = <&apps_smmu 0x5e0 0x0>,
				 <&apps_smmu 0x5e2 0x0>;
			reg = <0x1e40000 0x7000>,
			      <0x1e50000 0x4b20>,
			      <0x1e04000 0x2c000>;
			reg-names = "ipa-reg",
				    "ipa-shared",
				    "gsi";

			interrupts-extended = <&intc GIC_SPI 241 IRQ_TYPE_EDGE_RISING>,
					      <&intc GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>,
					      <&ipa_smp2p_in 0 IRQ_TYPE_EDGE_RISING>,
					      <&ipa_smp2p_in 1 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "ipa",
					  "gsi",
					  "ipa-clock-query",
					  "ipa-setup-ready";

			clocks = <&rpmhcc RPMH_IPA_CLK>;
			clock-names = "core";

			interconnects = <&system_noc MASTER_IPA &mc_virt SLAVE_EBI_CH0>,
					<&system_noc MASTER_IPA &system_noc SLAVE_OCIMEM>,
					<&mem_noc MASTER_AMPSS_M0 &system_noc SLAVE_IPA_CFG>;
			interconnect-names = "memory",
					     "imem",
					     "config";

			qcom,smem-states = <&ipa_smp2p_out 0>,
					   <&ipa_smp2p_out 1>;
			qcom,smem-state-names = "ipa-clock-enabled-valid",
						"ipa-clock-enabled";

			status = "disabled";
		};

		tcsr_mutex: hwlock@1f40000 {
			compatible = "qcom,tcsr-mutex";
			reg = <0x01f40000 0x40000>;
			#hwlock-cells = <1>;
		};

		tcsr: syscon@1fc0000 {
			compatible = "qcom,sdx55-tcsr", "syscon";
			reg = <0x01fc0000 0x1000>;
		};

		sdhc_1: mmc@8804000 {
			compatible = "qcom,sdx55-sdhci", "qcom,sdhci-msm-v5";
			reg = <0x08804000 0x1000>;
			interrupts = <GIC_SPI 210 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 227 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "hc_irq", "pwr_irq";
			clocks = <&gcc GCC_SDCC1_AHB_CLK>,
				 <&gcc GCC_SDCC1_APPS_CLK>;
			clock-names = "iface", "core";
			status = "disabled";
		};

		remoteproc_mpss: remoteproc@4080000 {
			compatible = "qcom,sdx55-mpss-pas";
			reg = <0x04080000 0x4040>;

			interrupts-extended = <&intc GIC_SPI 250 IRQ_TYPE_EDGE_RISING>,
					      <&modem_smp2p_in 0 IRQ_TYPE_EDGE_RISING>,
					      <&modem_smp2p_in 1 IRQ_TYPE_EDGE_RISING>,
					      <&modem_smp2p_in 2 IRQ_TYPE_EDGE_RISING>,
					      <&modem_smp2p_in 3 IRQ_TYPE_EDGE_RISING>,
					      <&modem_smp2p_in 7 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "wdog", "fatal", "ready", "handover",
					  "stop-ack", "shutdown-ack";

			clocks = <&rpmhcc RPMH_CXO_CLK>;
			clock-names = "xo";

			power-domains = <&rpmhpd SDX55_CX>,
					<&rpmhpd SDX55_MSS>;
			power-domain-names = "cx", "mss";

			qcom,smem-states = <&modem_smp2p_out 0>;
			qcom,smem-state-names = "stop";

			status = "disabled";

			glink-edge {
				interrupts = <GIC_SPI 114 IRQ_TYPE_EDGE_RISING>;
				label = "mpss";
				qcom,remote-pid = <1>;
				mboxes = <&apcs 15>;
			};
		};

		usb: usb@a6f8800 {
			compatible = "qcom,sdx55-dwc3", "qcom,dwc3";
			reg = <0x0a6f8800 0x400>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			clocks = <&gcc GCC_USB30_SLV_AHB_CLK>,
				 <&gcc GCC_USB30_MASTER_CLK>,
				 <&gcc GCC_USB30_MSTR_AXI_CLK>,
				 <&gcc GCC_USB30_SLEEP_CLK>,
				 <&gcc GCC_USB30_MOCK_UTMI_CLK>;
			clock-names = "cfg_noc",
				      "core",
				      "iface",
				      "sleep",
				      "mock_utmi";

			assigned-clocks = <&gcc GCC_USB30_MOCK_UTMI_CLK>,
					  <&gcc GCC_USB30_MASTER_CLK>;
			assigned-clock-rates = <19200000>, <200000000>;

			interrupts-extended = <&intc GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>,
					      <&intc GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>,
					      <&pdc 10 IRQ_TYPE_EDGE_BOTH>,
					      <&pdc 11 IRQ_TYPE_EDGE_BOTH>,
					      <&pdc 51 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "pwr_event",
					  "hs_phy_irq",
					  "dp_hs_phy_irq",
					  "dm_hs_phy_irq",
					  "ss_phy_irq";

			power-domains = <&gcc USB30_GDSC>;

			resets = <&gcc GCC_USB30_BCR>;

			usb_dwc3: usb@a600000 {
				compatible = "snps,dwc3";
				reg = <0x0a600000 0xcd00>;
				interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
				iommus = <&apps_smmu 0x1a0 0x0>;
				snps,dis_u2_susphy_quirk;
				snps,dis_enblslpm_quirk;
				phys = <&usb_hsphy>, <&usb_qmpphy>;
				phy-names = "usb2-phy", "usb3-phy";
			};
		};

		pdc: interrupt-controller@b210000 {
			compatible = "qcom,sdx55-pdc", "qcom,pdc";
			reg = <0x0b210000 0x30000>;
			qcom,pdc-ranges = <0 179 52>;
			#interrupt-cells = <2>;
			interrupt-parent = <&intc>;
			interrupt-controller;
		};

		restart@c264000 {
			compatible = "qcom,pshold";
			reg = <0x0c264000 0x1000>;
		};

		spmi_bus: spmi@c440000 {
			compatible = "qcom,spmi-pmic-arb";
			reg = <0x0c440000 0x0000d00>,
			      <0x0c600000 0x2000000>,
			      <0x0e600000 0x0100000>,
			      <0x0e700000 0x00a0000>,
			      <0x0c40a000 0x0000700>;
			reg-names = "core", "chnls", "obsrvr", "intr", "cnfg";
			interrupt-names = "periph_irq";
			interrupts = <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
			qcom,ee = <0>;
			qcom,channel = <0>;
			#address-cells = <2>;
			#size-cells = <0>;
			interrupt-controller;
			#interrupt-cells = <4>;
		};

		tlmm: pinctrl@f100000 {
			compatible = "qcom,sdx55-pinctrl";
			reg = <0xf100000 0x300000>;
			interrupts = <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-ranges = <&tlmm 0 0 108>;
		};

		sram@1468f000 {
			compatible = "qcom,sdx55-imem", "syscon", "simple-mfd";
			reg = <0x1468f000 0x1000>;

			#address-cells = <1>;
			#size-cells = <1>;

			ranges = <0x0 0x1468f000 0x1000>;

			pil-reloc@94c {
				compatible = "qcom,pil-reloc-info";
				reg = <0x94c 0x200>;
			};
		};

		apps_smmu: iommu@15000000 {
			compatible = "qcom,sdx55-smmu-500", "qcom,smmu-500", "arm,mmu-500";
			reg = <0x15000000 0x20000>;
			#iommu-cells = <2>;
			#global-interrupts = <1>;
			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		};

		intc: interrupt-controller@17800000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			interrupt-parent = <&intc>;
			#interrupt-cells = <3>;
			reg = <0x17800000 0x1000>,
			      <0x17802000 0x1000>;
		};

		a7pll: clock@17808000 {
			compatible = "qcom,sdx55-a7pll";
			reg = <0x17808000 0x1000>;
			clocks = <&rpmhcc RPMH_CXO_CLK>;
			clock-names = "bi_tcxo";
			#clock-cells = <0>;
		};

		apcs: mailbox@17810000 {
			compatible = "qcom,sdx55-apcs-gcc", "syscon";
			reg = <0x17810000 0x2000>;
			#mbox-cells = <1>;
			clocks = <&rpmhcc RPMH_CXO_CLK>, <&a7pll>, <&gcc GPLL0>;
			clock-names = "ref", "pll", "aux";
			#clock-cells = <0>;
		};

		watchdog@17817000 {
			compatible = "qcom,apss-wdt-sdx55", "qcom,kpss-wdt";
			reg = <0x17817000 0x1000>;
			clocks = <&sleep_clk>;
		};

		timer@17820000 {
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			compatible = "arm,armv7-timer-mem";
			reg = <0x17820000 0x1000>;
			clock-frequency = <19200000>;

			frame@17821000 {
				frame-number = <0>;
				interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17821000 0x1000>,
				      <0x17822000 0x1000>;
			};

			frame@17823000 {
				frame-number = <1>;
				interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17823000 0x1000>;
				status = "disabled";
			};

			frame@17824000 {
				frame-number = <2>;
				interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17824000 0x1000>;
				status = "disabled";
			};

			frame@17825000 {
				frame-number = <3>;
				interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17825000 0x1000>;
				status = "disabled";
			};

			frame@17826000 {
				frame-number = <4>;
				interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17826000 0x1000>;
				status = "disabled";
			};

			frame@17827000 {
				frame-number = <5>;
				interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17827000 0x1000>;
				status = "disabled";
			};

			frame@17828000 {
				frame-number = <6>;
				interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17828000 0x1000>;
				status = "disabled";
			};

			frame@17829000 {
				frame-number = <7>;
				interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
				reg = <0x17829000 0x1000>;
				status = "disabled";
			};
		};

		apps_rsc: rsc@17830000 {
			compatible = "qcom,rpmh-rsc";
			reg = <0x17830000 0x10000>, <0x17840000 0x10000>;
			reg-names = "drv-0", "drv-1";
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
			qcom,tcs-offset = <0xd00>;
			qcom,drv-id = <1>;
			qcom,tcs-config = <ACTIVE_TCS  2>, <SLEEP_TCS   2>,
					  <WAKE_TCS    2>, <CONTROL_TCS 1>;

			rpmhcc: clock-controller {
				compatible = "qcom,sdx55-rpmh-clk";
				#clock-cells = <1>;
				clock-names = "xo";
				clocks = <&xo_board>;
			};

			rpmhpd: power-controller {
				compatible = "qcom,sdx55-rpmhpd";
				#power-domain-cells = <1>;
				operating-points-v2 = <&rpmhpd_opp_table>;

				rpmhpd_opp_table: opp-table {
					compatible = "operating-points-v2";

					rpmhpd_opp_ret: opp1 {
						opp-level = <RPMH_REGULATOR_LEVEL_RETENTION>;
					};

					rpmhpd_opp_min_svs: opp2 {
						opp-level = <RPMH_REGULATOR_LEVEL_MIN_SVS>;
					};

					rpmhpd_opp_low_svs: opp3 {
						opp-level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;
					};

					rpmhpd_opp_svs: opp4 {
						opp-level = <RPMH_REGULATOR_LEVEL_SVS>;
					};

					rpmhpd_opp_svs_l1: opp5 {
						opp-level = <RPMH_REGULATOR_LEVEL_SVS_L1>;
					};

					rpmhpd_opp_nom: opp6 {
						opp-level = <RPMH_REGULATOR_LEVEL_NOM>;
					};

					rpmhpd_opp_nom_l1: opp7 {
						opp-level = <RPMH_REGULATOR_LEVEL_NOM_L1>;
					};

					rpmhpd_opp_nom_l2: opp8 {
						opp-level = <RPMH_REGULATOR_LEVEL_NOM_L2>;
					};

					rpmhpd_opp_turbo: opp9 {
						opp-level = <RPMH_REGULATOR_LEVEL_TURBO>;
					};

					rpmhpd_opp_turbo_l1: opp10 {
						opp-level = <RPMH_REGULATOR_LEVEL_TURBO_L1>;
					};
				};
			};

			apps_bcm_voter: bcm-voter {
				compatible = "qcom,bcm-voter";
			};
		};
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 12 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
		clock-frequency = <19200000>;
	};
};
