// SPDX-License-Identifier: (GPL-2.0+ OR MIT)

/dts-v1/;

#include "rk3036.dtsi"

/ {
	model = "Rockchip RK3036 KylinBoard";
	compatible = "rockchip,rk3036-kylin", "rockchip,rk3036";

	chosen {
		stdout-path = "serial2:115200n8";
	};

	memory@60000000 {
		device_type = "memory";
		reg = <0x60000000 0x20000000>;
	};

	hdmi_con: hdmi-con {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds: gpio-leds {
		compatible = "gpio-leds";

		work_led: led-0 {
			gpios = <&gpio2 RK_PD6 GPIO_ACTIVE_HIGH>;
			label = "kylin:red:led";
			pinctrl-names = "default";
			pinctrl-0 = <&led_ctl>;
		};
	};

	sdio_pwrseq: sdio-pwrseq {
		compatible = "mmc-pwrseq-simple";
		pinctrl-names = "default";
		pinctrl-0 = <&bt_wake_h>;

		/*
		 * On the module itself this is one of these (depending
		 * on the actual card populated):
		 * - SDIO_RESET_L_WL_REG_ON
		 * - SDIO_RESET_L_WL_RST
		 * - SDIO_RESET_L_BT_EN
		 */
		reset-gpios = <&gpio0 RK_PD2 GPIO_ACTIVE_LOW>, /* WL_REG_ON */
			      <&gpio0 RK_PD3 GPIO_ACTIVE_LOW>, /* WL_RST */
			      <&gpio2 RK_PB1 GPIO_ACTIVE_LOW>; /* BT_EN */
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "rockchip,rt5616-codec";
		simple-audio-card,mclk-fs = <512>;
		simple-audio-card,widgets =
			"Microphone", "Microphone Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"MIC1", "Microphone Jack",
			"MIC2", "Microphone Jack",
			"Microphone Jack", "micbias1",
			"Headphone Jack", "HPOL",
			"Headphone Jack", "HPOR";

		simple-audio-card,cpu {
			sound-dai = <&i2s>;
		};

		simple-audio-card,codec {
			sound-dai = <&rt5616>;
		};
	};

	vcc_sys: vsys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_sys";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		regulator-boot-on;
	};
};

&acodec {
	status = "okay";
};

&emac {
	phy = <&phy0>;
	phy-reset-duration = <10>; /* millisecond */
	phy-reset-gpios = <&gpio2 RK_PC6 GPIO_ACTIVE_LOW>; /* PHY_RST */
	pinctrl-names = "default";
	pinctrl-0 = <&emac_xfer>, <&emac_mdio>;
	status = "okay";

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;

		phy0: ethernet-phy@0 {
			reg = <0>;
		};
	};
};

&emmc {
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&i2c1 {
	clock-frequency = <400000>;

	status = "okay";

	rk808: pmic@1b {
		compatible = "rockchip,rk808";
		reg = <0x1b>;
		interrupt-parent = <&gpio2>;
		interrupts = <RK_PA2 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int &global_pwroff>;
		rockchip,system-power-controller;
		wakeup-source;
		#clock-cells = <1>;
		clock-output-names = "xin32k", "rk808-clkout2";

		vcc1-supply = <&vcc_sys>;
		vcc2-supply = <&vcc_sys>;
		vcc3-supply = <&vcc_sys>;
		vcc4-supply = <&vcc_sys>;
		vcc6-supply = <&vcc_sys>;
		vcc7-supply = <&vcc_sys>;
		vcc8-supply = <&vcc_18>;
		vcc9-supply = <&vcc_io>;
		vcc10-supply = <&vcc_io>;
		vcc11-supply = <&vcc_sys>;
		vcc12-supply = <&vcc_io>;
		vddio-supply = <&vccio_pmu>;

		regulators {
			vdd_cpu: DCDC_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <1350000>;
				regulator-name = "vdd_arm";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1250000>;
				regulator-name = "vdd_gpu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_ddr";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_io: DCDC_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_io";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vccio_pmu: LDO_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_pmu";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcc_tp: LDO_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_tp";
				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_10: LDO_REG3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-name = "vdd_10";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1000000>;
				};
			};

			vcc18_lcd: LDO_REG4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc18_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vccio_sd";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vout5: LDO_REG6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2500000>;
				regulator-name = "vout5";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_18: LDO_REG7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_18";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca_codec: LDO_REG8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcca_codec";
				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_wl: SWITCH_REG1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_wl";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_lcd: SWITCH_REG2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vcc_lcd";
				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};
		};
	};
};

&i2c2 {
	status = "okay";

	rt5616: audio-codec@1b {
		compatible = "realtek,rt5616";
		reg = <0x1b>;
		clocks = <&cru SCLK_I2S_OUT>;
		clock-names = "mclk";
		#sound-dai-cells = <0>;
	};
};

&i2s {
	status = "okay";
};

&sdio {
	status = "okay";

	bus-width = <4>;
	cap-sd-highspeed;
	cap-sdio-irq;
	rockchip,default-sample-phase = <90>;
	keep-power-in-suspend;
	mmc-pwrseq = <&sdio_pwrseq>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio_clk &sdio_cmd &sdio_bus4>;
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	card-detect-delay = <200>;
	disable-wp;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_clk>, <&sdmmc_cmd>, <&sdmmc_cd>, <&sdmmc_bus4>;
};

&uart0 {
	status = "okay";
};

&uart2 {
	status = "okay";
};

&usb_host {
	status = "okay";
};

&usb_otg {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&pinctrl {
	leds {
		led_ctl: led-ctl {
			rockchip,pins = <2 RK_PD6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pmic {
		pmic_int: pmic-int {
			rockchip,pins = <2 RK_PA2 RK_FUNC_GPIO &pcfg_pull_default>;
		};
	};

	sdio {
		bt_wake_h: bt-wake-h {
			rockchip,pins = <2 RK_PB0 RK_FUNC_GPIO &pcfg_pull_default>;
		};
	};

	sdmmc {
		sdmmc_pwr: sdmmc-pwr {
			rockchip,pins = <2 RK_PD4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	suspend {
		global_pwroff: global-pwroff {
			rockchip,pins = <2 RK_PA7 1 &pcfg_pull_none>;
		};
	};
};
