/*
 * Broadcom BCM470X / BCM5301X ARM platform code.
 * DTS for BCM4708 SoC.
 *
 * Copyright 2013-2014 Hauke Mehrtens <hauke@hauke-m.de>
 *
 * Licensed under the GNU/GPL. See COPYING for details.
 */

#include "bcm5301x.dtsi"

/ {
	compatible = "brcm,bcm4708";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "brcm,bcm-nsp-smp";

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			next-level-cache = <&L2>;
			reg = <0x0>;
		};

		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a9";
			next-level-cache = <&L2>;
			secondary-boot-reg = <0xffff0400>;
			reg = <0x1>;
		};
	};

};

&uart0 {
	status = "okay";
};
