// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/clock/qcom,gcc-msm8960.h>
#include <dt-bindings/clock/qcom,lcc-msm8960.h>
#include <dt-bindings/reset/qcom,gcc-msm8960.h>
#include <dt-bindings/clock/qcom,mmcc-msm8960.h>
#include <dt-bindings/clock/qcom,rpmcc.h>
#include <dt-bindings/soc/qcom,gsbi.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
/ {
	#address-cells = <1>;
	#size-cells = <1>;
	model = "Qualcomm APQ8064";
	compatible = "qcom,apq8064";
	interrupt-parent = <&intc>;

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		smem_region: smem@80000000 {
			reg = <0x80000000 0x200000>;
			no-map;
		};

		wcnss_mem: wcnss@8f000000 {
			reg = <0x8f000000 0x700000>;
			no-map;
		};
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		CPU0: cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
			cpu-idle-states = <&CPU_SPC>;
		};

		CPU1: cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
			cpu-idle-states = <&CPU_SPC>;
		};

		CPU2: cpu@2 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <2>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc2>;
			qcom,saw = <&saw2>;
			cpu-idle-states = <&CPU_SPC>;
		};

		CPU3: cpu@3 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <3>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc3>;
			qcom,saw = <&saw3>;
			cpu-idle-states = <&CPU_SPC>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			cache-unified;
		};

		idle-states {
			CPU_SPC: cpu-spc {
				compatible = "qcom,idle-state-spc",
						"arm,idle-state";
				entry-latency-us = <400>;
				exit-latency-us = <900>;
				min-residency-us = <3000>;
			};
		};
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x0>;
	};

	thermal-zones {
		cpu0-thermal {
			polling-delay-passive = <250>;
			polling-delay = <1000>;

			thermal-sensors = <&tsens 7>;
			coefficients = <1199 0>;

			trips {
				cpu_alert0: trip0 {
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};
				cpu_crit0: trip1 {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		cpu1-thermal {
			polling-delay-passive = <250>;
			polling-delay = <1000>;

			thermal-sensors = <&tsens 8>;
			coefficients = <1132 0>;

			trips {
				cpu_alert1: trip0 {
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};
				cpu_crit1: trip1 {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		cpu2-thermal {
			polling-delay-passive = <250>;
			polling-delay = <1000>;

			thermal-sensors = <&tsens 9>;
			coefficients = <1199 0>;

			trips {
				cpu_alert2: trip0 {
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};
				cpu_crit2: trip1 {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		cpu3-thermal {
			polling-delay-passive = <250>;
			polling-delay = <1000>;

			thermal-sensors = <&tsens 10>;
			coefficients = <1132 0>;

			trips {
				cpu_alert3: trip0 {
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};
				cpu_crit3: trip1 {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	clocks {
		cxo_board: cxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <19200000>;
		};

		pxo_board: pxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <27000000>;
		};

		sleep_clk: sleep_clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};
	};

	smem {
		compatible = "qcom,smem";
		memory-region = <&smem_region>;

		hwlocks = <&sfpb_mutex 3>;
	};

	smsm {
		compatible = "qcom,smsm";

		#address-cells = <1>;
		#size-cells = <0>;

		qcom,ipc-1 = <&l2cc 8 4>;
		qcom,ipc-2 = <&l2cc 8 14>;
		qcom,ipc-3 = <&l2cc 8 23>;
		qcom,ipc-4 = <&sps_sic_non_secure 0x4094 0>;

		apps_smsm: apps@0 {
			reg = <0>;
			#qcom,smem-state-cells = <1>;
		};

		modem_smsm: modem@1 {
			reg = <1>;
			interrupts = <GIC_SPI 38 IRQ_TYPE_EDGE_RISING>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		q6_smsm: q6@2 {
			reg = <2>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_EDGE_RISING>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		wcnss_smsm: wcnss@3 {
			reg = <3>;
			interrupts = <GIC_SPI 204 IRQ_TYPE_EDGE_RISING>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};

		dsps_smsm: dsps@4 {
			reg = <4>;
			interrupts = <GIC_SPI 137 IRQ_TYPE_EDGE_RISING>;

			interrupt-controller;
			#interrupt-cells = <2>;
		};
	};

	firmware {
		scm {
			compatible = "qcom,scm-apq8064", "qcom,scm";

			clocks = <&rpmcc RPM_DAYTONA_FABRIC_CLK>;
			clock-names = "core";
		};
	};

	replicator {
		compatible = "arm,coresight-static-replicator";

		clocks = <&rpmcc RPM_QDSS_CLK>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				replicator_in: endpoint {
					remote-endpoint = <&funnel_out>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				replicator_out0: endpoint {
					remote-endpoint = <&etb_in>;
				};
			};

			port@1 {
				reg = <1>;
				replicator_out1: endpoint {
					remote-endpoint = <&tpiu_in>;
				};
			};
		};
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		tlmm_pinmux: pinctrl@800000 {
			compatible = "qcom,apq8064-pinctrl";
			reg = <0x800000 0x4000>;

			gpio-controller;
			gpio-ranges = <&tlmm_pinmux 0 0 90>;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;

			pinctrl-names = "default";
			pinctrl-0 = <&ps_hold_default_state>;
		};

		sfpb_mutex: hwmutex@1200600 {
			compatible = "qcom,sfpb-mutex";
			reg = <0x01200600 0x100>;
			#hwlock-cells = <1>;
		};

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-wdt-apq8064", "qcom,kpss-timer",
				     "qcom,msm-timer";
			interrupts = <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 3 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <27000000>;
			clocks = <&sleep_clk>;
			clock-names = "sleep";
			cpu-offset = <0x80000>;
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu0_aux";
			#clock-cells = <0>;
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu1_aux";
			#clock-cells = <0>;
		};

		acc2: clock-controller@20a8000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x020a8000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu2_aux";
			#clock-cells = <0>;
		};

		acc3: clock-controller@20b8000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x020b8000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu3_aux";
			#clock-cells = <0>;
		};

		saw0: power-manager@2089000 {
			compatible = "qcom,apq8064-saw2-v1.1-cpu", "qcom,saw2";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;

			saw0_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		saw1: power-manager@2099000 {
			compatible = "qcom,apq8064-saw2-v1.1-cpu", "qcom,saw2";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;

			saw1_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		saw2: power-manager@20a9000 {
			compatible = "qcom,apq8064-saw2-v1.1-cpu", "qcom,saw2";
			reg = <0x020a9000 0x1000>, <0x02009000 0x1000>;

			saw2_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		saw3: power-manager@20b9000 {
			compatible = "qcom,apq8064-saw2-v1.1-cpu", "qcom,saw2";
			reg = <0x020b9000 0x1000>, <0x02009000 0x1000>;

			saw3_vreg: regulator {
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
			};
		};

		sps_sic_non_secure: sps-sic-non-secure@12100000 {
			compatible = "syscon";
			reg = <0x12100000 0x10000>;
		};

		gsbi1: gsbi@12440000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <1>;
			reg = <0x12440000 0x100>;
			clocks = <&gcc GSBI1_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			gsbi1_serial: serial@12450000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x12450000 0x100>,
				      <0x12400000 0x03>;
				interrupts = <GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI1_UART_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi1_i2c: i2c@12460000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				pinctrl-0 = <&i2c1_default_state>;
				pinctrl-1 = <&i2c1_sleep_state>;
				pinctrl-names = "default", "sleep";
				reg = <0x12460000 0x1000>;
				interrupts = <GIC_SPI 194 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI1_QUP_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};

		};

		gsbi2: gsbi@12480000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <2>;
			reg = <0x12480000 0x100>;
			clocks = <&gcc GSBI2_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			gsbi2_i2c: i2c@124a0000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x124a0000 0x1000>;
				pinctrl-0 = <&i2c2_default_state>;
				pinctrl-1 = <&i2c2_sleep_state>;
				pinctrl-names = "default", "sleep";
				interrupts = <GIC_SPI 196 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI2_QUP_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi3: gsbi@16200000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <3>;
			reg = <0x16200000 0x100>;
			clocks = <&gcc GSBI3_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			gsbi3_i2c: i2c@16280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				pinctrl-0 = <&i2c3_default_state>;
				pinctrl-1 = <&i2c3_sleep_state>;
				pinctrl-names = "default", "sleep";
				reg = <0x16280000 0x1000>;
				interrupts = <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI3_QUP_CLK>,
					 <&gcc GSBI3_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi4: gsbi@16300000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <4>;
			reg = <0x16300000 0x03>;
			clocks = <&gcc GSBI4_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			gsbi4_serial: serial@16340000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16340000 0x100>,
				      <0x16300000 0x3>;
				interrupts = <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
				pinctrl-0 = <&gsbi4_uart_pin_a>;
				pinctrl-names = "default";
				clocks = <&gcc GSBI4_UART_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi4_i2c: i2c@16380000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				pinctrl-0 = <&i2c4_default_state>;
				pinctrl-1 = <&i2c4_sleep_state>;
				pinctrl-names = "default", "sleep";
				reg = <0x16380000 0x1000>;
				interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI4_QUP_CLK>,
					 <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		gsbi5: gsbi@1a200000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <5>;
			reg = <0x1a200000 0x03>;
			clocks = <&gcc GSBI5_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			gsbi5_serial: serial@1a240000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x1a240000 0x100>,
				      <0x1a200000 0x03>;
				interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi5_spi: spi@1a280000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>;
				pinctrl-0 = <&spi5_default_state>;
				pinctrl-1 = <&spi5_sleep_state>;
				pinctrl-names = "default", "sleep";
				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		gsbi6: gsbi@16500000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <6>;
			reg = <0x16500000 0x03>;
			clocks = <&gcc GSBI6_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			gsbi6_serial: serial@16540000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16540000 0x100>,
				      <0x16500000 0x03>;
				interrupts = <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI6_UART_CLK>, <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi6_i2c: i2c@16580000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				pinctrl-0 = <&i2c6_default_state>;
				pinctrl-1 = <&i2c6_sleep_state>;
				pinctrl-names = "default", "sleep";
				reg = <0x16580000 0x1000>;
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI6_QUP_CLK>,
					 <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		gsbi7: gsbi@16600000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <7>;
			reg = <0x16600000 0x100>;
			clocks = <&gcc GSBI7_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			syscon-tcsr = <&tcsr>;

			gsbi7_serial: serial@16640000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16640000 0x1000>,
				      <0x16600000 0x1000>;
				interrupts = <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI7_UART_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi7_i2c: i2c@16680000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				pinctrl-0 = <&i2c7_default_state>;
				pinctrl-1 = <&i2c7_sleep_state>;
				pinctrl-names = "default", "sleep";
				reg = <0x16680000 0x1000>;
				interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI7_QUP_CLK>,
					 <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};
		};

		rng@1a500000 {
			compatible = "qcom,prng";
			reg = <0x1a500000 0x200>;
			clocks = <&gcc PRNG_CLK>;
			clock-names = "core";
		};

		ssbi2: ssbi@c00000 {
			compatible = "qcom,ssbi";
			reg = <0x00c00000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		ssbi: ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x00500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		qfprom: efuse@700000 {
			compatible = "qcom,apq8064-qfprom", "qcom,qfprom";
			reg = <0x00700000 0x1000>;
			#address-cells = <1>;
			#size-cells = <1>;

			tsens_calib: calib@404 {
				reg = <0x404 0x10>;
			};
			tsens_backup: backup_calib@414 {
				reg = <0x414 0x10>;
			};
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-apq8064", "syscon";
			reg = <0x00900000 0x4000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
			clocks = <&cxo_board>,
				 <&pxo_board>,
				 <&lcc PLL4>;
			clock-names = "cxo", "pxo", "pll4";

			tsens: thermal-sensor {
				compatible = "qcom,msm8960-tsens";

				nvmem-cells = <&tsens_calib>, <&tsens_backup>;
				nvmem-cell-names = "calib", "calib_backup";
				interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "uplow";

				#qcom,sensors = <11>;
				#thermal-sensor-cells = <1>;
			};
		};

		lcc: clock-controller@28000000 {
			compatible = "qcom,lcc-apq8064";
			reg = <0x28000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
			clocks = <&pxo_board>,
				 <&gcc PLL4_VOTE>,
				 <0>,
				 <0>, <0>,
				 <0>, <0>,
				 <0>;
			clock-names = "pxo",
				      "pll4_vote",
				      "mi2s_codec_clk",
				      "codec_i2s_mic_codec_clk",
				      "spare_i2s_mic_codec_clk",
				      "codec_i2s_spkr_codec_clk",
				      "spare_i2s_spkr_codec_clk",
				      "pcm_codec_clk";
		};

		mmcc: clock-controller@4000000 {
			compatible = "qcom,mmcc-apq8064";
			reg = <0x4000000 0x1000>;
			#clock-cells = <1>;
			#power-domain-cells = <1>;
			#reset-cells = <1>;
			clocks = <&pxo_board>,
				 <&gcc PLL3>,
				 <&gcc PLL8_VOTE>,
				 <&dsi0_phy 1>,
				 <&dsi0_phy 0>,
				 <&dsi1_phy 1>,
				 <&dsi1_phy 0>,
				 <&hdmi_phy>;
			clock-names = "pxo",
				      "pll3",
				      "pll8_vote",
				      "dsi1pll",
				      "dsi1pllbyte",
				      "dsi2pll",
				      "dsi2pllbyte",
				      "hdmipll";
		};

		l2cc: clock-controller@2011000 {
			compatible = "qcom,kpss-gcc-apq8064", "qcom,kpss-gcc", "syscon";
			reg = <0x2011000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			#clock-cells = <0>;
		};

		rpm: rpm@108000 {
			compatible = "qcom,rpm-apq8064";
			reg = <0x108000 0x1000>;
			qcom,ipc = <&l2cc 0x8 2>;

			interrupts = <GIC_SPI 19 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 21 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 22 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "ack", "err", "wakeup";

			rpmcc: clock-controller {
				compatible = "qcom,rpmcc-apq8064", "qcom,rpmcc";
				#clock-cells = <1>;
				clocks = <&pxo_board>, <&cxo_board>;
				clock-names = "pxo", "cxo";
			};
		};

		usb1: usb@12500000 {
			compatible = "qcom,ci-hdrc";
			reg = <0x12500000 0x200>,
			      <0x12500200 0x200>;
			interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc USB_HS1_XCVR_CLK>, <&gcc USB_HS1_H_CLK>;
			clock-names = "core", "iface";
			assigned-clocks = <&gcc USB_HS1_XCVR_CLK>;
			assigned-clock-rates = <60000000>;
			resets = <&gcc USB_HS1_RESET>;
			reset-names = "core";
			phy_type = "ulpi";
			ahb-burst-config = <0>;
			phys = <&usb_hs1_phy>;
			phy-names = "usb-phy";
			status = "disabled";
			#reset-cells = <1>;

			ulpi {
				usb_hs1_phy: phy {
					compatible = "qcom,usb-hs-phy-apq8064",
						     "qcom,usb-hs-phy";
					clocks = <&sleep_clk>, <&cxo_board>;
					clock-names = "sleep", "ref";
					resets = <&usb1 0>;
					reset-names = "por";
					#phy-cells = <0>;
				};
			};
		};

		usb3: usb@12520000 {
			compatible = "qcom,ci-hdrc";
			reg = <0x12520000 0x200>,
			      <0x12520200 0x200>;
			interrupts = <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc USB_HS3_XCVR_CLK>, <&gcc USB_HS3_H_CLK>;
			clock-names = "core", "iface";
			assigned-clocks = <&gcc USB_HS3_XCVR_CLK>;
			assigned-clock-rates = <60000000>;
			resets = <&gcc USB_HS3_RESET>;
			reset-names = "core";
			phy_type = "ulpi";
			ahb-burst-config = <0>;
			phys = <&usb_hs3_phy>;
			phy-names = "usb-phy";
			status = "disabled";
			#reset-cells = <1>;

			ulpi {
				usb_hs3_phy: phy {
					compatible = "qcom,usb-hs-phy-apq8064",
						     "qcom,usb-hs-phy";
					#phy-cells = <0>;
					clocks = <&sleep_clk>, <&cxo_board>;
					clock-names = "sleep", "ref";
					resets = <&usb3 0>;
					reset-names = "por";
				};
			};
		};

		usb4: usb@12530000 {
			compatible = "qcom,ci-hdrc";
			reg = <0x12530000 0x200>,
			      <0x12530200 0x200>;
			interrupts = <GIC_SPI 215 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc USB_HS4_XCVR_CLK>, <&gcc USB_HS4_H_CLK>;
			clock-names = "core", "iface";
			assigned-clocks = <&gcc USB_HS4_XCVR_CLK>;
			assigned-clock-rates = <60000000>;
			resets = <&gcc USB_HS4_RESET>;
			reset-names = "core";
			phy_type = "ulpi";
			ahb-burst-config = <0>;
			phys = <&usb_hs4_phy>;
			phy-names = "usb-phy";
			status = "disabled";
			#reset-cells = <1>;

			ulpi {
				usb_hs4_phy: phy {
					compatible = "qcom,usb-hs-phy-apq8064",
						     "qcom,usb-hs-phy";
					#phy-cells = <0>;
					clocks = <&sleep_clk>, <&cxo_board>;
					clock-names = "sleep", "ref";
					resets = <&usb4 0>;
					reset-names = "por";
				};
			};
		};

		sata_phy0: phy@1b400000 {
			compatible = "qcom,apq8064-sata-phy";
			status = "disabled";
			reg = <0x1b400000 0x200>;
			clocks = <&gcc SATA_PHY_CFG_CLK>;
			clock-names = "cfg";
			#phy-cells = <0>;
		};

		sata0: sata@29000000 {
			compatible = "qcom,apq8064-ahci", "generic-ahci";
			status	 = "disabled";
			reg	 = <0x29000000 0x180>;
			interrupts = <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&gcc SFAB_SATA_S_H_CLK>,
				 <&gcc SATA_H_CLK>,
				 <&gcc SATA_A_CLK>,
				 <&gcc SATA_RXOOB_CLK>,
				 <&gcc SATA_PMALIVE_CLK>;
			clock-names = "slave_iface",
				      "iface",
				      "core",
				      "rxoob",
				      "pmalive";

			assigned-clocks = <&gcc SATA_RXOOB_CLK>,
					  <&gcc SATA_PMALIVE_CLK>;
			assigned-clock-rates = <100000000>, <100000000>;

			phys = <&sata_phy0>;
			phy-names = "sata-phy";
			ports-implemented = <0x1>;
		};

		sdcc3: mmc@12180000 {
			compatible = "arm,pl18x", "arm,primecell";
			arm,primecell-periphid = <0x00051180>;
			status = "disabled";
			reg = <0x12180000 0x2000>;
			interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC3_CLK>, <&gcc SDC3_H_CLK>;
			clock-names = "mclk", "apb_pclk";
			bus-width = <4>;
			cap-sd-highspeed;
			cap-mmc-highspeed;
			max-frequency = <192000000>;
			no-1-8-v;
			dmas = <&sdcc3bam 2>, <&sdcc3bam 1>;
			dma-names = "tx", "rx";
		};

		sdcc3bam: dma-controller@12182000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12182000 0x8000>;
			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC3_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		sdcc4: mmc@121c0000 {
			compatible = "arm,pl18x", "arm,primecell";
			arm,primecell-periphid = <0x00051180>;
			status = "disabled";
			reg = <0x121c0000 0x2000>;
			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC4_CLK>, <&gcc SDC4_H_CLK>;
			clock-names = "mclk", "apb_pclk";
			bus-width = <4>;
			cap-sd-highspeed;
			cap-mmc-highspeed;
			max-frequency = <48000000>;
			dmas = <&sdcc4bam 2>, <&sdcc4bam 1>;
			dma-names = "tx", "rx";
			pinctrl-names = "default";
			pinctrl-0 = <&sdc4_default_state>;
		};

		sdcc4bam: dma-controller@121c2000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x121c2000 0x8000>;
			interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC4_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		sdcc1: mmc@12400000 {
			status = "disabled";
			compatible = "arm,pl18x", "arm,primecell";
			pinctrl-names = "default";
			pinctrl-0 = <&sdcc1_default_state>;
			arm,primecell-periphid = <0x00051180>;
			reg = <0x12400000 0x2000>;
			interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC1_CLK>, <&gcc SDC1_H_CLK>;
			clock-names = "mclk", "apb_pclk";
			bus-width = <8>;
			max-frequency = <96000000>;
			non-removable;
			cap-sd-highspeed;
			cap-mmc-highspeed;
			dmas = <&sdcc1bam 2>, <&sdcc1bam 1>;
			dma-names = "tx", "rx";
		};

		sdcc1bam: dma-controller@12402000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12402000 0x8000>;
			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC1_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		tcsr: syscon@1a400000 {
			compatible = "qcom,tcsr-apq8064", "syscon";
			reg = <0x1a400000 0x100>;
		};

		gpu: gpu@4300000 {
			compatible = "qcom,adreno-320.2", "qcom,adreno";
			reg = <0x04300000 0x20000>;
			reg-names = "kgsl_3d0_reg_memory";
			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "kgsl_3d0_irq";
			clock-names =
			    "core",
			    "iface",
			    "mem",
			    "mem_iface";
			clocks =
			    <&mmcc GFX3D_CLK>,
			    <&mmcc GFX3D_AHB_CLK>,
			    <&mmcc GFX3D_AXI_CLK>,
			    <&mmcc MMSS_IMEM_AHB_CLK>;

			iommus = <&gfx3d 0
				  &gfx3d 1
				  &gfx3d 2
				  &gfx3d 3
				  &gfx3d 4
				  &gfx3d 5
				  &gfx3d 6
				  &gfx3d 7
				  &gfx3d 8
				  &gfx3d 9
				  &gfx3d 10
				  &gfx3d 11
				  &gfx3d 12
				  &gfx3d 13
				  &gfx3d 14
				  &gfx3d 15
				  &gfx3d 16
				  &gfx3d 17
				  &gfx3d 18
				  &gfx3d 19
				  &gfx3d 20
				  &gfx3d 21
				  &gfx3d 22
				  &gfx3d 23
				  &gfx3d 24
				  &gfx3d 25
				  &gfx3d 26
				  &gfx3d 27
				  &gfx3d 28
				  &gfx3d 29
				  &gfx3d 30
				  &gfx3d 31
				  &gfx3d1 0
				  &gfx3d1 1
				  &gfx3d1 2
				  &gfx3d1 3
				  &gfx3d1 4
				  &gfx3d1 5
				  &gfx3d1 6
				  &gfx3d1 7
				  &gfx3d1 8
				  &gfx3d1 9
				  &gfx3d1 10
				  &gfx3d1 11
				  &gfx3d1 12
				  &gfx3d1 13
				  &gfx3d1 14
				  &gfx3d1 15
				  &gfx3d1 16
				  &gfx3d1 17
				  &gfx3d1 18
				  &gfx3d1 19
				  &gfx3d1 20
				  &gfx3d1 21
				  &gfx3d1 22
				  &gfx3d1 23
				  &gfx3d1 24
				  &gfx3d1 25
				  &gfx3d1 26
				  &gfx3d1 27
				  &gfx3d1 28
				  &gfx3d1 29
				  &gfx3d1 30
				  &gfx3d1 31>;

			operating-points-v2 = <&gpu_opp_table>;

			gpu_opp_table: opp-table {
				compatible = "operating-points-v2";

				opp-450000000 {
					opp-hz = /bits/ 64 <450000000>;
				};

				opp-27000000 {
					opp-hz = /bits/ 64 <27000000>;
				};
			};
		};

		mmss_sfpb: syscon@5700000 {
			compatible = "syscon";
			reg = <0x5700000 0x70>;
		};

		dsi0: dsi@4700000 {
			compatible = "qcom,apq8064-dsi-ctrl",
				     "qcom,mdss-dsi-ctrl";
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x04700000 0x200>;
			reg-names = "dsi_ctrl";

			clocks = <&mmcc DSI_M_AHB_CLK>,
				<&mmcc DSI_S_AHB_CLK>,
				<&mmcc AMP_AHB_CLK>,
				<&mmcc DSI_CLK>,
				<&mmcc DSI1_BYTE_CLK>,
				<&mmcc DSI_PIXEL_CLK>,
				<&mmcc DSI1_ESC_CLK>;
			clock-names = "iface", "bus", "core_mmss",
					"src", "byte", "pixel",
					"core";

			assigned-clocks = <&mmcc DSI1_BYTE_SRC>,
					<&mmcc DSI1_ESC_SRC>,
					<&mmcc DSI_SRC>,
					<&mmcc DSI_PIXEL_SRC>;
			assigned-clock-parents = <&dsi0_phy 0>,
						<&dsi0_phy 0>,
						<&dsi0_phy 1>,
						<&dsi0_phy 1>;
			syscon-sfpb = <&mmss_sfpb>;
			phys = <&dsi0_phy>;
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					dsi0_in: endpoint {
					};
				};

				port@1 {
					reg = <1>;
					dsi0_out: endpoint {
					};
				};
			};
		};


		dsi0_phy: phy@4700200 {
			compatible = "qcom,dsi-phy-28nm-8960";
			#clock-cells = <1>;
			#phy-cells = <0>;

			reg = <0x04700200 0x100>,
				<0x04700300 0x200>,
				<0x04700500 0x5c>;
			reg-names = "dsi_pll", "dsi_phy", "dsi_phy_regulator";
			clock-names = "iface", "ref";
			clocks = <&mmcc DSI_M_AHB_CLK>,
				 <&pxo_board>;
			status = "disabled";
		};

		dsi1: dsi@5800000 {
			compatible = "qcom,mdss-dsi-ctrl";
			interrupts = <GIC_SPI 166 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x05800000 0x200>;
			reg-names = "dsi_ctrl";

			clocks = <&mmcc DSI2_M_AHB_CLK>,
				 <&mmcc DSI2_S_AHB_CLK>,
				 <&mmcc AMP_AHB_CLK>,
				 <&mmcc DSI2_CLK>,
				 <&mmcc DSI2_BYTE_CLK>,
				 <&mmcc DSI2_PIXEL_CLK>,
				 <&mmcc DSI2_ESC_CLK>;
			clock-names = "iface",
				      "bus",
				      "core_mmss",
				      "src",
				      "byte",
				      "pixel",
				      "core";

			assigned-clocks = <&mmcc DSI2_BYTE_SRC>,
					  <&mmcc DSI2_ESC_SRC>,
					  <&mmcc DSI2_SRC>,
					  <&mmcc DSI2_PIXEL_SRC>;
			assigned-clock-parents = <&dsi1_phy 0>,
						 <&dsi1_phy 0>,
						 <&dsi1_phy 1>,
						 <&dsi1_phy 1>;

			syscon-sfpb = <&mmss_sfpb>;
			phys = <&dsi1_phy>;

			#address-cells = <1>;
			#size-cells = <0>;

			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					dsi1_in: endpoint {
					};
				};

				port@1 {
					reg = <1>;
					dsi1_out: endpoint {
					};
				};
			};
		};


		dsi1_phy: dsi-phy@5800200 {
			compatible = "qcom,dsi-phy-28nm-8960";
			reg = <0x05800200 0x100>,
			      <0x05800300 0x200>,
			      <0x05800500 0x5c>;
			reg-names = "dsi_pll",
				    "dsi_phy",
				    "dsi_phy_regulator";
			clock-names = "iface",
				      "ref";
			clocks = <&mmcc DSI2_M_AHB_CLK>,
				 <&pxo_board>;
			#clock-cells = <1>;
			#phy-cells = <0>;

			status = "disabled";
		};

		mdp_port0: iommu@7500000 {
			compatible = "qcom,apq8064-iommu";
			#iommu-cells = <1>;
			clock-names =
			    "smmu_pclk",
			    "iommu_clk";
			clocks =
			    <&mmcc SMMU_AHB_CLK>,
			    <&mmcc MDP_AXI_CLK>;
			reg = <0x07500000 0x100000>;
			interrupts =
			    <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>,
			    <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
			qcom,ncb = <2>;
		};

		mdp_port1: iommu@7600000 {
			compatible = "qcom,apq8064-iommu";
			#iommu-cells = <1>;
			clock-names =
			    "smmu_pclk",
			    "iommu_clk";
			clocks =
			    <&mmcc SMMU_AHB_CLK>,
			    <&mmcc MDP_AXI_CLK>;
			reg = <0x07600000 0x100000>;
			interrupts =
			    <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>,
			    <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
			qcom,ncb = <2>;
		};

		gfx3d: iommu@7c00000 {
			compatible = "qcom,apq8064-iommu";
			#iommu-cells = <1>;
			clock-names =
			    "smmu_pclk",
			    "iommu_clk";
			clocks =
			    <&mmcc SMMU_AHB_CLK>,
			    <&mmcc GFX3D_AXI_CLK>;
			reg = <0x07c00000 0x100000>;
			interrupts =
			    <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>,
			    <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
			qcom,ncb = <3>;
		};

		gfx3d1: iommu@7d00000 {
			compatible = "qcom,apq8064-iommu";
			#iommu-cells = <1>;
			clock-names =
			    "smmu_pclk",
			    "iommu_clk";
			clocks =
			    <&mmcc SMMU_AHB_CLK>,
			    <&mmcc GFX3D_AXI_CLK>;
			reg = <0x07d00000 0x100000>;
			interrupts =
			    <GIC_SPI 210 IRQ_TYPE_LEVEL_HIGH>,
			    <GIC_SPI 211 IRQ_TYPE_LEVEL_HIGH>;
			qcom,ncb = <3>;
		};

		pcie: pcie@1b500000 {
			compatible = "qcom,pcie-apq8064";
			reg = <0x1b500000 0x1000>,
			      <0x1b502000 0x80>,
			      <0x1b600000 0x100>,
			      <0x0ff00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <0>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;
			ranges = <0x81000000 0x0 0x00000000 0x0fe00000 0x0 0x00100000>, /* I/O */
				 <0x82000000 0x0 0x08000000 0x08000000 0x0 0x07e00000>; /* mem */
			interrupts = <GIC_SPI 238 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 36 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 37 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 38 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 39 IRQ_TYPE_LEVEL_HIGH>; /* int_d */
			clocks = <&gcc PCIE_A_CLK>,
				 <&gcc PCIE_H_CLK>,
				 <&gcc PCIE_PHY_REF_CLK>;
			clock-names = "core", "iface", "phy";
			resets = <&gcc PCIE_ACLK_RESET>,
				 <&gcc PCIE_HCLK_RESET>,
				 <&gcc PCIE_POR_RESET>,
				 <&gcc PCIE_PCI_RESET>,
				 <&gcc PCIE_PHY_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy";
			status = "disabled";

			pcie@0 {
				device_type = "pci";
				reg = <0x0 0x0 0x0 0x0 0x0>;
				bus-range = <0x01 0xff>;

				#address-cells = <3>;
				#size-cells = <2>;
				ranges;
			};
		};

		hdmi: hdmi-tx@4a00000 {
			compatible = "qcom,hdmi-tx-8960";
			pinctrl-names = "default";
			pinctrl-0 = <&hdmi_pinctrl>;
			reg = <0x04a00000 0x2f0>;
			reg-names = "core_physical";
			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&mmcc HDMI_APP_CLK>,
				 <&mmcc HDMI_M_AHB_CLK>,
				 <&mmcc HDMI_S_AHB_CLK>;
			clock-names = "core",
				      "master_iface",
				      "slave_iface";

			phys = <&hdmi_phy>;

			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					hdmi_in: endpoint {
					};
				};

				port@1 {
					reg = <1>;
					hdmi_out: endpoint {
					};
				};
			};
		};

		hdmi_phy: phy@4a00400 {
			compatible = "qcom,hdmi-phy-8960";
			reg = <0x4a00400 0x60>,
			      <0x4a00500 0x100>;
			reg-names = "hdmi_phy",
				    "hdmi_pll";

			clocks = <&mmcc HDMI_S_AHB_CLK>;
			clock-names = "slave_iface";
			#phy-cells = <0>;
			#clock-cells = <0>;

			status = "disabled";
		};

		mdp: display-controller@5100000 {
			compatible = "qcom,mdp4";
			reg = <0x05100000 0xf0000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&mmcc MDP_CLK>,
				 <&mmcc MDP_AHB_CLK>,
				 <&mmcc MDP_AXI_CLK>,
				 <&mmcc MDP_LUT_CLK>,
				 <&mmcc HDMI_TV_CLK>,
				 <&mmcc MDP_TV_CLK>;
			clock-names = "core_clk",
				      "iface_clk",
				      "bus_clk",
				      "lut_clk",
				      "hdmi_clk",
				      "tv_clk";

			iommus = <&mdp_port0 0
				  &mdp_port0 2
				  &mdp_port1 0
				  &mdp_port1 2>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					mdp_lvds_out: endpoint {
					};
				};

				port@1 {
					reg = <1>;
					mdp_dsi1_out: endpoint {
					};
				};

				port@2 {
					reg = <2>;
					mdp_dsi2_out: endpoint {
					};
				};

				port@3 {
					reg = <3>;
					mdp_dtv_out: endpoint {
					};
				};
			};
		};

		riva: riva-pil@3200800 {
			compatible = "qcom,riva-pil";

			reg = <0x03200800 0x1000>, <0x03202000 0x2000>, <0x03204000 0x100>;
			reg-names = "ccu", "dxe", "pmu";

			interrupts-extended = <&intc GIC_SPI 199 IRQ_TYPE_EDGE_RISING>,
					      <&wcnss_smsm 6 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "wdog", "fatal";

			memory-region = <&wcnss_mem>;

			status = "disabled";

			iris {
				compatible = "qcom,wcn3660";

				clocks = <&cxo_board>;
				clock-names = "xo";
			};

			smd-edge {
				interrupts = <GIC_SPI 198 IRQ_TYPE_EDGE_RISING>;

				qcom,ipc = <&l2cc 8 25>;
				qcom,smd-edge = <6>;

				label = "riva";

				wcnss {
					compatible = "qcom,wcnss";
					qcom,smd-channels = "WCNSS_CTRL";

					qcom,mmio = <&riva>;

					bluetooth {
						compatible = "qcom,wcnss-bt";
					};

					wifi {
						compatible = "qcom,wcnss-wlan";

						interrupts = <GIC_SPI 203 IRQ_TYPE_LEVEL_HIGH>,
							     <GIC_SPI 202 IRQ_TYPE_LEVEL_HIGH>;
						interrupt-names = "tx", "rx";

						qcom,smem-states = <&apps_smsm 10>, <&apps_smsm 9>;
						qcom,smem-state-names = "tx-enable", "tx-rings-empty";
					};
				};
			};
		};

		etb@1a01000 {
			compatible = "arm,coresight-etb10", "arm,primecell";
			reg = <0x1a01000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			in-ports {
				port {
					etb_in: endpoint {
						remote-endpoint = <&replicator_out0>;
					};
				};
			};
		};

		tpiu@1a03000 {
			compatible = "arm,coresight-tpiu", "arm,primecell";
			reg = <0x1a03000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			in-ports {
				port {
					tpiu_in: endpoint {
						remote-endpoint = <&replicator_out1>;
					};
				};
			};
		};

		funnel@1a04000 {
			compatible = "arm,coresight-dynamic-funnel", "arm,primecell";
			reg = <0x1a04000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			in-ports {
				#address-cells = <1>;
				#size-cells = <0>;

				/*
				 * Not described input ports:
				 * 2 - connected to STM component
				 * 3 - not-connected
				 * 6 - not-connected
				 * 7 - not-connected
				 */
				port@0 {
					reg = <0>;
					funnel_in0: endpoint {
						remote-endpoint = <&etm0_out>;
					};
				};
				port@1 {
					reg = <1>;
					funnel_in1: endpoint {
						remote-endpoint = <&etm1_out>;
					};
				};
				port@4 {
					reg = <4>;
					funnel_in4: endpoint {
						remote-endpoint = <&etm2_out>;
					};
				};
				port@5 {
					reg = <5>;
					funnel_in5: endpoint {
						remote-endpoint = <&etm3_out>;
					};
				};
			};

			out-ports {
				port {
					funnel_out: endpoint {
						remote-endpoint = <&replicator_in>;
					};
				};
			};
		};

		etm@1a1c000 {
			compatible = "arm,coresight-etm3x", "arm,primecell";
			reg = <0x1a1c000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			cpu = <&CPU0>;

			out-ports {
				port {
					etm0_out: endpoint {
						remote-endpoint = <&funnel_in0>;
					};
				};
			};
		};

		etm@1a1d000 {
			compatible = "arm,coresight-etm3x", "arm,primecell";
			reg = <0x1a1d000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			cpu = <&CPU1>;

			out-ports {
				port {
					etm1_out: endpoint {
						remote-endpoint = <&funnel_in1>;
					};
				};
			};
		};

		etm@1a1e000 {
			compatible = "arm,coresight-etm3x", "arm,primecell";
			reg = <0x1a1e000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			cpu = <&CPU2>;

			out-ports {
				port {
					etm2_out: endpoint {
						remote-endpoint = <&funnel_in4>;
					};
				};
			};
		};

		etm@1a1f000 {
			compatible = "arm,coresight-etm3x", "arm,primecell";
			reg = <0x1a1f000 0x1000>;

			clocks = <&rpmcc RPM_QDSS_CLK>;
			clock-names = "apb_pclk";

			cpu = <&CPU3>;

			out-ports {
				port {
					etm3_out: endpoint {
						remote-endpoint = <&funnel_in5>;
					};
				};
			};
		};
	};
};
#include "qcom-apq8064-pins.dtsi"
