/*
 *  BSD LICENSE
 *
 *  Copyright(c) 2015 Broadcom Corporation.  All rights reserved.
 *
 *  Redistribution and use in source and binary forms, with or without
 *  modification, are permitted provided that the following conditions
 *  are met:
 *
 *    * Redistributions of source code must retain the above copyright
 *      notice, this list of conditions and the following disclaimer.
 *    * Redistributions in binary form must reproduce the above copyright
 *      notice, this list of conditions and the following disclaimer in
 *      the documentation and/or other materials provided with the
 *      distribution.
 *    * Neither the name of Broadcom Corporation nor the names of its
 *      contributors may be used to endorse or promote products derived
 *      from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 *  OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/dts-v1/;

#include "bcm4708.dtsi"

/ {
	model = "NorthStar SVK (BCM953012K)";
	compatible = "brcm,bcm953012k", "brcm,bcm53012", "brcm,bcm4708";

	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0x10000000>;
	};
};

&nand_controller {
	nand@0 {
		compatible = "brcm,nandcs";
		reg = <0>;
		nand-on-flash-bbt;

		#address-cells = <1>;
		#size-cells = <1>;

		nand-ecc-strength = <4>;
		nand-ecc-step-size = <512>;

		partition@0 {
			label = "nboot";
			reg = <0x00000000 0x00200000>;
			read-only;
		};
		partition@200000 {
			label = "nenv";
			reg = <0x00200000 0x00400000>;
		};
		partition@600000 {
			label = "nsystem";
			reg = <0x00600000 0x00a00000>;
		};
		partition@1000000 {
			label = "nrootfs";
			reg = <0x01000000 0x07000000>;
		};
	};
};

&spi_nor {
	status = "okay";
	spi-max-frequency = <62500000>;
	m25p,default-addr-width = <3>;

	#address-cells = <1>;
	#size-cells = <1>;

	partition@0 {
		label = "boot";
		reg = <0x00000000 0x000d0000>;
	};
	partition@d000 {
		label = "env";
		reg = <0x000d0000 0x00030000>;
	};
	partition@100000 {
		label = "system";
		reg = <0x00100000 0x00600000>;
	};
	partition@700000 {
		label = "rootfs";
		reg = <0x00700000 0x00900000>;
	};
};

&uart0 {
	status = "okay";
};

&uart1 {
	status = "okay";
};

&usb3_phy {
	status = "okay";
};
