// SPDX-License-Identifier: GPL-2.0
#include "tegra20.dtsi"

/ {
	model = "Avionic Design Tamonten SOM";
	compatible = "ad,tamonten", "nvidia,tegra20";

	aliases {
		rtc0 = "/i2c@7000d000/tps6586x@34";
		rtc1 = "/rtc@7000e000";
		serial0 = &uartd;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	memory@0 {
		reg = <0x00000000 0x20000000>;
	};

	host1x@50000000 {
		hdmi@54280000 {
			vdd-supply = <&hdmi_vdd_reg>;
			pll-supply = <&hdmi_pll_reg>;

			nvidia,ddc-i2c-bus = <&hdmi_ddc>;
			nvidia,hpd-gpio = <&gpio TEGRA_GPIO(N, 7)
				GPIO_ACTIVE_HIGH>;
		};
	};

	pinmux@70000014 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			ata {
				nvidia,pins = "ata";
				nvidia,function = "ide";
			};
			atb {
				nvidia,pins = "atb", "gma", "gme";
				nvidia,function = "sdio4";
			};
			atc {
				nvidia,pins = "atc";
				nvidia,function = "nand";
			};
			atd {
				nvidia,pins = "atd", "ate", "gmb", "gmd", "gpu",
					"spia", "spib", "spic";
				nvidia,function = "gmi";
			};
			cdev1 {
				nvidia,pins = "cdev1";
				nvidia,function = "plla_out";
			};
			cdev2 {
				nvidia,pins = "cdev2";
				nvidia,function = "pllp_out4";
			};
			crtp {
				nvidia,pins = "crtp";
				nvidia,function = "crt";
			};
			csus {
				nvidia,pins = "csus";
				nvidia,function = "vi_sensor_clk";
			};
			dap1 {
				nvidia,pins = "dap1";
				nvidia,function = "dap1";
			};
			dap2 {
				nvidia,pins = "dap2";
				nvidia,function = "dap2";
			};
			dap3 {
				nvidia,pins = "dap3";
				nvidia,function = "dap3";
			};
			dap4 {
				nvidia,pins = "dap4";
				nvidia,function = "dap4";
			};
			dta {
				nvidia,pins = "dta", "dtd";
				nvidia,function = "sdio2";
			};
			dtb {
				nvidia,pins = "dtb", "dtc", "dte";
				nvidia,function = "rsvd1";
			};
			dtf {
				nvidia,pins = "dtf";
				nvidia,function = "i2c3";
			};
			gmc {
				nvidia,pins = "gmc";
				nvidia,function = "uartd";
			};
			gpu7 {
				nvidia,pins = "gpu7";
				nvidia,function = "rtck";
			};
			gpv {
				nvidia,pins = "gpv", "slxa", "slxk";
				nvidia,function = "pcie";
			};
			hdint {
				nvidia,pins = "hdint";
				nvidia,function = "hdmi";
			};
			i2cp {
				nvidia,pins = "i2cp";
				nvidia,function = "i2cp";
			};
			irrx {
				nvidia,pins = "irrx", "irtx";
				nvidia,function = "uarta";
			};
			kbca {
				nvidia,pins = "kbca", "kbcb", "kbcc", "kbcd",
					"kbce", "kbcf";
				nvidia,function = "kbc";
			};
			lcsn {
				nvidia,pins = "lcsn", "ld0", "ld1", "ld2",
					"ld3", "ld4", "ld5", "ld6", "ld7",
					"ld8", "ld9", "ld10", "ld11", "ld12",
					"ld13", "ld14", "ld15", "ld16", "ld17",
					"ldc", "ldi", "lhp0", "lhp1", "lhp2",
					"lhs", "lm0", "lm1", "lpp", "lpw0",
					"lpw1", "lpw2", "lsc0", "lsc1", "lsck",
					"lsda", "lsdi", "lspi", "lvp0", "lvp1",
					"lvs";
				nvidia,function = "displaya";
			};
			owc {
				nvidia,pins = "owc", "spdi", "spdo", "uac";
				nvidia,function = "rsvd2";
			};
			pmc {
				nvidia,pins = "pmc";
				nvidia,function = "pwr_on";
			};
			rm {
				nvidia,pins = "rm";
				nvidia,function = "i2c1";
			};
			sdb {
				nvidia,pins = "sdb", "sdc", "sdd";
				nvidia,function = "pwm";
			};
			sdio1 {
				nvidia,pins = "sdio1";
				nvidia,function = "sdio1";
			};
			slxc {
				nvidia,pins = "slxc", "slxd";
				nvidia,function = "spdif";
			};
			spid {
				nvidia,pins = "spid", "spie", "spif";
				nvidia,function = "spi1";
			};
			spig {
				nvidia,pins = "spig", "spih";
				nvidia,function = "spi2_alt";
			};
			uaa {
				nvidia,pins = "uaa", "uab", "uda";
				nvidia,function = "ulpi";
			};
			uad {
				nvidia,pins = "uad";
				nvidia,function = "irda";
			};
			uca {
				nvidia,pins = "uca", "ucb";
				nvidia,function = "uartc";
			};
			conf_ata {
				nvidia,pins = "ata", "atb", "atc", "atd", "ate",
					"cdev1", "cdev2", "dap1", "dtb", "dtf",
					"gma", "gmb", "gmc", "gmd", "gme", "gpu7",
					"gpv", "i2cp", "irrx", "irtx", "pta",
					"rm", "slxa", "slxk", "spia", "spib",
					"uac";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_ck32 {
				nvidia,pins = "ck32", "ddrc", "pmca", "pmcb",
					"pmcc", "pmcd", "pmce", "xm2c", "xm2d";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
			};
			conf_csus {
				nvidia,pins = "csus", "spid", "spif";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_crtp {
				nvidia,pins = "crtp", "dap2", "dap3", "dap4",
					"dtc", "dte", "gpu", "sdio1",
					"slxc", "slxd", "spdi", "spdo", "spig",
					"uda";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_ddc {
				nvidia,pins = "ddc", "dta", "dtd", "kbca",
					"kbcb", "kbcc", "kbcd", "kbce", "kbcf",
					"sdc", "uad", "uca";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_hdint {
				nvidia,pins = "hdint", "lcsn", "ldc", "lm1",
					"lpw1", "lsc1", "lsck", "lsda", "lsdi",
					"lvp0", "owc", "sdb";
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_sdd {
				nvidia,pins = "sdd", "spic", "spie", "spih",
					"uaa", "uab", "ucb";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_lc {
				nvidia,pins = "lc", "ls";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
			};
			conf_ld0 {
				nvidia,pins = "ld0", "ld1", "ld2", "ld3", "ld4",
					"ld5", "ld6", "ld7", "ld8", "ld9",
					"ld10", "ld11", "ld12", "ld13", "ld14",
					"ld15", "ld16", "ld17", "ldi", "lhp0",
					"lhp1", "lhp2", "lhs", "lm0", "lpp",
					"lpw0", "lpw2", "lsc0", "lspi", "lvp1",
					"lvs", "pmc";
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_ld17_0 {
				nvidia,pins = "ld17_0", "ld19_18", "ld21_20",
					"ld23_22";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
			};
		};

		state_i2cmux_ddc: pinmux-i2cmux-ddc {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "i2c2";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "rsvd4";
			};
		};

		state_i2cmux_idle: pinmux-i2cmux-idle {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "rsvd4";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "rsvd4";
			};
		};

		state_i2cmux_pta: pinmux-i2cmux-pta {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "rsvd4";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "i2c2";
			};
		};
	};

	i2s@70002800 {
		status = "okay";
	};

	serial@70006300 {
		/delete-property/ dmas;
		/delete-property/ dma-names;
		status = "okay";
	};

	i2c@7000c000 {
		clock-frequency = <400000>;
		status = "okay";
	};

	i2c@7000c400 {
		clock-frequency = <100000>;
		status = "okay";
	};

	i2c@7000d000 {
		clock-frequency = <400000>;
		status = "okay";

		pmic: tps6586x@34 {
			compatible = "ti,tps6586x";
			reg = <0x34>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;

			ti,system-power-controller;

			#gpio-cells = <2>;
			gpio-controller;

			/* vdd_5v0_reg must be provided by the base board */
			sys-supply = <&vdd_5v0_reg>;
			vin-sm0-supply = <&sys_reg>;
			vin-sm1-supply = <&sys_reg>;
			vin-sm2-supply = <&sys_reg>;
			vinldo01-supply = <&sm2_reg>;
			vinldo23-supply = <&sm2_reg>;
			vinldo4-supply = <&sm2_reg>;
			vinldo678-supply = <&sm2_reg>;
			vinldo9-supply = <&sm2_reg>;

			regulators {
				sys_reg: sys {
					regulator-name = "vdd_sys";
					regulator-always-on;
				};

				vdd_core: sm0 {
					regulator-name = "vdd_sys_sm0,vdd_core";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				sm1 {
					regulator-name = "vdd_sys_sm1,vdd_cpu";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				sm2_reg: sm2 {
					regulator-name = "vdd_sys_sm2,vin_ldo*";
					regulator-min-microvolt = <3700000>;
					regulator-max-microvolt = <3700000>;
					regulator-always-on;
				};

				pci_clk_reg: ldo0 {
					regulator-name = "vdd_ldo0,vddio_pex_clk";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
				};

				ldo1 {
					regulator-name = "vdd_ldo1,avdd_pll*";
					regulator-min-microvolt = <1100000>;
					regulator-max-microvolt = <1100000>;
					regulator-always-on;
				};

				ldo2 {
					regulator-name = "vdd_ldo2,vdd_rtc";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo3 {
					regulator-name = "vdd_ldo3,avdd_usb*";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};

				ldo4 {
					regulator-name = "vdd_ldo4,avdd_osc,vddio_sys";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo5 {
					regulator-name = "vdd_ldo5,vcore_mmc";
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
				};

				ldo6 {
					regulator-name = "vdd_ldo6,avdd_vdac";
					/*
					 * According to the Tegra 2 Automotive
					 * DataSheet, a typical value for this
					 * would be 2.8V, but the PMIC only
					 * supports 2.85V.
					 */
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
				};

				hdmi_vdd_reg: ldo7 {
					regulator-name = "vdd_ldo7,avdd_hdmi";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
				};

				hdmi_pll_reg: ldo8 {
					regulator-name = "vdd_ldo8,avdd_hdmi_pll";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo9 {
					regulator-name = "vdd_ldo9,vdd_ddr_rx,avdd_cam";
					/*
					 * According to the Tegra 2 Automotive
					 * DataSheet, a typical value for this
					 * would be 2.8V, but the PMIC only
					 * supports 2.85V.
					 */
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
					regulator-always-on;
				};

				ldo_rtc {
					regulator-name = "vdd_rtc_out";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};
			};
		};

		temperature-sensor@4c {
			compatible = "onnn,nct1008";
			reg = <0x4c>;
		};
	};

	pmc@7000e400 {
		nvidia,invert-interrupt;
		nvidia,suspend-mode = <1>;
		nvidia,cpu-pwr-good-time = <5000>;
		nvidia,cpu-pwr-off-time = <5000>;
		nvidia,core-pwr-good-time = <3845 3845>;
		nvidia,core-pwr-off-time = <3875>;
		nvidia,sys-clock-req-active-high;
		core-supply = <&vdd_core>;
	};

	pcie@80003000 {
		avdd-pex-supply = <&pci_vdd_reg>;
		vdd-pex-supply = <&pci_vdd_reg>;
		avdd-pex-pll-supply = <&pci_vdd_reg>;
		avdd-plle-supply = <&pci_vdd_reg>;
		vddio-pex-clk-supply = <&pci_clk_reg>;
	};

	usb@c5008000 {
		status = "okay";
	};

	usb-phy@c5008000 {
		status = "okay";
	};

	mmc@c8000600 {
		cd-gpios = <&gpio TEGRA_GPIO(H, 2) GPIO_ACTIVE_LOW>;
		wp-gpios = <&gpio TEGRA_GPIO(H, 3) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
		status = "okay";
	};

	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		#clock-cells = <0>;
	};

	i2cmux {
		compatible = "i2c-mux-pinctrl";
		#address-cells = <1>;
		#size-cells = <0>;

		i2c-parent = <&{/i2c@7000c400}>;

		pinctrl-names = "ddc", "pta", "idle";
		pinctrl-0 = <&state_i2cmux_ddc>;
		pinctrl-1 = <&state_i2cmux_pta>;
		pinctrl-2 = <&state_i2cmux_idle>;

		hdmi_ddc: i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};

	pci_vdd_reg: regulator-1v05 {
		compatible = "regulator-fixed";
		regulator-name = "vdd_1v05";
		regulator-min-microvolt = <1050000>;
		regulator-max-microvolt = <1050000>;
		gpio = <&pmic 2 0>;
		enable-active-high;
	};
};
