// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 *  sama7g5.dtsi - Device Tree Include file for SAMA7G5 family SoC
 *
 *  Copyright (C) 2020 Microchip Technology, Inc. and its subsidiaries
 *
 *  Author: Eugen Hristev <eugen.hristev@microchip.com>
 *  Author: Claudiu Beznea <claudiu.beznea@microchip.com>
 *
 */

#include <dt-bindings/iio/adc/at91-sama5d2_adc.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/at91.h>
#include <dt-bindings/dma/at91.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/mfd/at91-usart.h>
#include <dt-bindings/nvmem/microchip,sama7g5-otpc.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	model = "Microchip SAMA7G5 family SoC";
	compatible = "microchip,sama7g5";
	#address-cells = <1>;
	#size-cells = <1>;
	interrupt-parent = <&gic>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x0>;
			clocks = <&pmc PMC_TYPE_CORE PMC_CPUPLL>;
			clock-names = "cpu";
			operating-points-v2 = <&cpu_opp_table>;
			#cooling-cells = <2>; /* min followed by max */
		};
	};

	cpu_opp_table: opp-table {
		compatible = "operating-points-v2";

		opp-90000000 {
			opp-hz = /bits/ 64 <90000000>;
			opp-microvolt = <1050000 1050000 1225000>;
			clock-latency-ns = <320000>;
		};

		opp-250000000 {
			opp-hz = /bits/ 64 <250000000>;
			opp-microvolt = <1050000 1050000 1225000>;
			clock-latency-ns = <320000>;
		};

		opp-600000000 {
			opp-hz = /bits/ 64 <600000000>;
			opp-microvolt = <1050000 1050000 1225000>;
			clock-latency-ns = <320000>;
			opp-suspend;
		};

		opp-800000000 {
			opp-hz = /bits/ 64 <800000000>;
			opp-microvolt = <1150000 1125000 1225000>;
			clock-latency-ns = <320000>;
		};

		opp-1000000002 {
			opp-hz = /bits/ 64 <1000000002>;
			opp-microvolt = <1250000 1225000 1300000>;
			clock-latency-ns = <320000>;
		};
	};

	thermal-zones {
		cpu_thermal: cpu-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&thermal_sensor>;

			trips {
				cpu_normal: cpu-alert0 {
					temperature = <90000>;
					hysteresis = <0>;
					type = "passive";
				};

				cpu_hot: cpu-alert1 {
					temperature = <95000>;
					hysteresis = <0>;
					type = "passive";
				};

				cpu_critical: cpu-critical {
					temperature = <100000>;
					hysteresis = <0>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&cpu_normal>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};

				map1 {
					trip = <&cpu_hot>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};
		};
	};

	clocks {
		slow_xtal: slow_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
		};

		main_xtal: main_xtal {
			compatible = "fixed-clock";
			#clock-cells = <0>;
		};

		usb_clk: usb_clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <48000000>;
		};
	};

	vddout25: fixed-regulator-vddout25 {
		compatible = "regulator-fixed";

		regulator-name = "VDDOUT25";
		regulator-min-microvolt = <2500000>;
		regulator-max-microvolt = <2500000>;
		regulator-boot-on;
		status = "disabled";
	};

	ns_sram: sram@100000 {
		compatible = "mmio-sram";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0x100000 0x20000>;
		ranges;
	};

	thermal_sensor: thermal-sensor {
		compatible = "generic-adc-thermal";
		#thermal-sensor-cells = <0>;
		io-channels = <&adc AT91_SAMA7G5_ADC_TEMP_CHANNEL>;
		io-channel-names = "sensor-channel";
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		nfc_sram: sram@600000 {
			compatible = "mmio-sram";
			no-memory-wc;
			reg = <0x00600000 0x2400>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x00600000 0x2400>;
		};

		nfc_io: nfc-io@10000000 {
			compatible = "atmel,sama5d3-nfc-io", "syscon";
			reg = <0x10000000 0x8000000>;
		};

		ebi: ebi@40000000 {
			compatible = "atmel,sama5d3-ebi";
			#address-cells = <2>;
			#size-cells = <1>;
			atmel,smc = <&hsmc>;
			reg = <0x40000000 0x20000000>;
			ranges = <0x0 0x0 0x40000000 0x8000000
				  0x1 0x0 0x48000000 0x8000000
				  0x2 0x0 0x50000000 0x8000000
				  0x3 0x0 0x58000000 0x8000000>;
			clocks = <&pmc PMC_TYPE_CORE PMC_MCK1>;
			status = "disabled";

			nand_controller: nand-controller {
				compatible = "atmel,sama5d3-nand-controller";
				atmel,nfc-sram = <&nfc_sram>;
				atmel,nfc-io = <&nfc_io>;
				ecc-engine = <&pmecc>;
				#address-cells = <2>;
				#size-cells = <1>;
				ranges;
				status = "disabled";
			};
		};

		securam: sram@e0000000 {
			compatible = "microchip,sama7g5-securam", "atmel,sama5d2-securam", "mmio-sram";
			reg = <0xe0000000 0x4000>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 18>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0xe0000000 0x4000>;
			no-memory-wc;
		};

		secumod: secumod@e0004000 {
			compatible = "microchip,sama7g5-secumod", "atmel,sama5d2-secumod", "syscon";
			reg = <0xe0004000 0x4000>;
			gpio-controller;
			#gpio-cells = <2>;
		};

		sfrbu: sfr@e0008000 {
			compatible = "microchip,sama7g5-sfrbu", "atmel,sama5d2-sfrbu", "syscon";
			reg = <0xe0008000 0x20>;
		};

		pioA: pinctrl@e0014000 {
			compatible = "microchip,sama7g5-pinctrl";
			reg = <0xe0014000 0x800>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-controller;
			#gpio-cells = <2>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 11>;
		};

		pmc: clock-controller@e0018000 {
			compatible = "microchip,sama7g5-pmc", "syscon";
			reg = <0xe0018000 0x200>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			#clock-cells = <2>;
			clocks = <&clk32k 1>, <&clk32k 0>, <&main_xtal>;
			clock-names = "td_slck", "md_slck", "main_xtal";
		};

		reset_controller: reset-controller@e001d000 {
			compatible = "microchip,sama7g5-rstc";
			reg = <0xe001d000 0xc>, <0xe001d0e4 0x4>;
			#reset-cells = <1>;
			clocks = <&clk32k 0>;
		};

		shdwc: poweroff@e001d010 {
			compatible = "microchip,sama7g5-shdwc", "syscon";
			reg = <0xe001d010 0x10>;
			clocks = <&clk32k 0>;
			#address-cells = <1>;
			#size-cells = <0>;
			atmel,wakeup-rtc-timer;
			atmel,wakeup-rtt-timer;
			status = "disabled";
		};

		rtt: rtc@e001d020 {
			compatible = "microchip,sama7g5-rtt", "microchip,sam9x60-rtt", "atmel,at91sam9260-rtt";
			reg = <0xe001d020 0x30>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clk32k 1>;
		};

		clk32k: clock-controller@e001d050 {
			compatible = "microchip,sama7g5-sckc", "microchip,sam9x60-sckc";
			reg = <0xe001d050 0x4>;
			clocks = <&slow_xtal>;
			#clock-cells = <1>;
		};

		gpbr: gpbr@e001d060 {
			compatible = "microchip,sama7g5-gpbr", "syscon";
			reg = <0xe001d060 0x48>;
		};

		rtc: rtc@e001d0a8 {
			compatible = "microchip,sama7g5-rtc", "microchip,sam9x60-rtc";
			reg = <0xe001d0a8 0x30>;
			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clk32k 1>;
		};

		ps_wdt: watchdog@e001d180 {
			compatible = "microchip,sama7g5-wdt";
			reg = <0xe001d180 0x24>;
			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clk32k 0>;
		};

		chipid@e0020000 {
			compatible = "microchip,sama7g5-chipid";
			reg = <0xe0020000 0x8>;
		};

		tcb1: timer@e0800000 {
			compatible = "atmel,sama5d2-tcb", "simple-mfd", "syscon";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xe0800000 0x100>;
			interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 91>, <&pmc PMC_TYPE_PERIPHERAL 92>, <&pmc PMC_TYPE_PERIPHERAL 93>, <&clk32k 1>;
			clock-names = "t0_clk", "t1_clk", "t2_clk", "slow_clk";
		};

		hsmc: hsmc@e0808000 {
			compatible = "atmel,sama5d2-smc", "syscon", "simple-mfd";
			reg = <0xe0808000 0x1000>;
			interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 21>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			pmecc: ecc-engine@e0808070 {
				compatible = "atmel,sama5d2-pmecc";
				reg = <0xe0808070 0x490>,
				      <0xe0808500 0x200>;
			};
		};

		qspi0: spi@e080c000 {
			compatible = "microchip,sama7g5-ospi";
			reg = <0xe080c000 0x400>, <0x20000000 0x10000000>;
			reg-names = "qspi_base", "qspi_mmap";
			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(41)>,
			       <&dma0 AT91_XDMAC_DT_PERID(40)>;
			dma-names = "tx", "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 78>, <&pmc PMC_TYPE_GCK 78>;
			clock-names = "pclk", "gclk";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		qspi1: spi@e0810000 {
			compatible = "microchip,sama7g5-qspi";
			reg = <0xe0810000 0x400>, <0x30000000 0x10000000>;
			reg-names = "qspi_base", "qspi_mmap";
			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(43)>,
			       <&dma0 AT91_XDMAC_DT_PERID(42)>;
			dma-names = "tx", "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 79>, <&pmc PMC_TYPE_GCK 79>;
			clock-names = "pclk", "gclk";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		can0: can@e0828000 {
			compatible = "bosch,m_can";
			reg = <0xe0828000 0x100>, <0x100000 0x7800>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 61>, <&pmc PMC_TYPE_GCK 61>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 61>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0x3400 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		can1: can@e082c000 {
			compatible = "bosch,m_can";
			reg = <0xe082c000 0x100>, <0x100000 0xbc00>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 62>, <&pmc PMC_TYPE_GCK 62>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 62>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0x7800 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		can2: can@e0830000 {
			compatible = "bosch,m_can";
			reg = <0xe0830000 0x100>, <0x100000 0x10000>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 63>, <&pmc PMC_TYPE_GCK 63>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 63>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0xbc00 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		can3: can@e0834000 {
			compatible = "bosch,m_can";
			reg = <0xe0834000 0x100>, <0x110000 0x4400>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 64>, <&pmc PMC_TYPE_GCK 64>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 64>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0x0 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		can4: can@e0838000 {
			compatible = "bosch,m_can";
			reg = <0xe0838000 0x100>, <0x110000 0x8800>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 65>, <&pmc PMC_TYPE_GCK 65>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 65>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0x4400 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		can5: can@e083c000 {
			compatible = "bosch,m_can";
			reg = <0xe083c000 0x100>, <0x110000 0xcc00>;
			reg-names = "m_can", "message_ram";
			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "int0", "int1";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 66>, <&pmc PMC_TYPE_GCK 66>;
			clock-names = "hclk", "cclk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 66>;
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clock-rates = <40000000>;
			bosch,mram-cfg = <0x8800 0 0 64 0 0 32 32>;
			status = "disabled";
		};

		adc: adc@e1000000 {
			compatible = "microchip,sama7g5-adc";
			reg = <0xe1000000 0x200>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_GCK 26>;
			assigned-clocks = <&pmc PMC_TYPE_GCK 26>;
			assigned-clock-rates = <100000000>;
			clock-names = "adc_clk";
			dmas = <&dma0 AT91_XDMAC_DT_PERID(0)>;
			dma-names = "rx";
			atmel,min-sample-rate-hz = <200000>;
			atmel,max-sample-rate-hz = <20000000>;
			atmel,startup-time-ms = <4>;
			#io-channel-cells = <1>;
			nvmem-cells = <&temperature_calib>;
			nvmem-cell-names = "temperature_calib";
			status = "disabled";
		};

		sdmmc0: mmc@e1204000 {
			compatible = "microchip,sama7g5-sdhci", "microchip,sam9x60-sdhci";
			reg = <0xe1204000 0x4000>;
			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 80>, <&pmc PMC_TYPE_GCK 80>;
			clock-names = "hclock", "multclk";
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clocks = <&pmc PMC_TYPE_GCK 80>;
			assigned-clock-rates = <200000000>;
			microchip,sdcal-inverted;
			status = "disabled";
		};

		sdmmc1: mmc@e1208000 {
			compatible = "microchip,sama7g5-sdhci", "microchip,sam9x60-sdhci";
			reg = <0xe1208000 0x4000>;
			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 81>, <&pmc PMC_TYPE_GCK 81>;
			clock-names = "hclock", "multclk";
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clocks = <&pmc PMC_TYPE_GCK 81>;
			assigned-clock-rates = <200000000>;
			microchip,sdcal-inverted;
			status = "disabled";
		};

		sdmmc2: mmc@e120c000 {
			compatible = "microchip,sama7g5-sdhci", "microchip,sam9x60-sdhci";
			reg = <0xe120c000 0x4000>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 82>, <&pmc PMC_TYPE_GCK 82>;
			clock-names = "hclock", "multclk";
			assigned-clock-parents = <&pmc PMC_TYPE_CORE PMC_SYSPLL>;
			assigned-clocks = <&pmc PMC_TYPE_GCK 82>;
			assigned-clock-rates = <200000000>;
			microchip,sdcal-inverted;
			status = "disabled";
		};

		csi2dc: csi2dc@e1404000 {
			compatible = "microchip,sama7g5-csi2dc";
			reg = <0xe1404000 0x500>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 34>, <&xisc>;
			clock-names = "pclk", "scck";
			assigned-clocks = <&xisc>;
			assigned-clock-rates = <266000000>;
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;
				port@0 {
					reg = <0>;
					csi2dc_in: endpoint {
					};
				};

				port@1 {
					reg = <1>;
					csi2dc_out: endpoint {
						bus-width = <14>;
						hsync-active = <1>;
						vsync-active = <1>;
						remote-endpoint = <&xisc_in>;
					};
				};
			};
		};

		xisc: xisc@e1408000 {
			compatible = "microchip,sama7g5-isc";
			reg = <0xe1408000 0x2000>;
			interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 56>;
			clock-names = "hclock";
			#clock-cells = <0>;
			clock-output-names = "isc-mck";
			status = "disabled";

			port {
				xisc_in: endpoint {
					bus-type = <5>; /* Parallel */
					bus-width = <14>;
					hsync-active = <1>;
					vsync-active = <1>;
					remote-endpoint = <&csi2dc_out>;
				};
			};
		};

		pwm: pwm@e1604000 {
			compatible = "microchip,sama7g5-pwm", "atmel,sama5d2-pwm";
			reg = <0xe1604000 0x4000>;
			interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
			#pwm-cells = <3>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 77>;
			status = "disabled";
		};

		pdmc0: sound@e1608000 {
			compatible = "microchip,sama7g5-pdmc";
			reg = <0xe1608000 0x1000>;
			interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
			#sound-dai-cells = <0>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(37)>;
			dma-names = "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 68>, <&pmc PMC_TYPE_GCK 68>;
			clock-names = "pclk", "gclk";
			status = "disabled";
		};

		pdmc1: sound@e160c000 {
			compatible = "microchip,sama7g5-pdmc";
			reg = <0xe160c000 0x1000>;
			interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
			#sound-dai-cells = <0>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(38)>;
			dma-names = "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 69>, <&pmc PMC_TYPE_GCK 69>;
			clock-names = "pclk", "gclk";
			status = "disabled";
		};

		spdifrx: spdifrx@e1614000 {
			#sound-dai-cells = <0>;
			compatible = "microchip,sama7g5-spdifrx";
			reg = <0xe1614000 0x4000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(49)>;
			dma-names = "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 84>, <&pmc PMC_TYPE_GCK 84>;
			clock-names = "pclk", "gclk";
			status = "disabled";
		};

		spdiftx: spdiftx@e1618000 {
			#sound-dai-cells = <0>;
			compatible = "microchip,sama7g5-spdiftx";
			reg = <0xe1618000 0x4000>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(50)>;
			dma-names = "tx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 85>, <&pmc PMC_TYPE_GCK 85>;
			clock-names = "pclk", "gclk";
		};

		i2s0: i2s@e161c000 {
			compatible = "microchip,sama7g5-i2smcc";
			#sound-dai-cells = <0>;
			reg = <0xe161c000 0x4000>;
			interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(34)>, <&dma0 AT91_XDMAC_DT_PERID(33)>;
			dma-names = "tx", "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 57>, <&pmc PMC_TYPE_GCK 57>;
			clock-names = "pclk", "gclk";
			status = "disabled";
		};

		i2s1: i2s@e1620000 {
			compatible = "microchip,sama7g5-i2smcc";
			#sound-dai-cells = <0>;
			reg = <0xe1620000 0x4000>;
			interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dma0 AT91_XDMAC_DT_PERID(36)>, <&dma0 AT91_XDMAC_DT_PERID(35)>;
			dma-names = "tx", "rx";
			clocks = <&pmc PMC_TYPE_PERIPHERAL 58>, <&pmc PMC_TYPE_GCK 58>;
			clock-names = "pclk", "gclk";
			status = "disabled";
		};

		eic: interrupt-controller@e1628000 {
			compatible = "microchip,sama7g5-eic";
			reg = <0xe1628000 0xec>;
			interrupt-parent = <&gic>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 37>;
			clock-names = "pclk";
			status = "disabled";
		};

		pit64b0: timer@e1800000 {
			compatible = "microchip,sama7g5-pit64b", "microchip,sam9x60-pit64b";
			reg = <0xe1800000 0x4000>;
			interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 70>, <&pmc PMC_TYPE_GCK 70>;
			clock-names = "pclk", "gclk";
		};

		pit64b1: timer@e1804000 {
			compatible = "microchip,sama7g5-pit64b", "microchip,sam9x60-pit64b";
			reg = <0xe1804000 0x4000>;
			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 71>, <&pmc PMC_TYPE_GCK 71>;
			clock-names = "pclk", "gclk";
		};

		aes: crypto@e1810000 {
			compatible = "atmel,at91sam9g46-aes";
			reg = <0xe1810000 0x100>;
			interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 27>;
			clock-names = "aes_clk";
			dmas = <&dma0 AT91_XDMAC_DT_PERID(1)>,
			       <&dma0 AT91_XDMAC_DT_PERID(2)>;
			dma-names = "tx", "rx";
		};

		sha: crypto@e1814000 {
			compatible = "atmel,at91sam9g46-sha";
			reg = <0xe1814000 0x100>;
			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 83>;
			clock-names = "sha_clk";
			dmas = <&dma0 AT91_XDMAC_DT_PERID(48)>;
			dma-names = "tx";
		};

		flx0: flexcom@e1818000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe1818000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 38>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe1818000 0x800>;
			status = "disabled";

			uart0: serial@200 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0x200 0x200>;
				atmel,usart-mode = <AT91_USART_MODE_SERIAL>;
				interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 38>;
				clock-names = "usart";
				dmas = <&dma1 AT91_XDMAC_DT_PERID(6)>,
				       <&dma1 AT91_XDMAC_DT_PERID(5)>;
				dma-names = "tx", "rx";
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				status = "disabled";
			};
		};

		flx1: flexcom@e181c000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe181c000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 39>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe181c000 0x800>;
			status = "disabled";

			i2c1: i2c@600 {
				compatible = "microchip,sama7g5-i2c", "microchip,sam9x60-i2c";
				reg = <0x600 0x200>;
				interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 39>;
				atmel,fifo-size = <32>;
				dmas = <&dma0 AT91_XDMAC_DT_PERID(8)>,
				       <&dma0 AT91_XDMAC_DT_PERID(7)>;
				dma-names = "tx", "rx";
				status = "disabled";
			};
		};

		flx3: flexcom@e1824000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe1824000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 41>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe1824000 0x800>;
			status = "disabled";

			uart3: serial@200 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0x200 0x200>;
				atmel,usart-mode = <AT91_USART_MODE_SERIAL>;
				interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 41>;
				clock-names = "usart";
				dmas = <&dma1 AT91_XDMAC_DT_PERID(12)>,
				       <&dma1 AT91_XDMAC_DT_PERID(11)>;
				dma-names = "tx", "rx";
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				status = "disabled";
			};
		};

		trng: rng@e2010000 {
			compatible = "microchip,sama7g5-trng", "atmel,at91sam9g45-trng";
			reg = <0xe2010000 0x100>;
			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 97>;
			status = "disabled";
		};

		tdes: crypto@e2014000 {
			compatible = "atmel,at91sam9g46-tdes";
			reg = <0xe2014000 0x100>;
			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 96>;
			clock-names = "tdes_clk";
			dmas = <&dma0 AT91_XDMAC_DT_PERID(54)>,
			       <&dma0 AT91_XDMAC_DT_PERID(53)>;
			dma-names = "tx", "rx";
		};

		flx4: flexcom@e2018000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe2018000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 42>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe2018000 0x800>;
			status = "disabled";

			uart4: serial@200 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0x200 0x200>;
				atmel,usart-mode = <AT91_USART_MODE_SERIAL>;
				interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 42>;
				clock-names = "usart";
				dmas = <&dma1 AT91_XDMAC_DT_PERID(14)>,
				       <&dma1 AT91_XDMAC_DT_PERID(13)>;
				dma-names = "tx", "rx";
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				atmel,fifo-size = <32>;
				status = "disabled";
			};
		};

		flx7: flexcom@e2024000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe2024000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 45>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe2024000 0x800>;
			status = "disabled";

			uart7: serial@200 {
				compatible = "atmel,at91sam9260-usart";
				reg = <0x200 0x200>;
				atmel,usart-mode = <AT91_USART_MODE_SERIAL>;
				interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 45>;
				clock-names = "usart";
				dmas = <&dma1 AT91_XDMAC_DT_PERID(20)>,
				       <&dma1 AT91_XDMAC_DT_PERID(19)>;
				dma-names = "tx", "rx";
				atmel,use-dma-rx;
				atmel,use-dma-tx;
				atmel,fifo-size = <32>;
				status = "disabled";
			};
		};

		gmac0: ethernet@e2800000 {
			compatible = "microchip,sama7g5-gem";
			reg = <0xe2800000 0x1000>;
			interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 51>, <&pmc PMC_TYPE_PERIPHERAL 51>, <&pmc PMC_TYPE_GCK 51>, <&pmc PMC_TYPE_GCK 53>;
			clock-names = "pclk", "hclk", "tx_clk", "tsu_clk";
			assigned-clocks = <&pmc PMC_TYPE_GCK 51>;
			assigned-clock-rates = <125000000>;
			status = "disabled";
		};

		gmac1: ethernet@e2804000 {
			compatible = "microchip,sama7g5-emac";
			reg = <0xe2804000 0x1000>;
			interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 52>, <&pmc PMC_TYPE_PERIPHERAL 52>;
			clock-names = "pclk", "hclk";
			status = "disabled";
		};

		dma0: dma-controller@e2808000 {
			compatible = "microchip,sama7g5-dma";
			reg = <0xe2808000 0x1000>;
			interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
			#dma-cells = <1>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 22>;
			clock-names = "dma_clk";
			status = "disabled";
		};

		dma1: dma-controller@e280c000 {
			compatible = "microchip,sama7g5-dma";
			reg = <0xe280c000 0x1000>;
			interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>;
			#dma-cells = <1>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 23>;
			clock-names = "dma_clk";
			status = "disabled";
		};

		/* Place dma2 here despite it's address */
		dma2: dma-controller@e1200000 {
			compatible = "microchip,sama7g5-dma";
			reg = <0xe1200000 0x1000>;
			interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
			#dma-cells = <1>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 24>;
			clock-names = "dma_clk";
			dma-requests = <0>;
			status = "disabled";
		};

		tcb0: timer@e2814000 {
			compatible = "atmel,sama5d2-tcb", "simple-mfd", "syscon";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xe2814000 0x100>;
			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 88>, <&pmc PMC_TYPE_PERIPHERAL 89>, <&pmc PMC_TYPE_PERIPHERAL 90>, <&clk32k 1>;
			clock-names = "t0_clk", "t1_clk", "t2_clk", "slow_clk";
		};

		flx8: flexcom@e2818000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe2818000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 46>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe2818000 0x800>;
			status = "disabled";

			i2c8: i2c@600 {
				compatible = "microchip,sama7g5-i2c", "microchip,sam9x60-i2c";
				reg = <0x600 0x200>;
				interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 46>;
				atmel,fifo-size = <32>;
				dmas = <&dma0 AT91_XDMAC_DT_PERID(22)>,
				       <&dma0 AT91_XDMAC_DT_PERID(21)>;
				dma-names = "tx", "rx";
				status = "disabled";
			};
		};

		flx9: flexcom@e281c000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe281c000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 47>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe281c000 0x800>;
			status = "disabled";

			i2c9: i2c@600 {
				compatible = "microchip,sama7g5-i2c", "microchip,sam9x60-i2c";
				reg = <0x600 0x200>;
				interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 47>;
				atmel,fifo-size = <32>;
				dmas = <&dma0 AT91_XDMAC_DT_PERID(24)>,
				       <&dma0 AT91_XDMAC_DT_PERID(23)>;
				dma-names = "tx", "rx";
				status = "disabled";
			};
		};

		flx10: flexcom@e2820000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe2820000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 48>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe2820000 0x800>;
			status = "disabled";

			i2c10: i2c@600 {
				compatible = "microchip,sama7g5-i2c", "microchip,sam9x60-i2c";
				reg = <0x600 0x200>;
				interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 48>;
				atmel,fifo-size = <32>;
				dmas = <&dma0 AT91_XDMAC_DT_PERID(26)>,
				       <&dma0 AT91_XDMAC_DT_PERID(25)>;
				dma-names = "tx", "rx";
				status = "disabled";
			};
		};

		flx11: flexcom@e2824000 {
			compatible = "microchip,sama7g5-flexcom", "atmel,sama5d2-flexcom";
			reg = <0xe2824000 0x200>;
			clocks = <&pmc PMC_TYPE_PERIPHERAL 49>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe2824000 0x800>;
			status = "disabled";

			spi11: spi@400 {
				compatible = "atmel,at91rm9200-spi";
				reg = <0x400 0x200>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&pmc PMC_TYPE_PERIPHERAL 49>;
				clock-names = "spi_clk";
				#address-cells = <1>;
				#size-cells = <0>;
				atmel,fifo-size = <32>;
				dmas = <&dma0 AT91_XDMAC_DT_PERID(28)>,
				       <&dma0 AT91_XDMAC_DT_PERID(27)>;
				dma-names = "tx", "rx";
				status = "disabled";
			};
		};

		uddrc: uddrc@e3800000 {
			compatible = "microchip,sama7g5-uddrc";
			reg = <0xe3800000 0x4000>;
		};

		ddr3phy: ddr3phy@e3804000 {
			compatible = "microchip,sama7g5-ddr3phy";
			reg = <0xe3804000 0x1000>;
		};

		otpc: efuse@e8c00000 {
			compatible = "microchip,sama7g5-otpc", "syscon";
			reg = <0xe8c00000 0x100>;
			#address-cells = <1>;
			#size-cells = <1>;

			temperature_calib: calib@1 {
				reg = <OTP_PKT(1) 76>;
			};
		};

		gic: interrupt-controller@e8c11000 {
			compatible = "arm,cortex-a7-gic";
			#interrupt-cells = <3>;
			#address-cells = <0>;
			interrupt-controller;
			reg = <0xe8c11000 0x1000>,
				<0xe8c12000 0x2000>;
		};
	};
};
