// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright Altera Corporation (C) 2014. All rights reserved.
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/reset/altr,rst-mgr-a10.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "altr,socfpga-a10-smp";

		cpu0: cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
		};
		cpu1: cpu@1 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
		};
	};

	pmu: pmu@ff111000 {
		compatible = "arm,cortex-a9-pmu";
		interrupt-parent = <&intc>;
		interrupts = <0 124 4>, <0 125 4>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
		reg = <0xff111000 0x1000>,
		      <0xff113000 0x1000>;
	};

	intc: interrupt-controller@ffffd000 {
		compatible = "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0xffffd000 0x1000>,
		      <0xffffc100 0x100>;
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		device_type = "soc";
		interrupt-parent = <&intc>;
		ranges;

		amba {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			pdma: pdma@ffda1000 {
				compatible = "arm,pl330", "arm,primecell";
				reg = <0xffda1000 0x1000>;
				interrupts = <0 83 IRQ_TYPE_LEVEL_HIGH>,
					     <0 84 IRQ_TYPE_LEVEL_HIGH>,
					     <0 85 IRQ_TYPE_LEVEL_HIGH>,
					     <0 86 IRQ_TYPE_LEVEL_HIGH>,
					     <0 87 IRQ_TYPE_LEVEL_HIGH>,
					     <0 88 IRQ_TYPE_LEVEL_HIGH>,
					     <0 89 IRQ_TYPE_LEVEL_HIGH>,
					     <0 90 IRQ_TYPE_LEVEL_HIGH>,
					     <0 91 IRQ_TYPE_LEVEL_HIGH>;
				#dma-cells = <1>;
				clocks = <&l4_main_clk>;
				clock-names = "apb_pclk";
				resets = <&rst DMA_RESET>, <&rst DMA_OCP_RESET>;
				reset-names = "dma", "dma-ocp";
			};
		};

		base_fpga_region {
			#address-cells = <0x1>;
			#size-cells = <0x1>;

			compatible = "fpga-region";
			fpga-mgr = <&fpga_mgr>;
		};

		clkmgr@ffd04000 {
				compatible = "altr,clk-mgr";
				reg = <0xffd04000 0x1000>;

				clocks {
					#address-cells = <1>;
					#size-cells = <0>;

					cb_intosc_hs_div2_clk: cb_intosc_hs_div2_clk {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					cb_intosc_ls_clk: cb_intosc_ls_clk {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					f2s_free_clk: f2s_free_clk {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					osc1: osc1 {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					main_pll: main_pll@40 {
						#address-cells = <1>;
						#size-cells = <0>;
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-pll-clock";
						clocks = <&osc1>, <&cb_intosc_ls_clk>,
							 <&f2s_free_clk>;
						reg = <0x40>;

						main_mpu_base_clk: main_mpu_base_clk {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							div-reg = <0x140 0 11>;
						};

						main_noc_base_clk: main_noc_base_clk {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							div-reg = <0x144 0 11>;
						};

						main_emaca_clk: main_emaca_clk@68 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x68>;
						};

						main_emacb_clk: main_emacb_clk@6c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x6C>;
						};

						main_emac_ptp_clk: main_emac_ptp_clk@70 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x70>;
						};

						main_gpio_db_clk: main_gpio_db_clk@74 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x74>;
						};

						main_sdmmc_clk: main_sdmmc_clk@78 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk"
;
							clocks = <&main_pll>;
							reg = <0x78>;
						};

						main_s2f_usr0_clk: main_s2f_usr0_clk@7c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x7C>;
						};

						main_s2f_usr1_clk: main_s2f_usr1_clk@80 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x80>;
						};

						main_hmc_pll_ref_clk: main_hmc_pll_ref_clk@84 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x84>;
						};

						main_periph_ref_clk: main_periph_ref_clk@9c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&main_pll>;
							reg = <0x9C>;
						};
					};

					periph_pll: periph_pll@c0 {
						#address-cells = <1>;
						#size-cells = <0>;
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-pll-clock";
						clocks = <&osc1>, <&cb_intosc_ls_clk>,
							 <&f2s_free_clk>, <&main_periph_ref_clk>;
						reg = <0xC0>;

						peri_mpu_base_clk: peri_mpu_base_clk {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							div-reg = <0x140 16 11>;
						};

						peri_noc_base_clk: peri_noc_base_clk {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							div-reg = <0x144 16 11>;
						};

						peri_emaca_clk: peri_emaca_clk@e8 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xE8>;
						};

						peri_emacb_clk: peri_emacb_clk@ec {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xEC>;
						};

						peri_emac_ptp_clk: peri_emac_ptp_clk@f0 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xF0>;
						};

						peri_gpio_db_clk: peri_gpio_db_clk@f4 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xF4>;
						};

						peri_sdmmc_clk: peri_sdmmc_clk@f8 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xF8>;
						};

						peri_s2f_usr0_clk: peri_s2f_usr0_clk@fc {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0xFC>;
						};

						peri_s2f_usr1_clk: peri_s2f_usr1_clk@100 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x100>;
						};

						peri_hmc_pll_ref_clk: peri_hmc_pll_ref_clk@104 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-a10-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x104>;
						};
					};

					mpu_free_clk: mpu_free_clk@60 {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-perip-clk";
						clocks = <&main_mpu_base_clk>, <&peri_mpu_base_clk>,
							 <&osc1>, <&cb_intosc_hs_div2_clk>,
							 <&f2s_free_clk>;
						reg = <0x60>;
					};

					noc_free_clk: noc_free_clk@64 {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-perip-clk";
						clocks = <&main_noc_base_clk>, <&peri_noc_base_clk>,
							 <&osc1>, <&cb_intosc_hs_div2_clk>,
							 <&f2s_free_clk>;
						reg = <0x64>;
					};

					s2f_user1_free_clk: s2f_user1_free_clk@104 {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-perip-clk";
						clocks = <&main_s2f_usr1_clk>, <&peri_s2f_usr1_clk>,
							 <&osc1>, <&cb_intosc_hs_div2_clk>,
							 <&f2s_free_clk>;
						reg = <0x104>;
					};

					sdmmc_free_clk: sdmmc_free_clk@f8 {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-perip-clk";
						clocks = <&main_sdmmc_clk>, <&peri_sdmmc_clk>,
							 <&osc1>, <&cb_intosc_hs_div2_clk>,
							 <&f2s_free_clk>;
						fixed-divider = <4>;
						reg = <0xF8>;
					};

					l4_sys_free_clk: l4_sys_free_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-perip-clk";
						clocks = <&noc_free_clk>;
						fixed-divider = <4>;
					};

					l4_main_clk: l4_main_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&noc_free_clk>;
						div-reg = <0xA8 0 2>;
						clk-gate = <0x48 1>;
					};

					l4_mp_clk: l4_mp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&noc_free_clk>;
						div-reg = <0xA8 8 2>;
						clk-gate = <0x48 2>;
					};

					l4_sp_clk: l4_sp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&noc_free_clk>;
						div-reg = <0xA8 16 2>;
						clk-gate = <0x48 3>;
					};

					mpu_periph_clk: mpu_periph_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&mpu_free_clk>;
						fixed-divider = <4>;
						clk-gate = <0x48 0>;
					};

					sdmmc_clk: sdmmc_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&sdmmc_free_clk>;
						clk-gate = <0xC8 5>;
					};

					qspi_clk: qspi_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&l4_main_clk>;
						clk-gate = <0xC8 11>;
					};

					nand_x_clk: nand_x_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&l4_mp_clk>;
						clk-gate = <0xC8 10>;
					};

					nand_ecc_clk: nand_ecc_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&nand_x_clk>;
						clk-gate = <0xC8 10>;
					};

					nand_clk: nand_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&nand_x_clk>;
						fixed-divider = <4>;
						clk-gate = <0xC8 10>;
					};

					spi_m_clk: spi_m_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&l4_main_clk>;
						clk-gate = <0xC8 9>;
					};

					usb_clk: usb_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&l4_mp_clk>;
						clk-gate = <0xC8 8>;
					};

					s2f_usr1_clk: s2f_usr1_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-a10-gate-clk";
						clocks = <&peri_s2f_usr1_clk>;
						clk-gate = <0xC8 6>;
					};
				};
		};

		socfpga_axi_setup: stmmac-axi-config {
			snps,wr_osr_lmt = <0xf>;
			snps,rd_osr_lmt = <0xf>;
			snps,blen = <0 0 0 0 16 0 0>;
		};

		gmac0: ethernet@ff800000 {
			compatible = "altr,socfpga-stmmac-a10-s10", "snps,dwmac-3.72a", "snps,dwmac";
			altr,sysmgr-syscon = <&sysmgr 0x44 0>;
			reg = <0xff800000 0x2000>;
			interrupts = <0 92 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";
			/* Filled in by bootloader */
			mac-address = [00 00 00 00 00 00];
			snps,multicast-filter-bins = <256>;
			snps,perfect-filter-entries = <128>;
			tx-fifo-depth = <4096>;
			rx-fifo-depth = <16384>;
			clocks = <&l4_mp_clk>, <&peri_emac_ptp_clk>;
			clock-names = "stmmaceth", "ptp_ref";
			resets = <&rst EMAC0_RESET>, <&rst EMAC0_OCP_RESET>;
			reset-names = "stmmaceth", "stmmaceth-ocp";
			snps,axi-config = <&socfpga_axi_setup>;
			status = "disabled";
		};

		gmac1: ethernet@ff802000 {
			compatible = "altr,socfpga-stmmac-a10-s10", "snps,dwmac-3.72a", "snps,dwmac";
			altr,sysmgr-syscon = <&sysmgr 0x48 8>;
		        reg = <0xff802000 0x2000>;
			interrupts = <0 93 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";
			/* Filled in by bootloader */
			mac-address = [00 00 00 00 00 00];
			snps,multicast-filter-bins = <256>;
			snps,perfect-filter-entries = <128>;
			tx-fifo-depth = <4096>;
			rx-fifo-depth = <16384>;
			clocks = <&l4_mp_clk>, <&peri_emac_ptp_clk>;
			clock-names = "stmmaceth", "ptp_ref";
			resets = <&rst EMAC1_RESET>, <&rst EMAC1_OCP_RESET>;
			reset-names = "stmmaceth", "stmmaceth-ocp";
			snps,axi-config = <&socfpga_axi_setup>;
			status = "disabled";
		};

		gmac2: ethernet@ff804000 {
			compatible = "altr,socfpga-stmmac-a10-s10", "snps,dwmac-3.72a", "snps,dwmac";
			altr,sysmgr-syscon = <&sysmgr 0x4C 16>;
			reg = <0xff804000 0x2000>;
			interrupts = <0 94 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";
			/* Filled in by bootloader */
			mac-address = [00 00 00 00 00 00];
			snps,multicast-filter-bins = <256>;
			snps,perfect-filter-entries = <128>;
			tx-fifo-depth = <4096>;
			rx-fifo-depth = <16384>;
			clocks = <&l4_mp_clk>, <&peri_emac_ptp_clk>;
			clock-names = "stmmaceth", "ptp_ref";
			resets = <&rst EMAC2_RESET>, <&rst EMAC2_OCP_RESET>;
			reset-names = "stmmaceth", "stmmaceth-ocp";
			snps,axi-config = <&socfpga_axi_setup>;
			status = "disabled";
		};

		gpio0: gpio@ffc02900 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xffc02900 0x100>;
			resets = <&rst GPIO0_RESET>;
			status = "disabled";

			porta: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <29>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 112 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		gpio1: gpio@ffc02a00 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xffc02a00 0x100>;
			resets = <&rst GPIO1_RESET>;
			status = "disabled";

			portb: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <29>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 113 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		gpio2: gpio@ffc02b00 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xffc02b00 0x100>;
			resets = <&rst GPIO2_RESET>;
			status = "disabled";

			portc: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <27>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 114 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		fpga_mgr: fpga-mgr@ffd03000 {
			compatible = "altr,socfpga-a10-fpga-mgr";
			reg = <0xffd03000 0x100
			       0xffcfe400 0x20>;
			clocks = <&l4_mp_clk>;
			resets = <&rst FPGAMGR_RESET>;
			reset-names = "fpgamgr";
		};

		i2c0: i2c@ffc02200 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02200 0x100>;
			interrupts = <0 105 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sp_clk>;
			resets = <&rst I2C0_RESET>;
			status = "disabled";
		};

		i2c1: i2c@ffc02300 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02300 0x100>;
			interrupts = <0 106 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sp_clk>;
			resets = <&rst I2C1_RESET>;
			status = "disabled";
		};

		i2c2: i2c@ffc02400 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02400 0x100>;
			interrupts = <0 107 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sp_clk>;
			resets = <&rst I2C2_RESET>;
			status = "disabled";
		};

		i2c3: i2c@ffc02500 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02500 0x100>;
			interrupts = <0 108 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sp_clk>;
			resets = <&rst I2C3_RESET>;
			status = "disabled";
		};

		i2c4: i2c@ffc02600 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02600 0x100>;
			interrupts = <0 109 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sp_clk>;
			resets = <&rst I2C4_RESET>;
			status = "disabled";
		};

		spi0: spi@ffda4000 {
			compatible = "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xffda4000 0x100>;
			interrupts = <0 101 4>;
			num-cs = <4>;
			/*32bit_access;*/
			clocks = <&spi_m_clk>;
			resets = <&rst SPIM0_RESET>;
			reset-names = "spi";
			status = "disabled";
		};

		spi1: spi@ffda5000 {
			compatible = "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xffda5000 0x100>;
			interrupts = <0 102 4>;
			num-cs = <4>;
			/*32bit_access;*/
			tx-dma-channel = <&pdma 16>;
			rx-dma-channel = <&pdma 17>;
			clocks = <&spi_m_clk>;
			resets = <&rst SPIM1_RESET>;
			reset-names = "spi";
			status = "disabled";
		};

		sdr: sdr@ffcfb100 {
			compatible = "altr,sdr-ctl", "syscon";
			reg = <0xffcfb100 0x80>;
		};

		L2: cache-controller@fffff000 {
			compatible = "arm,pl310-cache";
			reg = <0xfffff000 0x1000>;
			interrupts = <0 18 IRQ_TYPE_LEVEL_HIGH>;
			cache-unified;
			cache-level = <2>;
			prefetch-data = <1>;
			prefetch-instr = <1>;
			arm,shared-override;
		};

		mmc: mmc@ff808000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "altr,socfpga-dw-mshc";
			reg = <0xff808000 0x1000>;
			interrupts = <0 98 IRQ_TYPE_LEVEL_HIGH>;
			fifo-depth = <0x400>;
			clocks = <&l4_mp_clk>, <&sdmmc_clk>;
			clock-names = "biu", "ciu";
			resets = <&rst SDMMC_RESET>;
			altr,sysmgr-syscon = <&sysmgr 0x28 4>;
			status = "disabled";
		};

		nand: nand-controller@ffb90000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "altr,socfpga-denali-nand";
			reg = <0xffb90000 0x72000>,
			      <0xffb80000 0x10000>;
			reg-names = "nand_data", "denali_reg";
			interrupts = <0 99 4>;
			clocks = <&nand_clk>, <&nand_x_clk>, <&nand_ecc_clk>;
			clock-names = "nand", "nand_x", "ecc";
			resets = <&rst NAND_RESET>;
			status = "disabled";
		};

		ocram: sram@ffe00000 {
			compatible = "mmio-sram";
			reg = <0xffe00000 0x40000>;
		};

		eccmgr: eccmgr {
			compatible = "altr,socfpga-a10-ecc-manager";
			altr,sysmgr-syscon = <&sysmgr>;
			#address-cells = <1>;
			#size-cells = <1>;
			interrupts = <0 2 IRQ_TYPE_LEVEL_HIGH>,
				     <0 0 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			ranges;

			sdramedac {
				compatible = "altr,sdram-edac-a10";
				altr,sdr-syscon = <&sdr>;
				interrupts = <17 IRQ_TYPE_LEVEL_HIGH>,
					     <49 IRQ_TYPE_LEVEL_HIGH>;
			};

			l2-ecc@ffd06010 {
				compatible = "altr,socfpga-a10-l2-ecc";
				reg = <0xffd06010 0x4>;
				interrupts = <0 IRQ_TYPE_LEVEL_HIGH>,
					     <32 IRQ_TYPE_LEVEL_HIGH>;
			};

			ocram-ecc@ff8c3000 {
				compatible = "altr,socfpga-a10-ocram-ecc";
				reg = <0xff8c3000 0x400>;
				interrupts = <1 IRQ_TYPE_LEVEL_HIGH>,
					     <33 IRQ_TYPE_LEVEL_HIGH>;
			};

			emac0-rx-ecc@ff8c0800 {
				compatible = "altr,socfpga-eth-mac-ecc";
				reg = <0xff8c0800 0x400>;
				altr,ecc-parent = <&gmac0>;
				interrupts = <4 IRQ_TYPE_LEVEL_HIGH>,
					     <36 IRQ_TYPE_LEVEL_HIGH>;
			};

			emac0-tx-ecc@ff8c0c00 {
				compatible = "altr,socfpga-eth-mac-ecc";
				reg = <0xff8c0c00 0x400>;
				altr,ecc-parent = <&gmac0>;
				interrupts = <5 IRQ_TYPE_LEVEL_HIGH>,
					     <37 IRQ_TYPE_LEVEL_HIGH>;
			};

			sdmmca-ecc@ff8c2c00 {
				compatible = "altr,socfpga-sdmmc-ecc";
				reg = <0xff8c2c00 0x400>;
				altr,ecc-parent = <&mmc>;
				interrupts = <15 IRQ_TYPE_LEVEL_HIGH>,
					     <47 IRQ_TYPE_LEVEL_HIGH>,
					     <16 IRQ_TYPE_LEVEL_HIGH>,
					     <48 IRQ_TYPE_LEVEL_HIGH>;
			};

			dma-ecc@ff8c8000 {
				compatible = "altr,socfpga-dma-ecc";
				reg = <0xff8c8000 0x400>;
				altr,ecc-parent = <&pdma>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH>,
					     <42 IRQ_TYPE_LEVEL_HIGH>;
			};

			usb0-ecc@ff8c8800 {
				compatible = "altr,socfpga-usb-ecc";
				reg = <0xff8c8800 0x400>;
				altr,ecc-parent = <&usb0>;
				interrupts = <2 IRQ_TYPE_LEVEL_HIGH>,
					     <34 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		qspi: spi@ff809000 {
			compatible = "intel,socfpga-qspi", "cdns,qspi-nor";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xff809000 0x100>,
			      <0xffa00000 0x100000>;
			interrupts = <0 100 IRQ_TYPE_LEVEL_HIGH>;
			cdns,fifo-depth = <128>;
			cdns,fifo-width = <4>;
			cdns,trigger-address = <0x00000000>;
			clocks = <&qspi_clk>;
			resets = <&rst QSPI_RESET>, <&rst QSPI_OCP_RESET>;
			reset-names = "qspi", "qspi-ocp";
			status = "disabled";
		};

		rst: rstmgr@ffd05000 {
			#reset-cells = <1>;
			compatible = "altr,rst-mgr";
			reg = <0xffd05000 0x100>;
			altr,modrst-offset = <0x20>;
		};

		scu: snoop-control-unit@ffffc000 {
			compatible = "arm,cortex-a9-scu";
			reg = <0xffffc000 0x100>;
		};

		sysmgr: sysmgr@ffd06000 {
			compatible = "altr,sys-mgr", "syscon";
			reg = <0xffd06000 0x300>;
			cpu1-start-addr = <0xffd06230>;
		};

		/* Local timer */
		timer@ffffc600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0xffffc600 0x100>;
			interrupts = <1 13 0xf01>;
			clocks = <&mpu_periph_clk>;
		};

		timer0: timer0@ffc02700 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 115 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0xffc02700 0x100>;
			clocks = <&l4_sp_clk>;
			clock-names = "timer";
			resets = <&rst SPTIMER0_RESET>;
			reset-names = "timer";
		};

		timer1: timer1@ffc02800 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 116 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0xffc02800 0x100>;
			clocks = <&l4_sp_clk>;
			clock-names = "timer";
			resets = <&rst SPTIMER1_RESET>;
			reset-names = "timer";
		};

		timer2: timer2@ffd00000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 117 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0xffd00000 0x100>;
			clocks = <&l4_sys_free_clk>;
			clock-names = "timer";
			resets = <&rst L4SYSTIMER0_RESET>;
			reset-names = "timer";
		};

		timer3: timer3@ffd00100 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 118 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0xffd00100 0x100>;
			clocks = <&l4_sys_free_clk>;
			clock-names = "timer";
			resets = <&rst L4SYSTIMER1_RESET>;
			reset-names = "timer";
		};

		uart0: serial@ffc02000 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc02000 0x100>;
			interrupts = <0 110 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&l4_sp_clk>;
			resets = <&rst UART0_RESET>;
			status = "disabled";
		};

		uart1: serial@ffc02100 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc02100 0x100>;
			interrupts = <0 111 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&l4_sp_clk>;
			resets = <&rst UART1_RESET>;
			status = "disabled";
		};

		usbphy0: usbphy {
			#phy-cells = <0>;
			compatible = "usb-nop-xceiv";
			status = "okay";
		};

		usb0: usb@ffb00000 {
			compatible = "snps,dwc2";
			reg = <0xffb00000 0xffff>;
			interrupts = <0 95 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&usb_clk>;
			clock-names = "otg";
			resets = <&rst USB0_RESET>;
			reset-names = "dwc2";
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			status = "disabled";
		};

		usb1: usb@ffb40000 {
			compatible = "snps,dwc2";
			reg = <0xffb40000 0xffff>;
			interrupts = <0 96 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&usb_clk>;
			clock-names = "otg";
			resets = <&rst USB1_RESET>;
			reset-names = "dwc2";
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			status = "disabled";
		};

		watchdog0: watchdog@ffd00200 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00200 0x100>;
			interrupts = <0 119 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sys_free_clk>;
			resets = <&rst L4WD0_RESET>;
			status = "disabled";
		};

		watchdog1: watchdog@ffd00300 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00300 0x100>;
			interrupts = <0 120 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&l4_sys_free_clk>;
			resets = <&rst L4WD1_RESET>;
			status = "disabled";
		};
	};
};
