&l4_cfg {						/* 0x4a000000 */
	compatible = "ti,dra7-l4-cfg", "simple-pm-bus";
	power-domains = <&prm_coreaon>;
	clocks = <&l4cfg_clkctrl DRA7_L4CFG_L4_CFG_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x4a000000 0x800>,
	      <0x4a000800 0x800>,
	      <0x4a001000 0x1000>;
	reg-names = "ap", "la", "ia0";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x4a000000 0x100000>,	/* segment 0 */
		 <0x00100000 0x4a100000 0x100000>,	/* segment 1 */
		 <0x00200000 0x4a200000 0x100000>;	/* segment 2 */
	dma-ranges;

	segment@0 {					/* 0x4a000000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 1 */
			 <0x00001000 0x00001000 0x001000>,	/* ap 2 */
			 <0x00002000 0x00002000 0x002000>,	/* ap 3 */
			 <0x00004000 0x00004000 0x001000>,	/* ap 4 */
			 <0x00005000 0x00005000 0x001000>,	/* ap 5 */
			 <0x00006000 0x00006000 0x001000>,	/* ap 6 */
			 <0x00008000 0x00008000 0x002000>,	/* ap 7 */
			 <0x0000a000 0x0000a000 0x001000>,	/* ap 8 */
			 <0x00056000 0x00056000 0x001000>,	/* ap 9 */
			 <0x00057000 0x00057000 0x001000>,	/* ap 10 */
			 <0x0005e000 0x0005e000 0x002000>,	/* ap 11 */
			 <0x00060000 0x00060000 0x001000>,	/* ap 12 */
			 <0x00080000 0x00080000 0x008000>,	/* ap 13 */
			 <0x00088000 0x00088000 0x001000>,	/* ap 14 */
			 <0x000a0000 0x000a0000 0x008000>,	/* ap 15 */
			 <0x000a8000 0x000a8000 0x001000>,	/* ap 16 */
			 <0x000d9000 0x000d9000 0x001000>,	/* ap 17 */
			 <0x000da000 0x000da000 0x001000>,	/* ap 18 */
			 <0x000dd000 0x000dd000 0x001000>,	/* ap 19 */
			 <0x000de000 0x000de000 0x001000>,	/* ap 20 */
			 <0x000e0000 0x000e0000 0x001000>,	/* ap 21 */
			 <0x000e1000 0x000e1000 0x001000>,	/* ap 22 */
			 <0x000f4000 0x000f4000 0x001000>,	/* ap 23 */
			 <0x000f5000 0x000f5000 0x001000>,	/* ap 24 */
			 <0x000f6000 0x000f6000 0x001000>,	/* ap 25 */
			 <0x000f7000 0x000f7000 0x001000>,	/* ap 26 */
			 <0x00090000 0x00090000 0x008000>,	/* ap 59 */
			 <0x00098000 0x00098000 0x001000>;	/* ap 60 */

		target-module@2000 {			/* 0x4a002000, ap 3 08.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x2000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2000 0x2000>;

			scm: scm@0 {
				compatible = "ti,dra7-scm-core", "simple-bus";
				reg = <0 0x2000>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x2000>;

				scm_conf: scm_conf@0 {
					compatible = "syscon", "simple-bus";
					reg = <0x0 0x1400>;
					#address-cells = <1>;
					#size-cells = <1>;
					ranges = <0 0x0 0x1400>;

					pbias_regulator: pbias_regulator@e00 {
						compatible = "ti,pbias-dra7", "ti,pbias-omap";
						reg = <0xe00 0x4>;
						syscon = <&scm_conf>;
						pbias_mmc_reg: pbias_mmc_omap5 {
							regulator-name = "pbias_mmc_omap5";
							regulator-min-microvolt = <1800000>;
							regulator-max-microvolt = <3300000>;
						};
					};

					phy_gmii_sel: phy-gmii-sel@554 {
						compatible = "ti,dra7xx-phy-gmii-sel";
						reg = <0x554 0x4>;
						#phy-cells = <1>;
					};

					scm_conf_clocks: clocks {
						#address-cells = <1>;
						#size-cells = <0>;
					};
				};

				dra7_pmx_core: pinmux@1400 {
					compatible = "ti,dra7-padconf",
						     "pinctrl-single";
					reg = <0x1400 0x0468>;
					#address-cells = <1>;
					#size-cells = <0>;
					#pinctrl-cells = <1>;
					#interrupt-cells = <1>;
					interrupt-controller;
					pinctrl-single,register-width = <32>;
					pinctrl-single,function-mask = <0x3fffffff>;
				};

				scm_conf1: scm_conf@1c04 {
					compatible = "syscon";
					reg = <0x1c04 0x0020>;
					#syscon-cells = <2>;
				};

				scm_conf_pcie: scm_conf@1c24 {
					compatible = "syscon";
					reg = <0x1c24 0x0024>;
				};

				sdma_xbar: dma-router@b78 {
					compatible = "ti,dra7-dma-crossbar";
					reg = <0xb78 0xfc>;
					#dma-cells = <1>;
					dma-requests = <205>;
					ti,dma-safe-map = <0>;
					dma-masters = <&sdma>;
				};

				edma_xbar: dma-router@c78 {
					compatible = "ti,dra7-dma-crossbar";
					reg = <0xc78 0x7c>;
					#dma-cells = <2>;
					dma-requests = <204>;
					ti,dma-safe-map = <0>;
					dma-masters = <&edma>;
				};
			};
		};

		target-module@5000 {			/* 0x4a005000, ap 5 10.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x5000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5000 0x1000>;

			cm_core_aon: cm_core_aon@0 {
				compatible = "ti,dra7-cm-core-aon",
					      "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0 0x2000>;
				ranges = <0 0 0x2000>;

				cm_core_aon_clocks: clocks {
					#address-cells = <1>;
					#size-cells = <0>;
				};

				cm_core_aon_clockdomains: clockdomains {
				};
			};
		};

		target-module@8000 {			/* 0x4a008000, ap 7 0e.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x8000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8000 0x2000>;

			cm_core: cm_core@0 {
				compatible = "ti,dra7-cm-core", "simple-bus";
				#address-cells = <1>;
				#size-cells = <1>;
				reg = <0 0x3000>;
				ranges = <0 0 0x3000>;

				cm_core_clocks: clocks {
					#address-cells = <1>;
					#size-cells = <0>;
				};

				cm_core_clockdomains: clockdomains {
				};
			};
		};

		target-module@56000 {			/* 0x4a056000, ap 9 02.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x56000 0x4>,
			      <0x5602c 0x4>,
			      <0x56028 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_EMUFREE |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): core_pwrdm, dma_clkdm */
			clocks = <&dma_clkctrl DRA7_DMA_DMA_SYSTEM_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x56000 0x1000>;

			sdma: dma-controller@0 {
				compatible = "ti,omap4430-sdma", "ti,omap-sdma";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
				#dma-cells = <1>;
				dma-channels = <32>;
				dma-requests = <127>;
			};
		};

		target-module@5e000 {			/* 0x4a05e000, ap 11 1a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5e000 0x2000>;
		};

		target-module@80000 {			/* 0x4a080000, ap 13 20.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x80000 0x4>,
			      <0x80010 0x4>,
			      <0x80014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_OCP2SCP1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x80000 0x8000>;

			ocp2scp@0 {
				compatible = "ti,omap-ocp2scp";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x8000>;
				reg = <0x0 0x20>;

				usb2_phy1: phy@4000 {
					compatible = "ti,dra7x-usb2", "ti,omap-usb2";
					reg = <0x4000 0x400>;
					syscon-phy-power = <&scm_conf 0x300>;
					clocks = <&usb_phy1_always_on_clk32k>,
						 <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS1_CLKCTRL 8>;
					clock-names =	"wkupclk",
							"refclk";
					#phy-cells = <0>;
				};

				usb2_phy2: phy@5000 {
					compatible = "ti,dra7x-usb2-phy2",
						     "ti,omap-usb2";
					reg = <0x5000 0x400>;
					syscon-phy-power = <&scm_conf 0xe74>;
					clocks = <&usb_phy2_always_on_clk32k>,
						 <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS2_CLKCTRL 8>;
					clock-names =	"wkupclk",
							"refclk";
					#phy-cells = <0>;
				};

				usb3_phy1: phy@4400 {
					compatible = "ti,omap-usb3";
					reg = <0x4400 0x80>,
					      <0x4800 0x64>,
					      <0x4c00 0x40>;
					reg-names = "phy_rx", "phy_tx", "pll_ctrl";
					syscon-phy-power = <&scm_conf 0x370>;
					clocks = <&usb_phy3_always_on_clk32k>,
						 <&sys_clkin1>,
						 <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS1_CLKCTRL 8>;
					clock-names =	"wkupclk",
							"sysclk",
							"refclk";
					#phy-cells = <0>;
				};
			};
		};

		target-module@90000 {			/* 0x4a090000, ap 59 42.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x90000 0x4>,
			      <0x90010 0x4>,
			      <0x90014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_OCP2SCP3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x90000 0x8000>;

			ocp2scp@0 {
				compatible = "ti,omap-ocp2scp";
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x8000>;
				reg = <0x0 0x20>;

				pcie1_phy: pciephy@4000 {
					compatible = "ti,phy-pipe3-pcie";
					reg = <0x4000 0x80>, /* phy_rx */
					      <0x4400 0x64>; /* phy_tx */
					reg-names = "phy_rx", "phy_tx";
					syscon-phy-power = <&scm_conf_pcie 0x1c>;
					syscon-pcs = <&scm_conf_pcie 0x10>;
					clocks = <&dpll_pcie_ref_ck>,
						 <&dpll_pcie_ref_m2ldo_ck>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE1_CLKCTRL 8>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE1_CLKCTRL 9>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE1_CLKCTRL 10>,
						 <&optfclk_pciephy_div>,
						 <&sys_clkin1>;
					clock-names = "dpll_ref", "dpll_ref_m2",
						      "wkupclk", "refclk",
						      "div-clk", "phy-div", "sysclk";
					#phy-cells = <0>;
				};

				pcie2_phy: pciephy@5000 {
					compatible = "ti,phy-pipe3-pcie";
					reg = <0x5000 0x80>, /* phy_rx */
					      <0x5400 0x64>; /* phy_tx */
					reg-names = "phy_rx", "phy_tx";
					syscon-phy-power = <&scm_conf_pcie 0x20>;
					syscon-pcs = <&scm_conf_pcie 0x10>;
					clocks = <&dpll_pcie_ref_ck>,
						 <&dpll_pcie_ref_m2ldo_ck>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE2_CLKCTRL 8>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE2_CLKCTRL 9>,
						 <&pcie_clkctrl DRA7_PCIE_PCIE2_CLKCTRL 10>,
						 <&optfclk_pciephy_div>,
						 <&sys_clkin1>;
					clock-names = "dpll_ref", "dpll_ref_m2",
						      "wkupclk", "refclk",
						      "div-clk", "phy-div", "sysclk";
					#phy-cells = <0>;
					status = "disabled";
				};

				sata_phy: phy@6000 {
					compatible = "ti,phy-pipe3-sata";
					reg = <0x6000 0x80>, /* phy_rx */
					      <0x6400 0x64>, /* phy_tx */
					      <0x6800 0x40>; /* pll_ctrl */
					reg-names = "phy_rx", "phy_tx", "pll_ctrl";
					syscon-phy-power = <&scm_conf 0x374>;
					clocks = <&sys_clkin1>,
						 <&l3init_clkctrl DRA7_L3INIT_SATA_CLKCTRL 8>;
					clock-names = "sysclk", "refclk";
					syscon-pllreset = <&scm_conf 0x3fc>;
					#phy-cells = <0>;
				};
			};
		};

		target-module@a0000 {			/* 0x4a0a0000, ap 15 40.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa0000 0x8000>;
		};

		target-module@d9000 {			/* 0x4a0d9000, ap 17 72.0 */
			compatible = "ti,sysc-omap4-sr", "ti,sysc";
			reg = <0xd9038 0x4>;
			reg-names = "sysc";
			ti,sysc-mask = <SYSC_OMAP3_SR_ENAWAKEUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): coreaon_pwrdm, coreaon_clkdm */
			clocks = <&coreaon_clkctrl DRA7_COREAON_SMARTREFLEX_MPU_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd9000 0x1000>;

			/* SmartReflex child device marked reserved in TRM */
		};

		target-module@dd000 {			/* 0x4a0dd000, ap 19 18.0 */
			compatible = "ti,sysc-omap4-sr", "ti,sysc";
			reg = <0xdd038 0x4>;
			reg-names = "sysc";
			ti,sysc-mask = <SYSC_OMAP3_SR_ENAWAKEUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): coreaon_pwrdm, coreaon_clkdm */
			clocks = <&coreaon_clkctrl DRA7_COREAON_SMARTREFLEX_CORE_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xdd000 0x1000>;

			/* SmartReflex child device marked reserved in TRM */
		};

		target-module@e0000 {			/* 0x4a0e0000, ap 21 28.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe0000 0x1000>;
		};

		target-module@f4000 {			/* 0x4a0f4000, ap 23 04.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xf4000 0x4>,
			      <0xf4010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xf4000 0x1000>;

			mailbox1: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <3>;
				ti,mbox-num-fifos = <8>;
				status = "disabled";
			};
		};

		target-module@f6000 {			/* 0x4a0f6000, ap 25 78.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xf6000 0x4>,
			      <0xf6010 0x4>,
			      <0xf6014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,syss-mask = <1>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_SPINLOCK_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xf6000 0x1000>;

			hwspinlock: spinlock@0 {
				compatible = "ti,omap4-hwspinlock";
				reg = <0x0 0x1000>;
				#hwlock-cells = <1>;
			};
		};
	};

	segment@100000 {					/* 0x4a100000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00002000 0x00102000 0x001000>,	/* ap 27 */
			 <0x00003000 0x00103000 0x001000>,	/* ap 28 */
			 <0x00008000 0x00108000 0x001000>,	/* ap 29 */
			 <0x00009000 0x00109000 0x001000>,	/* ap 30 */
			 <0x00040000 0x00140000 0x010000>,	/* ap 31 */
			 <0x00050000 0x00150000 0x001000>,	/* ap 32 */
			 <0x00051000 0x00151000 0x001000>,	/* ap 33 */
			 <0x00052000 0x00152000 0x001000>,	/* ap 34 */
			 <0x00053000 0x00153000 0x001000>,	/* ap 35 */
			 <0x00054000 0x00154000 0x001000>,	/* ap 36 */
			 <0x00055000 0x00155000 0x001000>,	/* ap 37 */
			 <0x00056000 0x00156000 0x001000>,	/* ap 38 */
			 <0x00057000 0x00157000 0x001000>,	/* ap 39 */
			 <0x00058000 0x00158000 0x001000>,	/* ap 40 */
			 <0x0005b000 0x0015b000 0x001000>,	/* ap 41 */
			 <0x0005c000 0x0015c000 0x001000>,	/* ap 42 */
			 <0x0005d000 0x0015d000 0x001000>,	/* ap 45 */
			 <0x0005e000 0x0015e000 0x001000>,	/* ap 46 */
			 <0x0005f000 0x0015f000 0x001000>,	/* ap 47 */
			 <0x00060000 0x00160000 0x001000>,	/* ap 48 */
			 <0x00061000 0x00161000 0x001000>,	/* ap 49 */
			 <0x00062000 0x00162000 0x001000>,	/* ap 50 */
			 <0x00063000 0x00163000 0x001000>,	/* ap 51 */
			 <0x00064000 0x00164000 0x001000>,	/* ap 52 */
			 <0x00065000 0x00165000 0x001000>,	/* ap 53 */
			 <0x00066000 0x00166000 0x001000>,	/* ap 54 */
			 <0x00067000 0x00167000 0x001000>,	/* ap 55 */
			 <0x00068000 0x00168000 0x001000>,	/* ap 56 */
			 <0x0006d000 0x0016d000 0x001000>,	/* ap 57 */
			 <0x0006e000 0x0016e000 0x001000>,	/* ap 58 */
			 <0x00071000 0x00171000 0x001000>,	/* ap 61 */
			 <0x00072000 0x00172000 0x001000>,	/* ap 62 */
			 <0x00073000 0x00173000 0x001000>,	/* ap 63 */
			 <0x00074000 0x00174000 0x001000>,	/* ap 64 */
			 <0x00075000 0x00175000 0x001000>,	/* ap 65 */
			 <0x00076000 0x00176000 0x001000>,	/* ap 66 */
			 <0x00077000 0x00177000 0x001000>,	/* ap 67 */
			 <0x00078000 0x00178000 0x001000>,	/* ap 68 */
			 <0x00081000 0x00181000 0x001000>,	/* ap 69 */
			 <0x00082000 0x00182000 0x001000>,	/* ap 70 */
			 <0x00083000 0x00183000 0x001000>,	/* ap 71 */
			 <0x00084000 0x00184000 0x001000>,	/* ap 72 */
			 <0x00085000 0x00185000 0x001000>,	/* ap 73 */
			 <0x00086000 0x00186000 0x001000>,	/* ap 74 */
			 <0x00087000 0x00187000 0x001000>,	/* ap 75 */
			 <0x00088000 0x00188000 0x001000>,	/* ap 76 */
			 <0x00069000 0x00169000 0x001000>,	/* ap 103 */
			 <0x0006a000 0x0016a000 0x001000>,	/* ap 104 */
			 <0x00079000 0x00179000 0x001000>,	/* ap 105 */
			 <0x0007a000 0x0017a000 0x001000>,	/* ap 106 */
			 <0x0006b000 0x0016b000 0x001000>,	/* ap 107 */
			 <0x0006c000 0x0016c000 0x001000>,	/* ap 108 */
			 <0x0007b000 0x0017b000 0x001000>,	/* ap 121 */
			 <0x0007c000 0x0017c000 0x001000>,	/* ap 122 */
			 <0x0007d000 0x0017d000 0x001000>,	/* ap 123 */
			 <0x0007e000 0x0017e000 0x001000>,	/* ap 124 */
			 <0x00059000 0x00159000 0x001000>,	/* ap 125 */
			 <0x0005a000 0x0015a000 0x001000>;	/* ap 126 */
		dma-ranges;

		target-module@2000 {			/* 0x4a102000, ap 27 3c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2000 0x1000>;
		};

		target-module@8000 {			/* 0x4a108000, ap 29 1e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8000 0x1000>;
		};

		target-module@40000 {			/* 0x4a140000, ap 31 06.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x400fc 4>,
			      <0x41100 4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			power-domains = <&prm_l3init>;
			clocks = <&l3init_clkctrl DRA7_L3INIT_SATA_CLKCTRL 0>;
			clock-names = "fck";
			#size-cells = <1>;
			#address-cells = <1>;
			ranges = <0x0 0x40000 0x10000>;

			sata: sata@0 {
				compatible = "snps,dwc-ahci";
				reg = <0 0x1100>, <0x1100 0x8>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
				phys = <&sata_phy>;
				phy-names = "sata-phy";
				clocks = <&l3init_clkctrl DRA7_L3INIT_SATA_CLKCTRL 8>;
				ports-implemented = <0x1>;
			};
		};

		target-module@51000 {			/* 0x4a151000, ap 33 50.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x51000 0x1000>;
		};

		target-module@53000 {			/* 0x4a153000, ap 35 54.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x53000 0x1000>;
		};

		target-module@55000 {			/* 0x4a155000, ap 37 46.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x55000 0x1000>;
		};

		target-module@57000 {			/* 0x4a157000, ap 39 58.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x57000 0x1000>;
		};

		target-module@59000 {			/* 0x4a159000, ap 125 6a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x59000 0x1000>;
		};

		target-module@5b000 {			/* 0x4a15b000, ap 41 60.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5b000 0x1000>;
		};

		target-module@5d000 {			/* 0x4a15d000, ap 45 3a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5d000 0x1000>;
		};

		target-module@5f000 {			/* 0x4a15f000, ap 47 56.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5f000 0x1000>;
		};

		target-module@61000 {			/* 0x4a161000, ap 49 32.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x61000 0x1000>;
		};

		target-module@63000 {			/* 0x4a163000, ap 51 5c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x63000 0x1000>;
		};

		target-module@65000 {			/* 0x4a165000, ap 53 4e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x65000 0x1000>;
		};

		target-module@67000 {			/* 0x4a167000, ap 55 5e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x67000 0x1000>;
		};

		target-module@69000 {			/* 0x4a169000, ap 103 4a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x69000 0x1000>;
		};

		target-module@6b000 {			/* 0x4a16b000, ap 107 52.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6b000 0x1000>;
		};

		target-module@6d000 {			/* 0x4a16d000, ap 57 68.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6d000 0x1000>;
		};

		target-module@71000 {			/* 0x4a171000, ap 61 48.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x71000 0x1000>;
		};

		target-module@73000 {			/* 0x4a173000, ap 63 2a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x73000 0x1000>;
		};

		target-module@75000 {			/* 0x4a175000, ap 65 64.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x75000 0x1000>;
		};

		target-module@77000 {			/* 0x4a177000, ap 67 66.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x77000 0x1000>;
		};

		target-module@79000 {			/* 0x4a179000, ap 105 34.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x79000 0x1000>;
		};

		target-module@7b000 {			/* 0x4a17b000, ap 121 7c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7b000 0x1000>;
		};

		target-module@7d000 {			/* 0x4a17d000, ap 123 7e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7d000 0x1000>;
		};

		target-module@81000 {			/* 0x4a181000, ap 69 26.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x81000 0x1000>;
		};

		target-module@83000 {			/* 0x4a183000, ap 71 2e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x83000 0x1000>;
		};

		target-module@85000 {			/* 0x4a185000, ap 73 36.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x85000 0x1000>;
		};

		target-module@87000 {			/* 0x4a187000, ap 75 74.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x87000 0x1000>;
		};
	};

	segment@200000 {					/* 0x4a200000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00018000 0x00218000 0x001000>,	/* ap 43 */
			 <0x00019000 0x00219000 0x001000>,	/* ap 44 */
			 <0x00000000 0x00200000 0x001000>,	/* ap 77 */
			 <0x00001000 0x00201000 0x001000>,	/* ap 78 */
			 <0x0000a000 0x0020a000 0x001000>,	/* ap 79 */
			 <0x0000b000 0x0020b000 0x001000>,	/* ap 80 */
			 <0x0000c000 0x0020c000 0x001000>,	/* ap 81 */
			 <0x0000d000 0x0020d000 0x001000>,	/* ap 82 */
			 <0x0000e000 0x0020e000 0x001000>,	/* ap 83 */
			 <0x0000f000 0x0020f000 0x001000>,	/* ap 84 */
			 <0x00010000 0x00210000 0x001000>,	/* ap 85 */
			 <0x00011000 0x00211000 0x001000>,	/* ap 86 */
			 <0x00012000 0x00212000 0x001000>,	/* ap 87 */
			 <0x00013000 0x00213000 0x001000>,	/* ap 88 */
			 <0x00014000 0x00214000 0x001000>,	/* ap 89 */
			 <0x00015000 0x00215000 0x001000>,	/* ap 90 */
			 <0x0002a000 0x0022a000 0x001000>,	/* ap 91 */
			 <0x0002b000 0x0022b000 0x001000>,	/* ap 92 */
			 <0x0001c000 0x0021c000 0x001000>,	/* ap 93 */
			 <0x0001d000 0x0021d000 0x001000>,	/* ap 94 */
			 <0x0001e000 0x0021e000 0x001000>,	/* ap 95 */
			 <0x0001f000 0x0021f000 0x001000>,	/* ap 96 */
			 <0x00020000 0x00220000 0x001000>,	/* ap 97 */
			 <0x00021000 0x00221000 0x001000>,	/* ap 98 */
			 <0x00024000 0x00224000 0x001000>,	/* ap 99 */
			 <0x00025000 0x00225000 0x001000>,	/* ap 100 */
			 <0x00026000 0x00226000 0x001000>,	/* ap 101 */
			 <0x00027000 0x00227000 0x001000>,	/* ap 102 */
			 <0x0002c000 0x0022c000 0x001000>,	/* ap 109 */
			 <0x0002d000 0x0022d000 0x001000>,	/* ap 110 */
			 <0x0002e000 0x0022e000 0x001000>,	/* ap 111 */
			 <0x0002f000 0x0022f000 0x001000>,	/* ap 112 */
			 <0x00030000 0x00230000 0x001000>,	/* ap 113 */
			 <0x00031000 0x00231000 0x001000>,	/* ap 114 */
			 <0x00032000 0x00232000 0x001000>,	/* ap 115 */
			 <0x00033000 0x00233000 0x001000>,	/* ap 116 */
			 <0x00034000 0x00234000 0x001000>,	/* ap 117 */
			 <0x00035000 0x00235000 0x001000>,	/* ap 118 */
			 <0x00036000 0x00236000 0x001000>,	/* ap 119 */
			 <0x00037000 0x00237000 0x001000>,	/* ap 120 */
			 <0x0001a000 0x0021a000 0x001000>,	/* ap 127 */
			 <0x0001b000 0x0021b000 0x001000>;	/* ap 128 */

		target-module@0 {			/* 0x4a200000, ap 77 3e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1000>;
		};

		target-module@a000 {			/* 0x4a20a000, ap 79 30.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa000 0x1000>;
		};

		target-module@c000 {			/* 0x4a20c000, ap 81 0c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc000 0x1000>;
		};

		target-module@e000 {			/* 0x4a20e000, ap 83 22.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xe000 0x1000>;
		};

		target-module@10000 {			/* 0x4a210000, ap 85 14.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x10000 0x1000>;
		};

		target-module@12000 {			/* 0x4a212000, ap 87 16.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x12000 0x1000>;
		};

		target-module@14000 {			/* 0x4a214000, ap 89 1c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x14000 0x1000>;
		};

		target-module@18000 {			/* 0x4a218000, ap 43 12.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x18000 0x1000>;
		};

		target-module@1a000 {			/* 0x4a21a000, ap 127 7a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1a000 0x1000>;
		};

		target-module@1c000 {			/* 0x4a21c000, ap 93 38.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1c000 0x1000>;
		};

		target-module@1e000 {			/* 0x4a21e000, ap 95 0a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1e000 0x1000>;
		};

		target-module@20000 {			/* 0x4a220000, ap 97 24.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x20000 0x1000>;
		};

		target-module@24000 {			/* 0x4a224000, ap 99 44.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x24000 0x1000>;
		};

		target-module@26000 {			/* 0x4a226000, ap 101 2c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x26000 0x1000>;
		};

		target-module@2a000 {			/* 0x4a22a000, ap 91 4c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2a000 0x1000>;
		};

		target-module@2c000 {			/* 0x4a22c000, ap 109 6c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2c000 0x1000>;
		};

		target-module@2e000 {			/* 0x4a22e000, ap 111 6e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2e000 0x1000>;
		};

		target-module@30000 {			/* 0x4a230000, ap 113 70.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x30000 0x1000>;
		};

		target-module@32000 {			/* 0x4a232000, ap 115 5a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x32000 0x1000>;
		};

		target-module@34000 {			/* 0x4a234000, ap 117 76.1 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x34000 0x1000>;
		};

		target-module@36000 {			/* 0x4a236000, ap 119 62.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x36000 0x1000>;
		};
	};
};

&l4_per1 {						/* 0x48000000 */
	compatible = "ti,dra7-l4-per1", "simple-pm-bus";
	power-domains = <&prm_l4per>;
	clocks = <&l4per_clkctrl DRA7_L4PER_L4_PER1_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x48000000 0x800>,
	      <0x48000800 0x800>,
	      <0x48001000 0x400>,
	      <0x48001400 0x400>,
	      <0x48001800 0x400>,
	      <0x48001c00 0x400>;
	reg-names = "ap", "la", "ia0", "ia1", "ia2", "ia3";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x48000000 0x200000>,	/* segment 0 */
		 <0x00200000 0x48200000 0x200000>;	/* segment 1 */

	segment@0 {					/* 0x48000000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 1 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 2 */
			 <0x00020000 0x00020000 0x001000>,	/* ap 3 */
			 <0x00021000 0x00021000 0x001000>,	/* ap 4 */
			 <0x00032000 0x00032000 0x001000>,	/* ap 5 */
			 <0x00033000 0x00033000 0x001000>,	/* ap 6 */
			 <0x00034000 0x00034000 0x001000>,	/* ap 7 */
			 <0x00035000 0x00035000 0x001000>,	/* ap 8 */
			 <0x00036000 0x00036000 0x001000>,	/* ap 9 */
			 <0x00037000 0x00037000 0x001000>,	/* ap 10 */
			 <0x0003e000 0x0003e000 0x001000>,	/* ap 11 */
			 <0x0003f000 0x0003f000 0x001000>,	/* ap 12 */
			 <0x00055000 0x00055000 0x001000>,	/* ap 13 */
			 <0x00056000 0x00056000 0x001000>,	/* ap 14 */
			 <0x00057000 0x00057000 0x001000>,	/* ap 15 */
			 <0x00058000 0x00058000 0x001000>,	/* ap 16 */
			 <0x00059000 0x00059000 0x001000>,	/* ap 17 */
			 <0x0005a000 0x0005a000 0x001000>,	/* ap 18 */
			 <0x0005b000 0x0005b000 0x001000>,	/* ap 19 */
			 <0x0005c000 0x0005c000 0x001000>,	/* ap 20 */
			 <0x0005d000 0x0005d000 0x001000>,	/* ap 21 */
			 <0x0005e000 0x0005e000 0x001000>,	/* ap 22 */
			 <0x00060000 0x00060000 0x001000>,	/* ap 23 */
			 <0x0006a000 0x0006a000 0x001000>,	/* ap 24 */
			 <0x0006b000 0x0006b000 0x001000>,	/* ap 25 */
			 <0x0006c000 0x0006c000 0x001000>,	/* ap 26 */
			 <0x0006d000 0x0006d000 0x001000>,	/* ap 27 */
			 <0x0006e000 0x0006e000 0x001000>,	/* ap 28 */
			 <0x0006f000 0x0006f000 0x001000>,	/* ap 29 */
			 <0x00070000 0x00070000 0x001000>,	/* ap 30 */
			 <0x00071000 0x00071000 0x001000>,	/* ap 31 */
			 <0x00072000 0x00072000 0x001000>,	/* ap 32 */
			 <0x00073000 0x00073000 0x001000>,	/* ap 33 */
			 <0x00061000 0x00061000 0x001000>,	/* ap 34 */
			 <0x00053000 0x00053000 0x001000>,	/* ap 35 */
			 <0x00054000 0x00054000 0x001000>,	/* ap 36 */
			 <0x000b2000 0x000b2000 0x001000>,	/* ap 37 */
			 <0x000b3000 0x000b3000 0x001000>,	/* ap 38 */
			 <0x00078000 0x00078000 0x001000>,	/* ap 39 */
			 <0x00079000 0x00079000 0x001000>,	/* ap 40 */
			 <0x00086000 0x00086000 0x001000>,	/* ap 41 */
			 <0x00087000 0x00087000 0x001000>,	/* ap 42 */
			 <0x00088000 0x00088000 0x001000>,	/* ap 43 */
			 <0x00089000 0x00089000 0x001000>,	/* ap 44 */
			 <0x00051000 0x00051000 0x001000>,	/* ap 45 */
			 <0x00052000 0x00052000 0x001000>,	/* ap 46 */
			 <0x00098000 0x00098000 0x001000>,	/* ap 47 */
			 <0x00099000 0x00099000 0x001000>,	/* ap 48 */
			 <0x0009a000 0x0009a000 0x001000>,	/* ap 49 */
			 <0x0009b000 0x0009b000 0x001000>,	/* ap 50 */
			 <0x0009c000 0x0009c000 0x001000>,	/* ap 51 */
			 <0x0009d000 0x0009d000 0x001000>,	/* ap 52 */
			 <0x00068000 0x00068000 0x001000>,	/* ap 53 */
			 <0x00069000 0x00069000 0x001000>,	/* ap 54 */
			 <0x00090000 0x00090000 0x002000>,	/* ap 55 */
			 <0x00092000 0x00092000 0x001000>,	/* ap 56 */
			 <0x000a4000 0x000a4000 0x001000>,	/* ap 57 */
			 <0x000a6000 0x000a6000 0x001000>,	/* ap 58 */
			 <0x000a8000 0x000a8000 0x004000>,	/* ap 59 */
			 <0x000ac000 0x000ac000 0x001000>,	/* ap 60 */
			 <0x000ad000 0x000ad000 0x001000>,	/* ap 61 */
			 <0x000ae000 0x000ae000 0x001000>,	/* ap 62 */
			 <0x00066000 0x00066000 0x001000>,	/* ap 63 */
			 <0x00067000 0x00067000 0x001000>,	/* ap 64 */
			 <0x000b4000 0x000b4000 0x001000>,	/* ap 65 */
			 <0x000b5000 0x000b5000 0x001000>,	/* ap 66 */
			 <0x000b8000 0x000b8000 0x001000>,	/* ap 67 */
			 <0x000b9000 0x000b9000 0x001000>,	/* ap 68 */
			 <0x000ba000 0x000ba000 0x001000>,	/* ap 69 */
			 <0x000bb000 0x000bb000 0x001000>,	/* ap 70 */
			 <0x000d1000 0x000d1000 0x001000>,	/* ap 71 */
			 <0x000d2000 0x000d2000 0x001000>,	/* ap 72 */
			 <0x000d5000 0x000d5000 0x001000>,	/* ap 73 */
			 <0x000d6000 0x000d6000 0x001000>,	/* ap 74 */
			 <0x000a2000 0x000a2000 0x001000>,	/* ap 75 */
			 <0x000a3000 0x000a3000 0x001000>,	/* ap 76 */
			 <0x00001400 0x00001400 0x000400>,	/* ap 77 */
			 <0x00001800 0x00001800 0x000400>,	/* ap 78 */
			 <0x00001c00 0x00001c00 0x000400>,	/* ap 79 */
			 <0x000a5000 0x000a5000 0x001000>,	/* ap 80 */
			 <0x0007a000 0x0007a000 0x001000>,	/* ap 81 */
			 <0x0007b000 0x0007b000 0x001000>,	/* ap 82 */
			 <0x0007c000 0x0007c000 0x001000>,	/* ap 83 */
			 <0x0007d000 0x0007d000 0x001000>;	/* ap 84 */

		target-module@20000 {			/* 0x48020000, ap 3 04.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x20050 0x4>,
			      <0x20054 0x4>,
			      <0x20058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_UART3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x20000 0x1000>;

			uart3: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
				dmas = <&sdma_xbar 53>, <&sdma_xbar 54>;
				dma-names = "tx", "rx";
			};
		};

		target-module@32000 {			/* 0x48032000, ap 5 3e.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x32000 0x4>,
			      <0x32010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x32000 0x1000>;

			timer2: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER2_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		timer3_target: target-module@34000 {	/* 0x48034000, ap 7 46.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x34000 0x4>,
			      <0x34010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x34000 0x1000>;

			timer3: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER3_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		timer4_target: target-module@36000 {	/* 0x48036000, ap 9 4e.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x36000 0x4>,
			      <0x36010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x36000 0x1000>;

			timer4: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER4_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@3e000 {			/* 0x4803e000, ap 11 56.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x3e000 0x4>,
			      <0x3e010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER9_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3e000 0x1000>;

			timer9: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER9_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		gpio7_target: target-module@51000 {		/* 0x48051000, ap 45 2e.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x51000 0x4>,
			      <0x51010 0x4>,
			      <0x51114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO7_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO7_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x51000 0x1000>;

			gpio7: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@53000 {			/* 0x48053000, ap 35 36.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x53000 0x4>,
			      <0x53010 0x4>,
			      <0x53114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO8_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO8_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x53000 0x1000>;

			gpio8: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		gpio2_target: target-module@55000 {		/* 0x48055000, ap 13 0e.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x55000 0x4>,
			      <0x55010 0x4>,
			      <0x55114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO2_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO2_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x55000 0x1000>;

			gpio2: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		gpio3_target: target-module@57000 {		/* 0x48057000, ap 15 06.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x57000 0x4>,
			      <0x57010 0x4>,
			      <0x57114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO3_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO3_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x57000 0x1000>;

			gpio3: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@59000 {			/* 0x48059000, ap 17 16.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x59000 0x4>,
			      <0x59010 0x4>,
			      <0x59114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO4_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO4_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x59000 0x1000>;

			gpio4: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@5b000 {			/* 0x4805b000, ap 19 1e.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x5b000 0x4>,
			      <0x5b010 0x4>,
			      <0x5b114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO5_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO5_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5b000 0x1000>;

			gpio5: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@5d000 {			/* 0x4805d000, ap 21 26.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x5d000 0x4>,
			      <0x5d010 0x4>,
			      <0x5d114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_GPIO6_CLKCTRL 0>,
				 <&l4per_clkctrl DRA7_L4PER_GPIO6_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5d000 0x1000>;

			gpio6: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@60000 {			/* 0x48060000, ap 23 32.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x60000 0x8>,
			      <0x60010 0x8>,
			      <0x60090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_I2C3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x60000 0x1000>;

			i2c3: i2c@0 {
				compatible = "ti,omap4-i2c";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@66000 {			/* 0x48066000, ap 63 14.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x66050 0x4>,
			      <0x66054 0x4>,
			      <0x66058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_UART5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x66000 0x1000>;

			uart5: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
				dmas = <&sdma_xbar 63>, <&sdma_xbar 64>;
				dma-names = "tx", "rx";
			};
		};

		target-module@68000 {			/* 0x48068000, ap 53 1c.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x68050 0x4>,
			      <0x68054 0x4>,
			      <0x68058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_UART6_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x68000 0x1000>;

			uart6: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
				dmas = <&sdma_xbar 79>, <&sdma_xbar 80>;
				dma-names = "tx", "rx";
			};
		};

		target-module@6a000 {			/* 0x4806a000, ap 24 24.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x6a050 0x4>,
			      <0x6a054 0x4>,
			      <0x6a058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_UART1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6a000 0x1000>;

			uart1: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts-extended = <&crossbar_mpu GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
				dmas = <&sdma_xbar 49>, <&sdma_xbar 50>;
				dma-names = "tx", "rx";
			};
		};

		target-module@6c000 {			/* 0x4806c000, ap 26 2c.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x6c050 0x4>,
			      <0x6c054 0x4>,
			      <0x6c058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_UART2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6c000 0x1000>;

			uart2: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 68 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
				dmas = <&sdma_xbar 51>, <&sdma_xbar 52>;
				dma-names = "tx", "rx";
			};
		};

		target-module@6e000 {			/* 0x4806e000, ap 28 0c.1 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x6e050 0x4>,
			      <0x6e054 0x4>,
			      <0x6e058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_UART4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6e000 0x1000>;

			uart4: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
			                        status = "disabled";
				dmas = <&sdma_xbar 55>, <&sdma_xbar 56>;
				dma-names = "tx", "rx";
			};
		};

		target-module@70000 {			/* 0x48070000, ap 30 22.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x70000 0x8>,
			      <0x70010 0x8>,
			      <0x70090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_I2C1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x70000 0x1000>;

			i2c1: i2c@0 {
				compatible = "ti,omap4-i2c";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@72000 {			/* 0x48072000, ap 32 2a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x72000 0x8>,
			      <0x72010 0x8>,
			      <0x72090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_I2C2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x72000 0x1000>;

			i2c2: i2c@0 {
				compatible = "ti,omap4-i2c";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@78000 {			/* 0x48078000, ap 39 0a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x78000 0x4>,
			      <0x78010 0x4>,
			      <0x78014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_ELM_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x78000 0x1000>;

			elm: elm@0 {
				compatible = "ti,am3352-elm";
				reg = <0x0 0xfc0>;      /* device IO registers */
				interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
			};
		};

		target-module@7a000 {			/* 0x4807a000, ap 81 3a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x7a000 0x8>,
			      <0x7a010 0x8>,
			      <0x7a090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_I2C4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7a000 0x1000>;

			i2c4: i2c@0 {
				compatible = "ti,omap4-i2c";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@7c000 {			/* 0x4807c000, ap 83 4a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x7c000 0x8>,
			      <0x7c010 0x8>,
			      <0x7c090 0x8>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_CLOCKACTIVITY |
					 SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_I2C5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7c000 0x1000>;

			i2c5: i2c@0 {
				compatible = "ti,omap4-i2c";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		target-module@86000 {			/* 0x48086000, ap 41 5e.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x86000 0x4>,
			      <0x86010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER10_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x86000 0x1000>;

			timer10: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER10_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@88000 {			/* 0x48088000, ap 43 66.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x88000 0x4>,
			      <0x88010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_TIMER11_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x88000 0x1000>;

			timer11: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per_clkctrl DRA7_L4PER_TIMER11_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@90000 {			/* 0x48090000, ap 55 12.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x91fe0 0x4>,
			      <0x91fe4 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP2_AUTOIDLE>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			/* Domains (P, C): l4per_pwrdm, l4sec_clkdm */
			clocks = <&l4sec_clkctrl DRA7_L4SEC_RNG_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x90000 0x2000>;

			rng: rng@0 {
				compatible = "ti,omap4-rng";
				reg = <0x0 0x2000>;
				interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&l3_iclk_div>;
				clock-names = "fck";
			};
		};

		target-module@98000 {			/* 0x48098000, ap 47 08.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x98000 0x4>,
			      <0x98010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MCSPI1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x98000 0x1000>;

			mcspi1: spi@0 {
				compatible = "ti,omap4-mcspi";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				ti,spi-num-cs = <4>;
				dmas = <&sdma_xbar 35>,
				       <&sdma_xbar 36>,
				       <&sdma_xbar 37>,
				       <&sdma_xbar 38>,
				       <&sdma_xbar 39>,
				       <&sdma_xbar 40>,
				       <&sdma_xbar 41>,
				       <&sdma_xbar 42>;
				dma-names = "tx0", "rx0", "tx1", "rx1",
					    "tx2", "rx2", "tx3", "rx3";
				status = "disabled";
			};
		};

		target-module@9a000 {			/* 0x4809a000, ap 49 10.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x9a000 0x4>,
			      <0x9a010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MCSPI2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x9a000 0x1000>;

			mcspi2: spi@0 {
				compatible = "ti,omap4-mcspi";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				ti,spi-num-cs = <2>;
				dmas = <&sdma_xbar 43>,
				       <&sdma_xbar 44>,
				       <&sdma_xbar 45>,
				       <&sdma_xbar 46>;
				dma-names = "tx0", "rx0", "tx1", "rx1";
				status = "disabled";
			};
		};

		target-module@9c000 {			/* 0x4809c000, ap 51 38.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x9c000 0x4>,
			      <0x9c010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_MMC1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x9c000 0x1000>;

			mmc1: mmc@0 {
				compatible = "ti,dra7-sdhci";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
				pbias-supply = <&pbias_mmc_reg>;
				max-frequency = <192000000>;
				mmc-ddr-1_8v;
				mmc-ddr-3_3v;
			};
		};

		target-module@a2000 {			/* 0x480a2000, ap 75 02.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa2000 0x1000>;
		};

		target-module@a4000 {			/* 0x480a4000, ap 57 42.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x00000000 0x000a4000 0x00001000>,
				 <0x00001000 0x000a5000 0x00001000>;
		};

		des_target: target-module@a5000 {	/* 0x480a5000 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xa5030 0x4>,
			      <0xa5034 0x4>,
			      <0xa5038 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4sec_clkdm */
			clocks = <&l4sec_clkctrl DRA7_L4SEC_DES_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0xa5000 0x00001000>;

			des: des@0 {
				compatible = "ti,omap4-des";
				reg = <0 0xa0>;
				interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
				dmas = <&sdma_xbar 117>, <&sdma_xbar 116>;
				dma-names = "tx", "rx";
				clocks = <&l3_iclk_div>;
				clock-names = "fck";
			};
		};

		target-module@a8000 {			/* 0x480a8000, ap 59 1a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa8000 0x4000>;
		};

		target-module@ad000 {			/* 0x480ad000, ap 61 20.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xad000 0x4>,
			      <0xad010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MMC3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xad000 0x1000>;

			mmc3: mmc@0 {
				compatible = "ti,dra7-sdhci";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
				/* Errata i887 limits max-frequency of MMC3 to 64 MHz */
				max-frequency = <64000000>;
				/* SDMA is not supported */
				sdhci-caps-mask = <0x0 0x400000>;
			};
		};

		target-module@b2000 {			/* 0x480b2000, ap 37 52.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xb2000 0x4>,
			      <0xb2014 0x4>,
			      <0xb2018 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,syss-mask = <1>;
			ti,no-reset-on-init;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_HDQ1W_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xb2000 0x1000>;

			hdqw1w: 1w@0 {
				compatible = "ti,omap3-1w";
				reg = <0x0 0x1000>;
				interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@b4000 {			/* 0x480b4000, ap 65 40.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xb4000 0x4>,
			      <0xb4010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_MMC2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xb4000 0x1000>;

			mmc2: mmc@0 {
				compatible = "ti,dra7-sdhci";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
				max-frequency = <192000000>;
				/* SDR104/DDR50/SDR50 bits in CAPA2 is not supported */
				sdhci-caps-mask = <0x7 0x0>;
				mmc-hs200-1_8v;
				mmc-ddr-1_8v;
				mmc-ddr-3_3v;
			};
		};

		target-module@b8000 {			/* 0x480b8000, ap 67 48.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xb8000 0x4>,
			      <0xb8010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MCSPI3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xb8000 0x1000>;

			mcspi3: spi@0 {
				compatible = "ti,omap4-mcspi";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				ti,spi-num-cs = <2>;
				dmas = <&sdma_xbar 15>, <&sdma_xbar 16>;
				dma-names = "tx0", "rx0";
				status = "disabled";
			};
		};

		target-module@ba000 {			/* 0x480ba000, ap 69 18.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xba000 0x4>,
			      <0xba010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MCSPI4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xba000 0x1000>;

			mcspi4: spi@0 {
				compatible = "ti,omap4-mcspi";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <0>;
				ti,spi-num-cs = <1>;
				dmas = <&sdma_xbar 70>, <&sdma_xbar 71>;
				dma-names = "tx0", "rx0";
				status = "disabled";
			};
		};

		target-module@d1000 {			/* 0x480d1000, ap 71 28.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xd1000 0x4>,
			      <0xd1010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per_clkdm */
			clocks = <&l4per_clkctrl DRA7_L4PER_MMC4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd1000 0x1000>;

			mmc4: mmc@0 {
				compatible = "ti,dra7-sdhci";
				reg = <0x0 0x400>;
				interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";
				max-frequency = <192000000>;
				/* SDMA is not supported */
				sdhci-caps-mask = <0x0 0x400000>;
			};
		};

		target-module@d5000 {			/* 0x480d5000, ap 73 30.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xd5000 0x1000>;
		};
	};

	segment@200000 {					/* 0x48200000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
	};
};

&l4_per2 {						/* 0x48400000 */
	compatible = "ti,dra7-l4-per2", "simple-pm-bus";
	power-domains = <&prm_l4per>;
	clocks = <&l4per2_clkctrl DRA7_L4PER2_L4_PER2_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x48400000 0x800>,
	      <0x48400800 0x800>,
	      <0x48401000 0x400>,
	      <0x48401400 0x400>,
	      <0x48401800 0x400>;
	reg-names = "ap", "la", "ia0", "ia1", "ia2";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x48400000 0x400000>,	/* segment 0 */
		 <0x45800000 0x45800000 0x400000>,	/* L3 data port */
		 <0x45c00000 0x45c00000 0x400000>,	/* L3 data port */
		 <0x46000000 0x46000000 0x400000>,	/* L3 data port */
		 <0x48436000 0x48436000 0x400000>,	/* L3 data port */
		 <0x4843a000 0x4843a000 0x400000>,	/* L3 data port */
		 <0x4844c000 0x4844c000 0x400000>,	/* L3 data port */
		 <0x48450000 0x48450000 0x400000>,	/* L3 data port */
		 <0x48454000 0x48454000 0x400000>;	/* L3 data port */

	segment@0 {					/* 0x48400000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 1 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 2 */
			 <0x00084000 0x00084000 0x004000>,	/* ap 3 */
			 <0x00001400 0x00001400 0x000400>,	/* ap 4 */
			 <0x00001800 0x00001800 0x000400>,	/* ap 5 */
			 <0x00088000 0x00088000 0x001000>,	/* ap 6 */
			 <0x0002c000 0x0002c000 0x001000>,	/* ap 7 */
			 <0x0002d000 0x0002d000 0x001000>,	/* ap 8 */
			 <0x00060000 0x00060000 0x002000>,	/* ap 9 */
			 <0x00062000 0x00062000 0x001000>,	/* ap 10 */
			 <0x00064000 0x00064000 0x002000>,	/* ap 11 */
			 <0x00066000 0x00066000 0x001000>,	/* ap 12 */
			 <0x00068000 0x00068000 0x002000>,	/* ap 13 */
			 <0x0006a000 0x0006a000 0x001000>,	/* ap 14 */
			 <0x0006c000 0x0006c000 0x002000>,	/* ap 15 */
			 <0x0006e000 0x0006e000 0x001000>,	/* ap 16 */
			 <0x00036000 0x00036000 0x001000>,	/* ap 17 */
			 <0x00037000 0x00037000 0x001000>,	/* ap 18 */
			 <0x00070000 0x00070000 0x002000>,	/* ap 19 */
			 <0x00072000 0x00072000 0x001000>,	/* ap 20 */
			 <0x0003a000 0x0003a000 0x001000>,	/* ap 21 */
			 <0x0003b000 0x0003b000 0x001000>,	/* ap 22 */
			 <0x0003c000 0x0003c000 0x001000>,	/* ap 23 */
			 <0x0003d000 0x0003d000 0x001000>,	/* ap 24 */
			 <0x0003e000 0x0003e000 0x001000>,	/* ap 25 */
			 <0x0003f000 0x0003f000 0x001000>,	/* ap 26 */
			 <0x00040000 0x00040000 0x001000>,	/* ap 27 */
			 <0x00041000 0x00041000 0x001000>,	/* ap 28 */
			 <0x00042000 0x00042000 0x001000>,	/* ap 29 */
			 <0x00043000 0x00043000 0x001000>,	/* ap 30 */
			 <0x00080000 0x00080000 0x002000>,	/* ap 31 */
			 <0x00082000 0x00082000 0x001000>,	/* ap 32 */
			 <0x0004a000 0x0004a000 0x001000>,	/* ap 33 */
			 <0x0004b000 0x0004b000 0x001000>,	/* ap 34 */
			 <0x00074000 0x00074000 0x002000>,	/* ap 35 */
			 <0x00076000 0x00076000 0x001000>,	/* ap 36 */
			 <0x00050000 0x00050000 0x001000>,	/* ap 37 */
			 <0x00051000 0x00051000 0x001000>,	/* ap 38 */
			 <0x00078000 0x00078000 0x002000>,	/* ap 39 */
			 <0x0007a000 0x0007a000 0x001000>,	/* ap 40 */
			 <0x00054000 0x00054000 0x001000>,	/* ap 41 */
			 <0x00055000 0x00055000 0x001000>,	/* ap 42 */
			 <0x0007c000 0x0007c000 0x002000>,	/* ap 43 */
			 <0x0007e000 0x0007e000 0x001000>,	/* ap 44 */
			 <0x0004c000 0x0004c000 0x001000>,	/* ap 45 */
			 <0x0004d000 0x0004d000 0x001000>,	/* ap 46 */
			 <0x00020000 0x00020000 0x001000>,	/* ap 47 */
			 <0x00021000 0x00021000 0x001000>,	/* ap 48 */
			 <0x00022000 0x00022000 0x001000>,	/* ap 49 */
			 <0x00023000 0x00023000 0x001000>,	/* ap 50 */
			 <0x00024000 0x00024000 0x001000>,	/* ap 51 */
			 <0x00025000 0x00025000 0x001000>,	/* ap 52 */
			 <0x00046000 0x00046000 0x001000>,	/* ap 53 */
			 <0x00047000 0x00047000 0x001000>,	/* ap 54 */
			 <0x00048000 0x00048000 0x001000>,	/* ap 55 */
			 <0x00049000 0x00049000 0x001000>,	/* ap 56 */
			 <0x00058000 0x00058000 0x002000>,	/* ap 57 */
			 <0x0005a000 0x0005a000 0x001000>,	/* ap 58 */
			 <0x0005b000 0x0005b000 0x001000>,	/* ap 59 */
			 <0x0005c000 0x0005c000 0x001000>,	/* ap 60 */
			 <0x0005d000 0x0005d000 0x001000>,	/* ap 61 */
			 <0x0005e000 0x0005e000 0x001000>,	/* ap 62 */
			 <0x45800000 0x45800000 0x400000>,	/* L3 data port */
			 <0x45c00000 0x45c00000 0x400000>,	/* L3 data port */
			 <0x46000000 0x46000000 0x400000>,	/* L3 data port */
			 <0x48436000 0x48436000 0x400000>,	/* L3 data port */
			 <0x4843a000 0x4843a000 0x400000>,	/* L3 data port */
			 <0x4844c000 0x4844c000 0x400000>,	/* L3 data port */
			 <0x48450000 0x48450000 0x400000>,	/* L3 data port */
			 <0x48454000 0x48454000 0x400000>;	/* L3 data port */

		target-module@20000 {			/* 0x48420000, ap 47 02.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x20050 0x4>,
			      <0x20054 0x4>,
			      <0x20058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_UART7_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x20000 0x1000>;

			uart7: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 218 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
			};
		};

		target-module@22000 {			/* 0x48422000, ap 49 0a.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x22050 0x4>,
			      <0x22054 0x4>,
			      <0x22058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_UART8_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x22000 0x1000>;

			uart8: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 219 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
			};
		};

		target-module@24000 {			/* 0x48424000, ap 51 12.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x24050 0x4>,
			      <0x24054 0x4>,
			      <0x24058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_UART9_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x24000 0x1000>;

			uart9: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 220 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
			};
		};

		target-module@2c000 {			/* 0x4842c000, ap 7 18.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2c000 0x1000>;
		};

		target-module@36000 {			/* 0x48436000, ap 17 06.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x36000 0x1000>;
		};

		target-module@3a000 {			/* 0x4843a000, ap 21 3e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3a000 0x1000>;
		};

		atl_tm: target-module@3c000 {		/* 0x4843c000, ap 23 08.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x3c000 0x4>;
			reg-names = "rev";
			clocks = <&atl_clkctrl DRA7_ATL_ATL_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3c000 0x1000>;

			atl: atl@0 {
				compatible = "ti,dra7-atl";
				reg = <0x0 0x3ff>;
				ti,provided-clocks = <&atl_clkin0_ck>, <&atl_clkin1_ck>,
						     <&atl_clkin2_ck>, <&atl_clkin3_ck>;
				clocks = <&atl_clkctrl DRA7_ATL_ATL_CLKCTRL 26>;
				clock-names = "fck";
				status = "disabled";
			};
		};

		target-module@3e000 {			/* 0x4843e000, ap 25 30.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x3e000 0x4>,
			      <0x3e004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_EPWMSS0_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3e000 0x1000>;

			epwmss0: epwmss@0 {
				compatible = "ti,dra746-pwmss", "ti,am33xx-pwmss";
				reg = <0x0 0x30>;
				#address-cells = <1>;
				#size-cells = <1>;
				status = "disabled";
				ranges = <0 0 0x1000>;

				ecap0: pwm@100 {
					compatible = "ti,dra746-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4_root_clk_div>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm0: pwm@200 {
					compatible = "ti,dra746-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm0_tbclk>, <&l4_root_clk_div>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@40000 {			/* 0x48440000, ap 27 38.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x40000 0x4>,
			      <0x40004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_EPWMSS1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x40000 0x1000>;

			epwmss1: epwmss@0 {
				compatible = "ti,dra746-pwmss", "ti,am33xx-pwmss";
				reg = <0x0 0x30>;
				#address-cells = <1>;
				#size-cells = <1>;
				status = "disabled";
				ranges = <0 0 0x1000>;

				ecap1: pwm@100 {
					compatible = "ti,dra746-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4_root_clk_div>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm1: pwm@200 {
					compatible = "ti,dra746-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm1_tbclk>, <&l4_root_clk_div>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@42000 {			/* 0x48442000, ap 29 20.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x42000 0x4>,
			      <0x42004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_EPWMSS2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x42000 0x1000>;

			epwmss2: epwmss@0 {
				compatible = "ti,dra746-pwmss", "ti,am33xx-pwmss";
				reg = <0x0 0x30>;
				#address-cells = <1>;
				#size-cells = <1>;
				status = "disabled";
				ranges = <0 0 0x1000>;

				ecap2: pwm@100 {
					compatible = "ti,dra746-ecap",
						     "ti,am3352-ecap";
					#pwm-cells = <3>;
					reg = <0x100 0x80>;
					clocks = <&l4_root_clk_div>;
					clock-names = "fck";
					status = "disabled";
				};

				ehrpwm2: pwm@200 {
					compatible = "ti,dra746-ehrpwm",
						     "ti,am3352-ehrpwm";
					#pwm-cells = <3>;
					reg = <0x200 0x80>;
					clocks = <&ehrpwm2_tbclk>, <&l4_root_clk_div>;
					clock-names = "tbclk", "fck";
					status = "disabled";
				};
			};
		};

		target-module@46000 {			/* 0x48446000, ap 53 40.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x46000 0x1000>;
		};

		target-module@48000 {			/* 0x48448000, ap 55 48.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x48000 0x1000>;
		};

		target-module@4a000 {			/* 0x4844a000, ap 33 1a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4a000 0x1000>;
		};

		target-module@4c000 {			/* 0x4844c000, ap 45 1c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4c000 0x1000>;
		};

		target-module@50000 {			/* 0x48450000, ap 37 24.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x50000 0x1000>;
		};

		target-module@54000 {			/* 0x48454000, ap 41 2c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x54000 0x1000>;
		};

		target-module@58000 {			/* 0x48458000, ap 57 28.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x58000 0x2000>;
		};

		target-module@5b000 {			/* 0x4845b000, ap 59 46.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5b000 0x1000>;
		};

		target-module@5d000 {			/* 0x4845d000, ap 61 22.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5d000 0x1000>;
		};

		target-module@60000 {			/* 0x48460000, ap 9 0e.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x60000 0x4>,
			      <0x60004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 0>,
				 <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 24>,
				 <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 28>;
			clock-names = "fck", "ahclkx", "ahclkr";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x60000 0x2000>,
				 <0x45800000 0x45800000 0x400000>;

			mcasp1: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x45800000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 129 1>, <&edma_xbar 128 1>;
				dma-names = "tx", "rx";
				clocks = <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 0>,
					 <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 24>,
					 <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 28>;
				clock-names = "fck", "ahclkx", "ahclkr";
				status = "disabled";
			};
		};

		target-module@64000 {			/* 0x48464000, ap 11 1e.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x64000 0x4>,
			      <0x64004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP2_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP2_CLKCTRL 24>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP2_CLKCTRL 28>;
			clock-names = "fck", "ahclkx", "ahclkr";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x64000 0x2000>,
				 <0x45c00000 0x45c00000 0x400000>;

			mcasp2: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x45c00000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 131 1>, <&edma_xbar 130 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP2_CLKCTRL 0>,
					 <&ipu_clkctrl DRA7_IPU_MCASP1_CLKCTRL 24>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP2_CLKCTRL 28>;
				clock-names = "fck", "ahclkx", "ahclkr";
				status = "disabled";
			};
		};

		target-module@68000 {			/* 0x48468000, ap 13 26.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x68000 0x4>,
			      <0x68004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP3_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP3_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x68000 0x2000>,
				 <0x46000000 0x46000000 0x400000>;

			mcasp3: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x46000000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 133 1>, <&edma_xbar 132 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP3_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP3_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@6c000 {			/* 0x4846c000, ap 15 2e.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x6c000 0x4>,
			      <0x6c004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP4_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP4_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6c000 0x2000>,
				 <0x48436000 0x48436000 0x400000>;

			mcasp4: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x48436000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 135 1>, <&edma_xbar 134 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP4_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP4_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@70000 {			/* 0x48470000, ap 19 36.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x70000 0x4>,
			      <0x70004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP5_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP5_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x70000 0x2000>,
				 <0x4843a000 0x4843a000 0x400000>;

			mcasp5: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x4843a000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 137 1>, <&edma_xbar 136 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP5_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP5_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@74000 {			/* 0x48474000, ap 35 14.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x74000 0x4>,
			      <0x74004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP6_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP6_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x74000 0x2000>,
				 <0x4844c000 0x4844c000 0x400000>;

			mcasp6: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x4844c000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 139 1>, <&edma_xbar 138 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP6_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP6_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@78000 {			/* 0x48478000, ap 39 0c.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x78000 0x4>,
			      <0x78004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP7_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP7_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x78000 0x2000>,
				 <0x48450000 0x48450000 0x400000>;

			mcasp7: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x48450000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 141 1>, <&edma_xbar 140 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP7_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP7_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@7c000 {			/* 0x4847c000, ap 43 04.0 */
			compatible = "ti,sysc-dra7-mcasp", "ti,sysc";
			reg = <0x7c000 0x4>,
			      <0x7c004 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): l4per_pwrdm, l4per2_clkdm */
			clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP8_CLKCTRL 0>,
				 <&l4per2_clkctrl DRA7_L4PER2_MCASP8_CLKCTRL 24>;
			clock-names = "fck", "ahclkx";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7c000 0x2000>,
				 <0x48454000 0x48454000 0x400000>;

			mcasp8: mcasp@0 {
				compatible = "ti,dra7-mcasp-audio";
				reg = <0x0 0x2000>,
				      <0x48454000 0x1000>;	/* L3 data port */
				reg-names = "mpu","dat";
				interrupts = <GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "tx", "rx";
				dmas = <&edma_xbar 143 1>, <&edma_xbar 142 1>;
				dma-names = "tx", "rx";
				clocks = <&l4per2_clkctrl DRA7_L4PER2_MCASP8_CLKCTRL 0>,
					 <&l4per2_clkctrl DRA7_L4PER2_MCASP8_CLKCTRL 24>;
				clock-names = "fck", "ahclkx";
				status = "disabled";
			};
		};

		target-module@80000 {			/* 0x48480000, ap 31 16.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x80020 0x4>;
			reg-names = "rev";
			clocks = <&l4per2_clkctrl DRA7_L4PER2_DCAN2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x80000 0x2000>;

			dcan2: can@0 {
				compatible = "ti,dra7-d_can";
				reg = <0x0 0x2000>;
				syscon-raminit = <&scm_conf 0x558 1>;
				interrupts = <GIC_SPI 225 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&sys_clkin1>;
				status = "disabled";
			};
		};

		target-module@84000 {			/* 0x48484000, ap 3 10.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x85200 0x4>,
			      <0x85208 0x4>,
			      <0x85204 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <0>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			ti,syss-mask = <1>;
			clocks = <&gmac_clkctrl DRA7_GMAC_GMAC_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x84000 0x4000>;
			/*
			 * Do not allow gating of cpsw clock as workaround
			 * for errata i877. Keeping internal clock disabled
			 * causes the device switching characteristics
			 * to degrade over time and eventually fail to meet
			 * the data manual delay time/skew specs.
			 */
			ti,no-idle;

			mac_sw: switch@0 {
				compatible = "ti,dra7-cpsw-switch","ti,cpsw-switch";
				reg = <0x0 0x4000>;
				ranges = <0 0 0x4000>;
				clocks = <&gmac_main_clk>;
				clock-names = "fck";
				#address-cells = <1>;
				#size-cells = <1>;
				syscon = <&scm_conf>;
				status = "disabled";

				interrupts = <GIC_SPI 334 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 335 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 336 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 337 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "rx_thresh", "rx", "tx", "misc";

				ethernet-ports {
					#address-cells = <1>;
					#size-cells = <0>;

					cpsw_port1: port@1 {
						reg = <1>;
						label = "port1";
						mac-address = [ 00 00 00 00 00 00 ];
						phys = <&phy_gmii_sel 1>;
					};

					cpsw_port2: port@2 {
						reg = <2>;
						label = "port2";
						mac-address = [ 00 00 00 00 00 00 ];
						phys = <&phy_gmii_sel 2>;
					};
				};

				davinci_mdio_sw: mdio@1000 {
					compatible = "ti,cpsw-mdio","ti,davinci_mdio";
					clocks = <&gmac_main_clk>;
					clock-names = "fck";
					#address-cells = <1>;
					#size-cells = <0>;
					bus_freq = <1000000>;
					reg = <0x1000 0x100>;
				};

				cpts {
					clocks = <&gmac_clkctrl DRA7_GMAC_GMAC_CLKCTRL 25>;
					clock-names = "cpts";
				};
			};
		};
	};
};

&l4_per3 {						/* 0x48800000 */
	compatible = "ti,dra7-l4-per3", "simple-pm-bus";
	power-domains = <&prm_l4per>;
	clocks = <&l4per3_clkctrl DRA7_L4PER3_L4_PER3_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x48800000 0x800>,
	      <0x48800800 0x800>,
	      <0x48801000 0x400>,
	      <0x48801400 0x400>,
	      <0x48801800 0x400>;
	reg-names = "ap", "la", "ia0", "ia1", "ia2";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x48800000 0x200000>;	/* segment 0 */

	segment@0 {					/* 0x48800000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 1 */
			 <0x00001000 0x00001000 0x000400>,	/* ap 2 */
			 <0x00001400 0x00001400 0x000400>,	/* ap 3 */
			 <0x00001800 0x00001800 0x000400>,	/* ap 4 */
			 <0x00020000 0x00020000 0x001000>,	/* ap 5 */
			 <0x00021000 0x00021000 0x001000>,	/* ap 6 */
			 <0x00022000 0x00022000 0x001000>,	/* ap 7 */
			 <0x00023000 0x00023000 0x001000>,	/* ap 8 */
			 <0x00024000 0x00024000 0x001000>,	/* ap 9 */
			 <0x00025000 0x00025000 0x001000>,	/* ap 10 */
			 <0x00026000 0x00026000 0x001000>,	/* ap 11 */
			 <0x00027000 0x00027000 0x001000>,	/* ap 12 */
			 <0x00028000 0x00028000 0x001000>,	/* ap 13 */
			 <0x00029000 0x00029000 0x001000>,	/* ap 14 */
			 <0x0002a000 0x0002a000 0x001000>,	/* ap 15 */
			 <0x0002b000 0x0002b000 0x001000>,	/* ap 16 */
			 <0x0002c000 0x0002c000 0x001000>,	/* ap 17 */
			 <0x0002d000 0x0002d000 0x001000>,	/* ap 18 */
			 <0x0002e000 0x0002e000 0x001000>,	/* ap 19 */
			 <0x0002f000 0x0002f000 0x001000>,	/* ap 20 */
			 <0x00170000 0x00170000 0x010000>,	/* ap 21 */
			 <0x00180000 0x00180000 0x001000>,	/* ap 22 */
			 <0x00190000 0x00190000 0x010000>,	/* ap 23 */
			 <0x001a0000 0x001a0000 0x001000>,	/* ap 24 */
			 <0x001b0000 0x001b0000 0x010000>,	/* ap 25 */
			 <0x001c0000 0x001c0000 0x001000>,	/* ap 26 */
			 <0x001d0000 0x001d0000 0x010000>,	/* ap 27 */
			 <0x001e0000 0x001e0000 0x001000>,	/* ap 28 */
			 <0x00038000 0x00038000 0x001000>,	/* ap 29 */
			 <0x00039000 0x00039000 0x001000>,	/* ap 30 */
			 <0x0005c000 0x0005c000 0x001000>,	/* ap 31 */
			 <0x0005d000 0x0005d000 0x001000>,	/* ap 32 */
			 <0x0003a000 0x0003a000 0x001000>,	/* ap 33 */
			 <0x0003b000 0x0003b000 0x001000>,	/* ap 34 */
			 <0x0003c000 0x0003c000 0x001000>,	/* ap 35 */
			 <0x0003d000 0x0003d000 0x001000>,	/* ap 36 */
			 <0x0003e000 0x0003e000 0x001000>,	/* ap 37 */
			 <0x0003f000 0x0003f000 0x001000>,	/* ap 38 */
			 <0x00040000 0x00040000 0x001000>,	/* ap 39 */
			 <0x00041000 0x00041000 0x001000>,	/* ap 40 */
			 <0x00042000 0x00042000 0x001000>,	/* ap 41 */
			 <0x00043000 0x00043000 0x001000>,	/* ap 42 */
			 <0x00044000 0x00044000 0x001000>,	/* ap 43 */
			 <0x00045000 0x00045000 0x001000>,	/* ap 44 */
			 <0x00046000 0x00046000 0x001000>,	/* ap 45 */
			 <0x00047000 0x00047000 0x001000>,	/* ap 46 */
			 <0x00048000 0x00048000 0x001000>,	/* ap 47 */
			 <0x00049000 0x00049000 0x001000>,	/* ap 48 */
			 <0x0004a000 0x0004a000 0x001000>,	/* ap 49 */
			 <0x0004b000 0x0004b000 0x001000>,	/* ap 50 */
			 <0x0004c000 0x0004c000 0x001000>,	/* ap 51 */
			 <0x0004d000 0x0004d000 0x001000>,	/* ap 52 */
			 <0x0004e000 0x0004e000 0x001000>,	/* ap 53 */
			 <0x0004f000 0x0004f000 0x001000>,	/* ap 54 */
			 <0x00050000 0x00050000 0x001000>,	/* ap 55 */
			 <0x00051000 0x00051000 0x001000>,	/* ap 56 */
			 <0x00052000 0x00052000 0x001000>,	/* ap 57 */
			 <0x00053000 0x00053000 0x001000>,	/* ap 58 */
			 <0x00054000 0x00054000 0x001000>,	/* ap 59 */
			 <0x00055000 0x00055000 0x001000>,	/* ap 60 */
			 <0x00056000 0x00056000 0x001000>,	/* ap 61 */
			 <0x00057000 0x00057000 0x001000>,	/* ap 62 */
			 <0x00058000 0x00058000 0x001000>,	/* ap 63 */
			 <0x00059000 0x00059000 0x001000>,	/* ap 64 */
			 <0x0005a000 0x0005a000 0x001000>,	/* ap 65 */
			 <0x0005b000 0x0005b000 0x001000>,	/* ap 66 */
			 <0x00064000 0x00064000 0x001000>,	/* ap 67 */
			 <0x00065000 0x00065000 0x001000>,	/* ap 68 */
			 <0x0005e000 0x0005e000 0x001000>,	/* ap 69 */
			 <0x0005f000 0x0005f000 0x001000>,	/* ap 70 */
			 <0x00060000 0x00060000 0x001000>,	/* ap 71 */
			 <0x00061000 0x00061000 0x001000>,	/* ap 72 */
			 <0x00062000 0x00062000 0x001000>,	/* ap 73 */
			 <0x00063000 0x00063000 0x001000>,	/* ap 74 */
			 <0x00140000 0x00140000 0x020000>,	/* ap 75 */
			 <0x00160000 0x00160000 0x001000>,	/* ap 76 */
			 <0x00016000 0x00016000 0x001000>,	/* ap 77 */
			 <0x00017000 0x00017000 0x001000>,	/* ap 78 */
			 <0x000c0000 0x000c0000 0x020000>,	/* ap 79 */
			 <0x000e0000 0x000e0000 0x001000>,	/* ap 80 */
			 <0x00004000 0x00004000 0x001000>,	/* ap 81 */
			 <0x00005000 0x00005000 0x001000>,	/* ap 82 */
			 <0x00080000 0x00080000 0x020000>,	/* ap 83 */
			 <0x000a0000 0x000a0000 0x001000>,	/* ap 84 */
			 <0x00100000 0x00100000 0x020000>,	/* ap 85 */
			 <0x00120000 0x00120000 0x001000>,	/* ap 86 */
			 <0x00010000 0x00010000 0x001000>,	/* ap 87 */
			 <0x00011000 0x00011000 0x001000>,	/* ap 88 */
			 <0x0000a000 0x0000a000 0x001000>,	/* ap 89 */
			 <0x0000b000 0x0000b000 0x001000>,	/* ap 90 */
			 <0x0001c000 0x0001c000 0x001000>,	/* ap 91 */
			 <0x0001d000 0x0001d000 0x001000>,	/* ap 92 */
			 <0x0001e000 0x0001e000 0x001000>,	/* ap 93 */
			 <0x0001f000 0x0001f000 0x001000>,	/* ap 94 */
			 <0x00002000 0x00002000 0x001000>,	/* ap 95 */
			 <0x00003000 0x00003000 0x001000>;	/* ap 96 */

		target-module@2000 {			/* 0x48802000, ap 95 7c.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x2000 0x4>,
			      <0x2010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX13_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2000 0x1000>;

			mailbox13: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 379 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 380 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 381 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 382 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@4000 {			/* 0x48804000, ap 81 20.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4000 0x1000>;
		};

		target-module@a000 {			/* 0x4880a000, ap 89 18.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xa000 0x1000>;
		};

		target-module@10000 {			/* 0x48810000, ap 87 28.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x10000 0x1000>;
		};

		target-module@16000 {			/* 0x48816000, ap 77 1e.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x16000 0x1000>;
		};

		target-module@1c000 {			/* 0x4881c000, ap 91 1c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1c000 0x1000>;
		};

		target-module@1e000 {			/* 0x4881e000, ap 93 2c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1e000 0x1000>;
		};

		target-module@20000 {			/* 0x48820000, ap 5 08.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x20000 0x4>,
			      <0x20010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_TIMER5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x20000 0x1000>;

			timer5: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&ipu_clkctrl DRA7_IPU_TIMER5_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@22000 {			/* 0x48822000, ap 7 24.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x22000 0x4>,
			      <0x22010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_TIMER6_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x22000 0x1000>;

			timer6: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&ipu_clkctrl DRA7_IPU_TIMER6_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@24000 {			/* 0x48824000, ap 9 26.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x24000 0x4>,
			      <0x24010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_TIMER7_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x24000 0x1000>;

			timer7: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&ipu_clkctrl DRA7_IPU_TIMER7_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 38 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@26000 {			/* 0x48826000, ap 11 0c.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x26000 0x4>,
			      <0x26010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): ipu_pwrdm, ipu_clkdm */
			clocks = <&ipu_clkctrl DRA7_IPU_TIMER8_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x26000 0x1000>;

			timer8: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&ipu_clkctrl DRA7_IPU_TIMER8_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		target-module@28000 {			/* 0x48828000, ap 13 16.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x28000 0x4>,
			      <0x28010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per3_clkdm */
			clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER13_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x28000 0x1000>;

			timer13: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER13_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 339 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
			};
		};

		target-module@2a000 {			/* 0x4882a000, ap 15 10.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x2a000 0x4>,
			      <0x2a010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per3_clkdm */
			clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER14_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2a000 0x1000>;

			timer14: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER14_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 340 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
			};
		};
		timer15_target: target-module@2c000 {	/* 0x4882c000, ap 17 02.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x2c000 0x4>,
			      <0x2c010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per3_clkdm */
			clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER15_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2c000 0x1000>;

			timer15: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER15_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 341 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
			};
		};

		timer16_target: target-module@2e000 {	/* 0x4882e000, ap 19 14.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x2e000 0x4>,
			      <0x2e010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l4per_pwrdm, l4per3_clkdm */
			clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER16_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2e000 0x1000>;

			timer16: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&l4per3_clkctrl DRA7_L4PER3_TIMER16_CLKCTRL 24>, <&timer_sys_clk_div>;
				clock-names = "fck", "timer_sys_ck";
				interrupts = <GIC_SPI 342 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-pwm;
			};
		};

		rtctarget: target-module@38000 {			/* 0x48838000, ap 29 12.0 */
			compatible = "ti,sysc-omap4-simple", "ti,sysc";
			reg = <0x38074 0x4>,
			      <0x38078 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): rtc_pwrdm, rtc_clkdm */
			clocks = <&rtc_clkctrl DRA7_RTC_RTCSS_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x38000 0x1000>;

			rtc: rtc@0 {
				compatible = "ti,am3352-rtc";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 217 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 217 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&sys_32k_ck>;
			};
		};

		target-module@3a000 {			/* 0x4883a000, ap 33 3e.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x3a000 0x4>,
			      <0x3a010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3a000 0x1000>;

			mailbox2: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 237 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 238 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 239 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 240 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@3c000 {			/* 0x4883c000, ap 35 3a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x3c000 0x4>,
			      <0x3c010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3c000 0x1000>;

			mailbox3: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 241 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 242 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 243 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 244 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@3e000 {			/* 0x4883e000, ap 37 46.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x3e000 0x4>,
			      <0x3e010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX4_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3e000 0x1000>;

			mailbox4: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 245 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 246 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 247 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 248 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@40000 {			/* 0x48840000, ap 39 64.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x40000 0x4>,
			      <0x40010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX5_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x40000 0x1000>;

			mailbox5: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 249 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 250 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 251 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 252 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@42000 {			/* 0x48842000, ap 41 4e.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x42000 0x4>,
			      <0x42010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX6_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x42000 0x1000>;

			mailbox6: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 253 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 254 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 255 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 256 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@44000 {			/* 0x48844000, ap 43 42.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x44000 0x4>,
			      <0x44010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX7_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x44000 0x1000>;

			mailbox7: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 257 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 258 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 259 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 260 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@46000 {			/* 0x48846000, ap 45 48.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x46000 0x4>,
			      <0x46010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX8_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x46000 0x1000>;

			mailbox8: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 261 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 262 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 263 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 264 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@48000 {			/* 0x48848000, ap 47 36.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x48000 0x1000>;
		};

		target-module@4a000 {			/* 0x4884a000, ap 49 38.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4a000 0x1000>;
		};

		target-module@4c000 {			/* 0x4884c000, ap 51 44.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4c000 0x1000>;
		};

		target-module@4e000 {			/* 0x4884e000, ap 53 4c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4e000 0x1000>;
		};

		target-module@50000 {			/* 0x48850000, ap 55 40.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x50000 0x1000>;
		};

		target-module@52000 {			/* 0x48852000, ap 57 54.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x52000 0x1000>;
		};

		target-module@54000 {			/* 0x48854000, ap 59 1a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x54000 0x1000>;
		};

		target-module@56000 {			/* 0x48856000, ap 61 22.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x56000 0x1000>;
		};

		target-module@58000 {			/* 0x48858000, ap 63 2a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x58000 0x1000>;
		};

		target-module@5a000 {			/* 0x4885a000, ap 65 5c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5a000 0x1000>;
		};

		target-module@5c000 {			/* 0x4885c000, ap 31 32.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5c000 0x1000>;
		};

		target-module@5e000 {			/* 0x4885e000, ap 69 6c.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x5e000 0x4>,
			      <0x5e010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX9_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5e000 0x1000>;

			mailbox9: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 265 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 266 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 267 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 268 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@60000 {			/* 0x48860000, ap 71 4a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x60000 0x4>,
			      <0x60010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX10_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x60000 0x1000>;

			mailbox10: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 269 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 270 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 271 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 272 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@62000 {			/* 0x48862000, ap 73 74.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x62000 0x4>,
			      <0x62010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX11_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x62000 0x1000>;

			mailbox11: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 273 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 274 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 275 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 276 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@64000 {			/* 0x48864000, ap 67 52.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x64000 0x4>,
			      <0x64010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_SOFTRESET>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			/* Domains (P, C): core_pwrdm, l4cfg_clkdm */
			clocks = <&l4cfg_clkctrl DRA7_L4CFG_MAILBOX12_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x64000 0x1000>;

			mailbox12: mailbox@0 {
				compatible = "ti,omap4-mailbox";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 277 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 278 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 279 IRQ_TYPE_LEVEL_HIGH>,
					     <GIC_SPI 280 IRQ_TYPE_LEVEL_HIGH>;
				#mbox-cells = <1>;
				ti,mbox-num-users = <4>;
				ti,mbox-num-fifos = <12>;
				status = "disabled";
			};
		};

		target-module@80000 {			/* 0x48880000, ap 83 0e.1 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x80000 0x4>,
			      <0x80010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_DMADISABLE>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x80000 0x20000>;

			omap_dwc3_1: omap_dwc3_1@0 {
				compatible = "ti,dwc3";
				reg = <0x0 0x10000>;
				interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				utmi-mode = <2>;
				ranges = <0 0 0x20000>;

				usb1: usb@10000 {
					compatible = "snps,dwc3";
					reg = <0x10000 0x17000>;
					interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "peripheral",
							  "host",
							  "otg";
					phys = <&usb2_phy1>, <&usb3_phy1>;
					phy-names = "usb2-phy", "usb3-phy";
					maximum-speed = "super-speed";
					dr_mode = "otg";
					snps,dis_u3_susphy_quirk;
					snps,dis_u2_susphy_quirk;
				};
			};
		};

		target-module@c0000 {			/* 0x488c0000, ap 79 06.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xc0000 0x4>,
			      <0xc0010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_DMADISABLE>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc0000 0x20000>;

			omap_dwc3_2: omap_dwc3_2@0 {
				compatible = "ti,dwc3";
				reg = <0x0 0x10000>;
				interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				utmi-mode = <2>;
				ranges = <0 0 0x20000>;

				usb2: usb@10000 {
					compatible = "snps,dwc3";
					reg = <0x10000 0x17000>;
					interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "peripheral",
							  "host",
							  "otg";
					phys = <&usb2_phy2>;
					phy-names = "usb2-phy";
					maximum-speed = "high-speed";
					dr_mode = "otg";
					snps,dis_u3_susphy_quirk;
					snps,dis_u2_susphy_quirk;
					snps,dis_metastability_quirk;
				};
			};
		};

		usb3_tm: target-module@100000 {		/* 0x48900000, ap 85 04.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x100000 0x4>,
			      <0x100010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <SYSC_OMAP4_DMADISABLE>;
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): l3init_pwrdm, l3init_clkdm */
			clocks = <&l3init_clkctrl DRA7_L3INIT_USB_OTG_SS3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x100000 0x20000>;

			omap_dwc3_3: omap_dwc3_3@0 {
				compatible = "ti,dwc3";
				reg = <0x0 0x10000>;
				interrupts = <GIC_SPI 344 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				utmi-mode = <2>;
				ranges = <0 0 0x20000>;
				status = "disabled";

				usb3: usb@10000 {
					compatible = "snps,dwc3";
					reg = <0x10000 0x17000>;
					interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>,
						     <GIC_SPI 344 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-names = "peripheral",
							  "host",
							  "otg";
					maximum-speed = "high-speed";
					dr_mode = "otg";
					snps,dis_u3_susphy_quirk;
					snps,dis_u2_susphy_quirk;
				};
			};
		};

		target-module@170000 {			/* 0x48970000, ap 21 0a.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x170010 0x4>;
			reg-names = "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			clocks = <&cam_clkctrl DRA7_CAM_VIP1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x170000 0x10000>;
			status = "disabled";
		};

		target-module@190000 {			/* 0x48990000, ap 23 2e.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x190010 0x4>;
			reg-names = "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			clocks = <&cam_clkctrl DRA7_CAM_VIP2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x190000 0x10000>;
			status = "disabled";
		};

		target-module@1b0000 {			/* 0x489b0000, ap 25 34.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x1b0000 0x4>,
			      <0x1b0010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			clocks = <&cam_clkctrl DRA7_CAM_VIP3_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1b0000 0x10000>;
			status = "disabled";
		};

		target-module@1d0010 {			/* 0x489d0000, ap 27 30.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x1d0010 0x4>;
			reg-names = "sysc";
			ti,sysc-midle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>;
			power-domains = <&prm_vpe>;
			clocks = <&vpe_clkctrl DRA7_VPE_VPE_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1d0000 0x10000>;

			vpe: vpe@0 {
				compatible = "ti,dra7-vpe";
				reg = <0x0000 0x120>,
				      <0x0700 0x80>,
				      <0x5700 0x18>,
				      <0xd000 0x400>;
				reg-names = "vpe_top",
					    "sc",
					    "csc",
					    "vpdma";
				interrupts = <GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>;
			};
		};
	};
};

&l4_wkup {						/* 0x4ae00000 */
	compatible = "ti,dra7-l4-wkup", "simple-pm-bus";
	power-domains = <&prm_wkupaon>;
	clocks = <&wkupaon_clkctrl DRA7_WKUPAON_L4_WKUP_CLKCTRL 0>;
	clock-names = "fck";
	reg = <0x4ae00000 0x800>,
	      <0x4ae00800 0x800>,
	      <0x4ae01000 0x1000>;
	reg-names = "ap", "la", "ia0";
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0x00000000 0x4ae00000 0x010000>,	/* segment 0 */
		 <0x00010000 0x4ae10000 0x010000>,	/* segment 1 */
		 <0x00020000 0x4ae20000 0x010000>,	/* segment 2 */
		 <0x00030000 0x4ae30000 0x010000>;	/* segment 3 */

	segment@0 {					/* 0x4ae00000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00000000 0x000800>,	/* ap 0 */
			 <0x00001000 0x00001000 0x001000>,	/* ap 1 */
			 <0x00000800 0x00000800 0x000800>,	/* ap 2 */
			 <0x00006000 0x00006000 0x002000>,	/* ap 3 */
			 <0x00008000 0x00008000 0x001000>,	/* ap 4 */
			 <0x00004000 0x00004000 0x001000>,	/* ap 15 */
			 <0x00005000 0x00005000 0x001000>,	/* ap 16 */
			 <0x0000c000 0x0000c000 0x001000>,	/* ap 17 */
			 <0x0000d000 0x0000d000 0x001000>;	/* ap 18 */

		target-module@4000 {			/* 0x4ae04000, ap 15 40.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x4000 0x4>,
			      <0x4010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_COUNTER_32K_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4000 0x1000>;

			counter32k: counter@0 {
				compatible = "ti,omap-counter32k";
				reg = <0x0 0x40>;
			};
		};

		target-module@6000 {			/* 0x4ae06000, ap 3 10.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0x6000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x6000 0x2000>;

			prm: prm@0 {
				compatible = "ti,dra7-prm", "simple-bus";
				reg = <0 0x3000>;
				interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0 0x3000>;

				prm_clocks: clocks {
					#address-cells = <1>;
					#size-cells = <0>;
				};

				prm_clockdomains: clockdomains {
				};
			};
		};

		target-module@c000 {			/* 0x4ae0c000, ap 17 50.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xc000 0x4>;
			reg-names = "rev";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc000 0x1000>;

			scm_wkup: scm_conf@0 {
				compatible = "syscon";
				reg = <0 0x1000>;
			};
		};
	};

	segment@10000 {					/* 0x4ae10000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00000000 0x00010000 0x001000>,	/* ap 5 */
			 <0x00001000 0x00011000 0x001000>,	/* ap 6 */
			 <0x00004000 0x00014000 0x001000>,	/* ap 7 */
			 <0x00005000 0x00015000 0x001000>,	/* ap 8 */
			 <0x00008000 0x00018000 0x001000>,	/* ap 9 */
			 <0x00009000 0x00019000 0x001000>,	/* ap 10 */
			 <0x0000c000 0x0001c000 0x001000>,	/* ap 11 */
			 <0x0000d000 0x0001d000 0x001000>;	/* ap 12 */

		target-module@0 {			/* 0x4ae10000, ap 5 20.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x0 0x4>,
			      <0x10 0x4>,
			      <0x114 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_GPIO1_CLKCTRL 0>,
				 <&wkupaon_clkctrl DRA7_WKUPAON_GPIO1_CLKCTRL 8>;
			clock-names = "fck", "dbclk";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1000>;

			gpio1: gpio@0 {
				compatible = "ti,omap4-gpio";
				reg = <0x0 0x200>;
				interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
				gpio-controller;
				#gpio-cells = <2>;
				interrupt-controller;
				#interrupt-cells = <2>;
			};
		};

		target-module@4000 {			/* 0x4ae14000, ap 7 28.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0x4000 0x4>,
			      <0x4010 0x4>,
			      <0x4014 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_EMUFREE |
					 SYSC_OMAP2_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_WD_TIMER2_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x4000 0x1000>;

			wdt2: wdt@0 {
				compatible = "ti,omap3-wdt";
				reg = <0x0 0x80>;
				interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		timer1_target: target-module@8000 {	/* 0x4ae18000, ap 9 30.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x8000 0x4>,
			      <0x8010 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_TIMER1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x8000 0x1000>;

			timer1: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				clocks = <&wkupaon_clkctrl DRA7_WKUPAON_TIMER1_CLKCTRL 24>;
				clock-names = "fck";
				interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-alwon;
			};
		};

		target-module@c000 {			/* 0x4ae1c000, ap 11 38.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc000 0x1000>;
		};
	};

	segment@20000 {					/* 0x4ae20000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x00006000 0x00026000 0x001000>,	/* ap 13 */
			 <0x0000a000 0x0002a000 0x001000>,	/* ap 14 */
			 <0x00000000 0x00020000 0x001000>,	/* ap 19 */
			 <0x00001000 0x00021000 0x001000>,	/* ap 20 */
			 <0x00002000 0x00022000 0x001000>,	/* ap 21 */
			 <0x00003000 0x00023000 0x001000>,	/* ap 22 */
			 <0x00007000 0x00027000 0x000400>,	/* ap 23 */
			 <0x00008000 0x00028000 0x000800>,	/* ap 24 */
			 <0x00009000 0x00029000 0x000100>,	/* ap 25 */
			 <0x00008800 0x00028800 0x000200>,	/* ap 26 */
			 <0x00008a00 0x00028a00 0x000100>,	/* ap 27 */
			 <0x0000b000 0x0002b000 0x001000>,	/* ap 28 */
			 <0x0000c000 0x0002c000 0x001000>,	/* ap 29 */
			 <0x0000f000 0x0002f000 0x001000>;	/* ap 32 */

		target-module@0 {			/* 0x4ae20000, ap 19 08.0 */
			compatible = "ti,sysc-omap4-timer", "ti,sysc";
			reg = <0x0 0x4>,
			      <0x10 0x4>;
			reg-names = "rev", "sysc";
			ti,sysc-mask = <(SYSC_OMAP4_FREEEMU |
					 SYSC_OMAP4_SOFTRESET)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_TIMER12_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1000>;

			timer12: timer@0 {
				compatible = "ti,omap5430-timer";
				reg = <0x0 0x80>;
				interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
				ti,timer-alwon;
				ti,timer-secure;
			};
		};

		target-module@2000 {			/* 0x4ae22000, ap 21 18.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x2000 0x1000>;
		};

		target-module@6000 {			/* 0x4ae26000, ap 13 48.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x00000000 0x00006000 0x00001000>,
				 <0x00001000 0x00007000 0x00000400>,
				 <0x00002000 0x00008000 0x00000800>,
				 <0x00002800 0x00008800 0x00000200>,
				 <0x00002a00 0x00008a00 0x00000100>,
				 <0x00003000 0x00009000 0x00000100>;
		};

		target-module@b000 {			/* 0x4ae2b000, ap 28 02.0 */
			compatible = "ti,sysc-omap2", "ti,sysc";
			reg = <0xb050 0x4>,
			      <0xb054 0x4>,
			      <0xb058 0x4>;
			reg-names = "rev", "sysc", "syss";
			ti,sysc-mask = <(SYSC_OMAP2_ENAWAKEUP |
					 SYSC_OMAP2_SOFTRESET |
					 SYSC_OMAP2_AUTOIDLE)>;
			ti,sysc-sidle = <SYSC_IDLE_FORCE>,
					<SYSC_IDLE_NO>,
					<SYSC_IDLE_SMART>,
					<SYSC_IDLE_SMART_WKUP>;
			ti,syss-mask = <1>;
			/* Domains (P, C): wkupaon_pwrdm, wkupaon_clkdm */
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_UART10_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xb000 0x1000>;

			uart10: serial@0 {
				compatible = "ti,dra742-uart";
				reg = <0x0 0x100>;
				interrupts = <GIC_SPI 221 IRQ_TYPE_LEVEL_HIGH>;
				clock-frequency = <48000000>;
				status = "disabled";
			};
		};

		target-module@f000 {			/* 0x4ae2f000, ap 32 58.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xf000 0x1000>;
		};
	};

	segment@30000 {					/* 0x4ae30000 */
		compatible = "simple-pm-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0x0000c000 0x0003c000 0x002000>,	/* ap 30 */
			 <0x0000e000 0x0003e000 0x001000>,	/* ap 31 */
			 <0x00000000 0x00030000 0x001000>,	/* ap 33 */
			 <0x00001000 0x00031000 0x001000>,	/* ap 34 */
			 <0x00002000 0x00032000 0x001000>,	/* ap 35 */
			 <0x00003000 0x00033000 0x001000>,	/* ap 36 */
			 <0x00004000 0x00034000 0x001000>,	/* ap 37 */
			 <0x00005000 0x00035000 0x001000>,	/* ap 38 */
			 <0x00006000 0x00036000 0x001000>,	/* ap 39 */
			 <0x00007000 0x00037000 0x001000>,	/* ap 40 */
			 <0x00008000 0x00038000 0x001000>,	/* ap 41 */
			 <0x00009000 0x00039000 0x001000>,	/* ap 42 */
			 <0x0000a000 0x0003a000 0x001000>;	/* ap 43 */

		target-module@1000 {			/* 0x4ae31000, ap 34 60.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x1000 0x1000>;
		};

		target-module@3000 {			/* 0x4ae33000, ap 36 0a.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x3000 0x1000>;
		};

		target-module@5000 {			/* 0x4ae35000, ap 38 0c.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x5000 0x1000>;
		};

		target-module@7000 {			/* 0x4ae37000, ap 40 68.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x7000 0x1000>;
		};

		target-module@9000 {			/* 0x4ae39000, ap 42 70.0 */
			compatible = "ti,sysc";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x9000 0x1000>;
		};

		target-module@c000 {			/* 0x4ae3c000, ap 30 04.0 */
			compatible = "ti,sysc-omap4", "ti,sysc";
			reg = <0xc020 0x4>;
			reg-names = "rev";
			clocks = <&wkupaon_clkctrl DRA7_WKUPAON_DCAN1_CLKCTRL 0>;
			clock-names = "fck";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0xc000 0x2000>;

			dcan1: can@0 {
				compatible = "ti,dra7-d_can";
				reg = <0x0 0x2000>;
				syscon-raminit = <&scm_conf 0x558 0>;
				interrupts = <GIC_SPI 222 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&wkupaon_clkctrl DRA7_WKUPAON_DCAN1_CLKCTRL 24>;
				status = "disabled";
			};
		};
	};
};

