// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (c) 2015 MediaTek Inc.
 * Author: Erin.Lo <erin.lo@mediatek.com>
 *
 */

#include <dt-bindings/clock/mt2701-clk.h>
#include <dt-bindings/phy/phy.h>
#include <dt-bindings/power/mt2701-power.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/memory/mt2701-larb-port.h>
#include <dt-bindings/reset/mt2701-resets.h>
#include "mt2701-pinfunc.h"

/ {
	#address-cells = <2>;
	#size-cells = <2>;
	compatible = "mediatek,mt2701";
	interrupt-parent = <&cirq>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "mediatek,mt81xx-tz-smp";

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x0>;
		};
		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x1>;
		};
		cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x2>;
		};
		cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0x3>;
		};
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		trustzone-bootinfo@80002000 {
			compatible = "mediatek,trustzone-bootinfo";
			reg = <0 0x80002000 0 0x1000>;
		};
	};

	system_clk: dummy13m {
		compatible = "fixed-clock";
		clock-frequency = <13000000>;
		#clock-cells = <0>;
	};

	rtc_clk: dummy32k {
		compatible = "fixed-clock";
		clock-frequency = <32000>;
		#clock-cells = <0>;
	};

	clk26m: oscillator@0 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <26000000>;
		clock-output-names = "clk26m";
	};

	rtc32k: oscillator@1 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32000>;
		clock-output-names = "rtc32k";
	};

	thermal-zones {
		cpu_thermal: cpu_thermal {
			polling-delay-passive = <1000>; /* milliseconds */
			polling-delay = <1000>; /* milliseconds */

			thermal-sensors = <&thermal 0>;
			sustainable-power = <1000>;

			trips {
				threshold: trip-point@0 {
					temperature = <68000>;
					hysteresis = <2000>;
					type = "passive";
				};

				target: trip-point@1 {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};

				cpu_crit: cpu_crit@0 {
					temperature = <115000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupt-parent = <&gic>;
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	topckgen: syscon@10000000 {
		compatible = "mediatek,mt2701-topckgen", "syscon";
		reg = <0 0x10000000 0 0x1000>;
		#clock-cells = <1>;
	};

	infracfg: syscon@10001000 {
		compatible = "mediatek,mt2701-infracfg", "syscon";
		reg = <0 0x10001000 0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	pericfg: syscon@10003000 {
		compatible = "mediatek,mt2701-pericfg", "syscon";
		reg = <0 0x10003000 0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	syscfg_pctl_a: syscfg@10005000 {
		compatible = "mediatek,mt2701-pctl-a-syscfg", "syscon";
		reg = <0 0x10005000 0 0x1000>;
	};

	scpsys: power-controller@10006000 {
		compatible = "mediatek,mt2701-scpsys", "syscon";
		#power-domain-cells = <1>;
		reg = <0 0x10006000 0 0x1000>;
		infracfg = <&infracfg>;
		clocks = <&topckgen CLK_TOP_MM_SEL>,
			 <&topckgen CLK_TOP_MFG_SEL>,
			 <&topckgen CLK_TOP_ETHIF_SEL>;
		clock-names = "mm", "mfg", "ethif";
	};

	watchdog: watchdog@10007000 {
		compatible = "mediatek,mt2701-wdt",
			     "mediatek,mt6589-wdt";
		reg = <0 0x10007000 0 0x100>;
	};

	timer: timer@10008000 {
		compatible = "mediatek,mt2701-timer",
			     "mediatek,mt6577-timer";
		reg = <0 0x10008000 0 0x80>;
		interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&system_clk>, <&rtc_clk>;
		clock-names = "system-clk", "rtc-clk";
	};

	pio: pinctrl@1000b000 {
		compatible = "mediatek,mt2701-pinctrl";
		reg = <0 0x1000b000 0 0x1000>;
		mediatek,pctl-regmap = <&syscfg_pctl_a>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
		interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
	};

	smi_common: smi@1000c000 {
		compatible = "mediatek,mt2701-smi-common";
		reg = <0 0x1000c000 0 0x1000>;
		clocks = <&infracfg CLK_INFRA_SMI>,
			 <&mmsys CLK_MM_SMI_COMMON>,
			 <&infracfg CLK_INFRA_SMI>;
		clock-names = "apb", "smi", "async";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_DISP>;
	};

	sysirq: interrupt-controller@10200100 {
		compatible = "mediatek,mt2701-sysirq",
			     "mediatek,mt6577-sysirq";
		interrupt-controller;
		#interrupt-cells = <3>;
		interrupt-parent = <&gic>;
		reg = <0 0x10200100 0 0x1c>;
	};

	cirq: interrupt-controller@10204000 {
		compatible = "mediatek,mt2701-cirq",
			     "mediatek,mtk-cirq";
		interrupt-controller;
		#interrupt-cells = <3>;
		interrupt-parent = <&sysirq>;
		reg = <0 0x10204000 0 0x400>;
		mediatek,ext-irq-range = <32 200>;
	};

	iommu: mmsys_iommu@10205000 {
		compatible = "mediatek,mt2701-m4u";
		reg = <0 0x10205000 0 0x1000>;
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&infracfg CLK_INFRA_M4U>;
		clock-names = "bclk";
		mediatek,larbs = <&larb0 &larb1 &larb2>;
		#iommu-cells = <1>;
	};

	apmixedsys: syscon@10209000 {
		compatible = "mediatek,mt2701-apmixedsys", "syscon";
		reg = <0 0x10209000 0 0x1000>;
		#clock-cells = <1>;
	};

	gic: interrupt-controller@10211000 {
		compatible = "arm,cortex-a7-gic";
		interrupt-controller;
		#interrupt-cells = <3>;
		interrupt-parent = <&gic>;
		reg = <0 0x10211000 0 0x1000>,
		      <0 0x10212000 0 0x2000>,
		      <0 0x10214000 0 0x2000>,
		      <0 0x10216000 0 0x2000>;
	};

	auxadc: adc@11001000 {
		compatible = "mediatek,mt2701-auxadc";
		reg = <0 0x11001000 0 0x1000>;
		clocks = <&pericfg CLK_PERI_AUXADC>;
		clock-names = "main";
		#io-channel-cells = <1>;
		status = "disabled";
	};

	uart0: serial@11002000 {
		compatible = "mediatek,mt2701-uart",
			     "mediatek,mt6577-uart";
		reg = <0 0x11002000 0 0x400>;
		interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_UART0_SEL>, <&pericfg CLK_PERI_UART0>;
		clock-names = "baud", "bus";
		status = "disabled";
	};

	uart1: serial@11003000 {
		compatible = "mediatek,mt2701-uart",
			     "mediatek,mt6577-uart";
		reg = <0 0x11003000 0 0x400>;
		interrupts = <GIC_SPI 52 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_UART1_SEL>, <&pericfg CLK_PERI_UART1>;
		clock-names = "baud", "bus";
		status = "disabled";
	};

	uart2: serial@11004000 {
		compatible = "mediatek,mt2701-uart",
			     "mediatek,mt6577-uart";
		reg = <0 0x11004000 0 0x400>;
		interrupts = <GIC_SPI 53 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_UART2_SEL>, <&pericfg CLK_PERI_UART2>;
		clock-names = "baud", "bus";
		status = "disabled";
	};

	uart3: serial@11005000 {
		compatible = "mediatek,mt2701-uart",
			     "mediatek,mt6577-uart";
		reg = <0 0x11005000 0 0x400>;
		interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_UART3_SEL>, <&pericfg CLK_PERI_UART3>;
		clock-names = "baud", "bus";
		status = "disabled";
	};

	i2c0: i2c@11007000 {
		compatible = "mediatek,mt2701-i2c",
			     "mediatek,mt6577-i2c";
		reg = <0 0x11007000 0 0x70>,
		      <0 0x11000200 0 0x80>;
		interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_LOW>;
		clock-div = <16>;
		clocks = <&pericfg CLK_PERI_I2C0>, <&pericfg CLK_PERI_AP_DMA>;
		clock-names = "main", "dma";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c1: i2c@11008000 {
		compatible = "mediatek,mt2701-i2c",
			     "mediatek,mt6577-i2c";
		reg = <0 0x11008000 0 0x70>,
		      <0 0x11000280 0 0x80>;
		interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_LOW>;
		clock-div = <16>;
		clocks = <&pericfg CLK_PERI_I2C1>, <&pericfg CLK_PERI_AP_DMA>;
		clock-names = "main", "dma";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c2: i2c@11009000 {
		compatible = "mediatek,mt2701-i2c",
			     "mediatek,mt6577-i2c";
		reg = <0 0x11009000 0 0x70>,
		      <0 0x11000300 0 0x80>;
		interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_LOW>;
		clock-div = <16>;
		clocks = <&pericfg CLK_PERI_I2C2>, <&pericfg CLK_PERI_AP_DMA>;
		clock-names = "main", "dma";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi0: spi@1100a000 {
		compatible = "mediatek,mt2701-spi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0 0x1100a000 0 0x100>;
		interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&topckgen CLK_TOP_SYSPLL3_D2>,
			 <&topckgen CLK_TOP_SPI0_SEL>,
			 <&pericfg CLK_PERI_SPI0>;
		clock-names = "parent-clk", "sel-clk", "spi-clk";
		status = "disabled";
	};

	thermal: thermal@1100b000 {
		#thermal-sensor-cells = <0>;
		compatible = "mediatek,mt2701-thermal";
		reg = <0 0x1100b000 0 0x1000>;
		interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_THERM>, <&pericfg CLK_PERI_AUXADC>;
		clock-names = "therm", "auxadc";
		resets = <&pericfg MT2701_PERI_THERM_SW_RST>;
		reset-names = "therm";
		mediatek,auxadc = <&auxadc>;
		mediatek,apmixedsys = <&apmixedsys>;
	};

	nandc: nand-controller@1100d000 {
		compatible = "mediatek,mt2701-nfc";
		reg = <0 0x1100d000 0 0x1000>;
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_NFI>,
			 <&pericfg CLK_PERI_NFI_PAD>;
		clock-names = "nfi_clk", "pad_clk";
		status = "disabled";
		ecc-engine = <&bch>;
		#address-cells = <1>;
		#size-cells = <0>;
	};

	bch: ecc@1100e000 {
		compatible = "mediatek,mt2701-ecc";
		reg = <0 0x1100e000 0 0x1000>;
		interrupts = <GIC_SPI 55 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&pericfg CLK_PERI_NFI_ECC>;
		clock-names = "nfiecc_clk";
		status = "disabled";
	};

	nor_flash: spi@11014000 {
		compatible = "mediatek,mt2701-nor",
			     "mediatek,mt8173-nor";
		reg = <0 0x11014000 0 0xe0>;
		clocks = <&pericfg CLK_PERI_FLASH>,
			 <&topckgen CLK_TOP_FLASH_SEL>;
		clock-names = "spi", "sf";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	spi1: spi@11016000 {
		compatible = "mediatek,mt2701-spi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0 0x11016000 0 0x100>;
		interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&topckgen CLK_TOP_SYSPLL3_D2>,
			 <&topckgen CLK_TOP_SPI1_SEL>,
			 <&pericfg CLK_PERI_SPI1>;
		clock-names = "parent-clk", "sel-clk", "spi-clk";
		status = "disabled";
	};

	spi2: spi@11017000 {
		compatible = "mediatek,mt2701-spi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0 0x11017000 0 0x1000>;
		interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&topckgen CLK_TOP_SYSPLL3_D2>,
			 <&topckgen CLK_TOP_SPI2_SEL>,
			 <&pericfg CLK_PERI_SPI2>;
		clock-names = "parent-clk", "sel-clk", "spi-clk";
		status = "disabled";
	};

	audsys: clock-controller@11220000 {
		compatible = "mediatek,mt2701-audsys", "syscon";
		reg = <0 0x11220000 0 0x2000>;
		#clock-cells = <1>;

		afe: audio-controller {
			compatible = "mediatek,mt2701-audio";
			interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_LOW>,
				      <GIC_SPI 132 IRQ_TYPE_LEVEL_LOW>;
			interrupt-names = "afe", "asys";
			power-domains = <&scpsys MT2701_POWER_DOMAIN_IFR_MSC>;

			clocks = <&infracfg CLK_INFRA_AUDIO>,
				 <&topckgen CLK_TOP_AUD_MUX1_SEL>,
				 <&topckgen CLK_TOP_AUD_MUX2_SEL>,
				 <&topckgen CLK_TOP_AUD_48K_TIMING>,
				 <&topckgen CLK_TOP_AUD_44K_TIMING>,
				 <&topckgen CLK_TOP_AUD_K1_SRC_SEL>,
				 <&topckgen CLK_TOP_AUD_K2_SRC_SEL>,
				 <&topckgen CLK_TOP_AUD_K3_SRC_SEL>,
				 <&topckgen CLK_TOP_AUD_K4_SRC_SEL>,
				 <&topckgen CLK_TOP_AUD_K1_SRC_DIV>,
				 <&topckgen CLK_TOP_AUD_K2_SRC_DIV>,
				 <&topckgen CLK_TOP_AUD_K3_SRC_DIV>,
				 <&topckgen CLK_TOP_AUD_K4_SRC_DIV>,
				 <&topckgen CLK_TOP_AUD_I2S1_MCLK>,
				 <&topckgen CLK_TOP_AUD_I2S2_MCLK>,
				 <&topckgen CLK_TOP_AUD_I2S3_MCLK>,
				 <&topckgen CLK_TOP_AUD_I2S4_MCLK>,
				 <&audsys CLK_AUD_I2SO1>,
				 <&audsys CLK_AUD_I2SO2>,
				 <&audsys CLK_AUD_I2SO3>,
				 <&audsys CLK_AUD_I2SO4>,
				 <&audsys CLK_AUD_I2SIN1>,
				 <&audsys CLK_AUD_I2SIN2>,
				 <&audsys CLK_AUD_I2SIN3>,
				 <&audsys CLK_AUD_I2SIN4>,
				 <&audsys CLK_AUD_ASRCO1>,
				 <&audsys CLK_AUD_ASRCO2>,
				 <&audsys CLK_AUD_ASRCO3>,
				 <&audsys CLK_AUD_ASRCO4>,
				 <&audsys CLK_AUD_AFE>,
				 <&audsys CLK_AUD_AFE_CONN>,
				 <&audsys CLK_AUD_A1SYS>,
				 <&audsys CLK_AUD_A2SYS>,
				 <&audsys CLK_AUD_AFE_MRGIF>;

			clock-names = "infra_sys_audio_clk",
				      "top_audio_mux1_sel",
				      "top_audio_mux2_sel",
				      "top_audio_a1sys_hp",
				      "top_audio_a2sys_hp",
				      "i2s0_src_sel",
				      "i2s1_src_sel",
				      "i2s2_src_sel",
				      "i2s3_src_sel",
				      "i2s0_src_div",
				      "i2s1_src_div",
				      "i2s2_src_div",
				      "i2s3_src_div",
				      "i2s0_mclk_en",
				      "i2s1_mclk_en",
				      "i2s2_mclk_en",
				      "i2s3_mclk_en",
				      "i2so0_hop_ck",
				      "i2so1_hop_ck",
				      "i2so2_hop_ck",
				      "i2so3_hop_ck",
				      "i2si0_hop_ck",
				      "i2si1_hop_ck",
				      "i2si2_hop_ck",
				      "i2si3_hop_ck",
				      "asrc0_out_ck",
				      "asrc1_out_ck",
				      "asrc2_out_ck",
				      "asrc3_out_ck",
				      "audio_afe_pd",
				      "audio_afe_conn_pd",
				      "audio_a1sys_pd",
				      "audio_a2sys_pd",
				      "audio_mrgif_pd";

			assigned-clocks = <&topckgen CLK_TOP_AUD_MUX1_SEL>,
					  <&topckgen CLK_TOP_AUD_MUX2_SEL>,
					  <&topckgen CLK_TOP_AUD_MUX1_DIV>,
					  <&topckgen CLK_TOP_AUD_MUX2_DIV>;
			assigned-clock-parents = <&topckgen CLK_TOP_AUD1PLL_98M>,
						 <&topckgen CLK_TOP_AUD2PLL_90M>;
			assigned-clock-rates = <0>, <0>, <49152000>, <45158400>;
		};
	};

	mmsys: syscon@14000000 {
		compatible = "mediatek,mt2701-mmsys", "syscon";
		reg = <0 0x14000000 0 0x1000>;
		#clock-cells = <1>;
	};

	bls: pwm@1400a000 {
		compatible = "mediatek,mt2701-disp-pwm";
		reg = <0 0x1400a000 0 0x1000>;
		#pwm-cells = <2>;
		clocks = <&mmsys CLK_MM_MDP_BLS_26M>, <&mmsys CLK_MM_DISP_BLS>;
		clock-names = "main", "mm";
		status = "disabled";
	};

	larb0: larb@14010000 {
		compatible = "mediatek,mt2701-smi-larb";
		reg = <0 0x14010000 0 0x1000>;
		mediatek,smi = <&smi_common>;
		mediatek,larb-id = <0>;
		clocks = <&mmsys CLK_MM_SMI_LARB0>,
			 <&mmsys CLK_MM_SMI_LARB0>;
		clock-names = "apb", "smi";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_DISP>;
	};

	imgsys: syscon@15000000 {
		compatible = "mediatek,mt2701-imgsys", "syscon";
		reg = <0 0x15000000 0 0x1000>;
		#clock-cells = <1>;
	};

	larb2: larb@15001000 {
		compatible = "mediatek,mt2701-smi-larb";
		reg = <0 0x15001000 0 0x1000>;
		mediatek,smi = <&smi_common>;
		mediatek,larb-id = <2>;
		clocks = <&imgsys CLK_IMG_SMI_COMM>,
			 <&imgsys CLK_IMG_SMI_COMM>;
		clock-names = "apb", "smi";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_ISP>;
	};

	jpegdec: jpegdec@15004000 {
		compatible = "mediatek,mt2701-jpgdec";
		reg = <0 0x15004000 0 0x1000>;
		interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&imgsys CLK_IMG_JPGDEC_SMI>,
			  <&imgsys CLK_IMG_JPGDEC>;
		clock-names = "jpgdec-smi",
			      "jpgdec";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_ISP>;
		iommus = <&iommu MT2701_M4U_PORT_JPGDEC_WDMA>,
			 <&iommu MT2701_M4U_PORT_JPGDEC_BSDMA>;
	};

	jpegenc: jpegenc@1500a000 {
		compatible = "mediatek,mt2701-jpgenc",
			     "mediatek,mtk-jpgenc";
		reg = <0 0x1500a000 0 0x1000>;
		interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&imgsys CLK_IMG_VENC>;
		clock-names = "jpgenc";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_ISP>;
		iommus = <&iommu MT2701_M4U_PORT_JPGENC_RDMA>,
			 <&iommu MT2701_M4U_PORT_JPGENC_BSDMA>;
	};

	vdecsys: syscon@16000000 {
		compatible = "mediatek,mt2701-vdecsys", "syscon";
		reg = <0 0x16000000 0 0x1000>;
		#clock-cells = <1>;
	};

	larb1: larb@16010000 {
		compatible = "mediatek,mt2701-smi-larb";
		reg = <0 0x16010000 0 0x1000>;
		mediatek,smi = <&smi_common>;
		mediatek,larb-id = <1>;
		clocks = <&vdecsys CLK_VDEC_CKGEN>,
			 <&vdecsys CLK_VDEC_LARB>;
		clock-names = "apb", "smi";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_VDEC>;
	};

	hifsys: syscon@1a000000 {
		compatible = "mediatek,mt2701-hifsys", "syscon";
		reg = <0 0x1a000000 0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	usb0: usb@1a1c0000 {
		compatible = "mediatek,mt2701-xhci", "mediatek,mtk-xhci";
		reg = <0 0x1a1c0000 0 0x1000>,
		      <0 0x1a1c4700 0 0x0100>;
		reg-names = "mac", "ippc";
		interrupts = <GIC_SPI 196 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&hifsys CLK_HIFSYS_USB0PHY>,
			 <&topckgen CLK_TOP_ETHIF_SEL>;
		clock-names = "sys_ck", "ref_ck";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_HIF>;
		phys = <&u2port0 PHY_TYPE_USB2>, <&u3port0 PHY_TYPE_USB3>;
		status = "disabled";
	};

	u3phy0: t-phy@1a1c4000 {
		compatible = "mediatek,mt2701-tphy",
			     "mediatek,generic-tphy-v1";
		reg = <0 0x1a1c4000 0 0x0700>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		status = "disabled";

		u2port0: usb-phy@1a1c4800 {
			reg = <0 0x1a1c4800 0 0x0100>;
			clocks = <&topckgen CLK_TOP_USB_PHY48M>;
			clock-names = "ref";
			#phy-cells = <1>;
			status = "okay";
		};

		u3port0: usb-phy@1a1c4900 {
			reg = <0 0x1a1c4900 0 0x0700>;
			clocks = <&clk26m>;
			clock-names = "ref";
			#phy-cells = <1>;
			status = "okay";
		};
	};

	usb1: usb@1a240000 {
		compatible = "mediatek,mt2701-xhci", "mediatek,mtk-xhci";
		reg = <0 0x1a240000 0 0x1000>,
		      <0 0x1a244700 0 0x0100>;
		reg-names = "mac", "ippc";
		interrupts = <GIC_SPI 197 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&hifsys CLK_HIFSYS_USB1PHY>,
			 <&topckgen CLK_TOP_ETHIF_SEL>;
		clock-names = "sys_ck", "ref_ck";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_HIF>;
		phys = <&u2port1 PHY_TYPE_USB2>, <&u3port1 PHY_TYPE_USB3>;
		status = "disabled";
	};

	u3phy1: t-phy@1a244000 {
		compatible = "mediatek,mt2701-tphy",
			     "mediatek,generic-tphy-v1";
		reg = <0 0x1a244000 0 0x0700>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		status = "disabled";

		u2port1: usb-phy@1a244800 {
			reg = <0 0x1a244800 0 0x0100>;
			clocks = <&topckgen CLK_TOP_USB_PHY48M>;
			clock-names = "ref";
			#phy-cells = <1>;
			status = "okay";
		};

		u3port1: usb-phy@1a244900 {
			reg = <0 0x1a244900 0 0x0700>;
			clocks = <&clk26m>;
			clock-names = "ref";
			#phy-cells = <1>;
			status = "okay";
		};
	};

	usb2: usb@11200000 {
		compatible = "mediatek,mt2701-musb",
			     "mediatek,mtk-musb";
		reg = <0 0x11200000 0 0x1000>;
		interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_LOW>;
		interrupt-names = "mc";
		phys = <&u2port2 PHY_TYPE_USB2>;
		dr_mode = "otg";
		clocks = <&pericfg CLK_PERI_USB0>,
			 <&pericfg CLK_PERI_USB0_MCU>,
			 <&pericfg CLK_PERI_USB_SLV>;
		clock-names = "main","mcu","univpll";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_IFR_MSC>;
		status = "disabled";
	};

	u2phy0: t-phy@11210000 {
		compatible = "mediatek,mt2701-tphy",
			     "mediatek,generic-tphy-v1";
		reg = <0 0x11210000 0 0x0800>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		status = "okay";

		u2port2: usb-phy@1a1c4800 {
			reg = <0 0x11210800 0 0x0100>;
			clocks = <&topckgen CLK_TOP_USB_PHY48M>;
			clock-names = "ref";
			#phy-cells = <1>;
			status = "okay";
		};
	};

	ethsys: syscon@1b000000 {
		compatible = "mediatek,mt2701-ethsys", "syscon";
		reg = <0 0x1b000000 0 0x1000>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	eth: ethernet@1b100000 {
		compatible = "mediatek,mt2701-eth", "syscon";
		reg = <0 0x1b100000 0 0x20000>;
		interrupts = <GIC_SPI 200 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 199 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 198 IRQ_TYPE_LEVEL_LOW>;
		clocks = <&topckgen CLK_TOP_ETHIF_SEL>,
			 <&ethsys CLK_ETHSYS_ESW>,
			 <&ethsys CLK_ETHSYS_GP1>,
			 <&ethsys CLK_ETHSYS_GP2>,
			 <&apmixedsys CLK_APMIXED_TRGPLL>;
		clock-names = "ethif", "esw", "gp1", "gp2", "trgpll";
		resets = <&ethsys MT2701_ETHSYS_FE_RST>,
			 <&ethsys MT2701_ETHSYS_GMAC_RST>,
			 <&ethsys MT2701_ETHSYS_PPE_RST>;
		reset-names = "fe", "gmac", "ppe";
		power-domains = <&scpsys MT2701_POWER_DOMAIN_ETH>;
		mediatek,ethsys = <&ethsys>;
		mediatek,pctl = <&syscfg_pctl_a>;
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	bdpsys: syscon@1c000000 {
		compatible = "mediatek,mt2701-bdpsys", "syscon";
		reg = <0 0x1c000000 0 0x1000>;
		#clock-cells = <1>;
	};
};
