/*
 * Copyright 2014 Hans de Goede <hdegoede@redhat.com>
 *
 * Hans de Goede <hdegoede@redhat.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;
#include "sun7i-a20.dtsi"
#include "sunxi-common-regulators.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	model = "LeMaker Banana Pi";
	compatible = "lemaker,bananapi", "allwinner,sun7i-a20";

	aliases {
		serial0 = &uart0;
		serial1 = &uart3;
		serial2 = &uart7;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	hdmi-connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led {
			label = "bananapi:green:usr";
			gpios = <&pio 7 24 GPIO_ACTIVE_HIGH>;
		};
	};

	reg_gmac_3v3: gmac-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "gmac-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <100000>;
		enable-active-high;
		gpio = <&pio 7 23 GPIO_ACTIVE_HIGH>;
	};
};

&ahci {
	status = "okay";
};

&codec {
	status = "okay";
};

&cpu0 {
	cpu-supply = <&reg_dcdc2>;
	operating-points =
		/* kHz	  uV */
		<960000	1400000>,
		<912000	1400000>,
		<864000	1350000>,
		<720000	1250000>,
		<528000	1150000>,
		<312000	1100000>,
		<144000	1050000>;
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&gmac {
	pinctrl-names = "default";
	pinctrl-0 = <&gmac_rgmii_pins>;
	phy-handle = <&phy1>;
	phy-mode = "rgmii-id";
	phy-supply = <&reg_gmac_3v3>;
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&i2c0 {
	status = "okay";

	axp209: pmic@34 {
		reg = <0x34>;
		interrupt-parent = <&nmi_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
	};
};

&i2c2 {
	status = "okay";
};

&ir0 {
	pinctrl-names = "default";
	pinctrl-0 = <&ir0_rx_pin>;
	status = "okay";
};

&gmac_mdio {
	phy1: ethernet-phy@1 {
		reg = <1>;
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 7 10 GPIO_ACTIVE_LOW>; /* PH10 */
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&otg_sram {
	status = "okay";
};

&pio {
	vcc-pa-supply = <&reg_vcc3v3>;
	vcc-pc-supply = <&reg_vcc3v3>;
	vcc-pe-supply = <&reg_vcc3v3>;
	vcc-pf-supply = <&reg_vcc3v3>;
	vcc-pg-supply = <&reg_vcc3v3>;
	gpio-line-names =
		/* PA */
		"ERXD3", "ERXD2", "ERXD1", "ERXD0", "ETXD3",
			"ETXD2", "ETXD1", "ETXD0",
		"ERXCK", "ERXERR", "ERXDV", "EMDC", "EMDIO",
			"ETXEN", "ETXCK", "ECRS",
		"ECOL", "ETXERR", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PB */
		"PMU-SCK", "PMU-SDA", "", "", "", "", "", "",
		"", "USB0-DRV", "", "", "", "", "", "",
		"", "", "", "", "SCL", "SDA", "", "",
		"", "", "", "", "", "", "", "",
		/* PC */
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PD */
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PE */
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PF */
		"SD0-D1", "SD0-D0", "SD0-CLK", "SD0-CMD", "SD0-D3",
			"SD0-D2", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PG */
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		"", "", "", "", "", "", "", "",
		/* PH */
		"TXD0", "RXD0", "IO-1", "PH3", "USB0-IDDET", "PH5", "", "",
		"", "", "SD0-DET", "", "", "", "", "",
		"", "", "", "", "IO-4", "IO-5", "", "EMAC-PWR-EN",
		"LED1", "", "", "", "", "", "", "",
		/* PI */
		"", "", "", "IO-GCLK", "", "", "", "",
		"", "", "SPI-CE0", "SPI-CLK", "SPI-MOSI",
			"SPI-MISO", "SPI-CE1", "",
		"IO-6", "IO-3", "IO-2", "IO-0", "", "", "", "",
		"", "", "", "", "", "", "", "";
};

#include "axp209.dtsi"

&reg_dcdc2 {
	regulator-always-on;
	regulator-min-microvolt = <1000000>;
	regulator-max-microvolt = <1400000>;
	regulator-name = "vdd-cpu";
};

&reg_dcdc3 {
	regulator-always-on;
	regulator-min-microvolt = <1000000>;
	regulator-max-microvolt = <1400000>;
	regulator-name = "vdd-int-dll";
};

&reg_ldo1 {
	regulator-name = "vdd-rtc";
};

&reg_ldo2 {
	regulator-always-on;
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
	regulator-name = "avcc";
};

&reg_usb0_vbus {
	status = "okay";
};

&reg_usb1_vbus {
	status = "okay";
};

&reg_usb2_vbus {
	status = "okay";
};

&spi0 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi0_pi_pins>,
		    <&spi0_cs0_pi_pin>,
		    <&spi0_cs1_pi_pin>;
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pb_pins>;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart3_ph_pins>;
	status = "okay";
};

&uart7 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart7_pi_pins>;
	status = "okay";
};

&usb_otg {
	dr_mode = "otg";
	status = "okay";
};

&usb_power_supply {
	status = "okay";
};

&usbphy {
	usb0_id_det-gpios = <&pio 7 4 (GPIO_ACTIVE_HIGH | GPIO_PULL_UP)>; /* PH4 */
	usb0_vbus_power-supply = <&usb_power_supply>;
	usb0_vbus-supply = <&reg_usb0_vbus>;
	usb1_vbus-supply = <&reg_usb1_vbus>;
	usb2_vbus-supply = <&reg_usb2_vbus>;
	status = "okay";
};
