// SPDX-License-Identifier: GPL-2.0+
/*
 * Copyright (C) 2012 Altera <www.altera.com>
 */

#include <dt-bindings/reset/altr,rst-mgr.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;

	aliases {
		serial0 = &uart0;
		serial1 = &uart1;
		timer0 = &timer0;
		timer1 = &timer1;
		timer2 = &timer2;
		timer3 = &timer3;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "altr,socfpga-smp";

		cpu0: cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
		};
		cpu1: cpu@1 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
		};
	};

	pmu: pmu@ff111000 {
		compatible = "arm,cortex-a9-pmu";
		interrupt-parent = <&intc>;
		interrupts = <0 176 4>, <0 177 4>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
		reg = <0xff111000 0x1000>,
		      <0xff113000 0x1000>;
	};

	intc: interrupt-controller@fffed000 {
		compatible = "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0xfffed000 0x1000>,
		      <0xfffec100 0x100>;
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		device_type = "soc";
		interrupt-parent = <&intc>;
		ranges;

		amba {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			pdma: pdma@ffe01000 {
				compatible = "arm,pl330", "arm,primecell";
				reg = <0xffe01000 0x1000>;
				interrupts = <0 104 4>,
					     <0 105 4>,
					     <0 106 4>,
					     <0 107 4>,
					     <0 108 4>,
					     <0 109 4>,
					     <0 110 4>,
					     <0 111 4>;
				#dma-cells = <1>;
				clocks = <&l4_main_clk>;
				clock-names = "apb_pclk";
				resets = <&rst DMA_RESET>;
				reset-names = "dma";
			};
		};

		base_fpga_region {
			compatible = "fpga-region";
			fpga-mgr = <&fpgamgr0>;

			#address-cells = <0x1>;
			#size-cells = <0x1>;
		};

		can0: can@ffc00000 {
			compatible = "bosch,d_can";
			reg = <0xffc00000 0x1000>;
			interrupts = <0 131 4>, <0 132 4>, <0 133 4>, <0 134 4>;
			clocks = <&can0_clk>;
			resets = <&rst CAN0_RESET>;
			status = "disabled";
		};

		can1: can@ffc01000 {
			compatible = "bosch,d_can";
			reg = <0xffc01000 0x1000>;
			interrupts = <0 135 4>, <0 136 4>, <0 137 4>, <0 138 4>;
			clocks = <&can1_clk>;
			resets = <&rst CAN1_RESET>;
			status = "disabled";
		};

		clkmgr@ffd04000 {
				compatible = "altr,clk-mgr";
				reg = <0xffd04000 0x1000>;

				clocks {
					#address-cells = <1>;
					#size-cells = <0>;

					osc1: osc1 {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					osc2: osc2 {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					f2s_periph_ref_clk: f2s_periph_ref_clk {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					f2s_sdram_ref_clk: f2s_sdram_ref_clk {
						#clock-cells = <0>;
						compatible = "fixed-clock";
					};

					main_pll: main_pll@40 {
						#address-cells = <1>;
						#size-cells = <0>;
						#clock-cells = <0>;
						compatible = "altr,socfpga-pll-clock";
						clocks = <&osc1>;
						reg = <0x40>;

						mpuclk: mpuclk@48 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>;
							div-reg = <0xe0 0 9>;
							reg = <0x48>;
						};

						mainclk: mainclk@4c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>;
							div-reg = <0xe4 0 9>;
							reg = <0x4C>;
						};

						dbg_base_clk: dbg_base_clk@50 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>, <&osc1>;
							div-reg = <0xe8 0 9>;
							reg = <0x50>;
						};

						main_qspi_clk: main_qspi_clk@54 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>;
							reg = <0x54>;
						};

						main_nand_sdmmc_clk: main_nand_sdmmc_clk@58 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>;
							reg = <0x58>;
						};

						cfg_h2f_usr0_clk: cfg_h2f_usr0_clk@5c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&main_pll>;
							reg = <0x5C>;
						};
					};

					periph_pll: periph_pll@80 {
						#address-cells = <1>;
						#size-cells = <0>;
						#clock-cells = <0>;
						compatible = "altr,socfpga-pll-clock";
						clocks = <&osc1>, <&osc2>, <&f2s_periph_ref_clk>;
						reg = <0x80>;

						emac0_clk: emac0_clk@88 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x88>;
						};

						emac1_clk: emac1_clk@8c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x8C>;
						};

						per_qspi_clk: per_qsi_clk@90 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x90>;
						};

						per_nand_mmc_clk: per_nand_mmc_clk@94 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x94>;
						};

						per_base_clk: per_base_clk@98 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x98>;
						};

						h2f_usr1_clk: h2f_usr1_clk@9c {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&periph_pll>;
							reg = <0x9C>;
						};
					};

					sdram_pll: sdram_pll@c0 {
						#address-cells = <1>;
						#size-cells = <0>;
						#clock-cells = <0>;
						compatible = "altr,socfpga-pll-clock";
						clocks = <&osc1>, <&osc2>, <&f2s_sdram_ref_clk>;
						reg = <0xC0>;

						ddr_dqs_clk: ddr_dqs_clk@c8 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&sdram_pll>;
							reg = <0xC8>;
						};

						ddr_2x_dqs_clk: ddr_2x_dqs_clk@cc {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&sdram_pll>;
							reg = <0xCC>;
						};

						ddr_dq_clk: ddr_dq_clk@d0 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&sdram_pll>;
							reg = <0xD0>;
						};

						h2f_usr2_clk: h2f_usr2_clk@d4 {
							#clock-cells = <0>;
							compatible = "altr,socfpga-perip-clk";
							clocks = <&sdram_pll>;
							reg = <0xD4>;
						};
					};

					mpu_periph_clk: mpu_periph_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-perip-clk";
						clocks = <&mpuclk>;
						fixed-divider = <4>;
					};

					mpu_l2_ram_clk: mpu_l2_ram_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-perip-clk";
						clocks = <&mpuclk>;
						fixed-divider = <2>;
					};

					l4_main_clk: l4_main_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&mainclk>;
						clk-gate = <0x60 0>;
					};

					l3_main_clk: l3_main_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-perip-clk";
						clocks = <&mainclk>;
						fixed-divider = <1>;
					};

					l3_mp_clk: l3_mp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&mainclk>;
						div-reg = <0x64 0 2>;
						clk-gate = <0x60 1>;
					};

					l3_sp_clk: l3_sp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&l3_mp_clk>;
						div-reg = <0x64 2 2>;
					};

					l4_mp_clk: l4_mp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&mainclk>, <&per_base_clk>;
						div-reg = <0x64 4 3>;
						clk-gate = <0x60 2>;
					};

					l4_sp_clk: l4_sp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&mainclk>, <&per_base_clk>;
						div-reg = <0x64 7 3>;
						clk-gate = <0x60 3>;
					};

					dbg_at_clk: dbg_at_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&dbg_base_clk>;
						div-reg = <0x68 0 2>;
						clk-gate = <0x60 4>;
					};

					dbg_clk: dbg_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&dbg_at_clk>;
						div-reg = <0x68 2 2>;
						clk-gate = <0x60 5>;
					};

					dbg_trace_clk: dbg_trace_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&dbg_base_clk>;
						div-reg = <0x6C 0 3>;
						clk-gate = <0x60 6>;
					};

					dbg_timer_clk: dbg_timer_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&dbg_base_clk>;
						clk-gate = <0x60 7>;
					};

					cfg_clk: cfg_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&cfg_h2f_usr0_clk>;
						clk-gate = <0x60 8>;
					};

					h2f_user0_clk: h2f_user0_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&cfg_h2f_usr0_clk>;
						clk-gate = <0x60 9>;
					};

					emac_0_clk: emac_0_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&emac0_clk>;
						clk-gate = <0xa0 0>;
					};

					emac_1_clk: emac_1_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&emac1_clk>;
						clk-gate = <0xa0 1>;
					};

					usb_mp_clk: usb_mp_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&per_base_clk>;
						clk-gate = <0xa0 2>;
						div-reg = <0xa4 0 3>;
					};

					spi_m_clk: spi_m_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&per_base_clk>;
						clk-gate = <0xa0 3>;
						div-reg = <0xa4 3 3>;
					};

					can0_clk: can0_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&per_base_clk>;
						clk-gate = <0xa0 4>;
						div-reg = <0xa4 6 3>;
					};

					can1_clk: can1_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&per_base_clk>;
						clk-gate = <0xa0 5>;
						div-reg = <0xa4 9 3>;
					};

					gpio_db_clk: gpio_db_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&per_base_clk>;
						clk-gate = <0xa0 6>;
						div-reg = <0xa8 0 24>;
					};

					h2f_user1_clk: h2f_user1_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&h2f_usr1_clk>;
						clk-gate = <0xa0 7>;
					};

					sdmmc_clk: sdmmc_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&f2s_periph_ref_clk>, <&main_nand_sdmmc_clk>, <&per_nand_mmc_clk>;
						clk-gate = <0xa0 8>;
					};

					sdmmc_clk_divided: sdmmc_clk_divided {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&sdmmc_clk>;
						clk-gate = <0xa0 8>;
						fixed-divider = <4>;
					};

					nand_x_clk: nand_x_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&f2s_periph_ref_clk>, <&main_nand_sdmmc_clk>, <&per_nand_mmc_clk>;
						clk-gate = <0xa0 9>;
					};

					nand_ecc_clk: nand_ecc_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&nand_x_clk>;
						clk-gate = <0xa0 9>;
					};

					nand_clk: nand_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&nand_x_clk>;
						clk-gate = <0xa0 10>;
						fixed-divider = <4>;
					};

					qspi_clk: qspi_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&f2s_periph_ref_clk>, <&main_qspi_clk>, <&per_qspi_clk>;
						clk-gate = <0xa0 11>;
					};

					ddr_dqs_clk_gate: ddr_dqs_clk_gate {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&ddr_dqs_clk>;
						clk-gate = <0xd8 0>;
					};

					ddr_2x_dqs_clk_gate: ddr_2x_dqs_clk_gate {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&ddr_2x_dqs_clk>;
						clk-gate = <0xd8 1>;
					};

					ddr_dq_clk_gate: ddr_dq_clk_gate {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&ddr_dq_clk>;
						clk-gate = <0xd8 2>;
					};

					h2f_user2_clk: h2f_user2_clk {
						#clock-cells = <0>;
						compatible = "altr,socfpga-gate-clk";
						clocks = <&h2f_usr2_clk>;
						clk-gate = <0xd8 3>;
					};

				};
		};

		fpga_bridge0: fpga_bridge@ff400000 {
			compatible = "altr,socfpga-lwhps2fpga-bridge";
			reg = <0xff400000 0x100000>;
			resets = <&rst LWHPS2FPGA_RESET>;
			clocks = <&l4_main_clk>;
			status = "disabled";
		};

		fpga_bridge1: fpga_bridge@ff500000 {
			compatible = "altr,socfpga-hps2fpga-bridge";
			reg = <0xff500000 0x10000>;
			resets = <&rst HPS2FPGA_RESET>;
			clocks = <&l4_main_clk>;
			status = "disabled";
		};

		fpga_bridge2: fpga-bridge@ff600000 {
			compatible = "altr,socfpga-fpga2hps-bridge";
			reg = <0xff600000 0x100000>;
			resets = <&rst FPGA2HPS_RESET>;
			clocks = <&l4_main_clk>;
			status = "disabled";
		};

		fpga_bridge3: fpga-bridge@ffc25080 {
			compatible = "altr,socfpga-fpga2sdram-bridge";
			reg = <0xffc25080 0x4>;
			status = "disabled";
		};

		fpgamgr0: fpgamgr@ff706000 {
			compatible = "altr,socfpga-fpga-mgr";
			reg = <0xff706000 0x1000
			       0xffb90000 0x4>;
			interrupts = <0 175 4>;
		};

		socfpga_axi_setup: stmmac-axi-config {
			snps,wr_osr_lmt = <0xf>;
			snps,rd_osr_lmt = <0xf>;
			snps,blen = <0 0 0 0 16 0 0>;
		};

		gmac0: ethernet@ff700000 {
			compatible = "altr,socfpga-stmmac", "snps,dwmac-3.70a", "snps,dwmac";
			altr,sysmgr-syscon = <&sysmgr 0x60 0>;
			reg = <0xff700000 0x2000>;
			interrupts = <0 115 4>;
			interrupt-names = "macirq";
			mac-address = [00 00 00 00 00 00];/* Filled in by U-Boot */
			clocks = <&emac_0_clk>;
			clock-names = "stmmaceth";
			resets = <&rst EMAC0_RESET>;
			reset-names = "stmmaceth";
			snps,multicast-filter-bins = <256>;
			snps,perfect-filter-entries = <128>;
			tx-fifo-depth = <4096>;
			rx-fifo-depth = <4096>;
			snps,axi-config = <&socfpga_axi_setup>;
			status = "disabled";
		};

		gmac1: ethernet@ff702000 {
			compatible = "altr,socfpga-stmmac", "snps,dwmac-3.70a", "snps,dwmac";
			altr,sysmgr-syscon = <&sysmgr 0x60 2>;
			reg = <0xff702000 0x2000>;
			interrupts = <0 120 4>;
			interrupt-names = "macirq";
			mac-address = [00 00 00 00 00 00];/* Filled in by U-Boot */
			clocks = <&emac_1_clk>;
			clock-names = "stmmaceth";
			resets = <&rst EMAC1_RESET>;
			reset-names = "stmmaceth";
			snps,multicast-filter-bins = <256>;
			snps,perfect-filter-entries = <128>;
			tx-fifo-depth = <4096>;
			rx-fifo-depth = <4096>;
			snps,axi-config = <&socfpga_axi_setup>;
			status = "disabled";
		};

		gpio0: gpio@ff708000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xff708000 0x1000>;
			clocks = <&l4_mp_clk>;
			resets = <&rst GPIO0_RESET>;
			status = "disabled";

			porta: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <29>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 164 4>;
			};
		};

		gpio1: gpio@ff709000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xff709000 0x1000>;
			clocks = <&l4_mp_clk>;
			resets = <&rst GPIO1_RESET>;
			status = "disabled";

			portb: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <29>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 165 4>;
			};
		};

		gpio2: gpio@ff70a000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xff70a000 0x1000>;
			clocks = <&l4_mp_clk>;
			resets = <&rst GPIO2_RESET>;
			status = "disabled";

			portc: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <27>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 166 4>;
			};
		};

		i2c0: i2c@ffc04000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc04000 0x1000>;
			resets = <&rst I2C0_RESET>;
			clocks = <&l4_sp_clk>;
			interrupts = <0 158 0x4>;
			status = "disabled";
		};

		i2c1: i2c@ffc05000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc05000 0x1000>;
			resets = <&rst I2C1_RESET>;
			clocks = <&l4_sp_clk>;
			interrupts = <0 159 0x4>;
			status = "disabled";
		};

		i2c2: i2c@ffc06000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc06000 0x1000>;
			resets = <&rst I2C2_RESET>;
			clocks = <&l4_sp_clk>;
			interrupts = <0 160 0x4>;
			status = "disabled";
		};

		i2c3: i2c@ffc07000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc07000 0x1000>;
			resets = <&rst I2C3_RESET>;
			clocks = <&l4_sp_clk>;
			interrupts = <0 161 0x4>;
			status = "disabled";
		};

		eccmgr: eccmgr {
			compatible = "altr,socfpga-ecc-manager";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			l2-ecc@ffd08140 {
				compatible = "altr,socfpga-l2-ecc";
				reg = <0xffd08140 0x4>;
				interrupts = <0 36 1>, <0 37 1>;
			};

			ocram-ecc@ffd08144 {
				compatible = "altr,socfpga-ocram-ecc";
				reg = <0xffd08144 0x4>;
				iram = <&ocram>;
				interrupts = <0 178 1>, <0 179 1>;
			};
		};

		L2: cache-controller@fffef000 {
			compatible = "arm,pl310-cache";
			reg = <0xfffef000 0x1000>;
			interrupts = <0 38 0x04>;
			cache-unified;
			cache-level = <2>;
			arm,tag-latency = <1 1 1>;
			arm,data-latency = <2 1 1>;
			prefetch-data = <1>;
			prefetch-instr = <1>;
			arm,shared-override;
			arm,double-linefill = <1>;
			arm,double-linefill-incr = <0>;
			arm,double-linefill-wrap = <1>;
			arm,prefetch-drop = <0>;
			arm,prefetch-offset = <7>;
		};

		l3regs@ff800000 {
			compatible = "altr,l3regs", "syscon";
			reg = <0xff800000 0x1000>;
		};

		mmc: mmc@ff704000 {
			compatible = "altr,socfpga-dw-mshc";
			reg = <0xff704000 0x1000>;
			interrupts = <0 139 4>;
			fifo-depth = <0x400>;
			#address-cells = <1>;
			#size-cells = <0>;
			clocks = <&l4_mp_clk>, <&sdmmc_clk_divided>;
			clock-names = "biu", "ciu";
			resets = <&rst SDMMC_RESET>;
			altr,sysmgr-syscon = <&sysmgr 0x108 3>;
			status = "disabled";
		};

		nand0: nand-controller@ff900000 {
			#address-cells = <0x1>;
			#size-cells = <0x0>;
			compatible = "altr,socfpga-denali-nand";
			reg = <0xff900000 0x100000>,
			      <0xffb80000 0x10000>;
			reg-names = "nand_data", "denali_reg";
			interrupts = <0x0 0x90 0x4>;
			clocks = <&nand_clk>, <&nand_x_clk>, <&nand_ecc_clk>;
			clock-names = "nand", "nand_x", "ecc";
			resets = <&rst NAND_RESET>;
			status = "disabled";
		};

		ocram: sram@ffff0000 {
			compatible = "mmio-sram";
			reg = <0xffff0000 0x10000>;
		};

		qspi: spi@ff705000 {
			compatible = "intel,socfpga-qspi", "cdns,qspi-nor";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xff705000 0x1000>,
			      <0xffa00000 0x1000>;
			interrupts = <0 151 4>;
			cdns,fifo-depth = <128>;
			cdns,fifo-width = <4>;
			cdns,trigger-address = <0x00000000>;
			clocks = <&qspi_clk>;
			resets = <&rst QSPI_RESET>;
			status = "disabled";
		};

		rst: rstmgr@ffd05000 {
			#reset-cells = <1>;
			compatible = "altr,rst-mgr";
			reg = <0xffd05000 0x1000>;
			altr,modrst-offset = <0x10>;
		};

		scu: snoop-control-unit@fffec000 {
			compatible = "arm,cortex-a9-scu";
			reg = <0xfffec000 0x100>;
		};

		sdr: sdr@ffc25000 {
			compatible = "altr,sdr-ctl", "syscon";
			reg = <0xffc25000 0x1000>;
			resets = <&rst SDR_RESET>;
		};

		sdramedac {
			compatible = "altr,sdram-edac";
			altr,sdr-syscon = <&sdr>;
			interrupts = <0 39 4>;
		};

		spi0: spi@fff00000 {
			compatible = "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xfff00000 0x1000>;
			interrupts = <0 154 4>;
			num-cs = <4>;
			clocks = <&spi_m_clk>;
			resets = <&rst SPIM0_RESET>;
			reset-names = "spi";
			status = "disabled";
		};

		spi1: spi@fff01000 {
			compatible = "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xfff01000 0x1000>;
			interrupts = <0 155 4>;
			num-cs = <4>;
			clocks = <&spi_m_clk>;
			resets = <&rst SPIM1_RESET>;
			reset-names = "spi";
			status = "disabled";
		};

		sysmgr: sysmgr@ffd08000 {
			compatible = "altr,sys-mgr", "syscon";
			reg = <0xffd08000 0x4000>;
		};

		/* Local timer */
		timer@fffec600 {
			compatible = "arm,cortex-a9-twd-timer";
			reg = <0xfffec600 0x100>;
			interrupts = <1 13 0xf01>;
			clocks = <&mpu_periph_clk>;
		};

		timer0: timer0@ffc08000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 167 4>;
			reg = <0xffc08000 0x1000>;
			clocks = <&l4_sp_clk>;
			clock-names = "timer";
			resets = <&rst SPTIMER0_RESET>;
			reset-names = "timer";
		};

		timer1: timer1@ffc09000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 168 4>;
			reg = <0xffc09000 0x1000>;
			clocks = <&l4_sp_clk>;
			clock-names = "timer";
			resets = <&rst SPTIMER1_RESET>;
			reset-names = "timer";
		};

		timer2: timer2@ffd00000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 169 4>;
			reg = <0xffd00000 0x1000>;
			clocks = <&osc1>;
			clock-names = "timer";
			resets = <&rst OSC1TIMER0_RESET>;
			reset-names = "timer";
		};

		timer3: timer3@ffd01000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 170 4>;
			reg = <0xffd01000 0x1000>;
			clocks = <&osc1>;
			clock-names = "timer";
			resets = <&rst OSC1TIMER1_RESET>;
			reset-names = "timer";
		};

		uart0: serial@ffc02000 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc02000 0x1000>;
			interrupts = <0 162 4>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&l4_sp_clk>;
			dmas = <&pdma 28>,
			       <&pdma 29>;
			dma-names = "tx", "rx";
			resets = <&rst UART0_RESET>;
		};

		uart1: serial@ffc03000 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc03000 0x1000>;
			interrupts = <0 163 4>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&l4_sp_clk>;
			dmas = <&pdma 30>,
			       <&pdma 31>;
			dma-names = "tx", "rx";
			resets = <&rst UART1_RESET>;
		};

		usbphy0: usbphy {
			#phy-cells = <0>;
			compatible = "usb-nop-xceiv";
			status = "okay";
		};

		usb0: usb@ffb00000 {
			compatible = "snps,dwc2";
			reg = <0xffb00000 0xffff>;
			interrupts = <0 125 4>;
			clocks = <&usb_mp_clk>;
			clock-names = "otg";
			resets = <&rst USB0_RESET>;
			reset-names = "dwc2";
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			status = "disabled";
		};

		usb1: usb@ffb40000 {
			compatible = "snps,dwc2";
			reg = <0xffb40000 0xffff>;
			interrupts = <0 128 4>;
			clocks = <&usb_mp_clk>;
			clock-names = "otg";
			resets = <&rst USB1_RESET>;
			reset-names = "dwc2";
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			status = "disabled";
		};

		watchdog0: watchdog@ffd02000 {
			compatible = "snps,dw-wdt";
			reg = <0xffd02000 0x1000>;
			interrupts = <0 171 4>;
			clocks = <&osc1>;
			resets = <&rst L4WD0_RESET>;
			status = "disabled";
		};

		watchdog1: watchdog@ffd03000 {
			compatible = "snps,dw-wdt";
			reg = <0xffd03000 0x1000>;
			interrupts = <0 172 4>;
			clocks = <&osc1>;
			resets = <&rst L4WD1_RESET>;
			status = "disabled";
		};
	};
};
