/* Copyright (c) 2015, The Linux Foundation. All rights reserved.
 *
 * Permission to use, copy, modify, and/or distribute this software for any
 * purpose with or without fee is hereby granted, provided that the above
 * copyright notice and this permission notice appear in all copies.
 *
 * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
 * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
 * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR
 * ANY SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
 * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN
 * ACTION OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF
 * OR IN CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
 *
 */

#include <dt-bindings/gpio/gpio.h>
#include "qcom-ipq4019.dtsi"

/ {
	model = "Qualcomm Technologies, Inc. IPQ4019/AP-DK01.1";

	aliases {
		serial0 = &blsp1_uart1;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};
};

&prng {
	status = "okay";
};

&tlmm {
	serial_pins: serial-state {
		pins = "gpio60", "gpio61";
		function = "blsp_uart0";
		bias-disable;
	};

	spi_0_pins: spi-0-state {
		spi0-pins {
			pins = "gpio55", "gpio56", "gpio57";
			function = "blsp_spi0";
			drive-strength = <12>;
			bias-disable;
		};
		spi0-cs-pins {
			pins = "gpio54";
			function = "gpio";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>;

	flash@0 {
		reg = <0>;
		compatible = "jedec,spi-nor";
		spi-max-frequency = <24000000>;
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&wifi0 {
	status = "okay";
};

&wifi1 {
	status = "okay";
};
