// SPDX-License-Identifier: GPL-2.0
/*
 * Keystone 2 Edison EVM device tree
 *
 * Copyright (C) 2013-2017 Texas Instruments Incorporated - https://www.ti.com/
 */
/dts-v1/;

#include "keystone.dtsi"
#include "keystone-k2e.dtsi"

/ {
	compatible = "ti,k2e-evm", "ti,k2e", "ti,keystone";
	model = "Texas Instruments Keystone 2 Edison EVM";

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		dsp_common_memory: dsp-common-memory@81f800000 {
			compatible = "shared-dma-pool";
			reg = <0x00000008 0x1f800000 0x00000000 0x800000>;
			reusable;
			status = "okay";
		};
	};
};

&soc0 {

		clocks {
			refclksys: refclksys {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <100000000>;
				clock-output-names = "refclk-sys";
			};

			refclkpass: refclkpass {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <100000000>;
				clock-output-names = "refclk-pass";
			};

			refclkddr3a: refclkddr3a {
				#clock-cells = <0>;
				compatible = "fixed-clock";
				clock-frequency = <100000000>;
				clock-output-names = "refclk-ddr3a";
			};
		};
};

&usb_phy {
	status = "okay";
};

&keystone_usb0 {
	status = "okay";
};

&usb0 {
	dr_mode = "host";
};

&usb1_phy {
	status = "okay";
};

&keystone_usb1 {
	status = "okay";
};

&usb1 {
	dr_mode = "peripheral";
};

&i2c0 {
	eeprom@50 {
		compatible = "atmel,24c1024";
		reg = <0x50>;
	};
};

&aemif {
	cs0 {
		#address-cells = <2>;
		#size-cells = <1>;
		clock-ranges;
		ranges;

		ti,cs-chipselect = <0>;
		/* all timings in nanoseconds */
		ti,cs-min-turnaround-ns = <12>;
		ti,cs-read-hold-ns = <6>;
		ti,cs-read-strobe-ns = <23>;
		ti,cs-read-setup-ns = <9>;
		ti,cs-write-hold-ns = <8>;
		ti,cs-write-strobe-ns = <23>;
		ti,cs-write-setup-ns = <8>;

		nand@0,0 {
			compatible = "ti,keystone-nand","ti,davinci-nand";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0 0 0x4000000
			       1 0 0x0000100>;

			ti,davinci-chipselect = <0>;
			ti,davinci-mask-ale = <0x2000>;
			ti,davinci-mask-cle = <0x4000>;
			ti,davinci-mask-chipsel = <0>;
			nand-ecc-mode = "hw";
			ti,davinci-ecc-bits = <4>;
			nand-on-flash-bbt;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x100000>;
				read-only;
			};

			partition@100000 {
				label = "params";
				reg = <0x100000 0x80000>;
				read-only;
			};

			partition@180000 {
				label = "ubifs";
				reg = <0x180000 0x1fe80000>;
			};
		};
	};
};

&spi0 {
	nor_flash: flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "micron,n25q128a11", "jedec,spi-nor";
		spi-max-frequency = <54000000>;
		m25p,fast-read;
		reg = <0>;

		partition@0 {
			label = "u-boot-spl";
			reg = <0x0 0x80000>;
			read-only;
		};

		partition@1 {
			label = "misc";
			reg = <0x80000 0xf80000>;
		};
	};
};

&mdio {
	status = "okay";
	ethphy0: ethernet-phy@0 {
		compatible = "marvell,88E1514", "marvell,88E1510", "ethernet-phy-ieee802.3-c22";
		reg = <0>;
	};

	ethphy1: ethernet-phy@1 {
		compatible = "marvell,88E1514", "marvell,88E1510", "ethernet-phy-ieee802.3-c22";
		reg = <1>;
	};
};

&dsp0 {
	memory-region = <&dsp_common_memory>;
	status = "okay";
};
