/*
 * Copyright (C) 2017 NutsBoard.Org
 *
 * Author: Wig Cheng <onlywig@gmail.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of the
 *     License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 */

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include "imx6q.dtsi"

/ {
	model = "NutsBoard i.MX6 Quad Pistachio board";
	compatible = "nutsboard,imx6q-pistachio", "fsl,imx6q";

	chosen {
		stdout-path = &uart4;
	};

	memory@10000000 {
		device_type = "memory";
		reg = <0x10000000 0x80000000>;
	};

	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		regulator-name = "3P3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	reg_1p8v: regulator-1p8v {
		compatible = "regulator-fixed";
		regulator-name = "1P8V";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	wlan_en_reg: regulator-wlan_en {
		compatible = "regulator-fixed";
		regulator-name = "wlan-en-regulator";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		gpio = <&gpio2 24 GPIO_ACTIVE_HIGH>;
		startup-delay-us = <70000>;
		enable-active-high;
	};

	reg_usb_otg_vbus: regulator-usb_vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb_otg_vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio3 22 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&swbst_reg>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_gpio_keys>;

		key-power {
			label = "Power Button";
			gpios = <&gpio2 12 GPIO_ACTIVE_LOW>;
			wakeup-source;
			linux,code = <KEY_POWER>;
		};
	};

	sound {
		compatible = "fsl,imx-sgtl5000",
			   "fsl,imx-audio-sgtl5000";
		model = "audio-sgtl5000";
		ssi-controller = <&ssi1>;
		audio-codec = <&codec>;
		audio-routing =
			"MIC_IN", "Mic Jack",
			"Mic Jack", "Mic Bias",
			"Headphone Jack", "HP_OUT";
		mux-int-port = <1>;
		mux-ext-port = <3>;
	};

	backlight_lvds: backlight-lvds {
		compatible = "pwm-backlight";
		pwms = <&pwm1 0 50000 0>;
		brightness-levels = <
			0  /*1  2  3  4  5  6*/  7  8  9
			10 11 12 13 14 15 16 17 18 19
			20 21 22 23 24 25 26 27 28 29
			30 31 32 33 34 35 36 37 38 39
			40 41 42 43 44 45 46 47 48 49
			50 51 52 53 54 55 56 57 58 59
			60 61 62 63 64 65 66 67 68 69
			70 71 72 73 74 75 76 77 78 79
			80 81 82 83 84 85 86 87 88 89
			90 91 92 93 94 95 96 97 98 99
			100
		>;
		default-brightness-level = <94>;
		status = "okay";
	};

	panel {
		compatible = "hannstar,hsd100pxn1";
		backlight = <&backlight_lvds>;

		port {
			panel_in: endpoint {
				remote-endpoint = <&lvds0_out>;
			};
		};
	};
};

&audmux {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_audmux>;
	status = "okay";
};

&can2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_flexcan2>;
	status = "okay";
};

&clks {
	assigned-clocks = <&clks IMX6QDL_CLK_LDB_DI0_SEL>,
			  <&clks IMX6QDL_CLK_LDB_DI1_SEL>;
	assigned-clock-parents = <&clks IMX6QDL_CLK_PLL3_USB_OTG>,
				 <&clks IMX6QDL_CLK_PLL3_USB_OTG>;
};

&fec {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_enet>;
	phy-mode = "rgmii";
	status = "okay";
};

&hdmi {
	ddc-i2c-bus = <&i2c2>;
	status = "okay";
};

&i2c1 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c1>;
	status = "okay";

	codec: sgtl5000@a {
		compatible = "fsl,sgtl5000";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c1_sgtl5000>;
		reg = <0x0a>;
		#sound-dai-cells = <0>;
		clocks = <&clks IMX6QDL_CLK_CKO>;
		VDDA-supply = <&reg_1p8v>;
		VDDIO-supply = <&reg_1p8v>;
	};
};

&i2c2 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c2>;
	status = "okay";

	pmic: pmic@8 {
		compatible = "fsl,pfuze100";
		reg = <0x08>;

		regulators {
			sw1a_reg: sw1ab {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw1c_reg: sw1c {
				regulator-min-microvolt = <300000>;
				regulator-max-microvolt = <1875000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw2_reg: sw2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-ramp-delay = <6250>;
			};

			sw3a_reg: sw3a {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw3b_reg: sw3b {
				regulator-min-microvolt = <400000>;
				regulator-max-microvolt = <1975000>;
				regulator-boot-on;
				regulator-always-on;
			};

			sw4_reg: sw4 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <3300000>;
			};

			swbst_reg: swbst {
				regulator-min-microvolt = <5000000>;
				regulator-max-microvolt = <5150000>;
			};

			snvs_reg: vsnvs {
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
			};

			vref_reg: vrefddr {
				regulator-boot-on;
				regulator-always-on;
			};

			vgen1_reg: vgen1 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen2_reg: vgen2 {
				regulator-min-microvolt = <800000>;
				regulator-max-microvolt = <1550000>;
			};

			vgen3_reg: vgen3 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
			};

			vgen4_reg: vgen4 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};

			vgen5_reg: vgen5 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
			vgen6_reg: vgen6 {
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-always-on;
			};
		};
	};

	ar1021@4d {
		compatible = "microchip,ar1021-i2c";
		reg = <0x4d>;
		interrupt-parent = <&gpio6>;
		interrupts = <8 IRQ_TYPE_EDGE_FALLING>;
	};
};

&i2c3 {
	clock-frequency = <100000>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_i2c3>;
	status = "okay";
};

&iomuxc {
	pinctrl-names = "default";

	pinctrl_hog: hoggrp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D22__GPIO3_IO22	0x1b0b0  /*pcie power*/
			MX6QDL_PAD_EIM_A25__GPIO5_IO02	0x1b0b0   /*LCD power*/
			MX6QDL_PAD_EIM_D16__GPIO3_IO16	0x1b0b0   /*backlight power*/
			MX6QDL_PAD_GPIO_2__GPIO1_IO02		0x1b0b1 /*SD3 CD pin*/
			MX6QDL_PAD_KEY_COL2__GPIO4_IO10	0x1b0b0 /*codec power*/
			MX6QDL_PAD_EIM_A16__GPIO2_IO22	0x1b0b0 /*touch reset*/
			MX6QDL_PAD_NANDF_ALE__GPIO6_IO08	0x1b0b01 /*touch irq*/
			MX6QDL_PAD_GPIO_7__GPIO1_IO07	 0x1b0b0/*backlight pwr*/
			MX6QDL_PAD_GPIO_16__GPIO7_IO11	0x1b0b0 /*gpio 5V_1*/
			MX6QDL_PAD_EIM_A19__GPIO2_IO19	0x1b0b0 /*gpio 5V_2*/
			MX6QDL_PAD_EIM_A24__GPIO5_IO04	0x1b0b0 /*gpio 5V_3*/
			MX6QDL_PAD_GPIO_17__GPIO7_IO12	0x1b0b0 /*gpio 5V_4*/
			MX6QDL_PAD_NANDF_CLE__GPIO6_IO07	0x1b0b0 /*AUX_5V_EN*/
			MX6QDL_PAD_NANDF_WP_B__GPIO6_IO09	0x1b0b0 /*AUX_5VB_EN*/
			MX6QDL_PAD_NANDF_RB0__GPIO6_IO10	0x1b0b0 /*AUX_3V3_EN*/
			MX6QDL_PAD_EIM_D21__GPIO3_IO21	0x1b0b0 /*I2C expander pwr*/
		>;
	};

	pinctrl_audmux: audmuxgrp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT7__AUD3_RXD		0x130b0
			MX6QDL_PAD_CSI0_DAT4__AUD3_TXC		0x130b0
			MX6QDL_PAD_CSI0_DAT5__AUD3_TXD		0x110b0
			MX6QDL_PAD_CSI0_DAT6__AUD3_TXFS		0x130b0
		>;
	};

	pinctrl_ecspi1: ecspi1grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL1__ECSPI1_MISO	0x100b1
			MX6QDL_PAD_KEY_ROW0__ECSPI1_MOSI	0x100b1
			MX6QDL_PAD_KEY_COL0__ECSPI1_SCLK	0x100b1
			MX6QDL_PAD_KEY_ROW1__GPIO4_IO09		0x1b0b0
		>;
	};

	pinctrl_enet: enetgrp {
		fsl,pins = <
			MX6QDL_PAD_ENET_MDIO__ENET_MDIO		0x1b8b0
			MX6QDL_PAD_ENET_MDC__ENET_MDC		0x1b0b0
			/* AR8035 reset */
			MX6QDL_PAD_EIM_A20__GPIO2_IO18		0x130b0
			/* AR8035 interrupt */
			MX6QDL_PAD_EIM_CS0__GPIO2_IO23		0x1b0b1
			MX6QDL_PAD_RGMII_TXC__RGMII_TXC		0x1b030
			MX6QDL_PAD_RGMII_TD0__RGMII_TD0		0x1b030
			MX6QDL_PAD_RGMII_TD1__RGMII_TD1		0x1b030
			MX6QDL_PAD_RGMII_TD2__RGMII_TD2		0x1b030
			MX6QDL_PAD_RGMII_TD3__RGMII_TD3		0x1b030
			MX6QDL_PAD_RGMII_TX_CTL__RGMII_TX_CTL	0x1b030
			/* AR8035 CLK_25M --> ENET_REF_CLK (V22) */
			MX6QDL_PAD_ENET_REF_CLK__ENET_TX_CLK	0x0a0b1
			/* AR8035 pin strapping: IO voltage: pull up */
			MX6QDL_PAD_RGMII_RXC__RGMII_RXC		0x1b030
			/* AR8035 pin strapping: PHYADDR#0: pull down */
			MX6QDL_PAD_RGMII_RD0__RGMII_RD0		0x13030
			/* AR8035 pin strapping: PHYADDR#1: pull down */
			MX6QDL_PAD_RGMII_RD1__RGMII_RD1		0x13030
			/* AR8035 pin strapping: MODE#1: pull up */
			MX6QDL_PAD_RGMII_RD2__RGMII_RD2		0x1b030
			/* AR8035 pin strapping: MODE#3: pull up */
			MX6QDL_PAD_RGMII_RD3__RGMII_RD3		0x1b030
			/* AR8035 pin strapping: MODE#0: pull down */
			MX6QDL_PAD_RGMII_RX_CTL__RGMII_RX_CTL	0x13030
		>;
	};

	pinctrl_flexcan2: flexcan2grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL4__FLEXCAN2_TX	0x1b0b0
			MX6QDL_PAD_KEY_ROW4__FLEXCAN2_RX	0x1b0b0
		>;
	};

	pinctrl_gpio_keys: gpio_keysgrp {
		fsl,pins = <
			MX6QDL_PAD_SD4_DAT4__GPIO2_IO12 0x1b0b0
		>;
	};

	pinctrl_hdmi_cec: hdmicecgrp {
		fsl,pins = <
			MX6QDL_PAD_KEY_ROW2__HDMI_TX_CEC_LINE 0x108b0
		>;
	};

	pinctrl_i2c1: i2c1grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT8__I2C1_SDA		0x4001b8b1
			MX6QDL_PAD_CSI0_DAT9__I2C1_SCL		0x4001b8b1
		>;
	};

	pinctrl_i2c2: i2c2grp {
		fsl,pins = <
			MX6QDL_PAD_KEY_COL3__I2C2_SCL		0x4001b8b1
			MX6QDL_PAD_KEY_ROW3__I2C2_SDA		0x4001b8b1
		>;
	};

	pinctrl_i2c3: i2c3grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_3__I2C3_SCL		0x4001b8b1
			MX6QDL_PAD_GPIO_6__I2C3_SDA		0x4001b8b1
		>;
	};

	pinctrl_i2c1_sgtl5000: i2c1-sgtl5000grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_0__CCM_CLKO1			0x000b0 /* sys_mclk */
			MX6QDL_PAD_SD3_RST__GPIO7_IO08		0x130b0 /*headphone det*/
			MX6QDL_PAD_GPIO_8__GPIO1_IO08			0x130b0 /*microphone det*/
		>;
	};

	pinctrl_pwm1: pwm1grp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_9__PWM1_OUT	    0x1b0b1
		>;
	};

	pinctrl_uart1: uart1grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT10__UART1_RX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT11__UART1_TX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D20__UART1_CTS_B	0x1b0b1
			MX6QDL_PAD_EIM_D19__UART1_RTS_B	0x1b0b1
			MX6QDL_PAD_EIM_D23__UART1_DCD_B	0x1b0b0
			MX6QDL_PAD_EIM_D24__UART1_DTR_B	0x1b0b0
			MX6QDL_PAD_EIM_D25__UART1_DSR_B	0x1b0b0
		>;
	};

	pinctrl_uart2: uart2grp {
		fsl,pins = <
			MX6QDL_PAD_EIM_D26__UART2_TX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D27__UART2_RX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D28__UART2_CTS_B	0x1b0b1
			MX6QDL_PAD_EIM_D29__UART2_RTS_B	0x1b0b1
		>;
	};

	pinctrl_uart3: uart3grp {
		fsl,pins = <
			MX6QDL_PAD_SD4_CLK__UART3_RX_DATA	0x1b0b1
			MX6QDL_PAD_SD4_CMD__UART3_TX_DATA	0x1b0b1
			MX6QDL_PAD_EIM_D30__UART3_CTS_B		0x1b0b1
			MX6QDL_PAD_EIM_D31__UART3_RTS_B		0x1b0b1
		>;
	};

	pinctrl_uart4: uart4grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT12__UART4_TX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT13__UART4_RX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT16__UART4_RTS_B	0x1b0b1
			MX6QDL_PAD_CSI0_DAT17__UART4_CTS_B	0x1b0b1
		>;
	};

	pinctrl_uart5: uart5grp {
		fsl,pins = <
			MX6QDL_PAD_CSI0_DAT14__UART5_TX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT15__UART5_RX_DATA	0x1b0b1
			MX6QDL_PAD_CSI0_DAT18__UART5_RTS_B	0x1b0b1
			MX6QDL_PAD_CSI0_DAT19__UART5_CTS_B	0x1b0b1
			MX6QDL_PAD_EIM_A21__GPIO2_IO17		 0x15059 /*BT_EN*/
		>;
	};

	pinctrl_usbotg: usbotggrp {
		fsl,pins = <
			MX6QDL_PAD_ENET_RX_ER__USB_OTG_ID	0x17059
		>;
	};

	pinctrl_usdhc1: usdhc1grp {
		fsl,pins = <
			MX6QDL_PAD_SD1_CMD__SD1_CMD		0x17059
			MX6QDL_PAD_SD1_CLK__SD1_CLK		0x10059
			MX6QDL_PAD_SD1_DAT0__SD1_DATA0		0x17059
			MX6QDL_PAD_SD1_DAT1__SD1_DATA1		0x17059
			MX6QDL_PAD_SD1_DAT2__SD1_DATA2		0x17059
			MX6QDL_PAD_SD1_DAT3__SD1_DATA3		0x17059
			MX6QDL_PAD_NANDF_D0__SD1_DATA4		0x17059
			MX6QDL_PAD_NANDF_D1__SD1_DATA5		0x17059
			MX6QDL_PAD_NANDF_D2__SD1_DATA6		0x17059
			MX6QDL_PAD_NANDF_D3__SD1_DATA7		0x17059
		>;
	};

	pinctrl_usdhc2: usdhc2grp {
		fsl,pins = <
			MX6QDL_PAD_SD2_CMD__SD2_CMD		0x17059
			MX6QDL_PAD_SD2_CLK__SD2_CLK		0x10059
			MX6QDL_PAD_SD2_DAT0__SD2_DATA0		0x17059
			MX6QDL_PAD_SD2_DAT1__SD2_DATA1		0x17059
			MX6QDL_PAD_SD2_DAT2__SD2_DATA2		0x17059
			MX6QDL_PAD_SD2_DAT3__SD2_DATA3		0x17059
			MX6QDL_PAD_EIM_RW__GPIO2_IO26			0x15059 /*WL_EN_LDO*/
			MX6QDL_PAD_EIM_CS1__GPIO2_IO24		0x15059 /*WL_EN*/
			MX6QDL_PAD_CSI0_PIXCLK__GPIO5_IO18	0x15059 /*WL_IRQ*/
		>;
	};

	pinctrl_usdhc3: usdhc3grp {
		fsl,pins = <
			MX6QDL_PAD_SD3_CMD__SD3_CMD		0x17071
			MX6QDL_PAD_SD3_CLK__SD3_CLK		0x10071
			MX6QDL_PAD_SD3_DAT0__SD3_DATA0		0x17071
			MX6QDL_PAD_SD3_DAT1__SD3_DATA1		0x17071
			MX6QDL_PAD_SD3_DAT2__SD3_DATA2		0x17071
			MX6QDL_PAD_SD3_DAT3__SD3_DATA3		0x17071
		>;
	};

	pinctrl_wdog: wdoggrp {
		fsl,pins = <
			MX6QDL_PAD_GPIO_1__WDOG2_B	0x1b0b00
		>;
	};
};

&ldb {
	status = "okay";

	lvds-channel@1 {
		fsl,data-mapping = "spwg";
		fsl,data-width = <18>;
		status = "okay";

		port@4 {
			reg = <4>;

			lvds0_out: endpoint {
				remote-endpoint = <&panel_in>;
			};
		};
	};
};

&pwm1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pwm1>;
	status = "okay";
};

&snvs_poweroff {
	status = "okay";
};

&ssi1 {
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart1>;
	uart-has-rtscts;
	fsl,dte-mode;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart2>;
	uart-has-rtscts;
	status = "okay";
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart3>;
	uart-has-rtscts;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart4>;
	uart-has-rtscts;
	status = "okay";
};

&uart5 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_uart5>;
	uart-has-rtscts;
	status = "okay";
};

&usbotg {
	vbus-supply = <&reg_usb_otg_vbus>;
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usbotg>;
	disable-over-current;
	srp-disable;
	hnp-disable;
	adp-disable;
	status = "okay";
};

&usbh1 {
	status = "okay";
};

&usbphy1 {
	fsl,tx-d-cal = <79>;
};

&usbphy2 {
	fsl,tx-d-cal = <79>;
};

&usdhc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc1>;
	bus-width = <8>;
	keep-power-in-suspend;
	vmmc-supply = <&reg_3p3v>;
	status = "okay";
};

&usdhc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc2>;
	bus-width = <4>;
	vmmc-supply = <&wlan_en_reg>;
	no-1-8-v;
	keep-power-in-suspend;
	non-removable;
	cap-power-off-card;
	status = "okay";

	#address-cells = <1>;
	#size-cells = <0>;
	wlcore: wlcore@2 {
		compatible = "ti,wl1835";
		reg = <2>;
		interrupt-parent = <&gpio5>;
		interrupts = <18 IRQ_TYPE_LEVEL_HIGH>;
		ref-clock-frequency = <38400000>;
		tcxo-clock-frequency = <26000000>;
	};
};

&usdhc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_usdhc3>;
	bus-width = <4>;
	cd-gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
	no-1-8-v;
	keep-power-in-suspend;
	wakeup-source;
	status = "okay";
};

&sata {
	status = "okay";
};

&wdog1 {
	status = "okay";
};
