// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2012 Texas Instruments Incorporated - https://www.ti.com/
 */

/*
 * VScom OnRISC
 * https://www.vscom.de
 */

/dts-v1/;

#include "am335x-baltos.dtsi"

/ {
	model = "NetCom Plus";
};

&am33xx_pinmux {
	pinctrl-names = "default";
	pinctrl-0 = <&dip_switches>;

	dip_switches: dip-switches-pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD12, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD13, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD14, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD15, PIN_INPUT_PULLDOWN, MUX_MODE7)
		>;
	};

	tca6416_pins: tca6416-pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_XDMA_EVENT_INTR1, PIN_INPUT_PULLUP, MUX_MODE7)
		>;
	};

	i2c2_pins: i2c2-pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART1_CTSN, PIN_INPUT_PULLDOWN, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_UART1_RTSN, PIN_INPUT_PULLDOWN, MUX_MODE3)
		>;
	};
};

&usb0_phy {
	status = "okay";
};

&usb1_phy {
	status = "okay";
};

&usb0 {
	status = "okay";
	dr_mode = "host";
};

&usb1 {
	status = "okay";
	dr_mode = "host";
};

&i2c1 {
	tca6416a: gpio@20 {
		compatible = "ti,tca6416";
		reg = <0x20>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-parent = <&gpio0>;
		interrupts = <20 IRQ_TYPE_EDGE_RISING>;
		pinctrl-names = "default";
		pinctrl-0 = <&tca6416_pins>;
		gpio-line-names = "GP_IN0", "GP_IN1", "GP_IN2", "GP_IN3",
				  "GP_IN4", "GP_IN5", "GP_IN6", "GP_IN7",
				  "GP_OUT0", "GP_OUT1", "GP_OUT2", "GP_OUT3",
				  "GP_OUT4", "GP_OUT5", "GP_OUT6", "GP_OUT7";
	};
};

&i2c2 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c2_pins>;

	status = "okay";
	clock-frequency = <400000>;

	tca6416b: gpio@20 {
		compatible = "ti,tca6416";
		reg = <0x20>;
		gpio-controller;
		#gpio-cells = <2>;
		gpio-line-names = "CH1_M0", "CH1_M1", "CH1_M2", "CH1_M3",
				  "CH2_M0", "CH2_M1", "CH2_M2", "CH2_M3",
				  "CH3_M0", "CH3_M1", "CH3_M2", "CH3_M3",
				  "CH4_M0", "CH4_M1", "CH4_M2", "CH4_M3";
	};

	tca6416c: gpio@21 {
		compatible = "ti,tca6416";
		reg = <0x21>;
		gpio-controller;
		#gpio-cells = <2>;
		gpio-line-names = "CH5_M0", "CH5_M1", "CH5_M2", "CH5_M3",
				  "CH6_M0", "CH6_M1", "CH6_M2", "CH6_M3",
				  "CH7_M0", "CH7_M1", "CH7_M2", "CH7_M3",
				  "CH8_M0", "CH8_M1", "CH8_M2", "CH8_M3";
	};
};

&davinci_mdio_sw {
	phy0: ethernet-phy@0 {
		reg = <1>;
	};
};

&cpsw_port1 {
	phy-mode = "rmii";
	ti,dual-emac-pvid = <1>;
	phy-handle = <&phy0>;
};

&cpsw_port2 {
	phy-mode = "rgmii-id";
	ti,dual-emac-pvid = <2>;
	phy-handle = <&phy1>;
};

&gpio0 {
	gpio-line-names =
		"MDIO",
		"MDC",
		"NC",
		"NC",
		"I2C1_SDA",
		"I2C1_SCL",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"I2C2_SDA",
		"I2C2_SCL",
		"NC",
		"NC",
		"onrisc:blue:wlan",
		"onrisc:green:app",
		"USB0_DRVVBUS",
		"ETH2_INT",
		"NC",
		"NC",
		"MMC1_DAT0",
		"MMC1_DAT1",
		"NC",
		"NC",
		"MMC1_DAT2",
		"MMC1_DAT3",
		"NC",
		"NC",
		"GPMC_WAIT0",
		"GPMC_WP_N";
};

&gpio1 {
	gpio-line-names =
		"GPMC_AD0",
		"GPMC_AD1",
		"GPMC_AD2",
		"GPMC_AD3",
		"GPMC_AD4",
		"GPMC_AD5",
		"GPMC_AD6",
		"GPMC_AD7",
		"NC",
		"NC",
		"CONSOLE_RX",
		"CONSOLE_TX",
		"SW2_0_alt",
		"SW2_1_alt",
		"SW2_2_alt",
		"SW2_3_alt",
		"RGMII2_TCTL",
		"RGMII2_RCTL",
		"RGMII2_TD3",
		"RGMII2_TD2",
		"RGMII2_TD1",
		"RGMII2_TD0",
		"RGMII2_TCLK",
		"RGMII2_RCLK",
		"RGMII2_RD3",
		"RGMII2_RD2",
		"RGMII2_RD1",
		"RGMII2_RD0",
		"PMIC_INT1",
		"GPMC_CSN0_Flash",
		"MMC1_CLK",
		"MMC1_CMD";
};

&gpio2 {
	gpio-line-names =
		"GPMC_CSN3_BUS",
		"GPMC_CLK",
		"GPMC_ADVN_ALE",
		"GPMC_OEN_RE_N",
		"GPMC_WE_N",
		"GPMC_BEN0_CLE",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"SW2_0",
		"SW2_1",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"MMC0_DAT3",
		"MMC0_DAT2",
		"MMC0_DAT1",
		"MMC0_DAT0",
		"MMC0_CLK",
		"MMC0_CMD";
};

&gpio3 {
	gpio-line-names =
		"onrisc:red:power",
		"NC",
		"NC",
		"NC",
		"3G_PWR_EN",
		"NC",
		"NC",
		"WLAN_IRQ",
		"WLAN_EN",
		"SW2_2",
		"SW2_3",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC",
		"NC";
};
