// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright 2013-2014 Freescale Semiconductor, Inc.
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	#address-cells = <2>;
	#size-cells = <2>;
	interrupt-parent = <&gic>;

	aliases {
		crypto = &crypto;
		ethernet0 = &enet0;
		ethernet1 = &enet1;
		ethernet2 = &enet2;
		rtc1 = &ftm_alarm0;
		serial0 = &lpuart0;
		serial1 = &lpuart1;
		serial2 = &lpuart2;
		serial3 = &lpuart3;
		serial4 = &lpuart4;
		serial5 = &lpuart5;
		sysclk = &sysclk;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@f00 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <0xf00>;
			clocks = <&clockgen 1 0>;
			#cooling-cells = <2>;
		};

		cpu1: cpu@f01 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <0xf01>;
			clocks = <&clockgen 1 0>;
			#cooling-cells = <2>;
		};
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x0 0x0 0x0>;
	};

	sysclk: sysclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "sysclk";
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
	};

	pmu {
		compatible = "arm,cortex-a7-pmu";
		interrupts = <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
	};

	reboot {
		compatible = "syscon-reboot";
		regmap = <&dcfg>;
		offset = <0xb0>;
		mask = <0x02>;
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		device_type = "soc";
		interrupt-parent = <&gic>;
		ranges;

		ddr: memory-controller@1080000 {
			compatible = "fsl,qoriq-memory-controller";
			reg = <0x0 0x1080000 0x0 0x1000>;
			interrupts = <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>;
			big-endian;
		};

		gic: interrupt-controller@1400000 {
			compatible = "arm,gic-400", "arm,cortex-a7-gic";
			#interrupt-cells = <3>;
			interrupt-controller;
			reg = <0x0 0x1401000 0x0 0x1000>,
			      <0x0 0x1402000 0x0 0x2000>,
			      <0x0 0x1404000 0x0 0x2000>,
			      <0x0 0x1406000 0x0 0x2000>;
			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_HIGH)>;

		};

		msi1: msi-controller@1570e00 {
			compatible = "fsl,ls1021a-msi";
			reg = <0x0 0x1570e00 0x0 0x8>;
			msi-controller;
			interrupts = <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>;
		};

		msi2: msi-controller@1570e08 {
			compatible = "fsl,ls1021a-msi";
			reg = <0x0 0x1570e08 0x0 0x8>;
			msi-controller;
			interrupts = <GIC_SPI 180 IRQ_TYPE_LEVEL_HIGH>;
		};

		ifc: memory-controller@1530000 {
			compatible = "fsl,ifc";
			reg = <0x0 0x1530000 0x0 0x10000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		sfp: efuse@1e80000 {
			compatible = "fsl,ls1021a-sfp";
			reg = <0x0 0x1e80000 0x0 0x10000>;
			clocks = <&clockgen 4 3>;
			clock-names = "sfp";
		};

		dcfg: dcfg@1ee0000 {
			compatible = "fsl,ls1021a-dcfg", "syscon";
			reg = <0x0 0x1ee0000 0x0 0x1000>;
			big-endian;
		};

		qspi: spi@1550000 {
			compatible = "fsl,ls1021a-qspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x1550000 0x0 0x10000>,
			      <0x0 0x40000000 0x0 0x20000000>;
			reg-names = "QuadSPI", "QuadSPI-memory";
			interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "qspi_en", "qspi";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
			status = "disabled";
		};

		esdhc: esdhc@1560000 {
			compatible = "fsl,ls1021a-esdhc", "fsl,esdhc";
			reg = <0x0 0x1560000 0x0 0x10000>;
			interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>;
			voltage-ranges = <1800 1800 3300 3300>;
			sdhci,auto-cmd12;
			big-endian;
			bus-width = <4>;
			status = "disabled";
		};

		sata: sata@3200000 {
			compatible = "fsl,ls1021a-ahci";
			reg = <0x0 0x3200000 0x0 0x10000>,
			      <0x0 0x20220520 0x0 0x4>;
			reg-names = "ahci", "sata-ecc";
			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			dma-coherent;
			status = "disabled";
		};

		scfg: scfg@1570000 {
			compatible = "fsl,ls1021a-scfg", "syscon";
			reg = <0x0 0x1570000 0x0 0x10000>;
			big-endian;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1570000 0x10000>;

			extirq: interrupt-controller@1ac {
				compatible = "fsl,ls1021a-extirq";
				#interrupt-cells = <2>;
				#address-cells = <0>;
				interrupt-controller;
				reg = <0x1ac 4>;
				interrupt-map =
					<0 0 &gic GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>,
					<1 0 &gic GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>,
					<2 0 &gic GIC_SPI 165 IRQ_TYPE_LEVEL_HIGH>,
					<3 0 &gic GIC_SPI 167 IRQ_TYPE_LEVEL_HIGH>,
					<4 0 &gic GIC_SPI 168 IRQ_TYPE_LEVEL_HIGH>,
					<5 0 &gic GIC_SPI 169 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-map-mask = <0x7 0x0>;
			};
		};

		crypto: crypto@1700000 {
			compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
			fsl,sec-era = <7>;
			#address-cells = <1>;
			#size-cells = <1>;
			reg		 = <0x0 0x1700000 0x0 0x100000>;
			ranges		 = <0x0 0x0 0x1700000 0x100000>;
			interrupts	 = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;

			sec_jr0: jr@10000 {
				compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
				reg = <0x10000 0x10000>;
				interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr1: jr@20000 {
				compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
				reg = <0x20000 0x10000>;
				interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr2: jr@30000 {
				compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
				reg = <0x30000 0x10000>;
				interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr3: jr@40000 {
				compatible = "fsl,sec-v5.0-job-ring",
				     "fsl,sec-v4.0-job-ring";
				reg = <0x40000 0x10000>;
				interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
			};

		};

		clockgen: clocking@1ee1000 {
			compatible = "fsl,ls1021a-clockgen";
			reg = <0x0 0x1ee1000 0x0 0x1000>;
			#clock-cells = <2>;
			clocks = <&sysclk>;
		};

		tmu: tmu@1f00000 {
			compatible = "fsl,qoriq-tmu";
			reg = <0x0 0x1f00000 0x0 0x10000>;
			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
			fsl,tmu-range = <0xb0000 0x9002c 0x6004e 0x30066>;
			fsl,tmu-calibration = <0x00000000 0x00000020>,
					      <0x00000001 0x00000024>,
					      <0x00000002 0x0000002a>,
					      <0x00000003 0x00000032>,
					      <0x00000004 0x00000038>,
					      <0x00000005 0x0000003e>,
					      <0x00000006 0x00000043>,
					      <0x00000007 0x0000004a>,
					      <0x00000008 0x00000050>,
					      <0x00000009 0x00000059>,
					      <0x0000000a 0x0000005f>,
					      <0x0000000b 0x00000066>,

					      <0x00010000 0x00000023>,
					      <0x00010001 0x0000002b>,
					      <0x00010002 0x00000033>,
					      <0x00010003 0x0000003a>,
					      <0x00010004 0x00000042>,
					      <0x00010005 0x0000004a>,
					      <0x00010006 0x00000054>,
					      <0x00010007 0x0000005c>,
					      <0x00010008 0x00000065>,
					      <0x00010009 0x0000006f>,

					      <0x00020000 0x00000029>,
					      <0x00020001 0x00000033>,
					      <0x00020002 0x0000003d>,
					      <0x00020003 0x00000048>,
					      <0x00020004 0x00000054>,
					      <0x00020005 0x00000060>,
					      <0x00020006 0x0000006c>,

					      <0x00030000 0x00000025>,
					      <0x00030001 0x00000033>,
					      <0x00030002 0x00000043>,
					      <0x00030003 0x00000055>;
			#thermal-sensor-cells = <1>;
		};

		dspi0: spi@2100000 {
			compatible = "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2100000 0x0 0x10000>;
			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen 4 1>;
			spi-num-chipselects = <6>;
			big-endian;
			status = "disabled";
		};

		dspi1: spi@2110000 {
			compatible = "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2110000 0x0 0x10000>;
			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen 4 1>;
			spi-num-chipselects = <6>;
			big-endian;
			status = "disabled";
		};

		i2c0: i2c@2180000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2180000 0x0 0x10000>;
			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			dma-names = "rx", "tx";
			dmas = <&edma0 1 38>, <&edma0 1 39>;
			status = "disabled";
		};

		i2c1: i2c@2190000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2190000 0x0 0x10000>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			dma-names = "rx", "tx";
			dmas = <&edma0 1 36>, <&edma0 1 37>;
			status = "disabled";
		};

		i2c2: i2c@21a0000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x21a0000 0x0 0x10000>;
			interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			dma-names = "rx", "tx";
			dmas = <&edma0 1 34>, <&edma0 1 35>;
			status = "disabled";
		};

		uart0: serial@21c0500 {
			compatible = "fsl,16550-FIFO64", "ns16550a";
			reg = <0x0 0x21c0500 0x0 0x100>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>;
			fifo-size = <15>;
			status = "disabled";
		};

		uart1: serial@21c0600 {
			compatible = "fsl,16550-FIFO64", "ns16550a";
			reg = <0x0 0x21c0600 0x0 0x100>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>;
			fifo-size = <15>;
			status = "disabled";
		};

		uart2: serial@21d0500 {
			compatible = "fsl,16550-FIFO64", "ns16550a";
			reg = <0x0 0x21d0500 0x0 0x100>;
			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>;
			fifo-size = <15>;
			status = "disabled";
		};

		uart3: serial@21d0600 {
			compatible = "fsl,16550-FIFO64", "ns16550a";
			reg = <0x0 0x21d0600 0x0 0x100>;
			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>;
			fifo-size = <15>;
			status = "disabled";
		};

		counter0: counter@29d0000 {
			compatible = "fsl,ftm-quaddec";
			reg = <0x0 0x29d0000 0x0 0x10000>;
			big-endian;
			status = "disabled";
		};

		counter1: counter@29e0000 {
			compatible = "fsl,ftm-quaddec";
			reg = <0x0 0x29e0000 0x0 0x10000>;
			big-endian;
			status = "disabled";
		};

		counter2: counter@29f0000 {
			compatible = "fsl,ftm-quaddec";
			reg = <0x0 0x29f0000 0x0 0x10000>;
			big-endian;
			status = "disabled";
		};

		counter3: counter@2a00000 {
			compatible = "fsl,ftm-quaddec";
			reg = <0x0 0x2a00000 0x0 0x10000>;
			big-endian;
			status = "disabled";
		};

		gpio0: gpio@2300000 {
			compatible = "fsl,ls1021a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2300000 0x0 0x10000>;
			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio1: gpio@2310000 {
			compatible = "fsl,ls1021a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2310000 0x0 0x10000>;
			interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio2: gpio@2320000 {
			compatible = "fsl,ls1021a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2320000 0x0 0x10000>;
			interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio3: gpio@2330000 {
			compatible = "fsl,ls1021a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2330000 0x0 0x10000>;
			interrupts = <GIC_SPI 166 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		lpuart0: serial@2950000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2950000 0x0 0x1000>;
			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&sysclk>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart1: serial@2960000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2960000 0x0 0x1000>;
			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart2: serial@2970000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2970000 0x0 0x1000>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart3: serial@2980000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2980000 0x0 0x1000>;
			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart4: serial@2990000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x2990000 0x0 0x1000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "ipg";
			status = "disabled";
		};

		lpuart5: serial@29a0000 {
			compatible = "fsl,ls1021a-lpuart";
			reg = <0x0 0x29a0000 0x0 0x1000>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "ipg";
			status = "disabled";
		};

		pwm0: pwm@29d0000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x29d0000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm1: pwm@29e0000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x29e0000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm2: pwm@29f0000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x29f0000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm3: pwm@2a00000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x2a00000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm4: pwm@2a10000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x2a10000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm5: pwm@2a20000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x2a20000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm6: pwm@2a30000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x2a30000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		pwm7: pwm@2a40000 {
			compatible = "fsl,vf610-ftm-pwm";
			#pwm-cells = <3>;
			reg = <0x0 0x2a40000 0x0 0x10000>;
			clock-names = "ftm_sys", "ftm_ext",
				"ftm_fix", "ftm_cnt_clk_en";
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				<&clockgen 4 1>, <&clockgen 4 1>;
			big-endian;
			status = "disabled";
		};

		wdog0: watchdog@2ad0000 {
			compatible = "fsl,imx21-wdt";
			reg = <0x0 0x2ad0000 0x0 0x10000>;
			interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>;
			clock-names = "wdog-en";
			big-endian;
		};

		sai1: sai@2b50000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0x2b50000 0x0 0x10000>;
			interrupts = <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				 <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 47>,
			       <&edma0 1 46>;
			status = "disabled";
		};

		sai2: sai@2b60000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0x2b60000 0x0 0x10000>;
			interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>,
				 <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 45>,
			       <&edma0 1 44>;
			status = "disabled";
		};

		edma0: dma-controller@2c00000 {
			#dma-cells = <2>;
			compatible = "fsl,vf610-edma";
			reg = <0x0 0x2c00000 0x0 0x10000>,
			      <0x0 0x2c10000 0x0 0x10000>,
			      <0x0 0x2c20000 0x0 0x10000>;
			interrupts = <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 135 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "edma-tx", "edma-err";
			dma-channels = <32>;
			big-endian;
			clock-names = "dmamux0", "dmamux1";
			clocks = <&clockgen 4 1>,
				 <&clockgen 4 1>;
		};

		dcu: dcu@2ce0000 {
			compatible = "fsl,ls1021a-dcu";
			reg = <0x0 0x2ce0000 0x0 0x10000>;
			interrupts = <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 0>,
				<&clockgen 4 0>;
			clock-names = "dcu", "pix";
			big-endian;
			status = "disabled";
		};

		mdio0: mdio@2d24000 {
			compatible = "gianfar";
			device_type = "mdio";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2d24000 0x0 0x4000>,
			      <0x0 0x2d10030 0x0 0x4>;
		};

		mdio1: mdio@2d64000 {
			compatible = "gianfar";
			device_type = "mdio";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2d64000 0x0 0x4000>,
			      <0x0 0x2d50030 0x0 0x4>;
		};

		ptp_clock@2d10e00 {
			compatible = "fsl,etsec-ptp";
			reg = <0x0 0x2d10e00 0x0 0xb0>;
			interrupts = <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>;
			fsl,tclk-period = <5>;
			fsl,tmr-prsc    = <2>;
			fsl,tmr-add     = <0xaaaaaaab>;
			fsl,tmr-fiper1  = <999999995>;
			fsl,tmr-fiper2  = <999999995>;
			fsl,max-adj     = <499999999>;
			fsl,extts-fifo;
		};

		enet0: ethernet@2d10000 {
			compatible = "fsl,etsec2";
			device_type = "network";
			#address-cells = <2>;
			#size-cells = <2>;
			interrupt-parent = <&gic>;
			model = "eTSEC";
			fsl,magic-packet;
			ranges;
			dma-coherent;

			queue-group@2d10000 {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d10000 0x0 0x1000>;
				interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>;
			};

			queue-group@2d14000  {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d14000 0x0 0x1000>;
				interrupts = <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		enet1: ethernet@2d50000 {
			compatible = "fsl,etsec2";
			device_type = "network";
			#address-cells = <2>;
			#size-cells = <2>;
			interrupt-parent = <&gic>;
			model = "eTSEC";
			ranges;
			dma-coherent;

			queue-group@2d50000  {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d50000 0x0 0x1000>;
				interrupts = <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;
			};

			queue-group@2d54000  {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d54000 0x0 0x1000>;
				interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		enet2: ethernet@2d90000 {
			compatible = "fsl,etsec2";
			device_type = "network";
			#address-cells = <2>;
			#size-cells = <2>;
			interrupt-parent = <&gic>;
			model = "eTSEC";
			ranges;
			dma-coherent;

			queue-group@2d90000  {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d90000 0x0 0x1000>;
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
			};

			queue-group@2d94000  {
				#address-cells = <2>;
				#size-cells = <2>;
				reg = <0x0 0x2d94000 0x0 0x1000>;
				interrupts = <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 162 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		usb2: usb@8600000 {
			compatible = "fsl-usb2-dr-v2.5", "fsl-usb2-dr";
			reg = <0x0 0x8600000 0x0 0x1000>;
			interrupts = <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			phy_type = "ulpi";
		};

		usb3: usb@3100000 {
			compatible = "snps,dwc3";
			reg = <0x0 0x3100000 0x0 0x10000>;
			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			snps,quirk-frame-length-adjustment = <0x20>;
			snps,dis_rxdet_inp3_quirk;
			usb3-lpm-capable;
			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
			snps,host-vbus-glitches;
		};

		pcie@3400000 {
			compatible = "fsl,ls1021a-pcie";
			reg = <0x00 0x03400000 0x0 0x00010000>, /* controller registers */
			      <0x40 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>; /* controller interrupt */
			fsl,pcie-scfg = <&scfg 0>;
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			num-viewport = <6>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000>, /* downstream I/O */
				 <0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&msi1>, <&msi2>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic GIC_SPI 91  IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic GIC_SPI 190 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic GIC_SPI 192 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		pcie@3500000 {
			compatible = "fsl,ls1021a-pcie";
			reg = <0x00 0x03500000 0x0 0x00010000>, /* controller registers */
			      <0x48 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
			fsl,pcie-scfg = <&scfg 1>;
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			num-viewport = <6>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000>, /* downstream I/O */
				 <0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&msi1>, <&msi2>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic GIC_SPI 92  IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic GIC_SPI 189 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		can0: can@2a70000 {
			compatible = "fsl,ls1021ar2-flexcan";
			reg = <0x0 0x2a70000 0x0 0x1000>;
			interrupts = <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "ipg", "per";
			big-endian;
			status = "disabled";
		};

		can1: can@2a80000 {
			compatible = "fsl,ls1021ar2-flexcan";
			reg = <0x0 0x2a80000 0x0 0x1000>;
			interrupts = <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "ipg", "per";
			big-endian;
			status = "disabled";
		};

		can2: can@2a90000 {
			compatible = "fsl,ls1021ar2-flexcan";
			reg = <0x0 0x2a90000 0x0 0x1000>;
			interrupts = <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "ipg", "per";
			big-endian;
			status = "disabled";
		};

		can3: can@2aa0000 {
			compatible = "fsl,ls1021ar2-flexcan";
			reg = <0x0 0x2aa0000 0x0 0x1000>;
			interrupts = <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen 4 1>, <&clockgen 4 1>;
			clock-names = "ipg", "per";
			big-endian;
			status = "disabled";
		};

		ocram1: sram@10000000 {
			compatible = "mmio-sram";
			reg = <0x0 0x10000000 0x0 0x10000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x10000000 0x10000>;
		};

		ocram2: sram@10010000 {
			compatible = "mmio-sram";
			reg = <0x0 0x10010000 0x0 0x10000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x10010000 0x10000>;
		};

		qdma: dma-controller@8390000 {
			compatible = "fsl,ls1021a-qdma";
			reg = <0x0 0x8388000 0x0 0x1000>, /* Controller regs */
			      <0x0 0x8389000 0x0 0x1000>, /* Status regs */
			      <0x0 0x838a000 0x0 0x2000>; /* Block regs */
			interrupts = <GIC_SPI 185 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "qdma-error",
				"qdma-queue0", "qdma-queue1";
			#dma-cells = <2>;
			dma-channels = <8>;
			block-number = <1>;
			block-offset = <0x1000>;
			fsl,dma-queues = <2>;
			status-sizes = <64>;
			queue-sizes = <64 64>;
			big-endian;
		};

		rcpm: power-controller@1ee2140 {
			compatible = "fsl,ls1021a-rcpm", "fsl,qoriq-rcpm-2.1+";
			reg = <0x0 0x1ee2140 0x0 0x8>;
			#fsl,rcpm-wakeup-cells = <2>;
			#power-domain-cells = <0>;
		};

		ftm_alarm0: timer0@29d0000 {
			compatible = "fsl,ls1021a-ftm-alarm";
			reg = <0x0 0x29d0000 0x0 0x10000>;
			reg-names = "ftm";
			fsl,rcpm-wakeup = <&rcpm 0x0 0x20000000>;
			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
			big-endian;
		};
	};

	thermal-zones {
		cpu_thermal: cpu-thermal {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;

			thermal-sensors = <&tmu 0>;

			trips {
				cpu_alert: cpu-alert {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};
				cpu_crit: cpu-crit {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&cpu_alert>;
					cooling-device =
						<&cpu0 THERMAL_NO_LIMIT
						THERMAL_NO_LIMIT>,
						<&cpu1 THERMAL_NO_LIMIT
						THERMAL_NO_LIMIT>;
				};
			};
		};
	};
};
