// SPDX-License-Identifier: GPL-2.0

/dts-v1/;

#include <dt-bindings/input/gpio-keys.h>
#include <dt-bindings/input/input.h>

#include "tegra114.dtsi"

/ {
	model = "Asus Transformer Pad TF701T";
	compatible = "asus,tf701t", "nvidia,tegra114";
	chassis-type = "convertible";

	aliases {
		mmc0 = "/mmc@78000600"; /* eMMC */
		mmc1 = "/mmc@78000400"; /* uSD slot */
		mmc2 = "/mmc@78000000"; /* WiFi */

		rtc0 = &palmas;
		rtc1 = "/rtc@7000e000";

		serial0 = &uartd; /* Console */
		serial1 = &uartc; /* Bluetooth */
		serial2 = &uartb; /* GPS */
	};

	firmware {
		trusted-foundations {
			compatible = "tlm,trusted-foundations";
			tlm,version-major = <2>;
			tlm,version-minor = <8>;
		};
	};

	memory@80000000 {
		reg = <0x80000000 0x80000000>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		linux,cma@80000000 {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x80000000 0x30000000>;
			size = <0x10000000>;
			linux,cma-default;
			reusable;
		};

		trustzone@bfe00000 {
			reg = <0xbfe00000 0x200000>;
			no-map;
		};
	};

	host1x@50000000 {
		hdmi@54280000 {
			status = "okay";

			hdmi-supply = <&hdmi_5v0_sys>;
			pll-supply = <&avdd_hdmi_pll>;
			vdd-supply = <&avdd_hdmi>;

			port {
				hdmi_out: endpoint {
					remote-endpoint = <&connector_in>;
				};
			};
		};

		dsi@54300000 {
			status = "okay";

			avdd-dsi-csi-supply = <&avdd_dsi_csi>;

			nvidia,ganged-mode = <&dsib>;

			panel_primary: panel@0 {
				compatible = "sharp,lq101r1sx01";
				reg = <0>;

				link2 = <&panel_secondary>;

				power-supply = <&dvdd_1v8_lcd>;
				backlight = <&backlight>;
			};
		};

		dsi@54400000 {
			status = "okay";

			avdd-dsi-csi-supply = <&avdd_dsi_csi>;

			panel_secondary: panel@0 {
				compatible = "sharp,lq101r1sx01";
				reg = <0>;
			};
		};
	};

	vde@6001a000 {
		assigned-clocks = <&tegra_car TEGRA114_CLK_VDE>;
		assigned-clock-parents = <&tegra_car TEGRA114_CLK_PLL_P>;
		assigned-clock-rates = <408000000>;
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			/* WLAN SDIO pinmux */
			sdmmc1-clk {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc1-cmd {
				nvidia,pins = "sdmmc1_cmd_pz1",
					      "sdmmc1_dat0_py7",
					      "sdmmc1_dat1_py6",
					      "sdmmc1_dat2_py5",
					      "sdmmc1_dat3_py4";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			wlan-power {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			wlan-reset {
				nvidia,pins = "gpio_x7_aud_px7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			wlan-host-wake {
				nvidia,pins = "pu5";
				nvidia,function = "pwm2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			wlan-3v3-com {
				nvidia,pins = "pu1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* UART-A pinmux */
			uarta-cts {
				nvidia,pins = "kb_row10_ps2";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uarta-rts {
				nvidia,pins = "kb_row9_ps1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* GNSS UART-B pinmux */
			uartb-cts {
				nvidia,pins = "uart2_cts_n_pj5";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uartb-rts {
				nvidia,pins = "uart2_rts_n_pj6";
				nvidia,function = "uartb";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			uartb-rxd {
				nvidia,pins = "uart2_rxd_pc3";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uartb-txd {
				nvidia,pins = "uart2_txd_pc2";
				nvidia,function = "irda";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Bluetooth UART-C pinmux */
			uartc-cts-rxd {
				nvidia,pins = "uart3_cts_n_pa1",
					      "uart3_rxd_pw7";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uartc-rts-txd {
				nvidia,pins = "uart3_rts_n_pc0",
					      "uart3_txd_pw6";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			bt-shutdown {
				nvidia,pins = "kb_col6_pq6",
					      "kb_col7_pq7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			bt-dev-wake {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			bt-host-wake {
				nvidia,pins = "pu6";
				nvidia,function = "pwm3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			bt-pcm-dap4-out {
				nvidia,pins = "dap4_fs_pp4",
					      "dap4_dout_pp6",
					      "dap4_sclk_pp7";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			bt-pcm-dap4-in {
				nvidia,pins = "dap4_din_pp5";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* UART-D pinmux */
			uartd-cts {
				nvidia,pins = "gmi_a17_pb0";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			uartd-rts {
				nvidia,pins = "gmi_a16_pj7",
					      "gmi_a19_pk7";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* MicroSD pinmux */
			sdmmc3-clk {
				nvidia,pins = "sdmmc3_clk_pa6";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc3-data {
				nvidia,pins = "sdmmc3_cmd_pa7",
					      "sdmmc3_dat0_pb7",
					      "sdmmc3_dat1_pb6",
					      "sdmmc3_dat2_pb5",
					      "sdmmc3_dat3_pb4",
					      "kb_col4_pq4",
					      "sdmmc3_cd_n_pv2",
					      "sdmmc3_clk_lb_out_pee4",
					      "sdmmc3_clk_lb_in_pee5";
				nvidia,function = "sdmmc3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			microsd-pwr {
				nvidia,pins = "gmi_clk_pk1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* EMMC pinmux */
			sdmmc4-clk-cmd {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sdmmc4-data {
				nvidia,pins = "sdmmc4_cmd_pt7",
					      "sdmmc4_dat0_paa0",
					      "sdmmc4_dat1_paa1",
					      "sdmmc4_dat2_paa2",
					      "sdmmc4_dat3_paa3",
					      "sdmmc4_dat4_paa4",
					      "sdmmc4_dat5_paa5",
					      "sdmmc4_dat6_paa6",
					      "sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* I2C pinmux */
			gen1-i2c {
				nvidia,pins = "gen1_i2c_scl_pc4",
					      "gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			gen2-i2c {
				nvidia,pins = "gen2_i2c_scl_pt5",
					      "gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			cam-i2c {
				nvidia,pins = "cam_i2c_scl_pbb1",
					      "cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};
			
			ddc-i2c {
				nvidia,pins = "ddc_scl_pv4",
					      "ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			pwr-i2c {
				nvidia,pins = "pwr_i2c_scl_pz6",
					      "pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			/* SPI pinmux */
			spi1-out {
				nvidia,pins = "ulpi_clk_py0",
					      "ulpi_nxt_py2",
					      "ulpi_stp_py3";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spi1-in {
				nvidia,pins = "ulpi_dir_py1";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			spi2 {
				nvidia,pins = "ulpi_data4_po5",
					      "ulpi_data7_po0";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			spi4-out {
				nvidia,pins = "gmi_ad6_pg6",
					      "gmi_wr_n_pi0";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spi4-in {
				nvidia,pins = "gmi_ad5_pg5",
					      "gmi_ad7_pg7";
				nvidia,function = "spi4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GPIO keys pinmux */
			hall-switch {
				nvidia,pins = "ulpi_data4_po5";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			lineout-switch {
				nvidia,pins = "gpio_x5_aud_px5";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			power-key {
				nvidia,pins = "kb_col0_pq0";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			volume-keys {
				nvidia,pins = "kb_row1_pr1",
					      "kb_row2_pr2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Sensors pinmux */
			nct-irq {
				nvidia,pins = "ulpi_data3_po4";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			mpu-irq {
				nvidia,pins = "kb_row3_pr3";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* HDMI pinmux */
			hdmi-hpd {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			hdmi-en {
				nvidia,pins = "dap3_dout_pp2";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			hdmi-cec {
				nvidia,pins = "hdmi_cec_pee3";
				nvidia,function = "cec";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* LED pinmux */
			backlight-pwm {
				nvidia,pins = "gmi_ad9_ph1";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			backlight-en {
				nvidia,pins = "gmi_ad10_ph2";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Touchscreen pinmux */
			touch-irq {
				nvidia,pins = "gmi_cs4_n_pk2";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			touch-rst {
				nvidia,pins = "gmi_cs3_n_pk4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			touch-pwr {
				nvidia,pins = "gmi_ad8_ph0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			touch-vio {
				nvidia,pins = "gmi_ad12_ph4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* AUDIO pinmux */
			audio-ldo1 {
				nvidia,pins = "sdmmc1_wp_n_pv3";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			hp-detect {
				nvidia,pins = "kb_row7_pr7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap-i2s0-in {
				nvidia,pins = "dap1_din_pn1";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap-i2s0-out {
				nvidia,pins = "dap1_dout_pn2",
					      "dap1_fs_pn0",
					      "dap1_sclk_pn3";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			dap-i2s1-in {
				nvidia,pins = "dap2_din_pa4";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap-i2s1-out {
				nvidia,pins = "dap2_dout_pa5",
					      "dap2_fs_pa2",
					      "dap2_sclk_pa3";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			dap-i2s2-in {
				nvidia,pins = "dap3_fs_pp0",
					      "dap3_sclk_pp3";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dap-i2s2-out {
				nvidia,pins = "dap3_din_pp1";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spdif-in {
				nvidia,pins = "spdif_in_pk6";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			spdif-out {
				nvidia,pins = "spdif_out_pk5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* AsusEC pinmux */
			ec-irq {
				nvidia,pins = "kb_col5_pq5";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ec-req {
				nvidia,pins = "kb_col2_pq2";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			hotplug-i2c {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ps2-irq {
				nvidia,pins = "gpio_w2_aud_pw2";
				nvidia,function = "spi6";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kbd-irq {
				nvidia,pins = "gmi_cs0_n_pj0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			dvfs-pin {
				nvidia,pins = "dvfs_pwm_px0",
					      "dvfs_clk_px2";
				nvidia,function = "cldvfs";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Core pinmux */
			clk-32k-out {
				nvidia,pins = "clk_32k_out_pa0";
				nvidia,function = "soc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			sys-clk-req {
				nvidia,pins = "sys_clk_req_pz5";
				nvidia,function = "sysclk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			core-pwr-req {
				nvidia,pins = "core_pwr_req";
				nvidia,function = "pwron";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			cpu-pwr-req {
				nvidia,pins = "cpu_pwr_req";
				nvidia,function = "cpu";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pwr-int-n {
				nvidia,pins = "pwr_int_n";
				nvidia,function = "pmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			clk-32k-in {
				nvidia,pins = "clk_32k_in";
				nvidia,function = "clk";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			owr {
				nvidia,pins = "owr";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			reset-out-n {
				nvidia,pins = "reset_out_n";
				nvidia,function = "reset_out_n";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* ULPI pinmux */
			ulpi-data0-6 {
				nvidia,pins = "ulpi_data0_po1",
					      "ulpi_data6_po7";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ulpi-data1-5 {
				nvidia,pins = "ulpi_data1_po2",
					      "ulpi_data5_po6";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ulpi-data2-3 {
				nvidia,pins = "ulpi_data2_po3",
					      "ulpi_data3_po4";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PORT V */
			pv0-gpio {
				nvidia,pins = "pv0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pv1-gpio {
				nvidia,pins = "pv1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PORT U */
			pu0-gpio {
				nvidia,pins = "pu0";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pu2-gpio {
				nvidia,pins = "pu2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PWM pinmux */
			pwm0 {
				nvidia,pins = "pu3";
				nvidia,function = "pwm0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pwm1 {
				nvidia,pins = "pu4";
				nvidia,function = "pwm1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* EXTPERIPH pinmux */
			clk1-out {
				nvidia,pins = "clk1_out_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk2-out {
				nvidia,pins = "clk2_out_pw5";
				nvidia,function = "extperiph2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk3-out {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			clk1-req {
				nvidia,pins = "clk1_req_pee2";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* GMI pinmux */
			gmi-wp-n {
				nvidia,pins = "gmi_wp_n_pc7";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-adv {
				nvidia,pins = "gmi_adv_n_pk0";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-ad0-ad1 {
				nvidia,pins = "gmi_ad0_pg0",
					      "gmi_ad1_pg1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi-ad2-ad3 {
				nvidia,pins = "gmi_ad2_pg2",
					      "gmi_ad3_pg3";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-iordy {
				nvidia,pins = "gmi_iordy_pi5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-a18 {
				nvidia,pins = "gmi_a18_pb1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-wait {
				nvidia,pins = "gmi_wait_pi7";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi-cs6-n {
				nvidia,pins = "gmi_cs6_n_pi3";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi-cs7-n {
				nvidia,pins = "gmi_cs7_n_pi6";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-dqs-p {
				nvidia,pins = "gmi_dqs_p_pj3";
				nvidia,function = "nand";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-cs2-ad {
				nvidia,pins = "gmi_cs2_n_pk3",
					      "gmi_ad14_ph6",
					      "gmi_ad15_ph7";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-cs4-clk {
				nvidia,pins = "gmi_cs4_n_pk2",
					      "gmi_clk_lb";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-ad11 {
				nvidia,pins = "gmi_ad11_ph3";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gmi-cs1-oe {
				nvidia,pins = "gmi_cs1_n_pj2",
					      "gmi_oe_n_pi1";
				nvidia,function = "soc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-ad4 {
				nvidia,pins = "gmi_ad4_pg4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-ad13 {
				nvidia,pins = "gmi_ad13_ph5";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gmi-rst-n {
				nvidia,pins = "gmi_rst_n_pi4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* PORT CC */
			pcc-gpio {
				nvidia,pins = "pcc1", "pcc2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* PORT BB */
			pbb3-gpio {
				nvidia,pins = "pbb3";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			pbb4-5-6-gpio {
				nvidia,pins = "pbb4", "pbb5", "pbb6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			pbb7-gpio {
				nvidia,pins = "pbb7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* KBC pinmux */
			kb-r0-c1 {
				nvidia,pins = "kb_row0_pr0",
					      "kb_col1_pq1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb-row4 {
				nvidia,pins = "kb_row4_pr4";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb-row5 {
				nvidia,pins = "kb_row5_pr5";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb-row6 {
				nvidia,pins = "kb_row6_pr6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			kb-r8-c3 {
				nvidia,pins = "kb_row8_ps0",
					      "kb_col3_pq3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* VI pinmux */
			cam-mclk {
				nvidia,pins = "cam_mclk_pcc0",
					      "pbb0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* AUD pinmux */
			gpio-x4-aud {
				nvidia,pins = "gpio_x4_aud_px4";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			gpio-x1-aud {
				nvidia,pins = "gpio_x1_aud_px1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gpio-x3-aud {
				nvidia,pins = "gpio_x3_aud_px3";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			gpio-x6-aud {
				nvidia,pins = "gpio_x6_aud_px6";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			usb-vbus {
				nvidia,pins = "usb_vbus_en0_pn4",
					      "usb_vbus_en1_pn5";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* GPIO power/drive control */
			drive-sdio1 {
				nvidia,pins = "drive_sdio1";
				nvidia,high-speed-mode = <TEGRA_PIN_ENABLE>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <36>;
				nvidia,pull-up-strength = <20>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_SLOW>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_SLOW>;
			};

			drive-sdio3 {
				nvidia,pins = "drive_sdio3";
				nvidia,high-speed-mode = <TEGRA_PIN_ENABLE>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <22>;
				nvidia,pull-up-strength = <36>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};

			drive-gma {
				nvidia,pins = "drive_gma";
				nvidia,high-speed-mode = <TEGRA_PIN_ENABLE>;
				nvidia,schmitt = <TEGRA_PIN_DISABLE>;
				nvidia,pull-down-strength = <2>;
				nvidia,pull-up-strength = <2>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};
		};
	};

	serial@70006040 {
		/* GPS */
	};

	serial@70006200 {
		compatible = "nvidia,tegra114-hsuart", "nvidia,tegra30-hsuart";
		reset-names = "serial";
		/delete-property/ reg-shift;
		status = "okay";

		nvidia,adjust-baud-rates = <0 9600 100>,
					   <9600 115200 200>,
					   <1000000 4000000 136>;

		bluetooth {
			compatible = "brcm,bcm4334-bt";
			max-speed = <4000000>;

			clocks = <&tegra_pmc TEGRA_PMC_CLK_BLINK>;
			clock-names = "txco";

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(U, 6) IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "host-wakeup";

			device-wakeup-gpios = <&gpio TEGRA_GPIO(EE, 1) GPIO_ACTIVE_HIGH>;
			shutdown-gpios = <&gpio TEGRA_GPIO(Q, 7) GPIO_ACTIVE_HIGH>;
			reset-gpios = <&gpio TEGRA_GPIO(Q, 6) GPIO_ACTIVE_LOW>;

			vbat-supply = <&vdd_3v3_com>;
			vddio-supply = <&vdd_1v8_vio>;
		};
	};

	serial@70006300 {
		/delete-property/ dmas;
		/delete-property/ dma-names;
		status = "okay";
	};

	pwm@7000a000 {
		status = "okay";
	};

	i2c@7000c000 {
		status = "okay";
		clock-frequency = <100000>;

		magnetometer@c {
			compatible = "asahi-kasei,ak09911";
			reg = <0xc>;

			/* no DRDY (polling) */

			vdd-supply = <&vdd_2v85_sen>;
			vid-supply = <&vdd_1v8_vio>;

			mount-matrix =  "0",  "1", "0",
					"1",  "0", "0",
					"0",  "0","-1";
		};

		rt5639: audio-codec@1c {
			compatible = "realtek,rt5639";
			reg = <0x1c>;

			realtek,ldo1-en-gpios =
				<&gpio TEGRA_GPIO(V, 3) GPIO_ACTIVE_HIGH>;

			clocks = <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;
			clock-names = "mclk";
		};

		temp_sensor: temperature-sensor@4c {
			compatible = "onnn,nct1008";
			reg = <0x4c>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(O, 4) IRQ_TYPE_EDGE_FALLING>;

			vcc-supply = <&vdd_1v8_vio>;
			#thermal-sensor-cells = <1>;
		};

		motion-tracker@68 {
			compatible = "invensense,mpu6500";
			reg = <0x68>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(R, 3) IRQ_TYPE_LEVEL_HIGH>;

			vdd-supply = <&vdd_2v85_sen>;
			vddio-supply = <&vdd_1v8_vio>;

			mount-matrix =  "0", "-1", "0",
					"1",  "0", "0",
					"0",  "0", "1";
		};
	};

	i2c@7000c400 {
		status = "okay";
		clock-frequency = <100000>;

		power-sensor@44 {
			compatible = "ti,ina230";
			reg = <0x44>;

			shunt-resistor = <5000>;
		};
	};

	i2c@7000c500 {
		status = "okay";
		clock-frequency = <400000>;

		light-sensor@1c {
			compatible = "dynaimage,al3320a";
			reg = <0x1c>;

			vdd-supply = <&vdd_1v8_vio>;
		};
	};

	hdmi_ddc: i2c@7000c700 {
		status = "okay";
		clock-frequency = <10000>;
	};

	i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		palmas: pmic@58 {
			compatible = "ti,tps65913", "ti,palmas";
			reg = <0x58>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;

			#interrupt-cells = <2>;
			interrupt-controller;

			ti,system-power-controller;

			palmas_gpadc: adc {
				compatible = "ti,palmas-gpadc";
				interrupts = <18 IRQ_TYPE_NONE>,
					     <16 IRQ_TYPE_NONE>,
					     <17 IRQ_TYPE_NONE>;

				ti,channel0-current-microamp = <5>;
				ti,channel3-current-microamp = <400>;
				ti,enable-extended-delay;

				#io-channel-cells = <1>;
			};

			palmas_extcon: extcon {
				compatible = "ti,palmas-usb-vid";
				ti,enable-vbus-detection;
				ti,enable-id-detection;
			};

			palmas_gpio: gpio {
				compatible = "ti,palmas-gpio";
				gpio-controller;
				#gpio-cells = <2>;
			};

			palmas_clk32kg@0 {
				compatible = "ti,palmas-clk32kg";
				#clock-cells = <0>;
			};

			pinmux {
				compatible = "ti,tps65913-pinctrl";
				ti,palmas-enable-dvfs1;

				pinctrl-names = "default";
				pinctrl-0 = <&palmas_default>;

				palmas_default: pinmux {
					pin_gpio0 {
						pins = "gpio0";
						function = "gpio";
					};

					pin_gpio1 {
						pins = "gpio1";
						function = "gpio";
					};

					pin_gpio2 {
						pins = "gpio2";
						function = "gpio";
					};

					pin_gpio3 {
						pins = "gpio3";
						function = "gpio";
					};

					pin_gpio4 {
						pins = "gpio4";
						function = "gpio";
					};

					pin_gpio5 {
						pins = "gpio5";
						function = "gpio";
					};

					pin_gpio6 {
						pins = "gpio6";
						function = "gpio";
					};

					pin_gpio7 {
						pins = "gpio7";
						function = "gpio";
					};

					pin_powergood {
						pins = "powergood";
						function = "powergood";
					};

					pin_vac {
						pins = "vac";
						function = "vac";
					};
				};
			};

			pmic {
				compatible = "ti,tps65913-pmic", "ti,palmas-pmic";

				ldo1-in-supply = <&vddio_ddr>;
				ldo2-in-supply = <&vddio_ddr>;
				ldo4-in-supply = <&vdd_1v8_vio>;
				ldo5-in-supply = <&vcore_emmc>;
				ldo6-in-supply = <&vcore_emmc>;
				ldo7-in-supply = <&vcore_emmc>;
				ldo9-in-supply = <&vcore_emmc>;
				ldoln-in-supply = <&vdd_smps10_out2>;

				regulators {
					vdd_cpu: smps123 {
						regulator-name = "vdd_cpu";
						regulator-min-microvolt = <900000>;
						regulator-max-microvolt = <1350000>;
						regulator-always-on;
						regulator-boot-on;
						ti,roof-floor = <1>;
						ti,mode-sleep = <3>;
					};

					vdd_core: smps45 {
						regulator-name = "vdd_core";
						regulator-min-microvolt = <900000>;
						regulator-max-microvolt = <1400000>;
						regulator-always-on;
						regulator-boot-on;
						ti,roof-floor = <3>;
					};

					/* smps6 disabled */

					vddio_ddr: smps7 {
						regulator-name = "vddio_ddr";
						regulator-min-microvolt = <1350000>;
						regulator-max-microvolt = <1350000>;
						regulator-always-on;
						regulator-boot-on;
					};

					vdd_1v8_vio: smps8 {
						regulator-name = "vdd_1v8";
						regulator-min-microvolt = <1800000>;
						regulator-max-microvolt = <1800000>;
						regulator-always-on;
						regulator-boot-on;
					};

					vcore_emmc: smps9 {
						regulator-name = "vdd_emmc";
						regulator-min-microvolt = <2900000>;
						regulator-max-microvolt = <2900000>;
						regulator-boot-on;
					};

					smps10_out1 {
						regulator-name = "vd_smps10_out1";
						regulator-min-microvolt = <5000000>;
						regulator-max-microvolt = <5000000>;
						regulator-always-on;
						regulator-boot-on;
					};

					vdd_smps10_out2: smps10_out2 {
						regulator-name = "vd_smps10_out2";
						regulator-min-microvolt = <5000000>;
						regulator-max-microvolt = <5000000>;
						regulator-always-on;
						regulator-boot-on;
					};

					avdd_hdmi_pll: ldo1 {
						regulator-name = "avdd_hdmi_pll";
						regulator-min-microvolt = <1050000>;
						regulator-max-microvolt = <1050000>;
						regulator-always-on;
						regulator-boot-on;
						ti,roof-floor = <3>;
					};

					avdd_dsi_csi: ldo2 {
						regulator-name = "avdd_dsi_csi";
						regulator-min-microvolt = <1200000>;
						regulator-max-microvolt = <1200000>;
						regulator-boot-on;
					};

					ldo3 {
						regulator-name = "vpp_fuse";
						regulator-min-microvolt = <1800000>;
						regulator-max-microvolt = <1800000>;
					};

					vdd_1v2_cam: ldo4 {
						regulator-name = "vdd_1v2_cam";
						regulator-min-microvolt = <1200000>;
						regulator-max-microvolt = <1200000>;
					};

					avdd_2v8_cam: ldo5 {
						regulator-name = "avdd_cam2";
						regulator-min-microvolt = <2800000>;
						regulator-max-microvolt = <2800000>;
					};

					vdd_2v85_sen: ldo6 {
						regulator-name = "vdd_dev";
						regulator-min-microvolt = <2850000>;
						regulator-max-microvolt = <2850000>;
					};

					avdd_2v8_af: ldo7 {
						regulator-name = "avdd_2v8_cam";
						regulator-min-microvolt = <2800000>;
						regulator-max-microvolt = <2800000>;
					};

					ldo8 {
						regulator-name = "vdd_rtc";
						regulator-min-microvolt = <950000>;
						regulator-max-microvolt = <950000>;
						regulator-always-on;
						regulator-boot-on;
						ti,enable-ldo8-tracking;
					};

					vddio_usd: ldo9 {
						regulator-name = "vddio_usd";
						/* min voltage of 1.8v is not stable */
						regulator-min-microvolt = <2900000>;
						regulator-max-microvolt = <2900000>;
					};

					avdd_hdmi: ldoln {
						regulator-name = "avdd_hdmi";
						regulator-min-microvolt = <3300000>;
						regulator-max-microvolt = <3300000>;
						regulator-boot-on;
					};

					avdd_usb: ldousb {
						regulator-name = "avdd_usb";
						regulator-min-microvolt = <3300000>;
						regulator-max-microvolt = <3300000>;
						regulator-boot-on;
					};
				};
			};

			rtc {
				compatible = "ti,palmas-rtc";
				interrupt-parent = <&palmas>;
				interrupts = <8 IRQ_TYPE_NONE>;
			};
		};
	};

	pmc@7000e400 {
		status = "okay";
		nvidia,suspend-mode = <2>;
		nvidia,cpu-pwr-good-time = <300>;
		nvidia,cpu-pwr-off-time = <300>;
		nvidia,core-pwr-good-time = <641 3845>;
		nvidia,core-pwr-off-time = <2000>;
		nvidia,core-power-req-active-high;
		nvidia,sys-clock-req-active-high;

		/* Clear DEV_ON bit in DEV_CTRL register of TPS65913 PMIC  */
		i2c-thermtrip {
			nvidia,i2c-controller-id = <4>;
			nvidia,bus-addr = <0x58>;
			nvidia,reg-addr = <0xA0>;
			nvidia,reg-data = <0x00>;
		};
	};

	ahub@70080000 {
		/* HIFI CODEC (i2s1) */
		i2s@70080400 {
			status = "okay";
		};

		/* BT SCO (i2s3) */
		i2s@70080600 {
			status = "okay";
		};
	};

	brcm_wifi_pwrseq: pwrseq-wifi {
		compatible = "mmc-pwrseq-simple";

		clocks = <&tegra_pmc TEGRA_PMC_CLK_BLINK>;
		clock-names = "ext_clock";

		reset-gpios = <&gpio TEGRA_GPIO(X, 7) GPIO_ACTIVE_LOW>;
		post-power-on-delay-ms = <300>;
		power-off-delay-us = <300>;
	};

	/* WiFi */
	mmc@78000000 {
		status = "okay";

		#address-cells = <1>;
		#size-cells = <0>;

		assigned-clocks = <&tegra_car TEGRA114_CLK_SDMMC1>;
		assigned-clock-parents = <&tegra_car TEGRA114_CLK_PLL_P>;
		assigned-clock-rates = <82000000>;

		max-frequency = <82000000>;
		keep-power-in-suspend;
		bus-width = <4>;
		non-removable;

		sd-uhs-ddr50;
		mmc-ddr-1_8v;

		power-gpios = <&gpio TEGRA_GPIO(CC, 5) GPIO_ACTIVE_HIGH>;

		nvidia,default-tap = <0x2>;
		nvidia,default-trim = <0x2>;

		mmc-pwrseq = <&brcm_wifi_pwrseq>;
		vmmc-supply = <&vdd_3v3_com>;
		vqmmc-supply = <&vdd_1v8_vio>;

		wifi@1 {
			compatible = "brcm,bcm4329-fmac";
			reg = <1>;

			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(U, 5) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "host-wake";
		};
	};

	/* MicroSD card */
	mmc@78000400 {
		status = "okay";

		bus-width = <4>;
		cd-gpios = <&gpio TEGRA_GPIO(V, 2) GPIO_ACTIVE_LOW>;

		nvidia,default-tap = <0x3>;
		nvidia,default-trim = <0x3>;

		vmmc-supply = <&vdd_2v9_usd>;
		vqmmc-supply = <&vddio_usd>;
	};

	/* eMMC */
	mmc@78000600 {
		status = "okay";
		bus-width = <8>;

		non-removable;
		mmc-ddr-1_8v;

		vmmc-supply = <&vcore_emmc>;
		vqmmc-supply = <&vdd_1v8_vio>;
	};

	/* Peripheral USB via ASUS connector */
	usb@7d000000 {
		compatible = "nvidia,tegra114-udc";
		status = "okay";
		dr_mode = "peripheral";
	};

	usb-phy@7d000000 {
		status = "okay";
		dr_mode = "peripheral";
		vbus-supply = <&avdd_usb>;
	};

	/* Host USB via dock */
	usb@7d008000 {
		status = "okay";
	};

	usb-phy@7d008000 {
		status = "okay";
		vbus-supply = <&vdd_5v0_sys>;
	};

	backlight: backlight {
		compatible = "pwm-backlight";

		power-supply = <&vdd_3v7_bl>;
		pwms = <&pwm 1 1000000>;

		brightness-levels = <1 255>;
		num-interpolated-steps = <254>;
		default-brightness-level = <224>;
	};

	/* PMIC has a built-in 32KHz oscillator which is used by PMC */
	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "pmic-oscillator";
	};

	connector {
		compatible = "hdmi-connector";
		type = "d";

		hpd-gpios = <&gpio TEGRA_GPIO(N, 7) GPIO_ACTIVE_HIGH>;
		ddc-i2c-bus = <&hdmi_ddc>;

		port {
			connector_in: endpoint {
				remote-endpoint = <&hdmi_out>;
			};
		};
	};

	extcon-keys {
		compatible = "gpio-keys";

		switch-hall-sensor {
			label = "Hall Effect Sensor";
			gpios = <&gpio TEGRA_GPIO(O, 5) GPIO_ACTIVE_LOW>;
			linux,input-type = <EV_SW>;
			linux,code = <SW_LID>;
			linux,can-disable;
			wakeup-source;
		};

		switch-lineout-detect {
			label = "Audio dock line-out detect";
			gpios = <&gpio TEGRA_GPIO(X, 5) GPIO_ACTIVE_LOW>;
			linux,input-type = <EV_SW>;
			linux,code = <SW_LINEOUT_INSERT>;
			debounce-interval = <10>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(Q, 0) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			debounce-interval = <10>;
			wakeup-source;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio TEGRA_GPIO(R, 1) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEDOWN>;
			debounce-interval = <10>;
		};

		key-volume-up {
			label = "Volume Up";
			gpios = <&gpio TEGRA_GPIO(R, 2) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VOLUMEUP>;
			debounce-interval = <10>;
		};
	};

	sound {
		compatible = "asus,tegra-audio-rt5639-tf701t",
			     "nvidia,tegra-audio-rt5640";
		nvidia,model = "Asus Transformer Pad TF701T RT5639";

		nvidia,audio-routing =
			"Headphones", "HPOR",
			"Headphones", "HPOL",
			"Speakers", "SPORP",
			"Speakers", "SPORN",
			"Speakers", "SPOLP",
			"Speakers", "SPOLN",
			"IN1P", "Mic Jack",
			"IN1N", "Mic Jack",
			"DMIC1", "Int Mic",
			"DMIC2", "Int Mic";

		nvidia,i2s-controller = <&tegra_i2s1>;
		nvidia,audio-codec = <&rt5639>;

		nvidia,hp-det-gpios = <&gpio TEGRA_GPIO(R, 7) GPIO_ACTIVE_LOW>;
		nvidia,int-mic-en-gpios = <&gpio TEGRA_GPIO(K, 3) GPIO_ACTIVE_HIGH>;

		clocks = <&tegra_car TEGRA114_CLK_PLL_A>,
			 <&tegra_car TEGRA114_CLK_PLL_A_OUT0>,
			 <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;
		clock-names = "pll_a", "pll_a_out0", "mclk";

		assigned-clocks = <&tegra_car TEGRA114_CLK_EXTERN1>,
				  <&tegra_pmc TEGRA_PMC_CLK_OUT_1>;

		assigned-clock-parents = <&tegra_car TEGRA114_CLK_PLL_A_OUT0>,
					 <&tegra_car TEGRA114_CLK_EXTERN1>;
	};

	vdd_5v0_sys: regulator-5v0-sys {
		compatible = "regulator-fixed";
		regulator-name = "vdd_5v0_sys";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	vdd_3v3_sys: regulator-3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v3_sys";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	dvdd_1v8_lcd: regulator-vdd-lcd {
		compatible = "regulator-fixed";
		regulator-name = "dvdd_1v8_lcd";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-boot-on;
		gpio = <&palmas_gpio 4 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_1v8_vio>;
	};

	vdd_3v7_bl: regulator-bl-en {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v7_bl";
		regulator-min-microvolt = <3700000>;
		regulator-max-microvolt = <3700000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(H, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_5v0_sys>;
	};

	hdmi_5v0_sys: regulator-hdmi {
		compatible = "regulator-fixed";
		regulator-name = "vdd_5v0_hdmi";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(P, 2) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_smps10_out2>;
	};

	vdd_2v9_usd: regulator-vdd-usd {
		compatible = "regulator-fixed";
		regulator-name = "vdd_sd_slot";
		regulator-min-microvolt = <2900000>;
		regulator-max-microvolt = <2900000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(K, 1) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vcore_emmc>;
	};

	vdd_1v8_cam: regulator-cam-vio {
		compatible = "regulator-fixed";
		regulator-name = "vdd_1v8_cam";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-boot-on;
		gpio = <&palmas_gpio 6 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_1v8_vio>;
	};

	vdd_1v2_xusb: regulator-xusb-vio {
		compatible = "regulator-fixed";
		regulator-name = "avddio_1v2_xusb";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <1200000>;
		regulator-boot-on;
		gpio = <&palmas_gpio 3 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vdd_3v3_xusb: regulator-xusb-vdd {
		compatible = "regulator-fixed";
		regulator-name = "hvdd_3v3_xusb";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		gpio = <&palmas_gpio 1 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vdd_3v3_com: regulator-com {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v3_com";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(U, 1) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_3v3_touch: regulator-touch-pwr {
		compatible = "regulator-fixed";
		regulator-name = "vdd_3v3_touch";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(H, 0) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};

	vdd_1v8_touch: regulator-touch-vio {
		compatible = "regulator-fixed";
		regulator-name = "vdd_1v8_touch";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-boot-on;
		gpio = <&gpio TEGRA_GPIO(H, 4) GPIO_ACTIVE_HIGH>;
		enable-active-high;
		vin-supply = <&vdd_3v3_sys>;
	};
};
