// SPDX-License-Identifier: GPL-2.0-only
/*
 * Copyright (C) 2013 Texas Instruments Incorporated - https://www.ti.com/
 */
#include "omap5.dtsi"
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>

/ {
	aliases {
		display0 = &hdmi0;
	};

	chosen {
		stdout-path = &uart3;
	};

	vmain: fixedregulator-vmain {
		compatible = "regulator-fixed";
		regulator-name = "vmain";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vsys_cobra: fixedregulator-vsys_cobra {
		compatible = "regulator-fixed";
		regulator-name = "vsys_cobra";
		vin-supply = <&vmain>;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vmmcsd_fixed: fixedregulator-mmcsd {
		compatible = "regulator-fixed";
		regulator-name = "vmmcsd_fixed";
		regulator-min-microvolt = <3000000>;
		regulator-max-microvolt = <3000000>;
	};

	mmc3_pwrseq: sdhci0_pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&clk32kgaudio>;
		clock-names = "ext_clock";
	};

	vmmcsdio_fixed: fixedregulator-mmcsdio {
		compatible = "regulator-fixed";
		regulator-name = "vmmcsdio_fixed";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		gpio = <&gpio5 12 GPIO_ACTIVE_HIGH>;	/* gpio140 WLAN_EN */
		enable-active-high;
		startup-delay-us = <70000>;
		pinctrl-names = "default";
		pinctrl-0 = <&wlan_pins>;
	};

	/* HS USB Host PHY on PORT 2 */
	hsusb2_phy: hsusb2-phy-pins {
		compatible = "usb-nop-xceiv";
		reset-gpios = <&gpio3 16 GPIO_ACTIVE_LOW>; /* gpio3_80 HUB_NRESET */
		clocks = <&auxclk1_ck>;
		clock-names = "main_clk";
		clock-frequency = <19200000>;
		#phy-cells = <0>;
	};

	/* HS USB Host PHY on PORT 3 */
	hsusb3_phy: hsusb3_phy {
		compatible = "usb-nop-xceiv";
		reset-gpios = <&gpio3 15 GPIO_ACTIVE_LOW>; /* gpio3_79 ETH_NRESET */
		#phy-cells = <0>;
	};

	tpd12s015: encoder {
		compatible = "ti,tpd12s015";

		pinctrl-names = "default";
		pinctrl-0 = <&tpd12s015_pins>;

		/* gpios defined in the board specific dts */

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				tpd12s015_in: endpoint {
					remote-endpoint = <&hdmi_out>;
				};
			};

			port@1 {
				reg = <1>;

				tpd12s015_out: endpoint {
					remote-endpoint = <&hdmi_connector_in>;
				};
			};
		};
	};

	hdmi0: connector {
		compatible = "hdmi-connector";
		label = "hdmi";

		type = "b";

		port {
			hdmi_connector_in: endpoint {
				remote-endpoint = <&tpd12s015_out>;
			};
		};
	};

	sound: sound {
		compatible = "ti,abe-twl6040";
		ti,model = "omap5-uevm";

		ti,jack-detection;
		ti,mclk-freq = <19200000>;

		ti,mcpdm = <&mcpdm>;

		ti,twl6040 = <&twl6040>;

		/* Audio routing */
		ti,audio-routing =
			"Headset Stereophone", "HSOL",
			"Headset Stereophone", "HSOR",
			"Line Out", "AUXL",
			"Line Out", "AUXR",
			"HSMIC", "Headset Mic",
			"Headset Mic", "Headset Mic Bias",
			"AFML", "Line In",
			"AFMR", "Line In";
	};
};

&gpio8 {
	/* TI trees use GPIO instead of msecure, see also muxing */
	msecure-hog {
		gpio-hog;
		gpios = <10 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "gpio8_234/msecure";
	};
};

&omap5_pmx_core {
	pinctrl-names = "default";
	pinctrl-0 = <
			&usbhost_pins
			&led_gpio_pins
	>;

	twl6040_pins: twl6040-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1be, PIN_OUTPUT | MUX_MODE6)	/* mcspi1_somi.gpio5_141 */
		>;
	};

	mcpdm_pins: mcpdm-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x182, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* abe_clks.abe_clks */
			OMAP5_IOPAD(0x19c, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* abemcpdm_ul_data.abemcpdm_ul_data */
			OMAP5_IOPAD(0x19e, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* abemcpdm_dl_data.abemcpdm_dl_data */
			OMAP5_IOPAD(0x1a0, PIN_INPUT_PULLUP | MUX_MODE0)	/* abemcpdm_frame.abemcpdm_frame */
			OMAP5_IOPAD(0x1a2, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* abemcpdm_lb_clk.abemcpdm_lb_clk */
		>;
	};

	mcbsp1_pins: mcbsp1-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x18c, PIN_INPUT | MUX_MODE1)		/* abedmic_clk2.abemcbsp1_fsx */
			OMAP5_IOPAD(0x18e, PIN_OUTPUT_PULLDOWN | MUX_MODE1)	/* abedmic_clk3.abemcbsp1_dx */
			OMAP5_IOPAD(0x190, PIN_INPUT | MUX_MODE1)		/* abeslimbus1_clock.abemcbsp1_clkx */
			OMAP5_IOPAD(0x192, PIN_INPUT_PULLDOWN | MUX_MODE1)	/* abeslimbus1_data.abemcbsp1_dr */
		>;
	};

	mcbsp2_pins: mcbsp2-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x194, PIN_INPUT_PULLDOWN | MUX_MODE0)	/* abemcbsp2_dr.abemcbsp2_dr */
			OMAP5_IOPAD(0x196, PIN_OUTPUT_PULLDOWN | MUX_MODE0)	/* abemcbsp2_dx.abemcbsp2_dx */
			OMAP5_IOPAD(0x198, PIN_INPUT | MUX_MODE0)		/* abemcbsp2_fsx.abemcbsp2_fsx */
			OMAP5_IOPAD(0x19a, PIN_INPUT | MUX_MODE0)		/* abemcbsp2_clkx.abemcbsp2_clkx */
		>;
	};

	i2c1_pins: i2c1-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1f2, PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c1_scl */
			OMAP5_IOPAD(0x1f4, PIN_INPUT_PULLUP | MUX_MODE0)	/* i2c1_sda */
		>;
	};

	mcspi2_pins: mcspi2-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x0fc, PIN_INPUT | MUX_MODE0)		/*  mcspi2_clk */
			OMAP5_IOPAD(0x0fe, PIN_INPUT | MUX_MODE0)		/*  mcspi2_simo */
			OMAP5_IOPAD(0x100, PIN_INPUT_PULLUP | MUX_MODE0)	/*  mcspi2_somi */
			OMAP5_IOPAD(0x102, PIN_OUTPUT | MUX_MODE0)		/*  mcspi2_cs0 */
		>;
	};

	mcspi3_pins: mcspi3-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x0b8, PIN_INPUT | MUX_MODE1)		/*  mcspi3_somi */
			OMAP5_IOPAD(0x0ba, PIN_INPUT | MUX_MODE1)		/*  mcspi3_cs0 */
			OMAP5_IOPAD(0x0bc, PIN_INPUT | MUX_MODE1)		/*  mcspi3_simo */
			OMAP5_IOPAD(0x0be, PIN_INPUT | MUX_MODE1)		/*  mcspi3_clk */
		>;
	};

	mmc3_pins: mmc3-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x01a4, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_clk */
			OMAP5_IOPAD(0x01a6, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_cmd */
			OMAP5_IOPAD(0x01a8, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_data0 */
			OMAP5_IOPAD(0x01aa, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_data1 */
			OMAP5_IOPAD(0x01ac, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_data2 */
			OMAP5_IOPAD(0x01ae, PIN_INPUT_PULLUP | MUX_MODE0) /* wlsdio_data3 */
		>;
	};

	wlan_pins: wlan-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1bc, PIN_OUTPUT | MUX_MODE6) /* mcspi1_clk.gpio5_140 */
		>;
	};

	/* TI trees use GPIO mode; msecure mode does not work reliably? */
	palmas_msecure_pins: palmas-msecure-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x180, PIN_OUTPUT | MUX_MODE6) /* gpio8_234 */
		>;
	};

	usbhost_pins: usbhost-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x0c4, PIN_INPUT | MUX_MODE0) /* usbb2_hsic_strobe */
			OMAP5_IOPAD(0x0c6, PIN_INPUT | MUX_MODE0) /* usbb2_hsic_data */

			OMAP5_IOPAD(0x1de, PIN_INPUT | MUX_MODE0) /* usbb3_hsic_strobe */
			OMAP5_IOPAD(0x1e0, PIN_INPUT | MUX_MODE0) /* usbb3_hsic_data */

			OMAP5_IOPAD(0x0b0, PIN_OUTPUT | MUX_MODE6) /* gpio3_80 HUB_NRESET */
			OMAP5_IOPAD(0x0ae, PIN_OUTPUT | MUX_MODE6) /* gpio3_79 ETH_NRESET */
		>;
	};

	led_gpio_pins: led-gpio-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1d6, PIN_OUTPUT | MUX_MODE6) /* uart3_cts_rctx.gpio5_153 */
		>;
	};

	uart1_pins: uart1-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x0a0, PIN_OUTPUT | MUX_MODE0) /* uart1_tx.uart1_cts */
			OMAP5_IOPAD(0x0a2, PIN_INPUT_PULLUP | MUX_MODE0) /* uart1_tx.uart1_cts */
			OMAP5_IOPAD(0x0a4, PIN_INPUT_PULLUP | MUX_MODE0) /* uart1_rx.uart1_rts */
			OMAP5_IOPAD(0x0a6, PIN_OUTPUT | MUX_MODE0) /* uart1_rx.uart1_rts */
		>;
	};

	uart3_pins: uart3-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1da, PIN_OUTPUT | MUX_MODE0) /* uart3_rts_irsd.uart3_tx_irtx */
			OMAP5_IOPAD(0x1dc, PIN_INPUT_PULLUP | MUX_MODE0) /* uart3_rx_irrx.uart3_usbb3_hsic */
		>;
	};

	uart5_pins: uart5-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x1b0, PIN_INPUT_PULLUP | MUX_MODE0) /* uart5_rx.uart5_rx */
			OMAP5_IOPAD(0x1b2, PIN_OUTPUT | MUX_MODE0) /* uart5_tx.uart5_tx */
			OMAP5_IOPAD(0x1b4, PIN_INPUT_PULLUP | MUX_MODE0) /* uart5_cts.uart5_rts */
			OMAP5_IOPAD(0x1b6, PIN_OUTPUT | MUX_MODE0) /* uart5_cts.uart5_rts */
		>;
	};

	dss_hdmi_pins: dss-hdmi-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x13c, PIN_INPUT | MUX_MODE0)	/* hdmi_cec.hdmi_cec */
			OMAP5_IOPAD(0x140, PIN_INPUT | MUX_MODE0)	/* hdmi_ddc_scl.hdmi_ddc_scl */
			OMAP5_IOPAD(0x142, PIN_INPUT | MUX_MODE0)	/* hdmi_ddc_sda.hdmi_ddc_sda */
		>;
	};

	tpd12s015_pins: tpd12s015-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x13e, PIN_INPUT_PULLDOWN | MUX_MODE6)	/* hdmi_hpd.gpio7_193 */
		>;
	};
};

&omap5_pmx_wkup {
	pinctrl-names = "default";
	pinctrl-0 = <
			&usbhost_wkup_pins
	>;

	palmas_sys_nirq_pins: palmas-sys-nirq-pins {
		pinctrl-single,pins = <
			/* sys_nirq1 is pulled down as the SoC is inverting it for GIC */
			OMAP5_IOPAD(0x068, PIN_INPUT_PULLUP | MUX_MODE0)
		>;
	};

	usbhost_wkup_pins: usbhost-wkup-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x05a, PIN_OUTPUT | MUX_MODE0) /* fref_clk1_out, USB hub clk */
		>;
	};

	wlcore_irq_pin: wlcore-irq-pin-pins {
		pinctrl-single,pins = <
			OMAP5_IOPAD(0x40, PIN_INPUT | MUX_MODE6)	/* llia_wakereqin.gpio1_wk14 */
		>;
	};
};

&mmc1 {
	vmmc-supply = <&ldo9_reg>;
	bus-width = <4>;
};

&mmc2 {
	vmmc-supply = <&vmmcsd_fixed>;
	bus-width = <8>;
	ti,non-removable;
};

&mmc3 {
	vmmc-supply = <&vmmcsdio_fixed>;
	mmc-pwrseq = <&mmc3_pwrseq>;
	bus-width = <4>;
	non-removable;
	cap-power-off-card;
	pinctrl-names = "default";
	pinctrl-0 = <&mmc3_pins>;
	interrupts-extended = <&wakeupgen GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH
			       &omap5_pmx_core 0x16a>;

	#address-cells = <1>;
	#size-cells = <0>;
	wlcore: wlcore@2 {
		compatible = "ti,wl1271";
		reg = <2>;
		pinctrl-names = "default";
		pinctrl-0 = <&wlcore_irq_pin>;
		interrupt-parent = <&gpio1>;
		interrupts = <14 IRQ_TYPE_LEVEL_HIGH>;	/* gpio 14 */
		ref-clock-frequency = <26000000>;
	};
};

&mmc4 {
	status = "disabled";
};

&mmc5 {
	status = "disabled";
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1_pins>;

	clock-frequency = <400000>;

	palmas: palmas@48 {
		compatible = "ti,palmas";
		/* sys_nirq/ext_sys_irq pins get inverted at mpuss wakeupgen */
		interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_LOW>;
		reg = <0x48>;
		interrupt-controller;
		#interrupt-cells = <2>;
		ti,system-power-controller;
		ti,mux-pad1 = <0xa1>;
		ti,mux-pad2 = <0x1b>;
		pinctrl-names = "default";
		pinctrl-0 = <&palmas_sys_nirq_pins &palmas_msecure_pins>;

		palmas_gpio: gpio {
			compatible = "ti,palmas-gpio";
			gpio-controller;
			#gpio-cells = <2>;
		};

		extcon_usb3: palmas_usb {
			compatible = "ti,palmas-usb-vid";
			ti,enable-vbus-detection;
			ti,enable-id-detection;
			ti,wakeup;
			id-gpios = <&palmas_gpio 0 GPIO_ACTIVE_HIGH>;
		};

		clk32kgaudio: palmas_clk32k@1 {
			compatible = "ti,palmas-clk32kgaudio";
			#clock-cells = <0>;
		};

		rtc {
			compatible = "ti,palmas-rtc";
			interrupt-parent = <&palmas>;
			interrupts = <8 IRQ_TYPE_NONE>;
			ti,backup-battery-chargeable;
			ti,backup-battery-charge-high-current;
		};

		gpadc: gpadc {
			compatible = "ti,palmas-gpadc";
			interrupts = <18 0>,
				     <16 0>,
				     <17 0>;
			#io-channel-cells = <1>;
			ti,channel0-current-microamp = <5>;
			ti,channel3-current-microamp = <10>;
		};

		palmas_pmic {
			compatible = "ti,palmas-pmic";
			interrupt-parent = <&palmas>;
			interrupts = <14 IRQ_TYPE_NONE>;
			interrupt-names = "short-irq";

			ti,ldo6-vibrator;

			smps123-in-supply = <&vsys_cobra>;
			smps45-in-supply = <&vsys_cobra>;
			smps6-in-supply = <&vsys_cobra>;
			smps7-in-supply = <&vsys_cobra>;
			smps8-in-supply = <&vsys_cobra>;
			smps9-in-supply = <&vsys_cobra>;
			smps10_out2-in-supply = <&vsys_cobra>;
			smps10_out1-in-supply = <&vsys_cobra>;
			ldo1-in-supply = <&vsys_cobra>;
			ldo2-in-supply = <&vsys_cobra>;
			ldo3-in-supply = <&vdds_1v8_main>;
			ldo4-in-supply = <&vdds_1v8_main>;
			ldo5-in-supply = <&vsys_cobra>;
			ldo6-in-supply = <&vdds_1v8_main>;
			ldo7-in-supply = <&vsys_cobra>;
			ldo8-in-supply = <&vsys_cobra>;
			ldo9-in-supply = <&vmmcsd_fixed>;
			ldoln-in-supply = <&vsys_cobra>;
			ldousb-in-supply = <&vsys_cobra>;

			regulators {
				smps123_reg: smps123 {
					/* VDD_OPP_MPU */
					regulator-name = "smps123";
					regulator-min-microvolt = < 600000>;
					regulator-max-microvolt = <1500000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps45_reg: smps45 {
					/* VDD_OPP_MM */
					regulator-name = "smps45";
					regulator-min-microvolt = < 600000>;
					regulator-max-microvolt = <1310000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps6_reg: smps6 {
					/* VDD_DDR3 - over VDD_SMPS6 */
					regulator-name = "smps6";
					regulator-min-microvolt = <1350000>;
					regulator-max-microvolt = <1350000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vdds_1v8_main:
				smps7_reg: smps7 {
					/* VDDS_1v8_OMAP over VDDS_1v8_MAIN */
					regulator-name = "smps7";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps8_reg: smps8 {
					/* VDD_OPP_CORE */
					regulator-name = "smps8";
					regulator-min-microvolt = < 600000>;
					regulator-max-microvolt = <1310000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps9_reg: smps9 {
					/* VDDA_2v1_AUD over VDD_2v1 */
					regulator-name = "smps9";
					regulator-min-microvolt = <2100000>;
					regulator-max-microvolt = <2100000>;
					ti,smps-range = <0x80>;
				};

				smps10_out2_reg: smps10_out2 {
					/* VBUS_5V_OTG */
					regulator-name = "smps10_out2";
					regulator-min-microvolt = <5000000>;
					regulator-max-microvolt = <5000000>;
					regulator-always-on;
					regulator-boot-on;
				};

				smps10_out1_reg: smps10_out1 {
					/* VBUS_5V_OTG */
					regulator-name = "smps10_out1";
					regulator-min-microvolt = <5000000>;
					regulator-max-microvolt = <5000000>;
				};

				ldo1_reg: ldo1 {
					/* VDDAPHY_CAM: vdda_csiport */
					regulator-name = "ldo1";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo2_reg: ldo2 {
					/* VCC_2V8_DISP: Does not go anywhere */
					regulator-name = "ldo2";
					regulator-min-microvolt = <2800000>;
					regulator-max-microvolt = <2800000>;
					/* Unused */
					status = "disabled";
				};

				ldo3_reg: ldo3 {
					/* VDDAPHY_MDM: vdda_lli */
					regulator-name = "ldo3";
					regulator-min-microvolt = <1500000>;
					regulator-max-microvolt = <1500000>;
					regulator-boot-on;
					/* Only if Modem is used */
					status = "disabled";
				};

				ldo4_reg: ldo4 {
					/* VDDAPHY_DISP: vdda_dsiport/hdmi */
					regulator-name = "ldo4";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo5_reg: ldo5 {
					/* VDDA_1V8_PHY: usb/sata/hdmi.. */
					regulator-name = "ldo5";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldo6_reg: ldo6 {
					/* VDDS_1V2_WKUP: hsic/ldo_emu_wkup */
					regulator-name = "ldo6";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldo7_reg: ldo7 {
					/* VDD_VPP: vpp1 */
					regulator-name = "ldo7";
					regulator-min-microvolt = <2000000>;
					regulator-max-microvolt = <2000000>;
					/* Only for efuse reprograming! */
					status = "disabled";
				};

				ldo8_reg: ldo8 {
					/* VDD_3v0: Does not go anywhere */
					regulator-name = "ldo8";
					regulator-min-microvolt = <3000000>;
					regulator-max-microvolt = <3000000>;
					regulator-boot-on;
					/* Unused */
					status = "disabled";
				};

				ldo9_reg: ldo9 {
					/* VCC_DV_SDIO: vdds_sdcard */
					regulator-name = "ldo9";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <3000000>;
					regulator-boot-on;
				};

				ldoln_reg: ldoln {
					/* VDDA_1v8_REF: vdds_osc/mm_l4per.. */
					regulator-name = "ldoln";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				ldousb_reg: ldousb {
					/* VDDA_3V_USB: VDDA_USBHS33 */
					regulator-name = "ldousb";
					regulator-min-microvolt = <3250000>;
					regulator-max-microvolt = <3250000>;
					regulator-always-on;
					regulator-boot-on;
				};

				regen3_reg: regen3 {
					/* REGEN3 controls LDO9 supply to card */
					regulator-name = "regen3";
					regulator-always-on;
					regulator-boot-on;
				};
			};
		};

		palmas_power_button: palmas_power_button {
			compatible = "ti,palmas-pwrbutton";
			interrupt-parent = <&palmas>;
			interrupts = <1 IRQ_TYPE_EDGE_FALLING>;
			wakeup-source;
		};
	};

	twl6040: twl@4b {
		compatible = "ti,twl6040";
		#clock-cells = <0>;
		reg = <0x4b>;

		pinctrl-names = "default";
		pinctrl-0 = <&twl6040_pins>;

		/* sys_nirq/ext_sys_irq pins get inverted at mpuss wakeupgen */
		interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_LOW>;

		/* audpwron gpio defined in the board specific dts */

		vio-supply = <&smps7_reg>;
		v2v1-supply = <&smps9_reg>;
		enable-active-high;

		clocks = <&clk32kgaudio>, <&fref_xtal_ck>;
		clock-names = "clk32k", "mclk";
	};
};

&mcpdm_module {
	/* Module on the SoC needs external clock from the PMIC */
	pinctrl-names = "default";
	pinctrl-0 = <&mcpdm_pins>;
	status = "okay";
};

&mcpdm {
	clocks = <&twl6040>;
	clock-names = "pdmclk";
};

&mcbsp1 {
	pinctrl-names = "default";
	pinctrl-0 = <&mcbsp1_pins>;
	status = "okay";
};

&mcbsp2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mcbsp2_pins>;
	status = "okay";
};

&usbhshost {
	port2-mode = "ehci-hsic";
	port3-mode = "ehci-hsic";
};

&usbhsehci {
	phys = <0 &hsusb2_phy &hsusb3_phy>;
};

&usb3 {
	extcon = <&extcon_usb3>;
	vbus-supply = <&smps10_out1_reg>;
};

&dwc3 {
	extcon = <&extcon_usb3>;
	dr_mode = "otg";
};

&mcspi1 {

};

&mcspi2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mcspi2_pins>;
};

&mcspi3 {
	pinctrl-names = "default";
	pinctrl-0 = <&mcspi3_pins>;
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;
};

&uart3 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart3_pins>;
	interrupts-extended = <&wakeupgen GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>,
			      <&omap5_pmx_core 0x19c>;
};

&uart5 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart5_pins>;
};

&cpu0 {
	cpu0-supply = <&smps123_reg>;
};

&dss {
	status = "okay";
};

&hdmi {
	status = "okay";

	/* vdda-supply populated in board specific dts file */

	pinctrl-names = "default";
	pinctrl-0 = <&dss_hdmi_pins>;

	port {
		hdmi_out: endpoint {
			remote-endpoint = <&tpd12s015_in>;
		};
	};
};
