// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/mfd/qcom-rpm.h>
#include <dt-bindings/clock/qcom,rpmcc.h>
#include <dt-bindings/clock/qcom,gcc-ipq806x.h>
#include <dt-bindings/clock/qcom,lcc-ipq806x.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/reset/qcom,gcc-ipq806x.h>
#include <dt-bindings/soc/qcom,gsbi.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	model = "Qualcomm IPQ8064";
	compatible = "qcom,ipq8064";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc0>;
			qcom,saw = <&saw0>;
		};

		cpu1: cpu@1 {
			compatible = "qcom,krait";
			enable-method = "qcom,kpss-acc-v1";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
			qcom,acc = <&acc1>;
			qcom,saw = <&saw1>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			cache-unified;
		};
	};

	thermal-zones {
		sensor0-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 0>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor1-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 1>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor2-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 2>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor3-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 3>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor4-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 4>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor5-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 5>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor6-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 6>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor7-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 7>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor8-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 8>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor9-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 9>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};

		sensor10-thermal {
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&tsens 10>;

			trips {
				cpu-critical {
					temperature = <105000>;
					hysteresis = <2000>;
					type = "critical";
				};

				cpu-hot {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "hot";
				};
			};
		};
	};

	memory {
		device_type = "memory";
		reg = <0x0 0x0>;
	};

	cpu-pmu {
		compatible = "qcom,krait-pmu";
		interrupts = <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) |
					  IRQ_TYPE_LEVEL_HIGH)>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		nss@40000000 {
			reg = <0x40000000 0x1000000>;
			no-map;
		};

		smem: smem@41000000 {
			compatible = "qcom,smem";
			reg = <0x41000000 0x200000>;
			no-map;

			hwlocks = <&sfpb_mutex 3>;
		};
	};

	clocks {
		cxo_board: cxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};

		pxo_board: pxo_board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};

		sleep_clk: sleep_clk {
			compatible = "fixed-clock";
			clock-frequency = <32768>;
			#clock-cells = <0>;
		};
	};

	firmware {
		scm {
			compatible = "qcom,scm-ipq806x", "qcom,scm";
		};
	};

	stmmac_axi_setup: stmmac-axi-config {
		snps,wr_osr_lmt = <7>;
		snps,rd_osr_lmt = <7>;
		snps,blen = <16 0 0 0 0 0 0>;
	};

	vsdcc_fixed: vsdcc-regulator {
		compatible = "regulator-fixed";
		regulator-name = "SDCC Power";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		rpm: rpm@108000 {
			compatible = "qcom,rpm-ipq8064";
			reg = <0x00108000 0x1000>;
			qcom,ipc = <&l2cc 0x8 2>;

			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>,
					<GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "ack", "err", "wakeup";

			clocks = <&gcc RPM_MSG_RAM_H_CLK>;
			clock-names = "ram";

			rpmcc: clock-controller {
				compatible = "qcom,rpmcc-ipq806x", "qcom,rpmcc";
				#clock-cells = <1>;
			};
		};

		ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x00500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		qfprom: efuse@700000 {
			compatible = "qcom,ipq8064-qfprom", "qcom,qfprom";
			reg = <0x00700000 0x1000>;
			#address-cells = <1>;
			#size-cells = <1>;
			speedbin_efuse: speedbin@c0 {
				reg = <0xc0 0x4>;
			};
			tsens_calib: calib@400 {
				reg = <0x400 0xb>;
			};
			tsens_calib_backup: calib_backup@410 {
				reg = <0x410 0xb>;
			};
		};

		qcom_pinmux: pinmux@800000 {
			compatible = "qcom,ipq8064-pinctrl";
			reg = <0x00800000 0x4000>;

			gpio-controller;
			gpio-ranges = <&qcom_pinmux 0 0 69>;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;

			pcie0_pins: pcie0-state {
				pins = "gpio3";
				function = "pcie1_rst";
				drive-strength = <12>;
				bias-disable;
			};

			pcie1_pins: pcie1-state {
				pins = "gpio48";
				function = "pcie2_rst";
				drive-strength = <12>;
				bias-disable;
			};

			pcie2_pins: pcie2-state {
				pins = "gpio63";
				function = "pcie3_rst";
				drive-strength = <12>;
				bias-disable;
			};

			i2c4_pins: i2c4-state {
				pins = "gpio12", "gpio13";
				function = "gsbi4";
				drive-strength = <12>;
				bias-disable;
			};

			spi_pins: spi-state {
				pins = "gpio18", "gpio19", "gpio21";
				function = "gsbi5";
				drive-strength = <10>;
				bias-disable;
			};

			leds_pins: leds-state {
				pins = "gpio7", "gpio8", "gpio9",
					"gpio26", "gpio53";
				function = "gpio";
				drive-strength = <2>;
				bias-pull-down;
				output-low;
			};

			buttons_pins: buttons-state {
				pins = "gpio54";
				drive-strength = <2>;
				bias-pull-up;
			};

			nand_pins: nand-state {
				nand-pins {
					pins = "gpio34", "gpio35", "gpio36",
					       "gpio37", "gpio38", "gpio39",
					       "gpio40", "gpio41", "gpio42",
					       "gpio43", "gpio44", "gpio45",
					       "gpio46", "gpio47";
					function = "nand";
					drive-strength = <10>;
					bias-disable;
				};

				nand-pullup-pins {
					pins = "gpio39";
					function = "nand";
					drive-strength = <10>;
					bias-pull-up;
				};

				nand-hold-pins {
					pins = "gpio40", "gpio41", "gpio42",
					       "gpio43", "gpio44", "gpio45",
					       "gpio46", "gpio47";
					function = "nand";
					drive-strength = <10>;
					bias-bus-hold;
				};
			};

			mdio0_pins: mdio0-state {
				pins = "gpio0", "gpio1";
				function = "mdio";
				drive-strength = <8>;
				bias-disable;
			};

			rgmii2_pins: rgmii2-state {
				pins = "gpio27", "gpio28", "gpio29",
					"gpio30", "gpio31", "gpio32",
					"gpio51", "gpio52", "gpio59",
					"gpio60", "gpio61", "gpio62";
				function = "rgmii2";
				drive-strength = <8>;
				bias-disable;
			};
		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-ipq8064", "syscon";
			clocks = <&pxo_board>, <&cxo_board>, <&lcc PLL4>;
			clock-names = "pxo", "cxo", "pll4";
			reg = <0x00900000 0x4000>;
			#clock-cells = <1>;
			#reset-cells = <1>;

			tsens: thermal-sensor {
				compatible = "qcom,ipq8064-tsens";

				nvmem-cells = <&tsens_calib>, <&tsens_calib_backup>;
				nvmem-cell-names = "calib", "calib_backup";
				interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-names = "uplow";

				#qcom,sensors = <11>;
				#thermal-sensor-cells = <1>;
			};
		};

		sfpb_mutex: hwlock@1200600 {
			compatible = "qcom,sfpb-mutex";
			reg = <0x01200600 0x100>;

			#hwlock-cells = <1>;
		};

		intc: interrupt-controller@2000000 {
			compatible = "qcom,msm-qgic2";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = <0x02000000 0x1000>,
			      <0x02002000 0x1000>;
		};

		timer@200a000 {
			compatible = "qcom,kpss-wdt-ipq8064", "qcom,kpss-timer",
				     "qcom,msm-timer";
			interrupts = <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(2) |
						 IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(2) |
						 IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 3 (GIC_CPU_MASK_SIMPLE(2) |
						 IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 4 (GIC_CPU_MASK_SIMPLE(2) |
						 IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 5 (GIC_CPU_MASK_SIMPLE(2) |
						 IRQ_TYPE_EDGE_RISING)>;
			reg = <0x0200a000 0x100>;
			clock-frequency = <25000000>;
			clocks = <&sleep_clk>;
			clock-names = "sleep";
			cpu-offset = <0x80000>;
		};

		l2cc: clock-controller@2011000 {
			compatible = "qcom,kpss-gcc-ipq8064", "qcom,kpss-gcc", "syscon";
			reg = <0x02011000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			#clock-cells = <0>;
		};

		acc0: clock-controller@2088000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02088000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu0_aux";
			#clock-cells = <0>;
		};

		saw0: power-manager@2089000 {
			compatible = "qcom,ipq8064-saw2-cpu", "qcom,saw2";
			reg = <0x02089000 0x1000>, <0x02009000 0x1000>;
		};

		acc1: clock-controller@2098000 {
			compatible = "qcom,kpss-acc-v1";
			reg = <0x02098000 0x1000>, <0x02008000 0x1000>;
			clocks = <&gcc PLL8_VOTE>, <&pxo_board>;
			clock-names = "pll8_vote", "pxo";
			clock-output-names = "acpu1_aux";
			#clock-cells = <0>;
		};

		saw1: power-manager@2099000 {
			compatible = "qcom,ipq8064-saw2-cpu", "qcom,saw2";
			reg = <0x02099000 0x1000>, <0x02009000 0x1000>;
		};

		nss_common: syscon@3000000 {
			compatible = "syscon";
			reg = <0x03000000 0x0000FFFF>;
		};

		usb3_0: usb@100f8800 {
			compatible = "qcom,ipq8064-dwc3", "qcom,dwc3";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x100f8800 0x8000>;
			clocks = <&gcc USB30_0_MASTER_CLK>;
			clock-names = "core";

			ranges;

			resets = <&gcc USB30_0_MASTER_RESET>;

			status = "disabled";

			dwc3_0: usb@10000000 {
				compatible = "snps,dwc3";
				reg = <0x10000000 0xcd00>;
				interrupts = <GIC_SPI 205 IRQ_TYPE_LEVEL_HIGH>;
				phys = <&hs_phy_0>, <&ss_phy_0>;
				phy-names = "usb2-phy", "usb3-phy";
				dr_mode = "host";
				snps,dis_u3_susphy_quirk;
			};
		};

		hs_phy_0: phy@100f8800 {
			compatible = "qcom,ipq806x-usb-phy-hs";
			reg = <0x100f8800 0x30>;
			clocks = <&gcc USB30_0_UTMI_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		ss_phy_0: phy@100f8830 {
			compatible = "qcom,ipq806x-usb-phy-ss";
			reg = <0x100f8830 0x30>;
			clocks = <&gcc USB30_0_MASTER_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		usb3_1: usb@110f8800 {
			compatible = "qcom,ipq8064-dwc3", "qcom,dwc3";
			#address-cells = <1>;
			#size-cells = <1>;
			reg = <0x110f8800 0x8000>;
			clocks = <&gcc USB30_1_MASTER_CLK>;
			clock-names = "core";

			ranges;

			resets = <&gcc USB30_1_MASTER_RESET>;

			status = "disabled";

			dwc3_1: usb@11000000 {
				compatible = "snps,dwc3";
				reg = <0x11000000 0xcd00>;
				interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
				phys = <&hs_phy_1>, <&ss_phy_1>;
				phy-names = "usb2-phy", "usb3-phy";
				dr_mode = "host";
				snps,dis_u3_susphy_quirk;
			};
		};

		hs_phy_1: phy@110f8800 {
			compatible = "qcom,ipq806x-usb-phy-hs";
			reg = <0x110f8800 0x30>;
			clocks = <&gcc USB30_1_UTMI_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		ss_phy_1: phy@110f8830 {
			compatible = "qcom,ipq806x-usb-phy-ss";
			reg = <0x110f8830 0x30>;
			clocks = <&gcc USB30_1_MASTER_CLK>;
			clock-names = "ref";
			#phy-cells = <0>;

			status = "disabled";
		};

		sdcc3bam: dma-controller@12182000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12182000 0x8000>;
			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC3_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		sdcc1bam: dma-controller@12402000 {
			compatible = "qcom,bam-v1.3.0";
			reg = <0x12402000 0x8000>;
			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&gcc SDC1_H_CLK>;
			clock-names = "bam_clk";
			#dma-cells = <1>;
			qcom,ee = <0>;
		};

		amba: amba {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			sdcc3: mmc@12180000 {
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				status = "disabled";
				reg = <0x12180000 0x2000>;
				interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC3_CLK>, <&gcc SDC3_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <8>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				max-frequency = <192000000>;
				sd-uhs-sdr104;
				sd-uhs-ddr50;
				vqmmc-supply = <&vsdcc_fixed>;
				dmas = <&sdcc3bam 2>, <&sdcc3bam 1>;
				dma-names = "tx", "rx";
			};

			sdcc1: mmc@12400000 {
				status = "disabled";
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				reg = <0x12400000 0x2000>;
				interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC1_CLK>, <&gcc SDC1_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <8>;
				max-frequency = <96000000>;
				non-removable;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				vmmc-supply = <&vsdcc_fixed>;
				dmas = <&sdcc1bam 2>, <&sdcc1bam 1>;
				dma-names = "tx", "rx";
			};
		};

		gsbi1: gsbi@12440000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x12440000 0x100>;
			cell-index = <1>;
			clocks = <&gcc GSBI1_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			status = "disabled";

			gsbi1_serial: serial@12450000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x12450000 0x100>,
				      <0x12400000 0x03>;
				interrupts = <GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI1_UART_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";

				status = "disabled";
			};

			gsbi1_i2c: i2c@12460000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x12460000 0x1000>;
				interrupts = <GIC_SPI 194 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI1_QUP_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;

				status = "disabled";
			};
		};

		gsbi2: gsbi@12480000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <2>;
			reg = <0x12480000 0x100>;
			clocks = <&gcc GSBI2_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi2_serial: serial@12490000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x12490000 0x1000>,
				      <0x12480000 0x1000>;
				interrupts = <GIC_SPI 195 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI2_UART_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi2_i2c: i2c@124a0000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x124a0000 0x1000>;
				interrupts = <GIC_SPI 196 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI2_QUP_CLK>, <&gcc GSBI2_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		gsbi4: gsbi@16300000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <4>;
			reg = <0x16300000 0x100>;
			clocks = <&gcc GSBI4_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi4_serial: serial@16340000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16340000 0x1000>,
				      <0x16300000 0x1000>;
				interrupts = <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI4_UART_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@16380000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16380000 0x1000>;
				interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI4_QUP_CLK>, <&gcc GSBI4_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		gsbi6: gsbi@16500000 {
			compatible = "qcom,gsbi-v1.0.0";
			reg = <0x16500000 0x100>;
			cell-index = <6>;
			clocks = <&gcc GSBI6_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			status = "disabled";

			gsbi6_i2c: i2c@16580000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16580000 0x1000>;
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI6_QUP_CLK>, <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";

				#address-cells = <1>;
				#size-cells = <0>;

				status = "disabled";
			};

			gsbi6_spi: spi@16580000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x16580000 0x1000>;
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI6_QUP_CLK>, <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";

				#address-cells = <1>;
				#size-cells = <0>;

				status = "disabled";
			};
		};

		gsbi7: gsbi@16600000 {
			status = "disabled";
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <7>;
			reg = <0x16600000 0x100>;
			clocks = <&gcc GSBI7_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			syscon-tcsr = <&tcsr>;

			gsbi7_serial: serial@16640000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16640000 0x1000>,
				      <0x16600000 0x1000>;
				interrupts = <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI7_UART_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi7_i2c: i2c@16680000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16680000 0x1000>;
				interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI7_QUP_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";

				#address-cells = <1>;
				#size-cells = <0>;

				status = "disabled";
			};
		};

		adm_dma: dma-controller@18300000 {
			compatible = "qcom,adm";
			reg = <0x18300000 0x100000>;
			interrupts = <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH>;
			#dma-cells = <1>;

			clocks = <&gcc ADM0_CLK>, <&gcc ADM0_PBUS_CLK>;
			clock-names = "core", "iface";

			resets = <&gcc ADM0_RESET>,
				 <&gcc ADM0_PBUS_RESET>,
				 <&gcc ADM0_C0_RESET>,
				 <&gcc ADM0_C1_RESET>,
				 <&gcc ADM0_C2_RESET>;
			reset-names = "clk", "pbus", "c0", "c1", "c2";
			qcom,ee = <0>;

			status = "disabled";
		};

		gsbi5: gsbi@1a200000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <5>;
			reg = <0x1a200000 0x100>;
			clocks = <&gcc GSBI5_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;

			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi5_serial: serial@1a240000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x1a240000 0x1000>,
				      <0x1a200000 0x1000>;
				interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI5_UART_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			i2c@1a280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};

			spi@1a280000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x1a280000 0x1000>;
				interrupts = <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>;

				clocks = <&gcc GSBI5_QUP_CLK>, <&gcc GSBI5_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";

				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		tcsr: syscon@1a400000 {
			compatible = "qcom,tcsr-ipq8064", "syscon";
			reg = <0x1a400000 0x100>;
		};

		rng@1a500000 {
			compatible = "qcom,prng";
			reg = <0x1a500000 0x200>;
			clocks = <&gcc PRNG_CLK>;
			clock-names = "core";
		};

		nand: nand-controller@1ac00000 {
			compatible = "qcom,ipq806x-nand";
			reg = <0x1ac00000 0x800>;

			pinctrl-0 = <&nand_pins>;
			pinctrl-names = "default";

			clocks = <&gcc EBI2_CLK>,
				 <&gcc EBI2_AON_CLK>;
			clock-names = "core", "aon";

			dmas = <&adm_dma 3>;
			dma-names = "rxtx";
			qcom,cmd-crci = <15>;
			qcom,data-crci = <3>;

			#address-cells = <1>;
			#size-cells = <0>;

			status = "disabled";
		};

		sata_phy: sata-phy@1b400000 {
			compatible = "qcom,ipq806x-sata-phy";
			reg = <0x1b400000 0x200>;

			clocks = <&gcc SATA_PHY_CFG_CLK>;
			clock-names = "cfg";

			#phy-cells = <0>;
			status = "disabled";
		};

		pcie0: pcie@1b500000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b500000 0x1000
			       0x1b502000 0x80
			       0x1b600000 0x100
			       0x0ff00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <0>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0x0 0x00000000 0x0fe00000 0x0 0x00010000   /* I/O */
				  0x82000000 0x0 0x08000000 0x08000000 0x0 0x07e00000>; /* MEM */

			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 36 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 37 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 38 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 39 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_A_CLK>,
				 <&gcc PCIE_H_CLK>,
				 <&gcc PCIE_PHY_CLK>,
				 <&gcc PCIE_AUX_CLK>,
				 <&gcc PCIE_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_ACLK_RESET>,
				 <&gcc PCIE_HCLK_RESET>,
				 <&gcc PCIE_POR_RESET>,
				 <&gcc PCIE_PCI_RESET>,
				 <&gcc PCIE_PHY_RESET>,
				 <&gcc PCIE_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie0_pins>;
			pinctrl-names = "default";

			status = "disabled";
			perst-gpios = <&qcom_pinmux 3 GPIO_ACTIVE_LOW>;

			pcie@0 {
				device_type = "pci";
				reg = <0x0 0x0 0x0 0x0 0x0>;
				bus-range = <0x01 0xff>;

				#address-cells = <3>;
				#size-cells = <2>;
				ranges;
			};
		};

		pcie1: pcie@1b700000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b700000 0x1000
			       0x1b702000 0x80
			       0x1b800000 0x100
			       0x31f00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <1>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0x0 0x00000000 0x31e00000 0x0 0x00010000   /* I/O */
				  0x82000000 0x0 0x2e000000 0x2e000000 0x0 0x03e00000>; /* MEM */

			interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 58 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 59 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 60 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 61 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_1_A_CLK>,
				 <&gcc PCIE_1_H_CLK>,
				 <&gcc PCIE_1_PHY_CLK>,
				 <&gcc PCIE_1_AUX_CLK>,
				 <&gcc PCIE_1_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_1_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_1_ACLK_RESET>,
				 <&gcc PCIE_1_HCLK_RESET>,
				 <&gcc PCIE_1_POR_RESET>,
				 <&gcc PCIE_1_PCI_RESET>,
				 <&gcc PCIE_1_PHY_RESET>,
				 <&gcc PCIE_1_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie1_pins>;
			pinctrl-names = "default";

			status = "disabled";
			perst-gpios = <&qcom_pinmux 48 GPIO_ACTIVE_LOW>;

			pcie@0 {
				device_type = "pci";
				reg = <0x0 0x0 0x0 0x0 0x0>;
				bus-range = <0x01 0xff>;

				#address-cells = <3>;
				#size-cells = <2>;
				ranges;
			};
		};

		pcie2: pcie@1b900000 {
			compatible = "qcom,pcie-ipq8064";
			reg = <0x1b900000 0x1000
			       0x1b902000 0x80
			       0x1ba00000 0x100
			       0x35f00000 0x100000>;
			reg-names = "dbi", "elbi", "parf", "config";
			device_type = "pci";
			linux,pci-domain = <2>;
			bus-range = <0x00 0xff>;
			num-lanes = <1>;
			#address-cells = <3>;
			#size-cells = <2>;

			ranges = <0x81000000 0x0 0x00000000 0x35e00000 0x0 0x00010000   /* I/O */
				  0x82000000 0x0 0x32000000 0x32000000 0x0 0x03e00000>; /* MEM */

			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "msi";
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 0x7>;
			interrupt-map = <0 0 0 1 &intc 0 72 IRQ_TYPE_LEVEL_HIGH>, /* int_a */
					<0 0 0 2 &intc 0 73 IRQ_TYPE_LEVEL_HIGH>, /* int_b */
					<0 0 0 3 &intc 0 74 IRQ_TYPE_LEVEL_HIGH>, /* int_c */
					<0 0 0 4 &intc 0 75 IRQ_TYPE_LEVEL_HIGH>; /* int_d */

			clocks = <&gcc PCIE_2_A_CLK>,
				 <&gcc PCIE_2_H_CLK>,
				 <&gcc PCIE_2_PHY_CLK>,
				 <&gcc PCIE_2_AUX_CLK>,
				 <&gcc PCIE_2_ALT_REF_CLK>;
			clock-names = "core", "iface", "phy", "aux", "ref";

			assigned-clocks = <&gcc PCIE_2_ALT_REF_CLK>;
			assigned-clock-rates = <100000000>;

			resets = <&gcc PCIE_2_ACLK_RESET>,
				 <&gcc PCIE_2_HCLK_RESET>,
				 <&gcc PCIE_2_POR_RESET>,
				 <&gcc PCIE_2_PCI_RESET>,
				 <&gcc PCIE_2_PHY_RESET>,
				 <&gcc PCIE_2_EXT_RESET>;
			reset-names = "axi", "ahb", "por", "pci", "phy", "ext";

			pinctrl-0 = <&pcie2_pins>;
			pinctrl-names = "default";

			status = "disabled";
			perst-gpios = <&qcom_pinmux 63 GPIO_ACTIVE_LOW>;

			pcie@0 {
				device_type = "pci";
				reg = <0x0 0x0 0x0 0x0 0x0>;
				bus-range = <0x01 0xff>;

				#address-cells = <3>;
				#size-cells = <2>;
				ranges;
			};
		};

		qsgmii_csr: syscon@1bb00000 {
			compatible = "syscon";
			reg = <0x1bb00000 0x000001FF>;
		};

		lcc: clock-controller@28000000 {
			compatible = "qcom,lcc-ipq8064";
			reg = <0x28000000 0x1000>;
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		lpass@28100000 {
			compatible = "qcom,lpass-cpu";
			status = "disabled";
			clocks = <&lcc AHBIX_CLK>,
					<&lcc MI2S_OSR_CLK>,
					<&lcc MI2S_BIT_CLK>;
			clock-names = "ahbix-clk",
					"mi2s-osr-clk",
					"mi2s-bit-clk";
			interrupts = <GIC_SPI 85 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "lpass-irq-lpaif";
			reg = <0x28100000 0x10000>;
			reg-names = "lpass-lpaif";
		};

		sata: sata@29000000 {
			compatible = "qcom,ipq806x-ahci", "generic-ahci";
			reg = <0x29000000 0x180>;

			interrupts = <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>;

			clocks = <&gcc SFAB_SATA_S_H_CLK>,
				 <&gcc SATA_H_CLK>,
				 <&gcc SATA_A_CLK>,
				 <&gcc SATA_RXOOB_CLK>,
				 <&gcc SATA_PMALIVE_CLK>;
			clock-names = "slave_iface", "iface", "core",
					"rxoob", "pmalive";

			assigned-clocks = <&gcc SATA_RXOOB_CLK>, <&gcc SATA_PMALIVE_CLK>;
			assigned-clock-rates = <100000000>, <100000000>;

			phys = <&sata_phy>;
			phy-names = "sata-phy";
			status = "disabled";
		};

		gmac0: ethernet@37000000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac", "snps,dwmac";
			reg = <0x37000000 0x200000>;
			interrupts = <GIC_SPI 220 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE1_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE1_RESET>,
				 <&gcc GMAC_AHB_RESET>;
			reset-names = "stmmaceth", "ahb";

			status = "disabled";
		};

		gmac1: ethernet@37200000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac", "snps,dwmac";
			reg = <0x37200000 0x200000>;
			interrupts = <GIC_SPI 223 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE2_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE2_RESET>,
				 <&gcc GMAC_AHB_RESET>;
			reset-names = "stmmaceth", "ahb";

			status = "disabled";
		};

		gmac2: ethernet@37400000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac", "snps,dwmac";
			reg = <0x37400000 0x200000>;
			interrupts = <GIC_SPI 226 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE3_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE3_RESET>,
				 <&gcc GMAC_AHB_RESET>;
			reset-names = "stmmaceth", "ahb";

			status = "disabled";
		};

		gmac3: ethernet@37600000 {
			device_type = "network";
			compatible = "qcom,ipq806x-gmac", "snps,dwmac";
			reg = <0x37600000 0x200000>;
			interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";

			snps,axi-config = <&stmmac_axi_setup>;
			snps,pbl = <32>;
			snps,aal;

			qcom,nss-common = <&nss_common>;
			qcom,qsgmii-csr = <&qsgmii_csr>;

			clocks = <&gcc GMAC_CORE4_CLK>;
			clock-names = "stmmaceth";

			resets = <&gcc GMAC_CORE4_RESET>,
				 <&gcc GMAC_AHB_RESET>;
			reset-names = "stmmaceth", "ahb";

			status = "disabled";
		};
	};
};
