// SPDX-License-Identifier: GPL-2.0
/*
 * Device Tree Source for the R-Mobile A1 (R8A77400) SoC
 *
 * Copyright (C) 2012 Renesas Solutions Corp.
 */

#include <dt-bindings/clock/r8a7740-clock.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	compatible = "renesas,r8a7740";
	interrupt-parent = <&gic>;
	#address-cells = <1>;
	#size-cells = <1>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		cpu@0 {
			compatible = "arm,cortex-a9";
			device_type = "cpu";
			reg = <0x0>;
			clock-frequency = <800000000>;
			power-domains = <&pd_a3sm>;
			next-level-cache = <&L2>;
		};
	};

	gic: interrupt-controller@c2800000 {
		compatible = "arm,pl390";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0xc2800000 0x1000>,
		      <0xc2000000 0x1000>;
	};

	L2: cache-controller@f0100000 {
		compatible = "arm,pl310-cache";
		reg = <0xf0100000 0x1000>;
		interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
		power-domains = <&pd_a3sm>;
		arm,data-latency = <3 3 3>;
		arm,tag-latency = <2 2 2>;
		arm,shared-override;
		cache-unified;
		cache-level = <2>;
	};

	dbsc3: memory-controller@fe400000 {
		compatible = "renesas,dbsc3-r8a7740";
		reg = <0xfe400000 0x400>;
		power-domains = <&pd_a4s>;
	};

	pmu {
		compatible = "arm,cortex-a9-pmu";
		interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
	};

	ptm {
		compatible = "arm,coresight-etm3x";
		power-domains = <&pd_d4>;
	};

	ceu0: ceu@fe910000 {
		reg = <0xfe910000 0x3000>;
		compatible = "renesas,r8a7740-ceu";
		interrupts = <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7740_CLK_CEU20>;
		power-domains = <&pd_a4r>;
		status = "disabled";
	};

	ceu1: ceu@fe914000 {
		reg = <0xfe914000 0x3000>;
		compatible = "renesas,r8a7740-ceu";
		interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7740_CLK_CEU21>;
		power-domains = <&pd_a4r>;
		status = "disabled";
	};

	cmt1: timer@e6138000 {
		compatible = "renesas,r8a7740-cmt1";
		reg = <0xe6138000 0x170>;
		interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_CMT1>;
		clock-names = "fck";
		power-domains = <&pd_c5>;
		status = "disabled";
	};

	/* irqpin0: IRQ0 - IRQ7 */
	irqpin0: interrupt-controller@e6900000 {
		compatible = "renesas,intc-irqpin-r8a7740", "renesas,intc-irqpin";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0xe6900000 4>,
			<0xe6900010 4>,
			<0xe6900020 1>,
			<0xe6900040 1>,
			<0xe6900060 1>;
		interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_INTCA>;
		power-domains = <&pd_a4s>;
	};

	/* irqpin1: IRQ8 - IRQ15 */
	irqpin1: interrupt-controller@e6900004 {
		compatible = "renesas,intc-irqpin-r8a7740", "renesas,intc-irqpin";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0xe6900004 4>,
			<0xe6900014 4>,
			<0xe6900024 1>,
			<0xe6900044 1>,
			<0xe6900064 1>;
		interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_INTCA>;
		power-domains = <&pd_a4s>;
	};

	/* irqpin2: IRQ16 - IRQ23 */
	irqpin2: interrupt-controller@e6900008 {
		compatible = "renesas,intc-irqpin-r8a7740", "renesas,intc-irqpin";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0xe6900008 4>,
			<0xe6900018 4>,
			<0xe6900028 1>,
			<0xe6900048 1>,
			<0xe6900068 1>;
		interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_INTCA>;
		power-domains = <&pd_a4s>;
	};

	/* irqpin3: IRQ24 - IRQ31 */
	irqpin3: interrupt-controller@e690000c {
		compatible = "renesas,intc-irqpin-r8a7740", "renesas,intc-irqpin";
		#interrupt-cells = <2>;
		interrupt-controller;
		reg = <0xe690000c 4>,
			<0xe690001c 4>,
			<0xe690002c 1>,
			<0xe690004c 1>,
			<0xe690006c 1>;
		interrupts = <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_INTCA>;
		power-domains = <&pd_a4s>;
	};

	ether: ethernet@e9a00000 {
		compatible = "renesas,gether-r8a7740";
		reg = <0xe9a00000 0x800>,
		      <0xe9a01800 0x800>;
		interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_GETHER>;
		power-domains = <&pd_a4s>;
		phy-mode = "mii";
		#address-cells = <1>;
		#size-cells = <0>;
		status = "disabled";
	};

	i2c0: i2c@fff20000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7740", "renesas,rmobile-iic";
		reg = <0xfff20000 0x425>;
		interrupts = <GIC_SPI 201 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 202 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 203 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 204 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7740_CLK_IIC0>;
		power-domains = <&pd_a4r>;
		status = "disabled";
	};

	i2c1: i2c@e6c20000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "renesas,iic-r8a7740", "renesas,rmobile-iic";
		reg = <0xe6c20000 0x425>;
		interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_IIC1>;
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa0: serial@e6c40000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6c40000 0x100>;
		interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA0>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa1: serial@e6c50000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6c50000 0x100>;
		interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA1>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa2: serial@e6c60000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6c60000 0x100>;
		interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA2>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa3: serial@e6c70000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6c70000 0x100>;
		interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA3>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa4: serial@e6c80000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6c80000 0x100>;
		interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA4>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa5: serial@e6cb0000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6cb0000 0x100>;
		interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA5>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa6: serial@e6cc0000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6cc0000 0x100>;
		interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA6>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifa7: serial@e6cd0000 {
		compatible = "renesas,scifa-r8a7740", "renesas,scifa";
		reg = <0xe6cd0000 0x100>;
		interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFA7>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	scifb: serial@e6c30000 {
		compatible = "renesas,scifb-r8a7740", "renesas,scifb";
		reg = <0xe6c30000 0x100>;
		interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp2_clks R8A7740_CLK_SCIFB>;
		clock-names = "fck";
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	pfc: pinctrl@e6050000 {
		compatible = "renesas,pfc-r8a7740";
		reg = <0xe6050000 0x8000>,
		      <0xe605800c 0x20>;
		gpio-controller;
		#gpio-cells = <2>;
		gpio-ranges = <&pfc 0 0 212>;
		interrupts-extended =
			<&irqpin0 0 0>, <&irqpin0 1 0>, <&irqpin0 2 0>, <&irqpin0 3 0>,
			<&irqpin0 4 0>, <&irqpin0 5 0>, <&irqpin0 6 0>, <&irqpin0 7 0>,
			<&irqpin1 0 0>, <&irqpin1 1 0>, <&irqpin1 2 0>, <&irqpin1 3 0>,
			<&irqpin1 4 0>, <&irqpin1 5 0>, <&irqpin1 6 0>, <&irqpin1 7 0>,
			<&irqpin2 0 0>, <&irqpin2 1 0>, <&irqpin2 2 0>, <&irqpin2 3 0>,
			<&irqpin2 4 0>, <&irqpin2 5 0>, <&irqpin2 6 0>, <&irqpin2 7 0>,
			<&irqpin3 0 0>, <&irqpin3 1 0>, <&irqpin3 2 0>, <&irqpin3 3 0>,
			<&irqpin3 4 0>, <&irqpin3 5 0>, <&irqpin3 6 0>, <&irqpin3 7 0>;
		power-domains = <&pd_c5>;
	};

	tpu: pwm@e6600000 {
		compatible = "renesas,tpu-r8a7740", "renesas,tpu";
		reg = <0xe6600000 0x148>;
		clocks = <&mstp3_clks R8A7740_CLK_TPU0>;
		power-domains = <&pd_a3sp>;
		status = "disabled";
		#pwm-cells = <3>;
	};

	mmcif0: mmc@e6bd0000 {
		compatible = "renesas,mmcif-r8a7740", "renesas,sh-mmcif";
		reg = <0xe6bd0000 0x100>;
		interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_MMC>;
		power-domains = <&pd_a3sp>;
		status = "disabled";
	};

	sdhi0: mmc@e6850000 {
		compatible = "renesas,sdhi-r8a7740";
		reg = <0xe6850000 0x100>;
		interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_SDHI0>;
		power-domains = <&pd_a3sp>;
		cap-sd-highspeed;
		cap-sdio-irq;
		status = "disabled";
	};

	sdhi1: mmc@e6860000 {
		compatible = "renesas,sdhi-r8a7740";
		reg = <0xe6860000 0x100>;
		interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp3_clks R8A7740_CLK_SDHI1>;
		power-domains = <&pd_a3sp>;
		cap-sd-highspeed;
		cap-sdio-irq;
		status = "disabled";
	};

	sdhi2: mmc@e6870000 {
		compatible = "renesas,sdhi-r8a7740";
		reg = <0xe6870000 0x100>;
		interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp4_clks R8A7740_CLK_SDHI2>;
		power-domains = <&pd_a3sp>;
		cap-sd-highspeed;
		cap-sdio-irq;
		status = "disabled";
	};

	sh_fsi2: sound@fe1f0000 {
		#sound-dai-cells = <1>;
		compatible = "renesas,fsi2-r8a7740", "renesas,sh_fsi2";
		reg = <0xfe1f0000 0x400>;
		interrupts = <GIC_SPI 9 0x4>;
		clocks = <&mstp3_clks R8A7740_CLK_FSI>;
		power-domains = <&pd_a4mp>;
		status = "disabled";
	};

	lcdc0: lcd-controller@fe940000 {
		compatible = "renesas,r8a7740-lcdc";
		reg = <0xfe940000 0x4000>;
		interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7740_CLK_LCDC0>,
			 <&cpg_clocks R8A7740_CLK_M3>, <&lcdlclk0_clk>,
			 <&vou_clk>;
		clock-names = "fck", "media", "lclk", "video";
		power-domains = <&pd_a4lc>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				lcdc0_rgb: endpoint {
				};
			};
		};
	};

	lcdc1: lcd-controller@fe944000 {
		compatible = "renesas,r8a7740-lcdc";
		reg = <0xfe944000 0x4000>;
		interrupts = <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&mstp1_clks R8A7740_CLK_LCDC1>,
			 <&cpg_clocks R8A7740_CLK_M3>, <&lcdlclk1_clk>,
			 <&vou_clk>;
		clock-names = "fck", "media", "lclk", "video";
		power-domains = <&pd_a4lc>;
		status = "disabled";

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;

				lcdc1_rgb: endpoint {
				};
			};

			port@1 {
				reg = <1>;

				lcdc1_hdmi: endpoint {
				};
			};
		};
	};

	tmu0: timer@fff80000 {
		compatible = "renesas,tmu-r8a7740", "renesas,tmu";
		reg = <0xfff80000 0x2c>;
		interrupts = <GIC_SPI 198 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 199 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 200 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "tuni0", "tuni1", "tuni2";
		clocks = <&mstp1_clks R8A7740_CLK_TMU0>;
		clock-names = "fck";
		power-domains = <&pd_a4r>;

		#renesas,channels = <3>;

		status = "disabled";
	};

	tmu1: timer@fff90000 {
		compatible = "renesas,tmu-r8a7740", "renesas,tmu";
		reg = <0xfff90000 0x2c>;
		interrupts = <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "tuni0", "tuni1", "tuni2";
		clocks = <&mstp1_clks R8A7740_CLK_TMU1>;
		clock-names = "fck";
		power-domains = <&pd_a4r>;

		#renesas,channels = <3>;

		status = "disabled";
	};

	clocks {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		/* External root clock */
		extalr_clk: extalr {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};
		extal1_clk: extal1 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		extal2_clk: extal2 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		dv_clk: dv {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <27000000>;
		};
		fmsick_clk: fmsick {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		fmsock_clk: fmsock {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		fsiack_clk: fsiack {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		fsibck_clk: fsibck {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		lcdlclk0_clk: lcdlclk0 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};
		lcdlclk1_clk: lcdlclk1 {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <0>;
		};

		/* Special CPG clocks */
		cpg_clocks: cpg_clocks@e6150000 {
			compatible = "renesas,r8a7740-cpg-clocks";
			reg = <0xe6150000 0x10000>;
			clocks = <&extal1_clk>, <&extal2_clk>, <&extalr_clk>;
			#clock-cells = <1>;
			clock-output-names = "system", "pllc0", "pllc1",
					     "pllc2", "r",
					     "usb24s",
					     "i", "zg", "b", "m1", "hp",
					     "hpp", "usbp", "s", "zb", "m3",
					     "cp";
		};

		/* Variable factor clocks (DIV6) */
		vclk1_clk: vclk1@e6150008 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150008 4>;
			clocks = <&pllc1_div2_clk>, <0>, <&dv_clk>,
				 <&cpg_clocks R8A7740_CLK_USB24S>,
				 <&extal1_div2_clk>, <&extalr_clk>, <0>,
				 <0>;
			#clock-cells = <0>;
		};
		vclk2_clk: vclk2@e615000c {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe615000c 4>;
			clocks = <&pllc1_div2_clk>, <0>, <&dv_clk>,
				 <&cpg_clocks R8A7740_CLK_USB24S>,
				 <&extal1_div2_clk>, <&extalr_clk>, <0>,
				 <0>;
			#clock-cells = <0>;
		};
		fmsi_clk: fmsi@e6150010 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150010 4>;
			clocks = <&pllc1_div2_clk>, <&fmsick_clk>, <0>, <0>;
			#clock-cells = <0>;
		};
		fmso_clk: fmso@e6150014 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150014 4>;
			clocks = <&pllc1_div2_clk>, <&fmsock_clk>, <0>, <0>;
			#clock-cells = <0>;
		};
		fsia_clk: fsia@e6150018 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150018 4>;
			clocks = <&pllc1_div2_clk>, <&fsiack_clk>, <0>, <0>;
			#clock-cells = <0>;
		};
		sub_clk: sub@e6150080 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150080 4>;
			clocks = <&pllc1_div2_clk>,
				 <&cpg_clocks R8A7740_CLK_USB24S>, <0>, <0>;
			#clock-cells = <0>;
		};
		spu_clk: spu@e6150084 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150084 4>;
			clocks = <&pllc1_div2_clk>,
				 <&cpg_clocks R8A7740_CLK_USB24S>, <0>, <0>;
			#clock-cells = <0>;
		};
		vou_clk: vou@e6150088 {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe6150088 4>;
			clocks = <&pllc1_div2_clk>, <&extal1_clk>, <&dv_clk>,
				 <0>;
			#clock-cells = <0>;
		};
		stpro_clk: stpro@e615009c {
			compatible = "renesas,r8a7740-div6-clock", "renesas,cpg-div6-clock";
			reg = <0xe615009c 4>;
			clocks = <&cpg_clocks R8A7740_CLK_PLLC0>;
			#clock-cells = <0>;
		};

		/* Fixed factor clocks */
		pllc1_div2_clk: pllc1_div2 {
			compatible = "fixed-factor-clock";
			clocks = <&cpg_clocks R8A7740_CLK_PLLC1>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
		};
		extal1_div2_clk: extal1_div2 {
			compatible = "fixed-factor-clock";
			clocks = <&extal1_clk>;
			#clock-cells = <0>;
			clock-div = <2>;
			clock-mult = <1>;
		};

		/* Gate clocks */
		subck_clks: subck_clks@e6150080 {
			compatible = "renesas,r8a7740-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0xe6150080 4>;
			clocks = <&sub_clk>, <&sub_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7740_CLK_SUBCK R8A7740_CLK_SUBCK2
			>;
			clock-output-names =
				"subck", "subck2";
		};
		mstp1_clks: mstp1_clks@e6150134 {
			compatible = "renesas,r8a7740-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0xe6150134 4>, <0xe6150038 4>;
			clocks = <&cpg_clocks R8A7740_CLK_S>,
				 <&cpg_clocks R8A7740_CLK_S>, <&sub_clk>,
				 <&cpg_clocks R8A7740_CLK_B>,
				 <&cpg_clocks R8A7740_CLK_HPP>, <&sub_clk>,
				 <&cpg_clocks R8A7740_CLK_B>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7740_CLK_CEU21 R8A7740_CLK_CEU20 R8A7740_CLK_TMU0
				R8A7740_CLK_LCDC1 R8A7740_CLK_IIC0 R8A7740_CLK_TMU1
				R8A7740_CLK_LCDC0
			>;
			clock-output-names =
				"ceu21", "ceu20", "tmu0", "lcdc1", "iic0",
				"tmu1", "lcdc0";
		};
		mstp2_clks: mstp2_clks@e6150138 {
			compatible = "renesas,r8a7740-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0xe6150138 4>, <0xe6150040 4>;
			clocks = <&sub_clk>, <&cpg_clocks R8A7740_CLK_HP>,
				 <&sub_clk>, <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&sub_clk>, <&sub_clk>, <&sub_clk>,
				 <&sub_clk>, <&sub_clk>, <&sub_clk>,
				 <&sub_clk>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7740_CLK_SCIFA6 R8A7740_CLK_INTCA
				R8A7740_CLK_SCIFA7
				R8A7740_CLK_DMAC1 R8A7740_CLK_DMAC2
				R8A7740_CLK_DMAC3 R8A7740_CLK_USBDMAC
				R8A7740_CLK_SCIFA5 R8A7740_CLK_SCIFB
				R8A7740_CLK_SCIFA0 R8A7740_CLK_SCIFA1
				R8A7740_CLK_SCIFA2 R8A7740_CLK_SCIFA3
				R8A7740_CLK_SCIFA4
			>;
			clock-output-names =
				"scifa6", "intca",
				"scifa7", "dmac1", "dmac2", "dmac3",
				"usbdmac", "scifa5", "scifb", "scifa0", "scifa1",
				"scifa2", "scifa3", "scifa4";
		};
		mstp3_clks: mstp3_clks@e615013c {
			compatible = "renesas,r8a7740-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0xe615013c 4>, <0xe6150048 4>;
			clocks = <&cpg_clocks R8A7740_CLK_R>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&sub_clk>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7740_CLK_CMT1 R8A7740_CLK_FSI R8A7740_CLK_IIC1
				R8A7740_CLK_USBF R8A7740_CLK_SDHI0 R8A7740_CLK_SDHI1
				R8A7740_CLK_MMC R8A7740_CLK_GETHER R8A7740_CLK_TPU0
			>;
			clock-output-names =
				"cmt1", "fsi", "iic1", "usbf", "sdhi0", "sdhi1",
				"mmc", "gether", "tpu0";
		};
		mstp4_clks: mstp4_clks@e6150140 {
			compatible = "renesas,r8a7740-mstp-clocks", "renesas,cpg-mstp-clocks";
			reg = <0xe6150140 4>, <0xe615004c 4>;
			clocks = <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>,
				 <&cpg_clocks R8A7740_CLK_HP>;
			#clock-cells = <1>;
			clock-indices = <
				R8A7740_CLK_USBH R8A7740_CLK_SDHI2
				R8A7740_CLK_USBFUNC R8A7740_CLK_USBPHY
			>;
			clock-output-names =
				"usbhost", "sdhi2", "usbfunc", "usphy";
		};
	};

	sysc: system-controller@e6180000 {
		compatible = "renesas,sysc-r8a7740", "renesas,sysc-rmobile";
		reg = <0xe6180000 0x8000>, <0xe6188000 0x8000>;

		pm-domains {
			pd_c5: c5 {
				#address-cells = <1>;
				#size-cells = <0>;
				#power-domain-cells = <0>;

				pd_a4lc: a4lc@1 {
					reg = <1>;
					#power-domain-cells = <0>;
				};

				pd_a4mp: a4mp@2 {
					reg = <2>;
					#power-domain-cells = <0>;
				};

				pd_d4: d4@3 {
					reg = <3>;
					#power-domain-cells = <0>;
				};

				pd_a4r: a4r@5 {
					reg = <5>;
					#address-cells = <1>;
					#size-cells = <0>;
					#power-domain-cells = <0>;

					pd_a3rv: a3rv@6 {
						reg = <6>;
						#power-domain-cells = <0>;
					};
				};

				pd_a4s: a4s@10 {
					reg = <10>;
					#address-cells = <1>;
					#size-cells = <0>;
					#power-domain-cells = <0>;

					pd_a3sp: a3sp@11 {
						reg = <11>;
						#power-domain-cells = <0>;
					};

					pd_a3sm: a3sm@12 {
						reg = <12>;
						#power-domain-cells = <0>;
					};

					pd_a3sg: a3sg@13 {
						reg = <13>;
						#power-domain-cells = <0>;
					};
				};

				pd_a4su: a4su@20 {
					reg = <20>;
					#power-domain-cells = <0>;
				};
			};
		};
	};
};
