/*
 * Copyright (C) 2013-2016 Marek Vasut <marek.vasut@gmail.com>
 *
 * This file is dual-licensed: you can use it either under the terms
 * of the GPL or the X11 license, at your option. Note that this dual
 * licensing only applies to this file, and not this project as a
 * whole.
 *
 *  a) This file is free software; you can redistribute it and/or
 *     modify it under the terms of the GNU General Public License as
 *     published by the Free Software Foundation; either version 2 of
 *     the License, or (at your option) any later version.
 *
 *     This file is distributed in the hope that it will be useful,
 *     but WITHOUT ANY WARRANTY; without even the implied warranty of
 *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
 *     GNU General Public License for more details.
 *
 * Or, alternatively,
 *
 *  b) Permission is hereby granted, free of charge, to any person
 *     obtaining a copy of this software and associated documentation
 *     files (the "Software"), to deal in the Software without
 *     restriction, including without limitation the rights to use,
 *     copy, modify, merge, publish, distribute, sublicense, and/or
 *     sell copies of the Software, and to permit persons to whom the
 *     Software is furnished to do so, subject to the following
 *     conditions:
 *
 *     The above copyright notice and this permission notice shall be
 *     included in all copies or substantial portions of the Software.
 *
 *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
 *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
 *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
 *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
 *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
 *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
 *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
 *     OTHER DEALINGS IN THE SOFTWARE.
 *
 */

/dts-v1/;
#include "imx23.dtsi"

/ {
	model = "Creative ZEN X-Fi3";
	compatible = "creative,x-fi3", "fsl,imx23";

	memory@40000000 {
		device_type = "memory";
		reg = <0x40000000 0x04000000>;
	};

	apb@80000000 {
		apbh-bus@80000000 {
			ssp0: spi@80010000 {
				compatible = "fsl,imx23-mmc";
				pinctrl-names = "default";
				pinctrl-0 = <&mmc0_4bit_pins_a &mmc0_pins_fixup>;
				bus-width = <4>;
				vmmc-supply = <&reg_vddio_sd0>;
				cd-inverted;
				status = "okay";
			};

			ssp1: spi@80034000 {
				compatible = "fsl,imx23-mmc";
				pinctrl-names = "default";
				pinctrl-0 = <&mmc1_4bit_pins_a>;
				bus-width = <4>;
				non-removable;
				status = "okay";
			};

			pinctrl@80018000 {
				pinctrl-names = "default";
				pinctrl-0 = <&hog_pins_a>;

				hog_pins_a: hog@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						MX23_PAD_GPMI_D07__GPIO_0_7
					>;
					fsl,drive-strength = <0>;
					fsl,voltage = <1>;
					fsl,pull-up = <0>;
				};

				key_pins_a: keys@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						MX23_PAD_ROTARYA__GPIO_2_7
						MX23_PAD_ROTARYB__GPIO_2_8
					>;
					fsl,drive-strength = <0>;
					fsl,voltage = <1>;
					fsl,pull-up = <1>;
				};
			};
		};

		apbx-bus@80040000 {
			i2c: i2c@80058000 {
				pinctrl-names = "default";
				pinctrl-0 = <&i2c_pins_a>;
				status = "okay";
			};

			pwm: pwm@80064000 {
				pinctrl-names = "default";
				pinctrl-0 = <&pwm2_pins_a>;
				status = "okay";
			};

			duart: serial@80070000 {
				pinctrl-names = "default";
				pinctrl-0 = <&duart_pins_a>;
				status = "okay";
			};

			auart1: serial@8006e000 {
				pinctrl-names = "default";
				pinctrl-0 = <&auart1_2pins_a>;
				status = "okay";
			};

			usbphy0: usbphy@8007c000 {
				status = "okay";
			};

			lradc@80050000 {
				status = "okay";
			};
		};
	};

	ahb@80080000 {
		usb0: usb@80080000 {
			dr_mode = "peripheral";
			status = "okay";
		};
	};

	reg_vddio_sd0: regulator-vddio-sd0 {
		compatible = "regulator-fixed";
		regulator-name = "vddio-sd0";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio0 7 0>;
	};

	backlight {
		compatible = "pwm-backlight";
		pwms = <&pwm 2 5000000 0>;
		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <6>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&key_pins_a>;

		key-voldown {
			label = "volume-down";
			linux,code = <114>;
			gpios = <&gpio2 7 0>;
			debounce-interval = <20>;
		};

		key-volup {
			label = "volume-up";
			linux,code = <115>;
			gpios = <&gpio2 8 0>;
			debounce-interval = <20>;
		};
	};
};
