// SPDX-License-Identifier: GPL-2.0
/*
 * Device Tree Source for the R-Car V2H (R8A77920) SoC
 *
 * Copyright (C) 2016 Cogent Embedded Inc.
 */

#include <dt-bindings/clock/r8a7792-cpg-mssr.h>
#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/power/r8a7792-sysc.h>

/ {
	compatible = "renesas,r8a7792";
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &iic3;
		spi0 = &qspi;
		spi1 = &msiof0;
		spi2 = &msiof1;
		vin0 = &vin0;
		vin1 = &vin1;
		vin2 = &vin2;
		vin3 = &vin3;
		vin4 = &vin4;
		vin5 = &vin5;
	};

	/* External CAN clock */
	can_clk: can {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		/* This value must be overridden by the board. */
		clock-frequency = <0>;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <0>;
			clock-frequency = <1000000000>;
			clocks = <&cpg CPG_CORE R8A7792_CLK_Z>;
			power-domains = <&sysc R8A7792_PD_CA15_CPU0>;
			enable-method = "renesas,apmu";
			next-level-cache = <&L2_CA15>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a15";
			reg = <1>;
			clock-frequency = <1000000000>;
			clocks = <&cpg CPG_CORE R8A7792_CLK_Z>;
			power-domains = <&sysc R8A7792_PD_CA15_CPU1>;
			enable-method = "renesas,apmu";
			next-level-cache = <&L2_CA15>;
		};

		L2_CA15: cache-controller-0 {
			compatible = "cache";
			cache-unified;
			cache-level = <2>;
			power-domains = <&sysc R8A7792_PD_CA15_SCU>;
		};
	};

	/* External root clock */
	extal_clk: extal {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		/* This value must be overridden by the board. */
		clock-frequency = <0>;
	};

	lbsc: lbsc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0 0 0x1c000000>;
	};

	pmu {
		compatible = "arm,cortex-a15-pmu";
		interrupts-extended = <&gic GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>,
				      <&gic GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>;
	};

	/* External SCIF clock */
	scif_clk: scif {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		/* This value must be overridden by the board. */
		clock-frequency = <0>;
	};

	soc {
		compatible = "simple-bus";
		interrupt-parent = <&gic>;

		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		rwdt: watchdog@e6020000 {
			compatible = "renesas,r8a7792-wdt",
				     "renesas,rcar-gen2-wdt";
			reg = <0 0xe6020000 0 0x0c>;
			interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 402>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 402>;
			status = "disabled";
		};

		gpio0: gpio@e6050000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6050000 0 0x50>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 0 29>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 912>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 912>;
		};

		gpio1: gpio@e6051000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6051000 0 0x50>;
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 32 23>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 911>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 911>;
		};

		gpio2: gpio@e6052000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6052000 0 0x50>;
			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 64 32>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 910>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 910>;
		};

		gpio3: gpio@e6053000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6053000 0 0x50>;
			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 96 28>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 909>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 909>;
		};

		gpio4: gpio@e6054000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6054000 0 0x50>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 128 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 908>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 908>;
		};

		gpio5: gpio@e6055000 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055000 0 0x50>;
			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 160 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 907>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 907>;
		};

		gpio6: gpio@e6055100 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055100 0 0x50>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 192 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 905>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 905>;
		};

		gpio7: gpio@e6055200 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055200 0 0x50>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 224 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 904>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 904>;
		};

		gpio8: gpio@e6055300 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055300 0 0x50>;
			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 256 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 921>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 921>;
		};

		gpio9: gpio@e6055400 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055400 0 0x50>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 288 17>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 919>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 919>;
		};

		gpio10: gpio@e6055500 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055500 0 0x50>;
			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 320 32>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 914>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 914>;
		};

		gpio11: gpio@e6055600 {
			compatible = "renesas,gpio-r8a7792",
				     "renesas,rcar-gen2-gpio";
			reg = <0 0xe6055600 0 0x50>;
			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
			#gpio-cells = <2>;
			gpio-controller;
			gpio-ranges = <&pfc 0 352 30>;
			#interrupt-cells = <2>;
			interrupt-controller;
			clocks = <&cpg CPG_MOD 913>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 913>;
		};

		pfc: pinctrl@e6060000 {
			compatible = "renesas,pfc-r8a7792";
			reg = <0 0xe6060000 0 0x144>;
		};

		cpg: clock-controller@e6150000 {
			compatible = "renesas,r8a7792-cpg-mssr";
			reg = <0 0xe6150000 0 0x1000>;
			clocks = <&extal_clk>;
			clock-names = "extal";
			#clock-cells = <2>;
			#power-domain-cells = <0>;
			#reset-cells = <1>;
		};

		apmu@e6152000 {
			compatible = "renesas,r8a7792-apmu", "renesas,apmu";
			reg = <0 0xe6152000 0 0x188>;
			cpus = <&cpu0>, <&cpu1>;
		};

		rst: reset-controller@e6160000 {
			compatible = "renesas,r8a7792-rst";
			reg = <0 0xe6160000 0 0x0100>;
		};

		sysc: system-controller@e6180000 {
			compatible = "renesas,r8a7792-sysc";
			reg = <0 0xe6180000 0 0x0200>;
			#power-domain-cells = <1>;
		};

		irqc: interrupt-controller@e61c0000 {
			compatible = "renesas,irqc-r8a7792", "renesas,irqc";
			#interrupt-cells = <2>;
			interrupt-controller;
			reg = <0 0xe61c0000 0 0x200>;
			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 407>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 407>;
		};

		tmu0: timer@e61e0000 {
			compatible = "renesas,tmu-r8a7792", "renesas,tmu";
			reg = <0 0xe61e0000 0 0x30>;
			interrupts = <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "tuni0", "tuni1", "tuni2";
			clocks = <&cpg CPG_MOD 125>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 125>;
			status = "disabled";
		};

		tmu1: timer@fff60000 {
			compatible = "renesas,tmu-r8a7792", "renesas,tmu";
			reg = <0 0xfff60000 0 0x30>;
			interrupts = <GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "tuni0", "tuni1", "tuni2", "ticpi2";
			clocks = <&cpg CPG_MOD 111>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 111>;
			status = "disabled";
		};

		tmu2: timer@fff70000 {
			compatible = "renesas,tmu-r8a7792", "renesas,tmu";
			reg = <0 0xfff70000 0 0x30>;
			interrupts = <GIC_SPI 303 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 304 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 305 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 306 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "tuni0", "tuni1", "tuni2", "ticpi2";
			clocks = <&cpg CPG_MOD 122>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 122>;
			status = "disabled";
		};

		tmu3: timer@fff80000 {
			compatible = "renesas,tmu-r8a7792", "renesas,tmu";
			reg = <0 0xfff80000 0 0x30>;
			interrupts = <GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 132 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "tuni0", "tuni1", "tuni2", "ticpi2";
			clocks = <&cpg CPG_MOD 121>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 121>;
			status = "disabled";
		};

		icram0:	sram@e63a0000 {
			compatible = "mmio-sram";
			reg = <0 0xe63a0000 0 0x12000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0 0xe63a0000 0x12000>;
		};

		icram1:	sram@e63c0000 {
			compatible = "mmio-sram";
			reg = <0 0xe63c0000 0 0x1000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0 0xe63c0000 0x1000>;

			smp-sram@0 {
				compatible = "renesas,smp-sram";
				reg = <0 0x100>;
			};
		};

		/* I2C doesn't need pinmux */
		i2c0: i2c@e6508000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6508000 0 0x40>;
			interrupts = <GIC_SPI 287 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 931>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 931>;
			i2c-scl-internal-delay-ns = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		i2c1: i2c@e6518000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6518000 0 0x40>;
			interrupts = <GIC_SPI 288 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 930>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 930>;
			i2c-scl-internal-delay-ns = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		i2c2: i2c@e6530000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6530000 0 0x40>;
			interrupts = <GIC_SPI 286 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 929>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 929>;
			i2c-scl-internal-delay-ns = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		i2c3: i2c@e6540000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6540000 0 0x40>;
			interrupts = <GIC_SPI 290 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 928>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 928>;
			i2c-scl-internal-delay-ns = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		i2c4: i2c@e6520000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6520000 0 0x40>;
			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 927>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 927>;
			i2c-scl-internal-delay-ns = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		i2c5: i2c@e6528000 {
			compatible = "renesas,i2c-r8a7792",
				     "renesas,rcar-gen2-i2c";
			reg = <0 0xe6528000 0 0x40>;
			interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 925>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 925>;
			i2c-scl-internal-delay-ns = <110>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		iic3: i2c@e60b0000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "renesas,iic-r8a7792",
				     "renesas,rcar-gen2-iic",
				     "renesas,rmobile-iic";
			reg = <0 0xe60b0000 0 0x425>;
			interrupts = <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 926>;
			dmas = <&dmac0 0x77>, <&dmac0 0x78>,
			       <&dmac1 0x77>, <&dmac1 0x78>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 926>;
			status = "disabled";
		};

		dmac0: dma-controller@e6700000 {
			compatible = "renesas,dmac-r8a7792",
				     "renesas,rcar-dmac";
			reg = <0 0xe6700000 0 0x20000>;
			interrupts = <GIC_SPI 197 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 200 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 201 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 202 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 203 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 204 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 205 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 206 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 207 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 210 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 211 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 213 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 214 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "error",
					  "ch0", "ch1", "ch2", "ch3",
					  "ch4", "ch5", "ch6", "ch7",
					  "ch8", "ch9", "ch10", "ch11",
					  "ch12", "ch13", "ch14";
			clocks = <&cpg CPG_MOD 219>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 219>;
			#dma-cells = <1>;
			dma-channels = <15>;
		};

		dmac1: dma-controller@e6720000 {
			compatible = "renesas,dmac-r8a7792",
				     "renesas,rcar-dmac";
			reg = <0 0xe6720000 0 0x20000>;
			interrupts = <GIC_SPI 220 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 216 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 217 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 218 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 219 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 308 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 309 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 310 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 311 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 312 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 313 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 314 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 315 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 316 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 317 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 318 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "error",
					  "ch0", "ch1", "ch2", "ch3",
					  "ch4", "ch5", "ch6", "ch7",
					  "ch8", "ch9", "ch10", "ch11",
					  "ch12", "ch13", "ch14";
			clocks = <&cpg CPG_MOD 218>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 218>;
			#dma-cells = <1>;
			dma-channels = <15>;
		};

		avb: ethernet@e6800000 {
			compatible = "renesas,etheravb-r8a7792",
				     "renesas,etheravb-rcar-gen2";
			reg = <0 0xe6800000 0 0x800>, <0 0xee0e8000 0 0x4000>;
			interrupts = <GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 812>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 812>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		qspi: spi@e6b10000 {
			compatible = "renesas,qspi-r8a7792", "renesas,qspi";
			reg = <0 0xe6b10000 0 0x2c>;
			interrupts = <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 917>;
			dmas = <&dmac0 0x17>, <&dmac0 0x18>,
			       <&dmac1 0x17>, <&dmac1 0x18>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 917>;
			num-cs = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		scif0: serial@e6e60000 {
			compatible = "renesas,scif-r8a7792",
				     "renesas,rcar-gen2-scif", "renesas,scif";
			reg = <0 0xe6e60000 0 64>;
			interrupts = <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 721>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x29>, <&dmac0 0x2a>,
			       <&dmac1 0x29>, <&dmac1 0x2a>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 721>;
			status = "disabled";
		};

		scif1: serial@e6e68000 {
			compatible = "renesas,scif-r8a7792",
				     "renesas,rcar-gen2-scif", "renesas,scif";
			reg = <0 0xe6e68000 0 64>;
			interrupts = <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 720>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x2d>, <&dmac0 0x2e>,
			       <&dmac1 0x2d>, <&dmac1 0x2e>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 720>;
			status = "disabled";
		};

		scif2: serial@e6e58000 {
			compatible = "renesas,scif-r8a7792",
				     "renesas,rcar-gen2-scif", "renesas,scif";
			reg = <0 0xe6e58000 0 64>;
			interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 719>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x2b>, <&dmac0 0x2c>,
			       <&dmac1 0x2b>, <&dmac1 0x2c>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 719>;
			status = "disabled";
		};

		scif3: serial@e6ea8000 {
			compatible = "renesas,scif-r8a7792",
				     "renesas,rcar-gen2-scif", "renesas,scif";
			reg = <0 0xe6ea8000 0 64>;
			interrupts = <GIC_SPI 23 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 718>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x2f>, <&dmac0 0x30>,
			       <&dmac1 0x2f>, <&dmac1 0x30>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 718>;
			status = "disabled";
		};

		hscif0: serial@e62c0000 {
			compatible = "renesas,hscif-r8a7792",
				     "renesas,rcar-gen2-hscif", "renesas,hscif";
			reg = <0 0xe62c0000 0 96>;
			interrupts = <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 717>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x39>, <&dmac0 0x3a>,
			       <&dmac1 0x39>, <&dmac1 0x3a>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 717>;
			status = "disabled";
		};

		hscif1: serial@e62c8000 {
			compatible = "renesas,hscif-r8a7792",
				     "renesas,rcar-gen2-hscif", "renesas,hscif";
			reg = <0 0xe62c8000 0 96>;
			interrupts = <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 716>,
				 <&cpg CPG_CORE R8A7792_CLK_ZS>, <&scif_clk>;
			clock-names = "fck", "brg_int", "scif_clk";
			dmas = <&dmac0 0x4d>, <&dmac0 0x4e>,
			       <&dmac1 0x4d>, <&dmac1 0x4e>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 716>;
			status = "disabled";
		};

		msiof0: spi@e6e20000 {
			compatible = "renesas,msiof-r8a7792",
				     "renesas,rcar-gen2-msiof";
			reg = <0 0xe6e20000 0 0x0064>;
			interrupts = <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 000>;
			dmas = <&dmac0 0x51>, <&dmac0 0x52>,
			       <&dmac1 0x51>, <&dmac1 0x52>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 000>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		msiof1: spi@e6e10000 {
			compatible = "renesas,msiof-r8a7792",
				     "renesas,rcar-gen2-msiof";
			reg = <0 0xe6e10000 0 0x0064>;
			interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 208>;
			dmas = <&dmac0 0x55>, <&dmac0 0x56>,
			       <&dmac1 0x55>, <&dmac1 0x56>;
			dma-names = "tx", "rx", "tx", "rx";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 208>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";
		};

		can0: can@e6e80000 {
			compatible = "renesas,can-r8a7792",
				     "renesas,rcar-gen2-can";
			reg = <0 0xe6e80000 0 0x1000>;
			interrupts = <GIC_SPI 186 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 916>,
				 <&cpg CPG_CORE R8A7792_CLK_RCAN>, <&can_clk>;
			clock-names = "clkp1", "clkp2", "can_clk";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 916>;
			status = "disabled";
		};

		can1: can@e6e88000 {
			compatible = "renesas,can-r8a7792",
				     "renesas,rcar-gen2-can";
			reg = <0 0xe6e88000 0 0x1000>;
			interrupts = <GIC_SPI 187 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 915>,
				 <&cpg CPG_CORE R8A7792_CLK_RCAN>, <&can_clk>;
			clock-names = "clkp1", "clkp2", "can_clk";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 915>;
			status = "disabled";
		};

		vin0: video@e6ef0000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef0000 0 0x1000>;
			interrupts = <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 811>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 811>;
			status = "disabled";
		};

		vin1: video@e6ef1000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef1000 0 0x1000>;
			interrupts = <GIC_SPI 189 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 810>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 810>;
			status = "disabled";
		};

		vin2: video@e6ef2000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef2000 0 0x1000>;
			interrupts = <GIC_SPI 190 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 809>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 809>;
			status = "disabled";
		};

		vin3: video@e6ef3000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef3000 0 0x1000>;
			interrupts = <GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 808>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 808>;
			status = "disabled";
		};

		vin4: video@e6ef4000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef4000 0 0x1000>;
			interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 805>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 805>;
			status = "disabled";
		};

		vin5: video@e6ef5000 {
			compatible = "renesas,vin-r8a7792",
				     "renesas,rcar-gen2-vin";
			reg = <0 0xe6ef5000 0 0x1000>;
			interrupts = <GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 804>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 804>;
			status = "disabled";
		};

		sdhi0: mmc@ee100000 {
			compatible = "renesas,sdhi-r8a7792",
				     "renesas,rcar-gen2-sdhi";
			reg = <0 0xee100000 0 0x328>;
			interrupts = <0 165 IRQ_TYPE_LEVEL_HIGH>;
			dmas = <&dmac0 0xcd>, <&dmac0 0xce>,
			       <&dmac1 0xcd>, <&dmac1 0xce>;
			dma-names = "tx", "rx", "tx", "rx";
			clocks = <&cpg CPG_MOD 314>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 314>;
			status = "disabled";
		};

		gic: interrupt-controller@f1001000 {
			compatible = "arm,gic-400";
			#interrupt-cells = <3>;
			interrupt-controller;
			reg = <0 0xf1001000 0 0x1000>,
			      <0 0xf1002000 0 0x2000>,
			      <0 0xf1004000 0 0x2000>,
			      <0 0xf1006000 0 0x2000>;
			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(2) |
				      IRQ_TYPE_LEVEL_HIGH)>;
			clocks = <&cpg CPG_MOD 408>;
			clock-names = "clk";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 408>;
		};

		vsp@fe928000 {
			compatible = "renesas,vsp1";
			reg = <0 0xfe928000 0 0x8000>;
			interrupts = <GIC_SPI 267 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 131>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 131>;
		};

		vsp@fe930000 {
			compatible = "renesas,vsp1";
			reg = <0 0xfe930000 0 0x8000>;
			interrupts = <GIC_SPI 246 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 128>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 128>;
		};

		vsp@fe938000 {
			compatible = "renesas,vsp1";
			reg = <0 0xfe938000 0 0x8000>;
			interrupts = <GIC_SPI 247 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 127>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 127>;
		};

		jpu: jpeg-codec@fe980000 {
			compatible = "renesas,jpu-r8a7792",
				     "renesas,rcar-gen2-jpu";
			reg = <0 0xfe980000 0 0x10300>;
			interrupts = <GIC_SPI 272 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 106>;
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 106>;
		};

		du: display@feb00000 {
			compatible = "renesas,du-r8a7792";
			reg = <0 0xfeb00000 0 0x40000>;
			interrupts = <GIC_SPI 256 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 268 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 724>, <&cpg CPG_MOD 723>;
			clock-names = "du.0", "du.1";
			resets = <&cpg 724>;
			reset-names = "du.0";
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					du_out_rgb0: endpoint {
					};
				};
				port@1 {
					reg = <1>;
					du_out_rgb1: endpoint {
					};
				};
			};
		};

		prr: chipid@ff000044 {
			compatible = "renesas,prr";
			reg = <0 0xff000044 0 4>;
		};

		cmt0: timer@ffca0000 {
			compatible = "renesas,r8a7792-cmt0",
				     "renesas,rcar-gen2-cmt0";
			reg = <0 0xffca0000 0 0x1004>;
			interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 124>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 124>;

			status = "disabled";
		};

		cmt1: timer@e6130000 {
			compatible = "renesas,r8a7792-cmt1",
				     "renesas,rcar-gen2-cmt1";
			reg = <0 0xe6130000 0 0x1004>;
			interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&cpg CPG_MOD 329>;
			clock-names = "fck";
			power-domains = <&sysc R8A7792_PD_ALWAYS_ON>;
			resets = <&cpg 329>;

			status = "disabled";
		};
	};

	timer {
		compatible = "arm,armv7-timer";
		interrupts-extended = <&gic GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				      <&gic GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				      <&gic GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				      <&gic GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
		interrupt-names = "sec-phys", "phys", "virt", "hyp-phys";
	};
};
