// SPDX-License-Identifier: GPL-2.0
/dts-v1/;

#include <dt-bindings/interrupt-controller/irq.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/qcom,gcc-msm8660.h>
#include <dt-bindings/soc/qcom,gsbi.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	model = "Qualcomm MSM8660";
	compatible = "qcom,msm8660";
	interrupt-parent = <&intc>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "qcom,scorpion";
			enable-method = "qcom,gcc-msm8660";
			device_type = "cpu";
			reg = <0>;
			next-level-cache = <&L2>;
		};

		cpu@1 {
			compatible = "qcom,scorpion";
			enable-method = "qcom,gcc-msm8660";
			device_type = "cpu";
			reg = <1>;
			next-level-cache = <&L2>;
		};

		L2: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			cache-unified;
		};
	};

	memory {
		device_type = "memory";
		reg = <0x0 0x0>;
	};

	cpu-pmu {
		compatible = "qcom,scorpion-mp-pmu";
		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	clocks {
		cxo_board: cxo-board-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <19200000>;
			clock-output-names = "cxo_board";
		};

		pxo_board: pxo-board-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <27000000>;
			clock-output-names = "pxo_board";
		};

		sleep-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32768>;
			clock-output-names = "sleep_clk";
		};
	};

	soc: soc {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";

		intc: interrupt-controller@2080000 {
			compatible = "qcom,msm-8660-qgic";
			interrupt-controller;
			#interrupt-cells = <3>;
			reg = < 0x02080000 0x1000 >,
			      < 0x02081000 0x1000 >;
		};

		timer@2000000 {
			compatible = "qcom,scss-timer", "qcom,msm-timer";
			interrupts = <GIC_PPI 0 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>,
				     <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_EDGE_RISING)>;
			reg = <0x02000000 0x100>;
			clock-frequency = <27000000>;
			cpu-offset = <0x40000>;
		};

		tlmm: pinctrl@800000 {
			compatible = "qcom,msm8660-pinctrl";
			reg = <0x800000 0x4000>;

			gpio-controller;
			gpio-ranges = <&tlmm 0 0 173>;
			#gpio-cells = <2>;
			interrupts = <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;

		};

		gcc: clock-controller@900000 {
			compatible = "qcom,gcc-msm8660";
			#clock-cells = <1>;
			#reset-cells = <1>;
			reg = <0x900000 0x4000>;
			clocks = <&pxo_board>, <&cxo_board>;
			clock-names = "pxo", "cxo";
		};

		gsbi1: gsbi@16000000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x16000000 0x100>;
			clocks = <&gcc GSBI1_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			status = "disabled";

			gsbi1_spi: spi@16080000 {
				compatible = "qcom,spi-qup-v1.1.1";
				reg = <0x16080000 0x1000>;
				interrupts = <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI1_QUP_CLK>, <&gcc GSBI1_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi3: gsbi@16200000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x16200000 0x100>;
			clocks = <&gcc GSBI3_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;
			status = "disabled";

			gsbi3_i2c: i2c@16280000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16280000 0x1000>;
				interrupts = <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI3_QUP_CLK>, <&gcc GSBI3_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi6: gsbi@16500000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x16500000 0x100>;
			clocks = <&gcc GSBI6_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi6_serial: serial@16540000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16540000 0x1000>,
				      <0x16500000 0x1000>;
				interrupts = <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI6_UART_CLK>, <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi6_i2c: i2c@16580000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16580000 0x1000>;
				interrupts = <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI6_QUP_CLK>, <&gcc GSBI6_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi7: gsbi@16600000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x16600000 0x100>;
			clocks = <&gcc GSBI7_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			status = "disabled";

			syscon-tcsr = <&tcsr>;

			gsbi7_serial: serial@16640000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x16640000 0x1000>,
				      <0x16600000 0x1000>;
				interrupts = <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI7_UART_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi7_i2c: i2c@16680000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x16680000 0x1000>;
				interrupts = <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI7_QUP_CLK>, <&gcc GSBI7_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi8: gsbi@19800000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x19800000 0x100>;
			clocks = <&gcc GSBI8_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;
			status = "disabled";

			gsbi8_i2c: i2c@19880000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x19880000 0x1000>;
				interrupts = <GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI8_QUP_CLK>, <&gcc GSBI8_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		gsbi12: gsbi@19c00000 {
			compatible = "qcom,gsbi-v1.0.0";
			cell-index = <12>;
			reg = <0x19c00000 0x100>;
			clocks = <&gcc GSBI12_H_CLK>;
			clock-names = "iface";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon-tcsr = <&tcsr>;

			gsbi12_serial: serial@19c40000 {
				compatible = "qcom,msm-uartdm-v1.3", "qcom,msm-uartdm";
				reg = <0x19c40000 0x1000>,
				      <0x19c00000 0x1000>;
				interrupts = <GIC_SPI 195 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI12_UART_CLK>, <&gcc GSBI12_H_CLK>;
				clock-names = "core", "iface";
				status = "disabled";
			};

			gsbi12_i2c: i2c@19c80000 {
				compatible = "qcom,i2c-qup-v1.1.1";
				reg = <0x19c80000 0x1000>;
				interrupts = <GIC_SPI 196 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc GSBI12_QUP_CLK>, <&gcc GSBI12_H_CLK>;
				clock-names = "core", "iface";
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		ebi2: external-bus@1a100000 {
			compatible = "qcom,msm8660-ebi2";
			#address-cells = <2>;
			#size-cells = <1>;
			ranges = <0 0x0 0x1a800000 0x00800000>,
				 <1 0x0 0x1b000000 0x00800000>,
				 <2 0x0 0x1b800000 0x00800000>,
				 <3 0x0 0x1d000000 0x08000000>,
				 <4 0x0 0x1c800000 0x00800000>,
				 <5 0x0 0x1c000000 0x00800000>;
			reg = <0x1a100000 0x1000>, <0x1a110000 0x1000>;
			reg-names = "ebi2", "xmem";
			clocks = <&gcc EBI2_2X_CLK>, <&gcc EBI2_CLK>;
			clock-names = "ebi2x", "ebi2";
			status = "disabled";
		};

		ssbi: ssbi@500000 {
			compatible = "qcom,ssbi";
			reg = <0x500000 0x1000>;
			qcom,controller-type = "pmic-arbiter";
		};

		l2cc: clock-controller@2082000 {
			compatible = "qcom,kpss-gcc-msm8660", "qcom,kpss-gcc", "syscon";
			reg = <0x02082000 0x1000>;
		};

		rpm: rpm@104000 {
			compatible = "qcom,rpm-msm8660";
			reg = <0x00104000 0x1000>;
			qcom,ipc = <&l2cc 0x8 2>;

			interrupts = <GIC_SPI 19 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 21 IRQ_TYPE_EDGE_RISING>,
				     <GIC_SPI 22 IRQ_TYPE_EDGE_RISING>;
			interrupt-names = "ack", "err", "wakeup";
			clocks = <&gcc RPM_MSG_RAM_H_CLK>;
			clock-names = "ram";

			rpmcc: clock-controller {
				compatible = "qcom,rpmcc-msm8660", "qcom,rpmcc";
				#clock-cells = <1>;
				clocks = <&pxo_board>;
				clock-names = "pxo";
			};
		};

		amba {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;
			sdcc1: mmc@12400000 {
				status = "disabled";
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				reg = <0x12400000 0x8000>;
				interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC1_CLK>, <&gcc SDC1_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <8>;
				max-frequency = <48000000>;
				non-removable;
				cap-sd-highspeed;
				cap-mmc-highspeed;
			};

			sdcc2: mmc@12140000 {
				status = "disabled";
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				reg = <0x12140000 0x8000>;
				interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC2_CLK>, <&gcc SDC2_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <8>;
				max-frequency = <48000000>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
			};

			sdcc3: mmc@12180000 {
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				status = "disabled";
				reg = <0x12180000 0x8000>;
				interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC3_CLK>, <&gcc SDC3_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <4>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				max-frequency = <48000000>;
				no-1-8-v;
			};

			sdcc4: mmc@121c0000 {
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				status = "disabled";
				reg = <0x121c0000 0x8000>;
				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC4_CLK>, <&gcc SDC4_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <4>;
				max-frequency = <48000000>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
			};

			sdcc5: mmc@12200000 {
				compatible = "arm,pl18x", "arm,primecell";
				arm,primecell-periphid = <0x00051180>;
				status = "disabled";
				reg = <0x12200000 0x8000>;
				interrupts = <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&gcc SDC5_CLK>, <&gcc SDC5_H_CLK>;
				clock-names = "mclk", "apb_pclk";
				bus-width = <4>;
				cap-sd-highspeed;
				cap-mmc-highspeed;
				max-frequency = <48000000>;
			};
		};

		tcsr: syscon@1a400000 {
			compatible = "qcom,tcsr-msm8660", "syscon";
			reg = <0x1a400000 0x100>;
		};
	};

};
