13:44:04.426635 14325 C5G_Tests.ttcn:324 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs-latest/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating'.
13:44:05.454122 14325 C5G_Tests.ttcn:324 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs-latest/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating' was executed successfully (exit status: 0).
13:44:05.454603 14325 C5G_Tests.ttcn:324 Test case TC_periodic_registration_updating started.
13:44:05.454761 14325 C5G_Tests.ttcn:324 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_periodic_registration_updating.
13:44:05.454898 14325 C5G_Tests.ttcn:324 Port NGAP_UNIT[0] was started.
13:44:05.454992 14325 C5G_Tests.ttcn:324 Port NGAP_PROC[0] was started.
13:44:05.455070 14325 C5G_Tests.ttcn:324 Port TEID0 was started.
13:44:05.455396 14325 C5G_Tests.ttcn:324 Component type C5G_Tests.MTC_CT was initialized.
13:44:05.455499 14325 C5G_Tests.ttcn:191 Start timer g_Tguard: 30 s
13:44:05.455568 14325 C5G_Tests.ttcn:192 Altstep as_Tguard was activated as default, id 1
13:44:05.455633 14325 C5G_Tests.ttcn:183 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
13:44:05.462364 14560 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
13:44:05.462405 14560 - TTCN-3 Parallel Test Component started on e9423b37bbd0. Component reference: GTP1U_EM(12), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
13:44:05.462427 14560 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
13:44:05.462550 14560 - Connected to MC.
13:44:05.462579 14560 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_periodic_registration_updating.
13:44:05.462619 14325 C5G_Tests.ttcn:183 PTC was created. Component reference: 12, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
13:44:05.462635 14325 C5G_Tests.ttcn:184 Mapping port GTP1U_EM(12):GTP1U to system:GTP1U.
13:44:05.463429 14560 - Port GTP1U was started.
13:44:05.463450 14560 - Port TEID0 was started.
13:44:05.463460 14560 - Port CLIENT was started.
13:44:05.463470 14560 - Port CLIENT_PROC was started.
13:44:05.463480 14560 - Port UECUPS was started.
13:44:05.463490 14560 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
13:44:05.463521 14560 - Port GTP1U was mapped to system:GTP1U.
13:44:05.463603 14325 C5G_Tests.ttcn:184 Map operation of GTP1U_EM(12):GTP1U to system:GTP1U finished.
13:44:05.463687 14325 C5G_Tests.ttcn:185 Connecting ports GTP1U_EM(12):TEID0 and mtc:TEID0.
13:44:05.464491 14325 C5G_Tests.ttcn:185 Port TEID0 is waiting for connection from GTP1U_EM(12):TEID0 on UNIX pathname /tmp/ttcn3-portconn-736ea674.
13:44:05.464830 14560 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
13:44:05.465164 14325 C5G_Tests.ttcn:185 Port TEID0 has accepted the connection from GTP1U_EM(12):TEID0.
13:44:05.465361 14325 C5G_Tests.ttcn:185 Connect operation on GTP1U_EM(12):TEID0 and mtc:TEID0 finished.
13:44:05.465454 14325 C5G_Tests.ttcn:186 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(12).
13:44:05.465715 14325 C5G_Tests.ttcn:186 Function was started.
13:44:05.465976 14560 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
13:44:05.465995 14325 C5G_Tests.ttcn:161 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
13:44:05.466687 14560 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 14.466679: srand48(-1051884989).
13:44:05.466774 14560 Osmocom_Types.ttcn:65 Function rnd() returned 0.298951.
13:44:05.466962 14560 Osmocom_Types.ttcn:65 Function rnd() returned 0.019449.
13:44:05.467192 14560 GTPv1U_Emulation.ttcnpp:214 Mapping port GTP1U_EM(12):UECUPS to system:UECUPS.
13:44:05.467387 14560 GTPv1U_Emulation.ttcnpp:214 Port UECUPS was mapped to system:UECUPS.
13:44:05.467578 14560 GTPv1U_Emulation.ttcnpp:214 Map operation of GTP1U_EM(12):UECUPS to system:UECUPS finished.
13:44:05.468318 14560 GTPv1U_Emulation.ttcnpp:215 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
13:44:05.468861 14560 GTPv1U_Emulation.ttcnpp:215 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
13:44:05.471837 14560 GTPv1U_Emulation.ttcnpp:190 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
13:44:05.472144 14560 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
13:44:05.472409 14560 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
13:44:05.472691 14560 GTPv1U_Emulation.ttcnpp:190 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
13:44:05.473133 14560 GTPv1U_Emulation.ttcnpp:191 Start timer T: 30 s
13:44:05.474028 14560 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
13:44:05.474279 14560 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
13:44:05.474517 14560 GTPv1U_Emulation.ttcnpp:194 Matching on port UECUPS succeeded:  matched
13:44:05.474601 14560 GTPv1U_Emulation.ttcnpp:194 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
13:44:05.474642 14561 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
13:44:05.474652 14560 GTPv1U_Emulation.ttcnpp:194 Message with id 1 was extracted from the queue of UECUPS.
13:44:05.474747 14561 - TTCN-3 Parallel Test Component started on e9423b37bbd0. Component reference: TC_periodic_registration_updating-NGAP0(13), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0. Version: 11.1.0.
13:44:05.474797 14561 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
13:44:05.474874 14560 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
13:44:05.474981 14560 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
13:44:05.475119 14561 - Connected to MC.
13:44:05.475172 14561 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_periodic_registration_updating.
13:44:05.475236 14560 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
13:44:05.475308 14325 C5G_Tests.ttcn:161 PTC was created. Component reference: 13, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
13:44:05.475355 14560 GTPv1U_Emulation.ttcnpp:192 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
13:44:05.475433 14325 C5G_Tests.ttcn:162 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
13:44:05.475512 14560 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS succeeded:  matched
13:44:05.475576 14560 GTPv1U_Emulation.ttcnpp:193 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
13:44:05.475623 14560 GTPv1U_Emulation.ttcnpp:193 Message with id 2 was extracted from the queue of UECUPS.
13:44:05.475747 14560 GTPv1U_Emulation.ttcnpp:225 Altstep as_uecups_ind was activated as default, id 1
13:44:05.478031 14561 - Port NGAP was started.
13:44:05.478104 14561 - Port NGAP_CLIENT was started.
13:44:05.478141 14561 - Port NGAP_PROC was started.
13:44:05.478176 14561 - Port NGAP_UNIT was started.
13:44:05.478210 14561 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
13:44:05.478319 14561 - Port NGAP was mapped to system:NGAP_CODEC_PT.
13:44:05.478426 14325 C5G_Tests.ttcn:162 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
13:44:05.478520 14325 C5G_Tests.ttcn:163 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0].
13:44:05.479094 14325 C5G_Tests.ttcn:163 Port NGAP_PROC[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-4256f519.
13:44:05.479274 14561 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
13:44:05.479561 14325 C5G_Tests.ttcn:163 Port NGAP_PROC[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
13:44:05.479667 14325 C5G_Tests.ttcn:163 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0] finished.
13:44:05.479724 14325 C5G_Tests.ttcn:164 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0].
13:44:05.480435 14325 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-534fec08.
13:44:05.480529 14561 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
13:44:05.480730 14325 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
13:44:05.480791 14325 C5G_Tests.ttcn:164 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
13:44:05.480841 14325 C5G_Tests.ttcn:165 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0") on component TC_periodic_registration_updating-NGAP0(13).
13:44:05.481007 14325 C5G_Tests.ttcn:165 Function was started.
13:44:05.481261 14561 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0").
13:44:05.483043 14561 NGAP_Emulation.ttcn:452 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
13:44:05.483191 14561 NGAP_Emulation.ttcn:452 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
13:44:05.483860 14561 NGAP_Emulation.ttcn:457 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
13:44:05.484304 14561 NGAP_Emulation.ttcn:457 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
13:44:05.485883 14561 NGAP_Emulation.ttcn:469 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
13:44:05.486048 14325 C5G_Tests.ttcn:166 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
13:44:05.486137 14325 C5G_Tests.ttcn:166 Matching on port NGAP_UNIT[0] succeeded:  matched
13:44:05.486177 14325 C5G_Tests.ttcn:166 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
13:44:05.486213 14325 C5G_Tests.ttcn:166 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
13:44:05.486559 14325 C5G_Tests.ttcn:268 Sent on NGAP_UNIT[0] to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
13:44:05.486631 14325 C5G_Tests.ttcn:269 Start timer T: 5 s
13:44:05.488203 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
13:44:05.490164 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
13:44:05.490439 14561 NGAP_Emulation.ttcn:542 Matching on port NGAP_UNIT succeeded:  matched
13:44:05.490497 14561 NGAP_Emulation.ttcn:542 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
13:44:05.490531 14561 NGAP_Emulation.ttcn:542 Message with id 1 was extracted from the queue of NGAP_UNIT.
13:44:05.492625 14561 NGAP_Emulation.ttcn:544 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.493209 14561 NGAP_Emulation.ttcn:544 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
13:44:05.493572 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
13:44:05.493626 14561 NGAP_Emulation.ttcn:600 Matching on port NGAP succeeded:  matched
13:44:05.493648 14561 NGAP_Emulation.ttcn:600 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
13:44:05.493663 14561 NGAP_Emulation.ttcn:600 Message with id 1 was extracted from the queue of NGAP.
13:44:05.493728 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
13:44:05.494617 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
13:44:05.494683 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.494704 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
13:44:05.494721 14561 NGAP_Emulation.ttcn:548 Message with id 2 was extracted from the queue of NGAP.
13:44:05.494796 14561 C5G_Tests.ttcn:128 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.495008 14325 C5G_Tests.ttcn:270 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
13:44:05.495036 14325 C5G_Tests.ttcn:271 Matching on port NGAP_UNIT[0] succeeded:  matched
13:44:05.495052 14325 C5G_Tests.ttcn:271 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
13:44:05.495068 14325 C5G_Tests.ttcn:271 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
13:44:05.495080 14325 C5G_Tests.ttcn:272 setverdict(pass): none -> pass
13:44:05.495122 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.447075.
13:44:05.495137 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.774472.
13:44:05.495148 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.113305.
13:44:05.495160 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.318835.
13:44:05.495171 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.402076.
13:44:05.495182 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.527690.
13:44:05.495193 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.640739.
13:44:05.495203 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.294521.
13:44:05.495214 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.378740.
13:44:05.495225 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.482089.
13:44:05.495236 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.641276.
13:44:05.495247 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.511270.
13:44:05.495258 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.454016.
13:44:05.495269 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.574276.
13:44:05.495280 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.731992.
13:44:05.495291 14325 Osmocom_Types.ttcn:65 Function rnd() returned 0.386037.
13:44:05.495326 14325 C5G_Tests.ttcn:216 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
13:44:05.497583 14562 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
13:44:05.497614 14562 - TTCN-3 Parallel Test Component started on e9423b37bbd0. Component reference: TC_periodic_registration_updating0(14), component type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0. Version: 11.1.0.
13:44:05.497630 14562 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
13:44:05.497673 14562 - Connected to MC.
13:44:05.497687 14562 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_periodic_registration_updating.
13:44:05.497697 14325 C5G_Tests.ttcn:216 PTC was created. Component reference: 14, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
13:44:05.497711 14325 C5G_Tests.ttcn:218 Connecting ports TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
13:44:05.497880 14561 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT is waiting for connection from TC_periodic_registration_updating0(14):NGAP on UNIX pathname /tmp/ttcn3-portconn-1273a15c.
13:44:05.498609 14562 - Port NGAP was started.
13:44:05.498630 14562 - Port NGAP_PROC was started.
13:44:05.498640 14562 - Port GTP1U[0] was started.
13:44:05.498650 14562 - Port GTP1U[1] was started.
13:44:05.498660 14562 - Port GTP1U[2] was started.
13:44:05.498670 14562 - Port GTP1U[3] was started.
13:44:05.498679 14562 - Port GTP1U_PROC[0] was started.
13:44:05.498689 14562 - Port GTP1U_PROC[1] was started.
13:44:05.498699 14562 - Port GTP1U_PROC[2] was started.
13:44:05.498709 14562 - Port GTP1U_PROC[3] was started.
13:44:05.498719 14562 - Component type ConnHdlr.ConnHdlr was initialized.
13:44:05.498752 14562 - Port NGAP has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT using transport type UNIX.
13:44:05.498799 14561 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT has accepted the connection from TC_periodic_registration_updating0(14):NGAP.
13:44:05.498806 14325 C5G_Tests.ttcn:218 Connect operation on TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT finished.
13:44:05.498819 14325 C5G_Tests.ttcn:219 Connecting ports TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
13:44:05.498959 14561 NGAP_Emulation.ttcn:485 Port NGAP_PROC is waiting for connection from TC_periodic_registration_updating0(14):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-869ae15.
13:44:05.498979 14562 - Port NGAP_PROC has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_PROC using transport type UNIX.
13:44:05.499021 14561 NGAP_Emulation.ttcn:485 Port NGAP_PROC has accepted the connection from TC_periodic_registration_updating0(14):NGAP_PROC.
13:44:05.499027 14325 C5G_Tests.ttcn:219 Connect operation on TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC finished.
13:44:05.499040 14325 C5G_Tests.ttcn:222 Connecting ports TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT.
13:44:05.499201 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT is waiting for connection from TC_periodic_registration_updating0(14):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-132bd238.
13:44:05.499219 14562 - Port GTP1U[0] has established the connection with GTP1U_EM(12):CLIENT using transport type UNIX.
13:44:05.499276 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT has accepted the connection from TC_periodic_registration_updating0(14):GTP1U[0].
13:44:05.499282 14325 C5G_Tests.ttcn:222 Connect operation on TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT finished.
13:44:05.499292 14325 C5G_Tests.ttcn:223 Connecting ports TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
13:44:05.499428 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC is waiting for connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-5170a655.
13:44:05.499450 14562 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(12):CLIENT_PROC using transport type UNIX.
13:44:05.499491 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC has accepted the connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
13:44:05.499497 14325 C5G_Tests.ttcn:223 Connect operation on TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC finished.
13:44:05.499506 14325 C5G_Tests.ttcn:227 Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '4713456234654573'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}) on component TC_periodic_registration_updating0(14).
13:44:05.499551 14325 C5G_Tests.ttcn:227 Function was started.
13:44:05.500102 14562 - Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '4713456234654573'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}).
13:44:05.501921 14562 ConnHdlr.ttcn:639 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
13:44:05.502216 14562 ConnHdlr.ttcn:639 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
13:44:05.504293 14562 ConnHdlr.ttcn:644 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
13:44:05.504968 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
13:44:05.505022 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.505041 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.505056 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.505071 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.505229 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.505261 14561 NGAP_Emulation.ttcn:513 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
13:44:05.505280 14561 NGAP_Emulation.ttcn:513 Message with id 1 was extracted from the queue of NGAP_CLIENT.
13:44:05.506178 14561 NGAP_Emulation.ttcn:519 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.506417 14561 NGAP_Emulation.ttcn:519 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
13:44:05.508157 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403E000003000A000200020055000200000026002B2A7E0056020200002101B5CAC8406A5D71FE5A9DB64E776376201091A1D720B54780002599600FCDE5D009'O
} id 3
13:44:05.508500 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002101B5CAC8406A5D71FE5A9DB64E776376201091A1D720B54780002599600FCDE5D009'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
13:44:05.508542 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.508567 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002101B5CAC8406A5D71FE5A9DB64E776376201091A1D720B54780002599600FCDE5D009'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
13:44:05.508589 14561 NGAP_Emulation.ttcn:548 Message with id 3 was extracted from the queue of NGAP.
13:44:05.508746 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0056020200002101B5CAC8406A5D71FE5A9DB64E776376201091A1D720B54780002599600FCDE5D009'O
13:44:05.509250 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '00000001101101011100101011001000010000000110101001011101011100011111111001011010100111011011011001001110011101110110001101110110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10010001101000011101011100100000101101010100011110000000000000000010010110011001011000000000111111001101111001011101000000001001'B
        },
        eapMessage := omit
    }
}
13:44:05.509477 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '00000001101101011100101011001000010000000110101001011101011100011111111001011010100111011011011001001110011101110110001101110110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10010001101000011101011100100000101101010100011110000000000000000010010110011001011000000000111111001101111001011101000000001001'B
        },
        eapMessage := omit
    }
}
13:44:05.509706 14562 ConnHdlr.ttcn:656 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '00000001101101011100101011001000010000000110101001011101011100011111111001011010100111011011011001001110011101110110001101110110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10010001101000011101011100100000101101010100011110000000000000000010010110011001011000000000111111001101111001011101000000001001'B
        },
        eapMessage := omit
    }
} id 1
13:44:05.509892 14562 ConnHdlr.ttcn:209 Matching on port NGAP succeeded:  matched
13:44:05.509928 14562 ConnHdlr.ttcn:209 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '00000001101101011100101011001000010000000110101001011101011100011111111001011010100111011011011001001110011101110110001101110110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10010001101000011101011100100000101101010100011110000000000000000010010110011001011000000000111111001101111001011101000000001001'B
        },
        eapMessage := omit
    }
} id 1
13:44:05.509951 14562 ConnHdlr.ttcn:209 Message with id 1 was extracted from the queue of NGAP.
13:44:05.511376 14562 ConnHdlr.ttcn:254 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '9DDC7ADF8A5B8A9E130CBFA342ADAAC85A928F4495C7A8EE63682C98F573E87D'O,
        k_nas_enc := 'C91CE78BE57520EA3F8A89827BF46AA2AC91168F1C252604F6487BB040385ADD'O
    }
}
13:44:05.511460 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '9DDC7ADF8A5B8A9E130CBFA342ADAAC85A928F4495C7A8EE63682C98F573E87D'O,
        k_nas_enc := 'C91CE78BE57520EA3F8A89827BF46AA2AC91168F1C252604F6487BB040385ADD'O
    }
} id 2
13:44:05.511507 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.511520 14562 ConnHdlr.ttcn:258 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '11110010111100000010110001100000001000101010000100111111100100110000111111010000001001001100111110100011011101100101011100111010'B
        },
        eapMessage := omit
    }
}
13:44:05.511525 14561 NGAP_Emulation.ttcn:487 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := '9DDC7ADF8A5B8A9E130CBFA342ADAAC85A928F4495C7A8EE63682C98F573E87D'O,
        k_nas_enc := 'C91CE78BE57520EA3F8A89827BF46AA2AC91168F1C252604F6487BB040385ADD'O
    }
} id 2
13:44:05.511540 14561 NGAP_Emulation.ttcn:487 Message with id 2 was extracted from the queue of NGAP_CLIENT.
13:44:05.511671 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '11110010111100000010110001100000001000101010000100111111100100110000111111010000001001001100111110100011011101100101011100111010'B
        },
        eapMessage := omit
    }
} id 3
13:44:05.511747 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.511764 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.511778 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.511791 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.511813 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.511849 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.511868 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '11110010111100000010110001100000001000101010000100111111100100110000111111010000001001001100111110100011011101100101011100111010'B
        },
        eapMessage := omit
    }
} id 3
13:44:05.511887 14561 NGAP_Emulation.ttcn:522 Message with id 3 was extracted from the queue of NGAP_CLIENT.
13:44:05.511933 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '11110010111100000010110001100000001000101010000100111111100100110000111111010000001001001100111110100011011101100101011100111010'B
        },
        eapMessage := omit
    }
}
13:44:05.512071 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D10F2F02C6022A13F930FD024CFA376573A'O
13:44:05.512627 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D10F2F02C6022A13F930FD024CFA376573A'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.512712 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403C000004000A0002000200550002000000260016157E00572D10F2F02C6022A13F930FD024CFA376573A0079400F4099F907000000000099F907000001'O
}
13:44:05.515490 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044027000003000A0002000200550002000000260014137E0352344613007E005D0102028040E1360102'O
} id 4
13:44:05.515565 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0352344613007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
13:44:05.515605 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.515625 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0352344613007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
13:44:05.515649 14561 NGAP_Emulation.ttcn:548 Message with id 4 was extracted from the queue of NGAP.
13:44:05.515670 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0352344613007E005D0102028040E1360102'O
13:44:05.515701 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := '52344613'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0102028040E1360102'O
    }
}
13:44:05.516097 14561 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0102028040E1360102'O
13:44:05.516279 14561 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
13:44:05.516451 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
13:44:05.516623 14562 ConnHdlr.ttcn:657 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
13:44:05.516804 14562 ConnHdlr.ttcn:270 Matching on port NGAP succeeded:  matched
13:44:05.516834 14562 ConnHdlr.ttcn:270 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
13:44:05.516856 14562 ConnHdlr.ttcn:270 Message with id 2 was extracted from the queue of NGAP.
13:44:05.516897 14562 ConnHdlr.ttcn:275 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
13:44:05.516935 14562 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
13:44:05.516945 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
13:44:05.516995 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
13:44:05.517018 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
13:44:05.517040 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.517057 14561 NGAP_Emulation.ttcn:499 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
13:44:05.517074 14561 NGAP_Emulation.ttcn:499 Message with id 4 was extracted from the queue of NGAP_CLIENT.
13:44:05.517087 14562 ConnHdlr.ttcn:290 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
13:44:05.517122 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
13:44:05.517142 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
13:44:05.517156 14562 ConnHdlr.ttcn:290 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004129000D0199F9072143000100000000002E028040'O
13:44:05.517158 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
13:44:05.517190 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
13:44:05.517211 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.517227 14561 NGAP_Emulation.ttcn:506 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
13:44:05.517243 14561 NGAP_Emulation.ttcn:506 Message with id 5 was extracted from the queue of NGAP_CLIENT.
13:44:05.517289 14562 ConnHdlr.ttcn:291 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '4713456234654573'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
13:44:05.517387 14562 NGAP_Emulation.ttcn:717 Called on NGAP_PROC to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
13:44:05.517440 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '4713456234654573'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
13:44:05.517495 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.517512 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.517528 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.517542 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.517561 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.517581 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.517602 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '4713456234654573'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
13:44:05.517619 14561 NGAP_Emulation.ttcn:522 Message with id 6 was extracted from the queue of NGAP_CLIENT.
13:44:05.517653 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '4713456234654573'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
13:44:05.517722 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090547134562346545737100177E004129000D0199F9072143000100000000002E028040'O
13:44:05.517978 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '6567DA35'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090547134562346545737100177E004129000D0199F9072143000100000000002E028040'O
    }
}
13:44:05.518008 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E046567DA35007E005E7700090547134562346545737100177E004129000D0199F9072143000100000000002E028040'O
13:44:05.518089 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E046567DA35007E005E7700090547134562346545737100177E004129000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.518137 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4057000004000A0002000200550002000000260031307E046567DA35007E005E7700090547134562346545737100177E004129000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
13:44:05.518225 14561 NGAP_Emulation.ttcn:485 Call enqueued on NGAP_PROC from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
13:44:05.518254 14561 NGAP_Emulation.ttcn:602 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
13:44:05.518270 14561 NGAP_Emulation.ttcn:606 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
13:44:05.518287 14561 NGAP_Emulation.ttcn:610 Matching on port NGAP_PROC succeeded: { } with { } matched
13:44:05.518331 14561 NGAP_Emulation.ttcn:610 Getcall operation on port NGAP_PROC succeeded, call from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
13:44:05.518350 14561 NGAP_Emulation.ttcn:610 Operation with id 1 was extracted from the queue of NGAP_PROC.
13:44:05.518377 14561 NGAP_Emulation.ttcn:613 Replied on NGAP_PROC to TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2
13:44:05.518446 14562 NGAP_Emulation.ttcn:717 Reply enqueued on NGAP_PROC from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
13:44:05.518528 14562 NGAP_Emulation.ttcn:718 Matching on port NGAP_PROC succeeded: { } with { } matched value 2 with ? matched
13:44:05.518579 14562 NGAP_Emulation.ttcn:718 Getreply operation on port NGAP_PROC succeeded, reply from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
13:44:05.518618 14562 NGAP_Emulation.ttcn:718 Operation with id 1 was extracted from the queue of NGAP_PROC.
13:44:05.524597 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044056000005000A000200020055000200000026002F2E7E022F2DE03B017E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
13:44:05.525386 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E022F2DE03B017E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
13:44:05.525476 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.525510 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E022F2DE03B017E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
13:44:05.525533 14561 NGAP_Emulation.ttcn:548 Message with id 5 was extracted from the queue of NGAP.
13:44:05.525562 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E022F2DE03B017E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192'O
13:44:05.525602 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '2F2DE03B'O,
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192'O
    }
}
13:44:05.525827 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000026C54074099F90700000115020101210201005E0192'O
13:44:05.526466 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
13:44:05.526940 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
13:44:05.527391 14562 ConnHdlr.ttcn:662 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
13:44:05.527768 14562 ConnHdlr.ttcn:662 Matching on port NGAP succeeded:  matched
13:44:05.527809 14562 ConnHdlr.ttcn:662 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
13:44:05.527834 14562 ConnHdlr.ttcn:662 Message with id 3 was extracted from the queue of NGAP.
13:44:05.527903 14562 ConnHdlr.ttcn:664 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
13:44:05.527954 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
13:44:05.527988 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.528003 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.528018 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.528032 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.528051 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.528069 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.528088 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
13:44:05.528106 14561 NGAP_Emulation.ttcn:522 Message with id 7 was extracted from the queue of NGAP_CLIENT.
13:44:05.528137 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
13:44:05.528165 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
13:44:05.528322 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '80DAD221'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
13:44:05.528346 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0280DAD221007E0043'O
13:44:05.528441 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0280DAD221007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.528497 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0280DAD221007E00430079400F4099F907000000000099F907000001'O
}
13:44:05.528878 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E02035DC40B027E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
} id 6
13:44:05.528943 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02035DC40B027E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
13:44:05.528972 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.528993 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02035DC40B027E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
13:44:05.529009 14561 NGAP_Emulation.ttcn:548 Message with id 6 was extracted from the queue of NGAP.
13:44:05.529030 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02035DC40B027E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
13:44:05.529053 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '035DC40B'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
    }
}
13:44:05.529230 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
13:44:05.529409 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
13:44:05.529589 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
13:44:05.529722 14562 ConnHdlr.ttcn:666 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
13:44:05.529870 14562 ConnHdlr.ttcn:299 Matching on port NGAP succeeded:  matched
13:44:05.529896 14562 ConnHdlr.ttcn:299 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
13:44:05.529914 14562 ConnHdlr.ttcn:299 Message with id 4 was extracted from the queue of NGAP.
13:44:05.529948 14562 ConnHdlr.ttcn:300 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
13:44:05.529990 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
13:44:05.530016 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530030 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530043 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530056 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530073 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.530088 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.530104 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
13:44:05.530119 14561 NGAP_Emulation.ttcn:522 Message with id 8 was extracted from the queue of NGAP_CLIENT.
13:44:05.530141 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
13:44:05.530148 14562 ConnHdlr.ttcn:678 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
13:44:05.530164 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
13:44:05.530311 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '76BD0019'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
13:44:05.530335 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0276BD0019007E0055'O
13:44:05.530398 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0276BD0019007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.530439 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0276BD0019007E00550079400F4099F907000000000099F907000001'O
}
13:44:05.530657 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
13:44:05.530801 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530819 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530833 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530846 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.530865 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.530888 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.530921 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
13:44:05.530939 14561 NGAP_Emulation.ttcn:522 Message with id 9 was extracted from the queue of NGAP_CLIENT.
13:44:05.530960 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000026C'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
13:44:05.531025 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00412B000BF299F907020040C000026C2E028040'O
13:44:05.531143 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'D78A87B2'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E00412B000BF299F907020040C000026C2E028040'O
    }
}
13:44:05.531158 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02D78A87B2007E00412B000BF299F907020040C000026C2E028040'O
13:44:05.531205 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02D78A87B2007E00412B000BF299F907020040C000026C2E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.531236 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4043000004000A000200020055000200000026001D1C7E02D78A87B2007E00412B000BF299F907020040C000026C2E0280400079400F4099F907000000000099F907000001'O
}
13:44:05.740244 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000004000A000200020055000200000026002F2E7E0296F70E81037E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192000000020001'O
} id 7
13:44:05.740824 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0296F70E81037E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
13:44:05.741131 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.741275 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0296F70E81037E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
13:44:05.741380 14561 NGAP_Emulation.ttcn:548 Message with id 7 was extracted from the queue of NGAP.
13:44:05.741512 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0296F70E81037E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192'O
13:44:05.741616 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '96F70E81'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192'O
    }
}
13:44:05.742412 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C00000EC54074099F90700000115020101210201005E0192'O
13:44:05.742786 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
13:44:05.743156 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
13:44:05.743688 14562 ConnHdlr.ttcn:690 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
13:44:05.744254 14562 ConnHdlr.ttcn:690 Matching on port NGAP succeeded:  matched
13:44:05.744436 14562 ConnHdlr.ttcn:690 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
13:44:05.744560 14562 ConnHdlr.ttcn:690 Message with id 5 was extracted from the queue of NGAP.
13:44:05.744696 14562 ConnHdlr.ttcn:692 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
13:44:05.744832 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
13:44:05.744917 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.744973 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.745026 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.745076 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.745139 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.745203 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.745265 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
13:44:05.745325 14561 NGAP_Emulation.ttcn:522 Message with id 10 was extracted from the queue of NGAP_CLIENT.
13:44:05.745418 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
13:44:05.745506 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
13:44:05.746132 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '80DAD221'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
13:44:05.746207 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0280DAD221007E0043'O
13:44:05.746514 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0280DAD221007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.746698 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0280DAD221007E00430079400F4099F907000000000099F907000001'O
}
13:44:05.748238 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E028CC60094047E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
} id 8
13:44:05.748435 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E028CC60094047E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
13:44:05.748544 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.748622 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E028CC60094047E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
13:44:05.748687 14561 NGAP_Emulation.ttcn:548 Message with id 8 was extracted from the queue of NGAP.
13:44:05.748765 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E028CC60094047E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
13:44:05.748852 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '8CC60094'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
    }
}
13:44:05.749604 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004762203031445000490100'O
13:44:05.749878 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
13:44:05.750124 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
13:44:05.750362 14562 ConnHdlr.ttcn:694 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
13:44:05.750590 14562 ConnHdlr.ttcn:299 Matching on port NGAP succeeded:  matched
13:44:05.750686 14562 ConnHdlr.ttcn:299 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '62'O ("b"),
            month := '20'O (" "),
            day := '30'O ("0"),
            hour := '31'O ("1"),
            minute := '44'O ("D"),
            second := '50'O ("P"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
13:44:05.750757 14562 ConnHdlr.ttcn:299 Message with id 6 was extracted from the queue of NGAP.
13:44:05.750835 14562 ConnHdlr.ttcn:300 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
13:44:05.750949 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
13:44:05.751043 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.751099 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.751152 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.751203 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.751267 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.751326 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.751388 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
13:44:05.751460 14561 NGAP_Emulation.ttcn:522 Message with id 11 was extracted from the queue of NGAP_CLIENT.
13:44:05.751493 14562 ConnHdlr.ttcn:766 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        }
    }
}
13:44:05.751545 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
13:44:05.751630 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
13:44:05.752235 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '76BD0019'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
13:44:05.752314 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0276BD0019007E0055'O
13:44:05.752547 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0276BD0019007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.752708 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0276BD0019007E00550079400F4099F907000000000099F907000001'O
}
13:44:05.753044 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        }
    }
} id 12
13:44:05.753186 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.753293 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.753338 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.753381 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.753437 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
13:44:05.753491 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.753549 14561 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        }
    }
} id 12
13:44:05.753605 14561 NGAP_Emulation.ttcn:522 Message with id 12 was extracted from the queue of NGAP_CLIENT.
13:44:05.753666 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00000EC'O
        }
    }
}
13:44:05.753784 14561 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C00000EC'O
13:44:05.754378 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '75983C03'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C00000EC'O
    }
}
13:44:05.754445 14561 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0275983C03007E004531000BF299F907020040C00000EC'O
13:44:05.754620 14561 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0275983C03007E004531000BF299F907020040C00000EC'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.754749 14561 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403F000004000A0002000200550002000000260019187E0275983C03007E004531000BF299F907020040C00000EC0079400F4099F907000000000099F907000001'O
}
13:44:05.969326 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401E000003000A000200020055000200000026000B0A7E0227ED183B057E0046'O
} id 9
13:44:05.969738 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0227ED183B057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
13:44:05.969952 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.970031 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0227ED183B057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
13:44:05.970095 14561 NGAP_Emulation.ttcn:548 Message with id 9 was extracted from the queue of NGAP.
13:44:05.970179 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0227ED183B057E0046'O
13:44:05.970269 14561 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '27ED183B'O,
        sequenceNumber := '05'O,
        plainNASMessage := '7E0046'O
    }
}
13:44:05.971104 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
13:44:05.971257 14561 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
13:44:05.971404 14561 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
13:44:05.971612 14562 ConnHdlr.ttcn:768 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
13:44:05.971783 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900100000020072000400020000000F400148'O
} id 10
13:44:05.971895 14562 ConnHdlr.ttcn:768 Matching on port NGAP succeeded:  matched
13:44:05.971976 14562 ConnHdlr.ttcn:768 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
13:44:05.972043 14562 ConnHdlr.ttcn:768 Message with id 7 was extracted from the queue of NGAP.
13:44:05.973191 14561 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
13:44:05.973326 14561 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
13:44:05.973407 14561 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
13:44:05.973493 14561 NGAP_Emulation.ttcn:548 Message with id 10 was extracted from the queue of NGAP.
13:44:05.973721 14561 NGAP_Emulation.ttcn:587 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.975468 14562 ConnHdlr.ttcn:769 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
13:44:05.976541 14562 ConnHdlr.ttcn:782 Matching on port NGAP succeeded:  matched
13:44:05.976636 14562 ConnHdlr.ttcn:782 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
13:44:05.976703 14562 ConnHdlr.ttcn:782 Message with id 8 was extracted from the queue of NGAP.
13:44:05.979335 14562 ConnHdlr.ttcn:783 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.979862 14562 - Function f_init_handler finished. PTC terminates.
13:44:05.979937 14562 - Terminating component type ConnHdlr.ConnHdlr.
13:44:05.979993 14562 - Removing unterminated connection between port NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
13:44:05.980094 14562 - Port NGAP was stopped.
13:44:05.980108 14561 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
13:44:05.980151 14562 - Removing unterminated connection between port NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
13:44:05.980224 14562 - Port NGAP_PROC was stopped.
13:44:05.980276 14562 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(12):CLIENT.
13:44:05.980294 14561 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.980345 14562 - Port GTP1U[0] was stopped.
13:44:05.980348 14561 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.980392 14560 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT to TC_periodic_registration_updating0(14):GTP1U[0] was closed unexpectedly by the peer.
13:44:05.980398 14562 - Port GTP1U[1] was stopped.
13:44:05.980410 14561 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.980449 14562 - Port GTP1U[2] was stopped.
13:44:05.980463 14561 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
13:44:05.980507 14562 - Port GTP1U[3] was stopped.
13:44:05.980535 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT was disconnected from TC_periodic_registration_updating0(14):GTP1U[0].
13:44:05.980558 14562 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
13:44:05.980631 14562 - Port GTP1U_PROC[0] was stopped.
13:44:05.980705 14560 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT_PROC to TC_periodic_registration_updating0(14):GTP1U_PROC[0] was closed unexpectedly by the peer.
13:44:05.980811 14562 - Port GTP1U_PROC[1] was stopped.
13:44:05.980832 14560 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC was disconnected from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
13:44:05.980866 14562 - Port GTP1U_PROC[2] was stopped.
13:44:05.980917 14562 - Port GTP1U_PROC[3] was stopped.
13:44:05.981006 14562 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_periodic_registration_updating.
13:44:05.981067 14562 - Final verdict of PTC: none
13:44:05.981068 14561 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
13:44:05.981158 14325 C5G_Tests.ttcn:331 PTC with component reference 14 is done.
13:44:05.981160 14561 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
13:44:05.981220 14561 NGAP_Emulation.ttcn:535 Matching on port NGAP_CLIENT succeeded:  matched
13:44:05.981245 14562 - Disconnected from MC.
13:44:05.981295 14562 - TTCN-3 Parallel Test Component finished.
13:44:05.981316 14561 NGAP_Emulation.ttcn:535 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
13:44:05.981317 14325 C5G_Tests.ttcn:331 Terminating component type C5G_Tests.MTC_CT.
13:44:05.981379 14561 NGAP_Emulation.ttcn:535 Message with id 13 was extracted from the queue of NGAP_CLIENT.
13:44:05.981388 14325 C5G_Tests.ttcn:331 Default with id 1 (altstep as_Tguard) was deactivated.
13:44:05.981459 14325 C5G_Tests.ttcn:331 Stop timer g_Tguard: 30 s
13:44:05.981734 14325 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_UNIT[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
13:44:05.981941 14325 C5G_Tests.ttcn:331 Port NGAP_UNIT[0] was stopped.
13:44:05.982121 14325 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_PROC[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
13:44:05.982241 14325 C5G_Tests.ttcn:331 Port NGAP_PROC[0] was stopped.
13:44:05.982406 14325 C5G_Tests.ttcn:331 Removing unterminated connection between port TEID0 and GTP1U_EM(12):TEID0.
13:44:05.982705 14325 C5G_Tests.ttcn:331 Port TEID0 was stopped.
13:44:05.982712 14560 GTPv1U_Emulation.ttcnpp:265 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
13:44:05.982842 14560 GTPv1U_Emulation.ttcnpp:265 Port TEID0 was disconnected from mtc:TEID0.
13:44:05.982856 14561 NGAP_Emulation.ttcn:538 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
13:44:05.982882 14325 C5G_Tests.ttcn:331 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_periodic_registration_updating.
13:44:05.982976 14325 C5G_Tests.ttcn:331 Waiting for PTCs to finish.
13:44:05.983112 14560 GTPv1U_Emulation.ttcnpp:265 Kill was requested from MC.
13:44:05.983159 14561 NGAP_Emulation.ttcn:538 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290022000003000A400200020055400200000079400F4099F907000000000099F907000001'O
}
13:44:05.983166 14560 GTPv1U_Emulation.ttcnpp:265 Terminating test component execution.
13:44:05.983634 14561 NGAP_Emulation.ttcn:485 Connection of port NGAP_CLIENT to TC_periodic_registration_updating0(14):NGAP was closed unexpectedly by the peer.
13:44:05.983706 14561 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT was disconnected from TC_periodic_registration_updating0(14):NGAP.
13:44:05.983803 14561 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to TC_periodic_registration_updating0(14):NGAP_PROC was closed unexpectedly by the peer.
13:44:05.983871 14561 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from TC_periodic_registration_updating0(14):NGAP_PROC.
13:44:05.983941 14561 NGAP_Emulation.ttcn:485 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
13:44:05.984005 14561 NGAP_Emulation.ttcn:485 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
13:44:05.984068 14561 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
13:44:05.984112 14561 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
13:44:05.984153 14560 - Function main was stopped. PTC terminates.
13:44:05.984174 14561 NGAP_Emulation.ttcn:485 Kill was requested from MC.
13:44:05.984217 14561 NGAP_Emulation.ttcn:485 Terminating test component execution.
13:44:05.984262 14560 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
13:44:05.984353 14560 - Default with id 1 (altstep as_uecups_ind) was deactivated.
13:44:05.984427 14560 - Removing unterminated mapping between port GTP1U and system:GTP1U.
13:44:05.984516 14560 - Port GTP1U was unmapped from system:GTP1U.
13:44:05.984573 14560 - Port GTP1U was stopped.
13:44:05.984617 14560 - Port TEID0 was stopped.
13:44:05.984656 14560 - Port CLIENT was stopped.
13:44:05.984694 14560 - Port CLIENT_PROC was stopped.
13:44:05.984733 14560 - Removing unterminated mapping between port UECUPS and system:UECUPS.
13:44:05.984978 14561 - Function main was stopped. PTC terminates.
13:44:05.985126 14561 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
13:44:05.985241 14561 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
13:44:05.985260 14560 - Port UECUPS was unmapped from system:UECUPS.
13:44:05.985357 14560 - Port UECUPS was stopped.
13:44:05.985427 14560 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
13:44:05.985487 14560 - Final verdict of PTC: none
13:44:05.985630 14560 - Disconnected from MC.
13:44:05.985682 14560 - TTCN-3 Parallel Test Component finished.
13:44:05.985750 14561 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
13:44:05.985849 14561 - Port NGAP was stopped.
13:44:05.985902 14561 - Port NGAP_CLIENT was stopped.
13:44:05.985958 14561 - Port NGAP_PROC was stopped.
13:44:05.986005 14561 - Port NGAP_UNIT was stopped.
13:44:05.986049 14561 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
13:44:05.986102 14561 - Final verdict of PTC: none
13:44:05.986227 14561 - Disconnected from MC.
13:44:05.986264 14325 C5G_Tests.ttcn:331 Setting final verdict of the test case.
13:44:05.986289 14561 - TTCN-3 Parallel Test Component finished.
13:44:05.986422 14325 C5G_Tests.ttcn:331 Local verdict of MTC: pass
13:44:05.986539 14325 C5G_Tests.ttcn:331 Local verdict of PTC GTP1U_EM(12): none (pass -> pass)
13:44:05.986690 14325 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating-NGAP0(13): none (pass -> pass)
13:44:05.986792 14325 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating0(14): none (pass -> pass)
13:44:05.986896 14325 C5G_Tests.ttcn:331 Test case TC_periodic_registration_updating finished. Verdict: pass
13:44:05.987002 14325 C5G_Tests.ttcn:331 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs-latest/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass'.
13:44:08.044764 14325 C5G_Tests.ttcn:331 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs-latest/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass' was executed successfully (exit status: 0).
13:44:08.044876 14325 C5G_Tests.ttcn:339 Switching to log file `C5G_Tests-TC_ue_context_release_no_pdu_session-e9423b37bbd0-mtc-14325.log'
