09:30:15.443508 13836 C5G_Tests.ttcn:324 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating'.
09:30:16.478223 13836 C5G_Tests.ttcn:324 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating' was executed successfully (exit status: 0).
09:30:16.478805 13836 C5G_Tests.ttcn:324 Test case TC_periodic_registration_updating started.
09:30:16.479152 13836 C5G_Tests.ttcn:324 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_periodic_registration_updating.
09:30:16.479525 13836 C5G_Tests.ttcn:324 Port NGAP_UNIT[0] was started.
09:30:16.479631 13836 C5G_Tests.ttcn:324 Port NGAP_PROC[0] was started.
09:30:16.479720 13836 C5G_Tests.ttcn:324 Port TEID0 was started.
09:30:16.480083 13836 C5G_Tests.ttcn:324 Component type C5G_Tests.MTC_CT was initialized.
09:30:16.480203 13836 C5G_Tests.ttcn:191 Start timer g_Tguard: 30 s
09:30:16.480275 13836 C5G_Tests.ttcn:192 Altstep as_Tguard was activated as default, id 1
09:30:16.480337 13836 C5G_Tests.ttcn:183 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:30:16.489291 14071 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:16.489487 14071 - TTCN-3 Parallel Test Component started on 81fd22231848. Component reference: GTP1U_EM(12), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
09:30:16.489596 14071 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:16.489848 14071 - Connected to MC.
09:30:16.489952 14071 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_periodic_registration_updating.
09:30:16.490085 13836 C5G_Tests.ttcn:183 PTC was created. Component reference: 12, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:30:16.490180 13836 C5G_Tests.ttcn:184 Mapping port GTP1U_EM(12):GTP1U to system:GTP1U.
09:30:16.493670 14071 - Port GTP1U was started.
09:30:16.493765 14071 - Port TEID0 was started.
09:30:16.493813 14071 - Port CLIENT was started.
09:30:16.493860 14071 - Port CLIENT_PROC was started.
09:30:16.493906 14071 - Port UECUPS was started.
09:30:16.493952 14071 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
09:30:16.494093 14071 - Port GTP1U was mapped to system:GTP1U.
09:30:16.494287 13836 C5G_Tests.ttcn:184 Map operation of GTP1U_EM(12):GTP1U to system:GTP1U finished.
09:30:16.494353 13836 C5G_Tests.ttcn:185 Connecting ports GTP1U_EM(12):TEID0 and mtc:TEID0.
09:30:16.494918 13836 C5G_Tests.ttcn:185 Port TEID0 is waiting for connection from GTP1U_EM(12):TEID0 on UNIX pathname /tmp/ttcn3-portconn-8a6fa674.
09:30:16.495109 14071 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
09:30:16.495209 13836 C5G_Tests.ttcn:185 Port TEID0 has accepted the connection from GTP1U_EM(12):TEID0.
09:30:16.495320 13836 C5G_Tests.ttcn:185 Connect operation on GTP1U_EM(12):TEID0 and mtc:TEID0 finished.
09:30:16.495377 13836 C5G_Tests.ttcn:186 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(12).
09:30:16.495568 13836 C5G_Tests.ttcn:186 Function was started.
09:30:16.495825 13836 C5G_Tests.ttcn:161 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:30:16.495875 14071 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
09:30:16.496693 14071 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 14.496685: srand48(-1282480293).
09:30:16.496789 14071 Osmocom_Types.ttcn:65 Function rnd() returned 0.208308.
09:30:16.497004 14071 Osmocom_Types.ttcn:65 Function rnd() returned 0.721680.
09:30:16.497288 14071 GTPv1U_Emulation.ttcnpp:214 Mapping port GTP1U_EM(12):UECUPS to system:UECUPS.
09:30:16.497478 14071 GTPv1U_Emulation.ttcnpp:214 Port UECUPS was mapped to system:UECUPS.
09:30:16.497654 14071 GTPv1U_Emulation.ttcnpp:214 Map operation of GTP1U_EM(12):UECUPS to system:UECUPS finished.
09:30:16.498505 14071 GTPv1U_Emulation.ttcnpp:215 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
09:30:16.499122 14071 GTPv1U_Emulation.ttcnpp:215 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:30:16.502407 14071 GTPv1U_Emulation.ttcnpp:190 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
09:30:16.502739 14071 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
09:30:16.503037 14071 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
09:30:16.503375 14071 GTPv1U_Emulation.ttcnpp:190 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
09:30:16.503909 14071 GTPv1U_Emulation.ttcnpp:191 Start timer T: 30 s
09:30:16.504032 14072 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:16.504178 14072 - TTCN-3 Parallel Test Component started on 81fd22231848. Component reference: TC_periodic_registration_updating-NGAP0(13), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0. Version: 11.1.0.
09:30:16.504249 14072 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:16.504415 14072 - Connected to MC.
09:30:16.504470 14072 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_periodic_registration_updating.
09:30:16.504623 13836 C5G_Tests.ttcn:161 PTC was created. Component reference: 13, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:30:16.504736 13836 C5G_Tests.ttcn:162 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:30:16.505018 14071 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:16.505407 14071 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
09:30:16.505679 14071 GTPv1U_Emulation.ttcnpp:194 Matching on port UECUPS succeeded:  matched
09:30:16.505843 14071 GTPv1U_Emulation.ttcnpp:194 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:16.506015 14071 GTPv1U_Emulation.ttcnpp:194 Message with id 1 was extracted from the queue of UECUPS.
09:30:16.506366 14071 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
09:30:16.506563 14071 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
09:30:16.506916 14071 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
09:30:16.507049 14071 GTPv1U_Emulation.ttcnpp:192 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:30:16.507221 14071 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS succeeded:  matched
09:30:16.507283 14071 GTPv1U_Emulation.ttcnpp:193 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:30:16.507336 14071 GTPv1U_Emulation.ttcnpp:193 Message with id 2 was extracted from the queue of UECUPS.
09:30:16.507467 14071 GTPv1U_Emulation.ttcnpp:225 Altstep as_uecups_ind was activated as default, id 1
09:30:16.507677 14072 - Port NGAP was started.
09:30:16.507747 14072 - Port NGAP_CLIENT was started.
09:30:16.507785 14072 - Port NGAP_PROC was started.
09:30:16.507821 14072 - Port NGAP_UNIT was started.
09:30:16.507857 14072 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:30:16.507951 14072 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:30:16.508079 13836 C5G_Tests.ttcn:162 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:30:16.508132 13836 C5G_Tests.ttcn:163 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0].
09:30:16.508796 13836 C5G_Tests.ttcn:163 Port NGAP_PROC[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-bb57f519.
09:30:16.508986 14072 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
09:30:16.509066 13836 C5G_Tests.ttcn:163 Port NGAP_PROC[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:16.509118 13836 C5G_Tests.ttcn:163 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0] finished.
09:30:16.509160 13836 C5G_Tests.ttcn:164 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0].
09:30:16.509484 13836 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-aa4eec08.
09:30:16.509579 14072 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
09:30:16.509653 13836 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:30:16.509705 13836 C5G_Tests.ttcn:164 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
09:30:16.509751 13836 C5G_Tests.ttcn:165 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0") on component TC_periodic_registration_updating-NGAP0(13).
09:30:16.509923 13836 C5G_Tests.ttcn:165 Function was started.
09:30:16.510156 14072 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0").
09:30:16.512146 14072 NGAP_Emulation.ttcn:452 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:30:16.512292 14072 NGAP_Emulation.ttcn:452 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:30:16.513135 14072 NGAP_Emulation.ttcn:457 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
09:30:16.513706 14072 NGAP_Emulation.ttcn:457 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:30:16.516040 14072 NGAP_Emulation.ttcn:469 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:30:16.516259 13836 C5G_Tests.ttcn:166 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:30:16.516331 13836 C5G_Tests.ttcn:166 Matching on port NGAP_UNIT[0] succeeded:  matched
09:30:16.516395 13836 C5G_Tests.ttcn:166 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:30:16.516453 13836 C5G_Tests.ttcn:166 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
09:30:16.517005 13836 C5G_Tests.ttcn:268 Sent on NGAP_UNIT[0] to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
09:30:16.517109 13836 C5G_Tests.ttcn:269 Start timer T: 5 s
09:30:16.519941 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:16.523107 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:16.523486 14072 NGAP_Emulation.ttcn:542 Matching on port NGAP_UNIT succeeded:  matched
09:30:16.523558 14072 NGAP_Emulation.ttcn:542 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:16.523600 14072 NGAP_Emulation.ttcn:542 Message with id 1 was extracted from the queue of NGAP_UNIT.
09:30:16.526477 14072 NGAP_Emulation.ttcn:544 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.527287 14072 NGAP_Emulation.ttcn:544 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
09:30:16.527761 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:30:16.527824 14072 NGAP_Emulation.ttcn:600 Matching on port NGAP succeeded:  matched
09:30:16.527848 14072 NGAP_Emulation.ttcn:600 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:16.527866 14072 NGAP_Emulation.ttcn:600 Message with id 1 was extracted from the queue of NGAP.
09:30:16.527940 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
09:30:16.528910 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:16.528972 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.528993 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:16.529009 14072 NGAP_Emulation.ttcn:548 Message with id 2 was extracted from the queue of NGAP.
09:30:16.529086 14072 C5G_Tests.ttcn:128 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.529301 13836 C5G_Tests.ttcn:270 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:16.529328 13836 C5G_Tests.ttcn:271 Matching on port NGAP_UNIT[0] succeeded:  matched
09:30:16.529342 13836 C5G_Tests.ttcn:271 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:16.529357 13836 C5G_Tests.ttcn:271 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
09:30:16.529368 13836 C5G_Tests.ttcn:272 setverdict(pass): none -> pass
09:30:16.529407 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.104257.
09:30:16.529420 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.802728.
09:30:16.529431 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.879426.
09:30:16.529441 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.100829.
09:30:16.529451 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.092164.
09:30:16.529461 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.593189.
09:30:16.529496 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.865117.
09:30:16.529507 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.783191.
09:30:16.529543 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.715263.
09:30:16.529553 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.417727.
09:30:16.529563 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.632739.
09:30:16.529573 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.622217.
09:30:16.529583 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.710408.
09:30:16.529593 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.705804.
09:30:16.529603 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.439721.
09:30:16.529613 13836 Osmocom_Types.ttcn:65 Function rnd() returned 0.498712.
09:30:16.529648 13836 C5G_Tests.ttcn:216 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:30:16.531953 14073 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:16.531990 14073 - TTCN-3 Parallel Test Component started on 81fd22231848. Component reference: TC_periodic_registration_updating0(14), component type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0. Version: 11.1.0.
09:30:16.532008 14073 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:16.532060 14073 - Connected to MC.
09:30:16.532076 14073 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_periodic_registration_updating.
09:30:16.532102 13836 C5G_Tests.ttcn:216 PTC was created. Component reference: 14, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:30:16.532120 13836 C5G_Tests.ttcn:218 Connecting ports TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:30:16.532269 14072 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT is waiting for connection from TC_periodic_registration_updating0(14):NGAP on UNIX pathname /tmp/ttcn3-portconn-b7da15c.
09:30:16.533318 14073 - Port NGAP was started.
09:30:16.533345 14073 - Port NGAP_PROC was started.
09:30:16.533359 14073 - Port GTP1U[0] was started.
09:30:16.533373 14073 - Port GTP1U[1] was started.
09:30:16.533386 14073 - Port GTP1U[2] was started.
09:30:16.533399 14073 - Port GTP1U[3] was started.
09:30:16.533412 14073 - Port GTP1U_PROC[0] was started.
09:30:16.533426 14073 - Port GTP1U_PROC[1] was started.
09:30:16.533439 14073 - Port GTP1U_PROC[2] was started.
09:30:16.533453 14073 - Port GTP1U_PROC[3] was started.
09:30:16.533466 14073 - Component type ConnHdlr.ConnHdlr was initialized.
09:30:16.533510 14073 - Port NGAP has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT using transport type UNIX.
09:30:16.533542 14072 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT has accepted the connection from TC_periodic_registration_updating0(14):NGAP.
09:30:16.533557 13836 C5G_Tests.ttcn:218 Connect operation on TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT finished.
09:30:16.533577 13836 C5G_Tests.ttcn:219 Connecting ports TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:16.533708 14072 NGAP_Emulation.ttcn:485 Port NGAP_PROC is waiting for connection from TC_periodic_registration_updating0(14):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-1167ae15.
09:30:16.533739 14073 - Port NGAP_PROC has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_PROC using transport type UNIX.
09:30:16.533766 14072 NGAP_Emulation.ttcn:485 Port NGAP_PROC has accepted the connection from TC_periodic_registration_updating0(14):NGAP_PROC.
09:30:16.533780 13836 C5G_Tests.ttcn:219 Connect operation on TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC finished.
09:30:16.533797 13836 C5G_Tests.ttcn:222 Connecting ports TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT.
09:30:16.533942 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT is waiting for connection from TC_periodic_registration_updating0(14):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-425d238.
09:30:16.533972 14073 - Port GTP1U[0] has established the connection with GTP1U_EM(12):CLIENT using transport type UNIX.
09:30:16.534021 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT has accepted the connection from TC_periodic_registration_updating0(14):GTP1U[0].
09:30:16.534034 13836 C5G_Tests.ttcn:222 Connect operation on TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT finished.
09:30:16.534051 13836 C5G_Tests.ttcn:223 Connecting ports TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:30:16.534177 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC is waiting for connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-467ea655.
09:30:16.534208 14073 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(12):CLIENT_PROC using transport type UNIX.
09:30:16.534233 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC has accepted the connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:30:16.534247 13836 C5G_Tests.ttcn:223 Connect operation on TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC finished.
09:30:16.534263 13836 C5G_Tests.ttcn:227 Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '1881058774667744'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}) on component TC_periodic_registration_updating0(14).
09:30:16.534343 13836 C5G_Tests.ttcn:227 Function was started.
09:30:16.535187 14073 - Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '1881058774667744'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}).
09:30:16.538477 14073 ConnHdlr.ttcn:539 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:16.539149 14073 ConnHdlr.ttcn:539 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
09:30:16.544020 14073 ConnHdlr.ttcn:544 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:30:16.545155 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:16.545234 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.545261 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.545283 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.545304 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.545556 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.545601 14072 NGAP_Emulation.ttcn:513 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:16.545628 14072 NGAP_Emulation.ttcn:513 Message with id 1 was extracted from the queue of NGAP_CLIENT.
09:30:16.547258 14072 NGAP_Emulation.ttcn:519 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.547704 14072 NGAP_Emulation.ttcn:519 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
09:30:16.553101 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403E000003000A000200020055000200000026002B2A7E00560202000021E46A1C401085CD521A8C9237DC7F17AE2010371B5F80154E8000B0CD35436A15F4FB'O
} id 3
09:30:16.554099 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560202000021E46A1C401085CD521A8C9237DC7F17AE2010371B5F80154E8000B0CD35436A15F4FB'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:30:16.554224 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.554285 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00560202000021E46A1C401085CD521A8C9237DC7F17AE2010371B5F80154E8000B0CD35436A15F4FB'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:30:16.554336 14072 NGAP_Emulation.ttcn:548 Message with id 3 was extracted from the queue of NGAP.
09:30:16.554741 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E00560202000021E46A1C401085CD521A8C9237DC7F17AE2010371B5F80154E8000B0CD35436A15F4FB'O
09:30:16.555933 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11100100011010100001110001000000000100001000010111001101010100100001101010001100100100100011011111011100011111110001011110101110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '00110111000110110101111110000000000101010100111010000000000000001011000011001101001101010100001101101010000101011111010011111011'B
        },
        eapMessage := omit
    }
}
09:30:16.556440 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11100100011010100001110001000000000100001000010111001101010100100001101010001100100100100011011111011100011111110001011110101110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '00110111000110110101111110000000000101010100111010000000000000001011000011001101001101010100001101101010000101011111010011111011'B
        },
        eapMessage := omit
    }
}
09:30:16.556934 14073 ConnHdlr.ttcn:556 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11100100011010100001110001000000000100001000010111001101010100100001101010001100100100100011011111011100011111110001011110101110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '00110111000110110101111110000000000101010100111010000000000000001011000011001101001101010100001101101010000101011111010011111011'B
        },
        eapMessage := omit
    }
} id 1
09:30:16.557299 14073 ConnHdlr.ttcn:189 Matching on port NGAP succeeded:  matched
09:30:16.557375 14073 ConnHdlr.ttcn:189 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '11100100011010100001110001000000000100001000010111001101010100100001101010001100100100100011011111011100011111110001011110101110'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '00110111000110110101111110000000000101010100111010000000000000001011000011001101001101010100001101101010000101011111010011111011'B
        },
        eapMessage := omit
    }
} id 1
09:30:16.557427 14073 ConnHdlr.ttcn:189 Message with id 1 was extracted from the queue of NGAP.
09:30:16.560678 14073 ConnHdlr.ttcn:234 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'C146A6B014F813967014217D33F8FE628A9F542D543395FE2545F850A01498A0'O,
        k_nas_enc := '131C2DB0496E38F2AD6A8B4BD913E7CE59DDB165EFF697102E35600841D7658D'O
    }
}
09:30:16.560930 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'C146A6B014F813967014217D33F8FE628A9F542D543395FE2545F850A01498A0'O,
        k_nas_enc := '131C2DB0496E38F2AD6A8B4BD913E7CE59DDB165EFF697102E35600841D7658D'O
    }
} id 2
09:30:16.561026 14073 ConnHdlr.ttcn:238 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01110110111101110110101110000110111100010111110011101010010100011100011010101101010110001101001101011011001000101111110010111011'B
        },
        eapMessage := omit
    }
}
09:30:16.561057 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.561102 14072 NGAP_Emulation.ttcn:487 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'C146A6B014F813967014217D33F8FE628A9F542D543395FE2545F850A01498A0'O,
        k_nas_enc := '131C2DB0496E38F2AD6A8B4BD913E7CE59DDB165EFF697102E35600841D7658D'O
    }
} id 2
09:30:16.561137 14072 NGAP_Emulation.ttcn:487 Message with id 2 was extracted from the queue of NGAP_CLIENT.
09:30:16.561442 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01110110111101110110101110000110111100010111110011101010010100011100011010101101010110001101001101011011001000101111110010111011'B
        },
        eapMessage := omit
    }
} id 3
09:30:16.561600 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.561634 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.561663 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.561690 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.561733 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.561805 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.561846 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01110110111101110110101110000110111100010111110011101010010100011100011010101101010110001101001101011011001000101111110010111011'B
        },
        eapMessage := omit
    }
} id 3
09:30:16.561879 14072 NGAP_Emulation.ttcn:522 Message with id 3 was extracted from the queue of NGAP_CLIENT.
09:30:16.561977 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01110110111101110110101110000110111100010111110011101010010100011100011010101101010110001101001101011011001000101111110010111011'B
        },
        eapMessage := omit
    }
}
09:30:16.562296 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D1076F76B86F17CEA51C6AD58D35B22FCBB'O
09:30:16.563509 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D1076F76B86F17CEA51C6AD58D35B22FCBB'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.563678 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403C000004000A0002000200550002000000260016157E00572D1076F76B86F17CEA51C6AD58D35B22FCBB0079400F4099F907000000000099F907000001'O
}
09:30:16.568618 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044027000003000A0002000200550002000000260014137E03D843482D007E005D0102028040E1360102'O
} id 4
09:30:16.568812 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03D843482D007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:30:16.568889 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.568946 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03D843482D007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:30:16.568987 14072 NGAP_Emulation.ttcn:548 Message with id 4 was extracted from the queue of NGAP.
09:30:16.569029 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E03D843482D007E005D0102028040E1360102'O
09:30:16.569089 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := 'D843482D'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0102028040E1360102'O
    }
}
09:30:16.570224 14072 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0102028040E1360102'O
09:30:16.570511 14072 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:30:16.570800 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:30:16.571073 14073 ConnHdlr.ttcn:557 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:30:16.571333 14073 ConnHdlr.ttcn:250 Matching on port NGAP succeeded:  matched
09:30:16.571379 14073 ConnHdlr.ttcn:250 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:30:16.571407 14073 ConnHdlr.ttcn:250 Message with id 2 was extracted from the queue of NGAP.
09:30:16.571462 14073 ConnHdlr.ttcn:255 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
09:30:16.571514 14073 ConnHdlr.ttcn:260 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
09:30:16.571530 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:30:16.571605 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:30:16.571638 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:30:16.571666 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.571689 14072 NGAP_Emulation.ttcn:499 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:30:16.571713 14072 NGAP_Emulation.ttcn:499 Message with id 4 was extracted from the queue of NGAP_CLIENT.
09:30:16.571727 14073 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:16.571789 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:30:16.571819 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:30:16.571829 14073 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004129000D0199F9072143000100000000002E028040'O
09:30:16.571843 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:30:16.571890 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
09:30:16.571920 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.571943 14072 NGAP_Emulation.ttcn:506 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:30:16.571965 14072 NGAP_Emulation.ttcn:506 Message with id 5 was extracted from the queue of NGAP_CLIENT.
09:30:16.572021 14073 ConnHdlr.ttcn:271 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1881058774667744'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:30:16.572175 14073 NGAP_Emulation.ttcn:717 Called on NGAP_PROC to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
09:30:16.572255 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1881058774667744'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:30:16.572360 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.572384 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.572406 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.572428 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.572456 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.572484 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.572514 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1881058774667744'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:30:16.572540 14072 NGAP_Emulation.ttcn:522 Message with id 6 was extracted from the queue of NGAP_CLIENT.
09:30:16.572595 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '1881058774667744'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:30:16.572717 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090518810587746677447100177E004129000D0199F9072143000100000000002E028040'O
09:30:16.573481 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '7C2482D3'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090518810587746677447100177E004129000D0199F9072143000100000000002E028040'O
    }
}
09:30:16.573522 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E047C2482D3007E005E7700090518810587746677447100177E004129000D0199F9072143000100000000002E028040'O
09:30:16.573632 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E047C2482D3007E005E7700090518810587746677447100177E004129000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.573698 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4057000004000A0002000200550002000000260031307E047C2482D3007E005E7700090518810587746677447100177E004129000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
09:30:16.573825 14072 NGAP_Emulation.ttcn:485 Call enqueued on NGAP_PROC from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:30:16.573935 14072 NGAP_Emulation.ttcn:602 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
09:30:16.573955 14072 NGAP_Emulation.ttcn:606 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
09:30:16.573975 14072 NGAP_Emulation.ttcn:610 Matching on port NGAP_PROC succeeded: { } with { } matched
09:30:16.574017 14072 NGAP_Emulation.ttcn:610 Getcall operation on port NGAP_PROC succeeded, call from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:30:16.574041 14072 NGAP_Emulation.ttcn:610 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:30:16.574075 14072 NGAP_Emulation.ttcn:613 Replied on NGAP_PROC to TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2
09:30:16.574170 14073 NGAP_Emulation.ttcn:717 Reply enqueued on NGAP_PROC from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:30:16.574234 14073 NGAP_Emulation.ttcn:718 Matching on port NGAP_PROC succeeded: { } with { } matched value 2 with ? matched
09:30:16.574314 14073 NGAP_Emulation.ttcn:718 Getreply operation on port NGAP_PROC succeeded, reply from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:30:16.574345 14073 NGAP_Emulation.ttcn:718 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:30:16.584639 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044056000005000A000200020055000200000026002F2E7E0248ADB14D017E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
09:30:16.585961 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0248ADB14D017E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:30:16.586165 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.586271 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0248ADB14D017E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:30:16.586337 14072 NGAP_Emulation.ttcn:548 Message with id 5 was extracted from the queue of NGAP.
09:30:16.586422 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0248ADB14D017E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192'O
09:30:16.586508 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '48ADB14D'O,
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192'O
    }
}
09:30:16.587443 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C00003FD54074099F90700000115020101210201005E0192'O
09:30:16.589412 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:16.591266 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:16.592492 14073 ConnHdlr.ttcn:562 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:30:16.593281 14073 ConnHdlr.ttcn:562 Matching on port NGAP succeeded:  matched
09:30:16.593385 14073 ConnHdlr.ttcn:562 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:30:16.593446 14073 ConnHdlr.ttcn:562 Message with id 3 was extracted from the queue of NGAP.
09:30:16.593595 14073 ConnHdlr.ttcn:564 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:16.593777 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:30:16.593950 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.594026 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.594097 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.594163 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.594259 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.594347 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.594426 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:30:16.594503 14072 NGAP_Emulation.ttcn:522 Message with id 7 was extracted from the queue of NGAP_CLIENT.
09:30:16.594610 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:16.594728 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:30:16.595734 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'CC32CEC5'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:30:16.595833 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02CC32CEC5007E0043'O
09:30:16.596132 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02CC32CEC5007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.596324 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E02CC32CEC5007E00430079400F4099F907000000000099F907000001'O
}
09:30:16.597915 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E02C37ED7BD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
} id 6
09:30:16.598145 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02C37ED7BD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:30:16.598283 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.598395 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02C37ED7BD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:30:16.598460 14072 NGAP_Emulation.ttcn:548 Message with id 6 was extracted from the queue of NGAP.
09:30:16.598542 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02C37ED7BD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
09:30:16.598631 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'C37ED7BD'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
    }
}
09:30:16.599576 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
09:30:16.600167 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:16.600742 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:16.600993 14073 ConnHdlr.ttcn:566 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:30:16.601249 14073 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:30:16.601298 14073 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:30:16.601330 14073 ConnHdlr.ttcn:279 Message with id 4 was extracted from the queue of NGAP.
09:30:16.601392 14073 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:16.601465 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:30:16.601519 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.601550 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.601572 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.601594 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.601622 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.601648 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.601674 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:30:16.601701 14072 NGAP_Emulation.ttcn:522 Message with id 8 was extracted from the queue of NGAP_CLIENT.
09:30:16.601736 14073 ConnHdlr.ttcn:578 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:16.601740 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:16.601784 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:30:16.602071 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '17CE0742'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:30:16.602113 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0217CE0742007E0055'O
09:30:16.602223 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0217CE0742007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.602305 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0217CE0742007E00550079400F4099F907000000000099F907000001'O
}
09:30:16.602721 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:30:16.602961 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.603000 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.603033 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.603059 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.603099 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.603145 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.603200 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:30:16.603237 14072 NGAP_Emulation.ttcn:522 Message with id 9 was extracted from the queue of NGAP_CLIENT.
09:30:16.603277 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00003FD'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:16.603424 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00412B000BF299F907020040C00003FD2E028040'O
09:30:16.603779 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'C96A22B9'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E00412B000BF299F907020040C00003FD2E028040'O
    }
}
09:30:16.603821 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02C96A22B9007E00412B000BF299F907020040C00003FD2E028040'O
09:30:16.603952 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02C96A22B9007E00412B000BF299F907020040C00003FD2E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.604041 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4043000004000A000200020055000200000026001D1C7E02C96A22B9007E00412B000BF299F907020040C00003FD2E0280400079400F4099F907000000000099F907000001'O
}
09:30:16.807864 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000004000A000200020055000200000026002F2E7E0214900DE4037E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192000000020001'O
} id 7
09:30:16.808271 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0214900DE4037E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:30:16.808498 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.808598 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0214900DE4037E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:30:16.808683 14072 NGAP_Emulation.ttcn:548 Message with id 7 was extracted from the queue of NGAP.
09:30:16.808770 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0214900DE4037E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192'O
09:30:16.808920 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '14900DE4'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192'O
    }
}
09:30:16.809715 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000045C54074099F90700000115020101210201005E0192'O
09:30:16.810031 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:16.810358 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:16.810741 14073 ConnHdlr.ttcn:590 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:30:16.811211 14073 ConnHdlr.ttcn:590 Matching on port NGAP succeeded:  matched
09:30:16.811340 14073 ConnHdlr.ttcn:590 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:30:16.811423 14073 ConnHdlr.ttcn:590 Message with id 5 was extracted from the queue of NGAP.
09:30:16.811536 14073 ConnHdlr.ttcn:592 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:16.811660 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:30:16.811743 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.811796 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.811844 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.811891 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.811952 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.812010 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.812068 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:30:16.812125 14072 NGAP_Emulation.ttcn:522 Message with id 10 was extracted from the queue of NGAP_CLIENT.
09:30:16.812206 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:16.812284 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:30:16.812925 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'CC32CEC5'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:30:16.813356 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02CC32CEC5007E0043'O
09:30:16.813618 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02CC32CEC5007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.813788 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E02CC32CEC5007E00430079400F4099F907000000000099F907000001'O
}
09:30:16.816584 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E027FC11C20047E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
} id 8
09:30:16.817120 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E027FC11C20047E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:16.817383 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:16.817518 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E027FC11C20047E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:16.817636 14072 NGAP_Emulation.ttcn:548 Message with id 8 was extracted from the queue of NGAP.
09:30:16.817775 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E027FC11C20047E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
09:30:16.817915 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '7FC11C20'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
    }
}
09:30:16.819330 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752214090036100490100'O
09:30:16.819716 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:16.820062 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:16.820336 14073 ConnHdlr.ttcn:594 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:30:16.820560 14073 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:30:16.820678 14073 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '21'O ("!"),
            day := '40'O ("@"),
            hour := '90'O,
            minute := '03'O,
            second := '61'O ("a"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:30:16.820745 14073 ConnHdlr.ttcn:279 Message with id 6 was extracted from the queue of NGAP.
09:30:16.820825 14073 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:16.820959 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:30:16.821105 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.821190 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.821268 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.821344 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.821424 14073 ConnHdlr.ttcn:608 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        }
    }
}
09:30:16.821450 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.821550 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.821639 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:30:16.821725 14072 NGAP_Emulation.ttcn:522 Message with id 11 was extracted from the queue of NGAP_CLIENT.
09:30:16.821843 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:16.821962 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:30:16.823141 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '17CE0742'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:30:16.823258 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0217CE0742007E0055'O
09:30:16.823590 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0217CE0742007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.823825 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0217CE0742007E00550079400F4099F907000000000099F907000001'O
}
09:30:16.824340 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        }
    }
} id 12
09:30:16.824679 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.824891 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.825041 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.825228 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:16.825315 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:16.825394 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:16.825472 14072 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        }
    }
} id 12
09:30:16.825538 14072 NGAP_Emulation.ttcn:522 Message with id 12 was extracted from the queue of NGAP_CLIENT.
09:30:16.825625 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000045C'O
        }
    }
}
09:30:16.825787 14072 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C000045C'O
09:30:16.826451 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'C763A3D0'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C000045C'O
    }
}
09:30:16.826525 14072 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02C763A3D0007E004531000BF299F907020040C000045C'O
09:30:16.826746 14072 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02C763A3D0007E004531000BF299F907020040C000045C'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:16.826905 14072 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403F000004000A0002000200550002000000260019187E02C763A3D0007E004531000BF299F907020040C000045C0079400F4099F907000000000099F907000001'O
}
09:30:17.041223 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401E000003000A000200020055000200000026000B0A7E022A46A5DC057E0046'O
} id 9
09:30:17.041596 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E022A46A5DC057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:30:17.041864 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:17.041945 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E022A46A5DC057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:30:17.042009 14072 NGAP_Emulation.ttcn:548 Message with id 9 was extracted from the queue of NGAP.
09:30:17.042092 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E022A46A5DC057E0046'O
09:30:17.042178 14072 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '2A46A5DC'O,
        sequenceNumber := '05'O,
        plainNASMessage := '7E0046'O
    }
}
09:30:17.042837 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
09:30:17.042933 14072 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:30:17.043047 14072 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:30:17.043245 14073 ConnHdlr.ttcn:610 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:30:17.043305 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900100000020072000400020000000F400148'O
} id 10
09:30:17.043458 14073 ConnHdlr.ttcn:610 Matching on port NGAP succeeded:  matched
09:30:17.043530 14073 ConnHdlr.ttcn:610 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:30:17.043594 14073 ConnHdlr.ttcn:610 Message with id 7 was extracted from the queue of NGAP.
09:30:17.044585 14072 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:30:17.044723 14072 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:17.044797 14072 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:30:17.044876 14072 NGAP_Emulation.ttcn:548 Message with id 10 was extracted from the queue of NGAP.
09:30:17.045090 14072 NGAP_Emulation.ttcn:587 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:17.046793 14073 ConnHdlr.ttcn:611 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:17.047884 14073 ConnHdlr.ttcn:624 Matching on port NGAP succeeded:  matched
09:30:17.047978 14073 ConnHdlr.ttcn:624 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:17.048042 14073 ConnHdlr.ttcn:624 Message with id 8 was extracted from the queue of NGAP.
09:30:17.050556 14073 ConnHdlr.ttcn:625 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:17.050993 14073 - Function f_init_handler finished. PTC terminates.
09:30:17.051052 14073 - Terminating component type ConnHdlr.ConnHdlr.
09:30:17.051097 14073 - Removing unterminated connection between port NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:30:17.051176 14073 - Port NGAP was stopped.
09:30:17.051212 14072 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:30:17.051220 14073 - Removing unterminated connection between port NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:17.051288 14073 - Port NGAP_PROC was stopped.
09:30:17.051329 14073 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(12):CLIENT.
09:30:17.051374 14072 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:17.051391 14073 - Port GTP1U[0] was stopped.
09:30:17.051425 14072 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:17.051426 14073 - Port GTP1U[1] was stopped.
09:30:17.051437 14071 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT to TC_periodic_registration_updating0(14):GTP1U[0] was closed unexpectedly by the peer.
09:30:17.051467 14073 - Port GTP1U[2] was stopped.
09:30:17.051477 14072 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:17.051514 14073 - Port GTP1U[3] was stopped.
09:30:17.051522 14072 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:17.051553 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT was disconnected from TC_periodic_registration_updating0(14):GTP1U[0].
09:30:17.051554 14073 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:30:17.051611 14073 - Port GTP1U_PROC[0] was stopped.
09:30:17.051648 14073 - Port GTP1U_PROC[1] was stopped.
09:30:17.051687 14071 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT_PROC to TC_periodic_registration_updating0(14):GTP1U_PROC[0] was closed unexpectedly by the peer.
09:30:17.051708 14073 - Port GTP1U_PROC[2] was stopped.
09:30:17.051734 14071 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC was disconnected from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:30:17.051745 14073 - Port GTP1U_PROC[3] was stopped.
09:30:17.051779 14073 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_periodic_registration_updating.
09:30:17.051842 14073 - Final verdict of PTC: none
09:30:17.051911 13836 C5G_Tests.ttcn:331 PTC with component reference 14 is done.
09:30:17.051984 13836 C5G_Tests.ttcn:331 Terminating component type C5G_Tests.MTC_CT.
09:30:17.052003 14072 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:30:17.052005 14073 - Disconnected from MC.
09:30:17.052027 13836 C5G_Tests.ttcn:331 Default with id 1 (altstep as_Tguard) was deactivated.
09:30:17.052072 13836 C5G_Tests.ttcn:331 Stop timer g_Tguard: 30 s
09:30:17.052084 14072 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
09:30:17.052113 14073 - TTCN-3 Parallel Test Component finished.
09:30:17.052205 14072 NGAP_Emulation.ttcn:535 Matching on port NGAP_CLIENT succeeded:  matched
09:30:17.052242 13836 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_UNIT[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:30:17.052275 14072 NGAP_Emulation.ttcn:535 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:30:17.052332 14072 NGAP_Emulation.ttcn:535 Message with id 13 was extracted from the queue of NGAP_CLIENT.
09:30:17.052344 13836 C5G_Tests.ttcn:331 Port NGAP_UNIT[0] was stopped.
09:30:17.052401 13836 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_PROC[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:17.052525 13836 C5G_Tests.ttcn:331 Port NGAP_PROC[0] was stopped.
09:30:17.052563 13836 C5G_Tests.ttcn:331 Removing unterminated connection between port TEID0 and GTP1U_EM(12):TEID0.
09:30:17.052653 13836 C5G_Tests.ttcn:331 Port TEID0 was stopped.
09:30:17.052713 13836 C5G_Tests.ttcn:331 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:17.052739 14071 GTPv1U_Emulation.ttcnpp:265 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
09:30:17.052784 14071 GTPv1U_Emulation.ttcnpp:265 Port TEID0 was disconnected from mtc:TEID0.
09:30:17.052851 13836 C5G_Tests.ttcn:331 Waiting for PTCs to finish.
09:30:17.052989 14071 GTPv1U_Emulation.ttcnpp:265 Kill was requested from MC.
09:30:17.053025 14071 GTPv1U_Emulation.ttcnpp:265 Terminating test component execution.
09:30:17.053363 14072 NGAP_Emulation.ttcn:538 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:17.053553 14072 NGAP_Emulation.ttcn:538 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290022000003000A400200020055400200000079400F4099F907000000000099F907000001'O
}
09:30:17.053658 14071 - Function main was stopped. PTC terminates.
09:30:17.053726 14071 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
09:30:17.053785 14071 - Default with id 1 (altstep as_uecups_ind) was deactivated.
09:30:17.053818 14072 NGAP_Emulation.ttcn:485 Connection of port NGAP_CLIENT to TC_periodic_registration_updating0(14):NGAP was closed unexpectedly by the peer.
09:30:17.053888 14072 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT was disconnected from TC_periodic_registration_updating0(14):NGAP.
09:30:17.053962 14072 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to TC_periodic_registration_updating0(14):NGAP_PROC was closed unexpectedly by the peer.
09:30:17.054014 14071 - Removing unterminated mapping between port GTP1U and system:GTP1U.
09:30:17.054099 14072 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from TC_periodic_registration_updating0(14):NGAP_PROC.
09:30:17.054175 14071 - Port GTP1U was unmapped from system:GTP1U.
09:30:17.054225 14071 - Port GTP1U was stopped.
09:30:17.054253 14071 - Port TEID0 was stopped.
09:30:17.054285 14071 - Port CLIENT was stopped.
09:30:17.054299 14072 NGAP_Emulation.ttcn:485 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
09:30:17.054327 14071 - Port CLIENT_PROC was stopped.
09:30:17.054352 14071 - Removing unterminated mapping between port UECUPS and system:UECUPS.
09:30:17.054369 14072 NGAP_Emulation.ttcn:485 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
09:30:17.054459 14072 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
09:30:17.054520 14072 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
09:30:17.054604 14072 NGAP_Emulation.ttcn:485 Kill was requested from MC.
09:30:17.054663 14072 NGAP_Emulation.ttcn:485 Terminating test component execution.
09:30:17.054689 14071 - Port UECUPS was unmapped from system:UECUPS.
09:30:17.054725 14071 - Port UECUPS was stopped.
09:30:17.054749 14071 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:17.054781 14071 - Final verdict of PTC: none
09:30:17.054860 14071 - Disconnected from MC.
09:30:17.054887 14071 - TTCN-3 Parallel Test Component finished.
09:30:17.055659 14072 - Function main was stopped. PTC terminates.
09:30:17.055779 14072 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:30:17.055829 14072 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:30:17.056364 14072 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:30:17.056430 14072 - Port NGAP was stopped.
09:30:17.056473 14072 - Port NGAP_CLIENT was stopped.
09:30:17.056510 14072 - Port NGAP_PROC was stopped.
09:30:17.056546 14072 - Port NGAP_UNIT was stopped.
09:30:17.056581 14072 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:17.056713 14072 - Final verdict of PTC: none
09:30:17.056815 14072 - Disconnected from MC.
09:30:17.056839 13836 C5G_Tests.ttcn:331 Setting final verdict of the test case.
09:30:17.056866 14072 - TTCN-3 Parallel Test Component finished.
09:30:17.056912 13836 C5G_Tests.ttcn:331 Local verdict of MTC: pass
09:30:17.056971 13836 C5G_Tests.ttcn:331 Local verdict of PTC GTP1U_EM(12): none (pass -> pass)
09:30:17.057025 13836 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating-NGAP0(13): none (pass -> pass)
09:30:17.057076 13836 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating0(14): none (pass -> pass)
09:30:17.057127 13836 C5G_Tests.ttcn:331 Test case TC_periodic_registration_updating finished. Verdict: pass
09:30:17.057180 13836 C5G_Tests.ttcn:331 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass'.
09:30:19.115453 13836 C5G_Tests.ttcn:331 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass' was executed successfully (exit status: 0).
09:30:19.115566 13836 C5G_Tests.ttcn:339 Switching to log file `C5G_Tests-TC_ue_context_release_no_pdu_session-81fd22231848-mtc-13836.log'
