14:44:47.197254 9884 BSC_Tests.ttcn:3129 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2_ncc_permitted'.
14:44:48.206044 9884 BSC_Tests.ttcn:3129 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2_ncc_permitted' was executed successfully (exit status: 0).
14:44:48.206207 9884 BSC_Tests.ttcn:3129 Test case TC_si2_ncc_permitted started.
14:44:48.206239 9884 BSC_Tests.ttcn:3129 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_si2_ncc_permitted.
14:44:48.206359 9884 BSC_Tests.ttcn:3129 Port IPA_CTRL was started.
14:44:48.206386 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[0] was started.
14:44:48.206405 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[1] was started.
14:44:48.206424 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[2] was started.
14:44:48.206441 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][0] was started.
14:44:48.206458 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][1] was started.
14:44:48.206475 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][2] was started.
14:44:48.206491 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][3] was started.
14:44:48.206508 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][0] was started.
14:44:48.206524 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][1] was started.
14:44:48.206540 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][2] was started.
14:44:48.206556 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][3] was started.
14:44:48.206573 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][0] was started.
14:44:48.206589 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][1] was started.
14:44:48.206605 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][2] was started.
14:44:48.206622 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][3] was started.
14:44:48.206639 9884 BSC_Tests.ttcn:3129 Port IPA was started.
14:44:48.206655 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CTRL was started.
14:44:48.206675 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][0] was started.
14:44:48.206697 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][1] was started.
14:44:48.206716 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][2] was started.
14:44:48.206733 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][3] was started.
14:44:48.206750 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][0] was started.
14:44:48.206766 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][1] was started.
14:44:48.206782 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][2] was started.
14:44:48.206798 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][3] was started.
14:44:48.206814 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][0] was started.
14:44:48.206830 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][1] was started.
14:44:48.206846 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][2] was started.
14:44:48.206863 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][3] was started.
14:44:48.206879 9884 BSC_Tests.ttcn:3129 Port BSCVTY was started.
14:44:48.206895 9884 BSC_Tests.ttcn:3129 Port STPVTY was started.
14:44:48.206911 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[0] was started.
14:44:48.206928 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[1] was started.
14:44:48.206944 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[2] was started.
14:44:48.206960 9884 BSC_Tests.ttcn:3129 Port BSSAP was started.
14:44:48.206976 9884 BSC_Tests.ttcn:3129 Port BSSAP_LE was started.
14:44:48.206992 9884 BSC_Tests.ttcn:3129 Component type BSC_Tests.test_CT was initialized.
14:44:48.207019 9884 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
14:44:48.207232 9884 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
14:44:48.207264 9884 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
14:44:48.207303 9884 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
14:44:48.207333 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
14:44:48.207356 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
14:44:48.207377 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
14:44:48.207429 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
14:44:48.207469 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.207497 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:44:48.207515 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:44:48.207533 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:44:48.207550 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:44:48.207567 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:44:48.207587 9884 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
14:44:48.207608 9884 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
14:44:48.207627 9884 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
14:44:48.207654 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
14:44:48.207728 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.207773 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.207786 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
14:44:48.207799 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
14:44:48.207811 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.207828 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.207854 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.207915 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
14:44:48.207935 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.207953 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.207975 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.207986 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
14:44:48.207997 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
14:44:48.208008 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208019 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
14:44:48.208033 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208068 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
14:44:48.208085 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208101 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208120 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208131 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
14:44:48.208141 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
14:44:48.208155 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208166 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
14:44:48.208179 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208207 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
14:44:48.208223 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208238 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208256 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208267 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
14:44:48.208276 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
14:44:48.208286 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208296 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
14:44:48.208308 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208330 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
14:44:48.208345 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208360 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208378 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208388 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
14:44:48.208397 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
14:44:48.208407 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208417 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:44:48.208429 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208447 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
14:44:48.208462 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208477 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.208487 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
14:44:48.208497 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
14:44:48.208507 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208517 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.208529 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208555 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
14:44:48.208571 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208585 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208603 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208614 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
14:44:48.208625 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
14:44:48.208635 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208645 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
14:44:48.208656 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208678 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 9
14:44:48.208693 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208707 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208725 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208735 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 9
14:44:48.208745 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
14:44:48.208755 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208764 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
14:44:48.208776 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208808 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 10
14:44:48.208823 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208838 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.208856 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.208866 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 10
14:44:48.208875 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
14:44:48.208885 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.208895 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "ncc-permitted 6 7 8"
14:44:48.208907 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.208963 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 11
14:44:48.208978 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.208992 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.209009 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.209019 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 11
14:44:48.209029 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
14:44:48.209038 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209048 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:44:48.209059 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209085 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
14:44:48.209099 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209115 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.209125 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
14:44:48.209134 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
14:44:48.209144 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209154 9884 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
14:44:48.209165 9884 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
14:44:48.209177 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.209189 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209241 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 13
14:44:48.209256 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209271 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.209289 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.209300 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 13
14:44:48.209310 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 13 was extracted from the queue of BSCVTY.
14:44:48.209320 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209330 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:44:48.209342 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209365 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 14
14:44:48.209380 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209395 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.209414 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.209424 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 14
14:44:48.209434 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 14 was extracted from the queue of BSCVTY.
14:44:48.209444 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209454 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:44:48.209466 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209496 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 15
14:44:48.209511 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209525 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.209543 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.209553 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 15
14:44:48.209562 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 15 was extracted from the queue of BSCVTY.
14:44:48.209572 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209582 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.209595 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209616 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 16
14:44:48.209631 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209645 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.209663 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.209673 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 16
14:44:48.209682 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 16 was extracted from the queue of BSCVTY.
14:44:48.209693 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209702 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.209714 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.209732 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
14:44:48.209746 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.209761 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.209771 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
14:44:48.209781 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
14:44:48.209791 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.209802 9884 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:44:48.212377 11672 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.212411 11672 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: VirtMSC-STATS(251), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
14:44:48.212427 11672 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:48.212462 11672 - Connected to MC.
14:44:48.212474 11672 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_si2_ncc_permitted.
14:44:48.212498 9884 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 251, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:44:48.212511 9884 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(251).
14:44:48.212537 9884 StatsD_Checker.ttcnpp:417 Function was started.
14:44:48.212548 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
14:44:48.212562 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.212616 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 18
14:44:48.212633 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.212649 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.212659 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 18
14:44:48.212669 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 18 was extracted from the queue of BSCVTY.
14:44:48.212679 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.212690 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
14:44:48.212702 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.212745 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
14:44:48.212761 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.212777 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.212787 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
14:44:48.212796 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
14:44:48.212808 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.212819 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
14:44:48.212831 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.212872 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 20
14:44:48.212887 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.212902 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.212911 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 20
14:44:48.212920 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 20 was extracted from the queue of BSCVTY.
14:44:48.212930 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.212964 9884 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:44:48.213854 11672 - Port STATSVTY was started.
14:44:48.213876 11672 - Port STATSD_PROC was started.
14:44:48.213887 11672 - Port STATS was started.
14:44:48.213896 11672 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
14:44:48.213968 11672 - Starting function main("127.0.0.1", 8125, 5.000000).
14:44:48.214153 11672 StatsD_Checker.ttcnpp:125 Mapping port VirtMSC-STATS(251):STATS to system:STATS.
14:44:48.214202 11672 StatsD_Checker.ttcnpp:125 Port STATS was mapped to system:STATS.
14:44:48.214230 11672 StatsD_Checker.ttcnpp:125 Map operation of VirtMSC-STATS(251):STATS to system:STATS finished.
14:44:48.214365 11672 StatsD_Checker.ttcnpp:126 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
14:44:48.215119 11672 StatsD_Checker.ttcnpp:134 Mapping port VirtMSC-STATS(251):STATSVTY to system:STATSVTY.
14:44:48.215471 11672 StatsD_Checker.ttcnpp:134 Message enqueued on STATSVTY from system integer : 2 id 1
14:44:48.215521 11673 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.215533 11672 StatsD_Checker.ttcnpp:134 Port STATSVTY was mapped to system:STATSVTY.
14:44:48.215557 11672 StatsD_Checker.ttcnpp:134 Map operation of VirtMSC-STATS(251):STATSVTY to system:STATSVTY finished.
14:44:48.215581 11673 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_si2_ncc_permitted.
14:44:48.215599 9884 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 252, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:44:48.215620 9884 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:44:48.215702 11672 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
14:44:48.215771 11672 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
14:44:48.215792 11672 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
14:44:48.215910 11672 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
14:44:48.215969 11672 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.216015 11672 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
14:44:48.216028 11672 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
14:44:48.216037 11672 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
14:44:48.216046 11672 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
14:44:48.216063 11672 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
14:44:48.216115 11672 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
14:44:48.216138 11672 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
14:44:48.216151 11672 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
14:44:48.216222 11672 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
14:44:48.216285 11672 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.216309 11672 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.216320 11672 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
14:44:48.216334 11672 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
14:44:48.216355 11672 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.216375 11672 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
14:44:48.216392 11672 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.216431 11672 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
14:44:48.216450 11672 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.216467 11672 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.216477 11672 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
14:44:48.216487 11672 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
14:44:48.216497 11672 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.216701 11673 - Component type SCCP_Emulation.SCCP_CT was initialized.
14:44:48.217955 11674 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.218046 11674 - Initializing variables, timers and ports of component type M3UA_Emulation.M3UA_CT inside testcase TC_si2_ncc_permitted.
14:44:48.218074 9884 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 253, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:44:48.218091 9884 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(253):SCTP_PORT to system:sctp.
14:44:48.219051 11674 - Component type M3UA_Emulation.M3UA_CT was initialized.
14:44:48.219086 9884 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(253):SCTP_PORT to system:sctp finished.
14:44:48.219098 9884 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(253):MTP3_SP_PORT and VirtMSC-SCCP(252):MTP3_SCCP_PORT.
14:44:48.219299 9884 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(253):MTP3_SP_PORT and VirtMSC-SCCP(252):MTP3_SCCP_PORT finished.
14:44:48.219311 9884 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({
    local_sctp_port := 23905,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 1) on component VirtMSC-M3UA(253).
14:44:48.219337 9884 SCCP_Adapter.ttcnpp:127 Function was started.
14:44:48.219350 9884 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT.
14:44:48.219371 11674 - Starting function f_M3UA_Emulation({
    local_sctp_port := 23905,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 1).
14:44:48.219447 9884 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(252):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-d77fb81d.
14:44:48.219501 9884 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(252):SCCP_SP_PORT.
14:44:48.219512 9884 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT finished.
14:44:48.219523 9884 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(252).
14:44:48.219557 9884 SCCP_Adapter.ttcnpp:165 Function was started.
14:44:48.219639 9884 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(252) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 0,
                        causeValue := '0000000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
14:44:48.219657 9884 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 0,
                    causeValue := '0000000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
14:44:48.219698 11673 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
14:44:48.219699 9884 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
14:44:48.219732 9884 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
}
14:44:48.219809 9884 BSC_Tests.ttcn:899 Start timer T: 5 s
14:44:48.424882 9884 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(252) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
} id 1
14:44:48.425030 9884 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
14:44:48.425283 9884 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 1,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
14:44:48.425431 9884 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
14:44:48.425580 9884 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
14:44:48.425703 9884 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(252): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
14:44:48.425770 9884 BSC_Tests.ttcn:901 Message with id 1 was extracted from the queue of BSSAP.
14:44:48.425838 9884 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
14:44:48.425936 9884 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:44:48.428752 11675 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.428787 11675 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: VirtSMLC-SCCP(254), component type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP. Version: 11.1.0.
14:44:48.428803 11675 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:48.428852 11675 - Connected to MC.
14:44:48.428867 11675 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_si2_ncc_permitted.
14:44:48.428889 9884 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 254, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:44:48.428904 9884 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:44:48.430096 11675 - Port SCCP_SP_PORT was started.
14:44:48.430121 11675 - Port MTP3_SCCP_PORT was started.
14:44:48.430133 11675 - Component type SCCP_Emulation.SCCP_CT was initialized.
14:44:48.431640 11676 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.431672 11676 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: VirtSMLC-M3UA(255), component type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA. Version: 11.1.0.
14:44:48.431701 11676 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:48.431739 11676 - Connected to MC.
14:44:48.431761 11676 - Initializing variables, timers and ports of component type M3UA_Emulation.M3UA_CT inside testcase TC_si2_ncc_permitted.
14:44:48.431771 9884 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 255, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:44:48.431786 9884 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(255):SCTP_PORT to system:sctp.
14:44:48.432718 11676 - Port MTP3_SP_PORT was started.
14:44:48.432749 11676 - Port SCTP_PORT was started.
14:44:48.432762 11676 - Component type M3UA_Emulation.M3UA_CT was initialized.
14:44:48.432780 11676 - Port SCTP_PORT was mapped to system:sctp.
14:44:48.432809 9884 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(255):SCTP_PORT to system:sctp finished.
14:44:48.432823 9884 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(255):MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT.
14:44:48.433035 11675 - Port MTP3_SCCP_PORT is waiting for connection from VirtSMLC-M3UA(255):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-b373f483.
14:44:48.433066 11676 - Port MTP3_SP_PORT has established the connection with VirtSMLC-SCCP(254):MTP3_SCCP_PORT using transport type UNIX.
14:44:48.433115 11675 - Port MTP3_SCCP_PORT has accepted the connection from VirtSMLC-M3UA(255):MTP3_SP_PORT.
14:44:48.433124 9884 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(255):MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT finished.
14:44:48.433137 9884 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({
    local_sctp_port := 23908,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 6) on component VirtSMLC-M3UA(255).
14:44:48.433167 9884 BSSAP_LE_Adapter.ttcn:105 Function was started.
14:44:48.433182 9884 BSC_Tests.ttcn:1290 Connecting ports mtc:BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT.
14:44:48.433204 11676 - Starting function f_M3UA_Emulation({
    local_sctp_port := 23908,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 6).
14:44:48.433351 9884 BSC_Tests.ttcn:1290 Port BSSAP_LE is waiting for connection from VirtSMLC-SCCP(254):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-9033e71d.
14:44:48.433376 11675 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP_LE using transport type UNIX.
14:44:48.433422 9884 BSC_Tests.ttcn:1290 Port BSSAP_LE has accepted the connection from VirtSMLC-SCCP(254):SCCP_SP_PORT.
14:44:48.433437 9884 BSC_Tests.ttcn:1290 Connect operation on mtc:BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT finished.
14:44:48.433448 11676 M3UA_Emulation.ttcn:512 *************************************************
14:44:48.433450 9884 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 190,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 252
}) on component VirtSMLC-SCCP(254).
14:44:48.433467 11676 M3UA_Emulation.ttcn:513 M3UA emulation initiated, the test can be started
14:44:48.433482 11676 M3UA_Emulation.ttcn:514 *************************************************
14:44:48.433492 9884 BSSAP_LE_Adapter.ttcn:122 Function was started.
14:44:48.433567 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
14:44:48.433613 11675 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 190,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 252
}).
14:44:48.433615 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.433821 11675 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
14:44:48.434088 11676 M3UA_Emulation.ttcn:554 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP_ConnectFrom : {
    local_hostname := "127.0.0.1",
    local_portnumber := 23908,
    peer_hostname := "127.0.0.1",
    peer_portnumber := 2905
}
14:44:48.435191 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" id 21
14:44:48.435221 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
14:44:48.436410 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.437431 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.438446 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:44:48.439543 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:44:48.440583 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with ? matched
14:44:48.441668 9884 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" id 21
14:44:48.441698 9884 Osmocom_VTY_Functions.ttcn:85 Message with id 21 was extracted from the queue of BSCVTY.
14:44:48.441721 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.441742 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.441753 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
14:44:48.441764 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
14:44:48.441775 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.441794 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.441820 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.441936 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
14:44:48.441956 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.441974 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.441997 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.442009 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
14:44:48.442021 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
14:44:48.442033 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442044 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:44:48.442064 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.442161 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
14:44:48.442185 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.442202 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.442222 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.442234 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
14:44:48.442244 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
14:44:48.442255 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442267 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
14:44:48.442280 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.442354 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
14:44:48.442370 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.442385 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.442404 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.442415 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
14:44:48.442425 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
14:44:48.442435 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442445 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.442458 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.442524 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
14:44:48.442540 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.442555 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.442573 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.442584 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
14:44:48.442594 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
14:44:48.442605 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442615 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.442628 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.442691 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
14:44:48.442707 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.442730 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.442751 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
14:44:48.442764 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
14:44:48.442778 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442792 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.442806 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.442881 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
14:44:48.442904 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.442924 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.442945 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.442959 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
14:44:48.442972 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
14:44:48.442985 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.442998 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
14:44:48.443013 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.443084 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
14:44:48.443102 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.443183 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.443244 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.443271 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
14:44:48.443297 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
14:44:48.443320 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.443346 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
14:44:48.443382 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.443451 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
14:44:48.443494 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.443529 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.443570 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.443602 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
14:44:48.443625 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
14:44:48.443647 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.443671 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.443732 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.443791 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
14:44:48.443831 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.443865 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.443912 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.443935 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
14:44:48.443956 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
14:44:48.443977 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.444001 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.444031 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.444071 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
14:44:48.444106 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.444141 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.444163 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
14:44:48.444184 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
14:44:48.444205 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.444231 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:48.444261 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.444305 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
14:44:48.444341 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.444374 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.444412 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.444435 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
14:44:48.444455 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
14:44:48.444477 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.444498 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
14:44:48.444527 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.444570 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 34
14:44:48.444606 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.444638 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.444676 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.444699 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 34
14:44:48.444720 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
14:44:48.444741 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.444763 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
14:44:48.444791 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.444834 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 35
14:44:48.444869 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.444906 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.444944 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.444967 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 35
14:44:48.444987 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
14:44:48.445007 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.445028 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.445057 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.445140 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 36
14:44:48.445176 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.445209 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:48.445247 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:48.445269 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 36
14:44:48.445289 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
14:44:48.445310 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.445331 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:44:48.445359 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:48.445430 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
14:44:48.445465 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:48.445499 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:48.445520 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
14:44:48.445541 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
14:44:48.445561 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:48.445584 9884 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:44:48.448731 11677 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.448769 11677 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: IPA-CTRL-CLI-IPA(256), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
14:44:48.448786 11677 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:48.448839 11677 - Connected to MC.
14:44:48.448862 11677 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_si2_ncc_permitted.
14:44:48.448915 9884 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 256, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:44:48.448958 9884 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(256):IPA_PORT to system:IPA_CODEC_PT.
14:44:48.450346 11677 - Port IPA_PORT was started.
14:44:48.450399 11677 - Port CFG_PORT was started.
14:44:48.450411 11677 - Port MTP3_SP_PORT was started.
14:44:48.450423 11677 - Port IPA_MGCP_PORT was started.
14:44:48.450434 11677 - Port IPA_RSL_PORT was started.
14:44:48.450484 11677 - Port IPA_OML_PORT was started.
14:44:48.450493 11677 - Port IPA_CTRL_PORT was started.
14:44:48.450502 11677 - Port IPA_SP_PORT was started.
14:44:48.450511 11677 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
14:44:48.450558 11677 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
14:44:48.450606 9884 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(256):IPA_PORT to system:IPA_CODEC_PT finished.
14:44:48.450650 9884 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT and mtc:IPA_CTRL.
14:44:48.450828 9884 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-2435f21f.
14:44:48.450857 11677 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
14:44:48.450898 9884 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT.
14:44:48.450925 9884 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
14:44:48.450946 9884 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(256).
14:44:48.451001 9884 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
14:44:48.451023 9884 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
14:44:48.451115 11677 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
14:44:48.451304 11677 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
14:44:48.452456 11677 IPA_Emulation.ttcnpp:409 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
14:44:48.452548 9884 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
14:44:48.452580 9884 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
14:44:48.452603 9884 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
14:44:48.452622 9884 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
14:44:48.452649 9884 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:44:48.455798 11678 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:48.455831 11678 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: VirtMGW-MGCP-0(257), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
14:44:48.455845 11678 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:48.455882 11678 - Connected to MC.
14:44:48.455895 11678 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_si2_ncc_permitted.
14:44:48.455908 9884 BSC_Tests.ttcn:1073 PTC was created. Component reference: 257, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:44:48.455932 9884 BSC_Tests.ttcn:1074 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := false
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(257).
14:44:48.455996 9884 BSC_Tests.ttcn:1074 Function was started.
14:44:48.456018 9884 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:44:48.456040 9884 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.860811.
14:44:48.456073 9884 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
14:44:48.456098 9884 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:44:48.456197 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
14:44:48.456294 11677 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
14:44:48.456321 11677 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
14:44:48.456339 11677 IPA_Emulation.ttcnpp:921 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
14:44:48.456365 11677 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Encoding @Osmocom_CTRL_Types.CtrlMessage: {
    cmd := {
        verb := "GET",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
14:44:48.456450 11677 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Stream after encoding: "GET 860810752 bts.0.oml-connection-state"
14:44:48.456848 11677 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 860810752 bts.0.oml-connection-state")
}
14:44:48.456923 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '47455420383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 860810752 bts.0.oml-connection-state")
}
14:44:48.457026 11678 - Port MGCP was started.
14:44:48.457045 11678 - Port MGCP_CLIENT was started.
14:44:48.457050 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0029EE0047455420383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
14:44:48.457055 11678 - Port MGCP_CLIENT_MULTI was started.
14:44:48.457066 11678 - Port MGCP_PROC was started.
14:44:48.457074 11678 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
14:44:48.457108 11677 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
14:44:48.457135 11678 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := false
}, "VirtMGW-MGCP-0").
14:44:48.457340 11678 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(257):MGCP to system:MGCP_CODEC_PT.
14:44:48.457377 11678 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
14:44:48.457402 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 44965,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0038EE004745545F5245504C5920383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 1
14:44:48.457402 11678 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(257):MGCP to system:MGCP_CODEC_PT finished.
14:44:48.457422 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0038EE004745545F5245504C5920383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
14:44:48.457505 11678 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
14:44:48.457532 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 56,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '4745545F5245504C5920383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 860810752 bts.0.oml-connection-state degraded")
}
14:44:48.457561 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 860810752 bts.0.oml-connection-state degraded")
} id 1
14:44:48.457615 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:48.457636 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383630383130373532206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 860810752 bts.0.oml-connection-state degraded")
} id 1
14:44:48.457649 11677 IPA_Emulation.ttcnpp:790 Message with id 1 was extracted from the queue of IPA_PORT.
14:44:48.457674 11677 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Stream before decoding: "GET_REPLY 860810752 bts.0.oml-connection-state degraded"
14:44:48.457736 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 860810752 bts.0.oml-connection-state degraded
14:44:48.457746 11677 IPA_Emulation.ttcnpp:653 match_begin token: null_match
14:44:48.457755 11677 IPA_Emulation.ttcnpp:653 match_begin result: 0
14:44:48.457810 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 860810752 bts.0.oml-connection-state degraded
14:44:48.457822 11677 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET)|(SET)))"
14:44:48.457833 11677 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
14:44:48.457843 11677 IPA_Emulation.ttcnpp:653 match_begin result: 3
14:44:48.457852 11677 IPA_Emulation.ttcnpp:653 match_begin data: _REPLY 860810752 bts.0.oml-connection-state degraded
14:44:48.457861 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:48.457870 11677 IPA_Emulation.ttcnpp:653 match_begin result: -1
14:44:48.457903 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 860810752 bts.0.oml-connection-state degraded
14:44:48.457914 11677 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET_REPLY)|(SET_REPLY)))"
14:44:48.457924 11677 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
14:44:48.457934 11677 IPA_Emulation.ttcnpp:653 match_begin result: 9
14:44:48.457943 11677 IPA_Emulation.ttcnpp:653 match_begin data:  860810752 bts.0.oml-connection-state degraded
14:44:48.457952 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:48.457962 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:48.457972 11677 IPA_Emulation.ttcnpp:653 match_first data: 860810752 bts.0.oml-connection-state degraded
14:44:48.457981 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:48.457990 11677 IPA_Emulation.ttcnpp:653 match_first result: 9
14:44:48.457999 11677 IPA_Emulation.ttcnpp:653 match_list data: 860810752 bts.0.oml-connection-state degraded
14:44:48.458008 11677 IPA_Emulation.ttcnpp:653 match_list result: 9
14:44:48.458017 11677 IPA_Emulation.ttcnpp:653 match_begin data:  bts.0.oml-connection-state degraded
14:44:48.458026 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:48.458035 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:48.458044 11677 IPA_Emulation.ttcnpp:653 match_first data: bts.0.oml-connection-state degraded
14:44:48.458055 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:48.458064 11677 IPA_Emulation.ttcnpp:653 match_first result: 26
14:44:48.458073 11677 IPA_Emulation.ttcnpp:653 match_list data: bts.0.oml-connection-state degraded
14:44:48.458082 11677 IPA_Emulation.ttcnpp:653 match_list result: 26
14:44:48.458091 11677 IPA_Emulation.ttcnpp:653 match_begin data:  degraded
14:44:48.458100 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:48.458109 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:48.458118 11677 IPA_Emulation.ttcnpp:653 match_first data: degraded
14:44:48.458127 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:48.458136 11677 IPA_Emulation.ttcnpp:653 match_first result: -1
14:44:48.458145 11677 IPA_Emulation.ttcnpp:653 match_list data: degraded
14:44:48.458154 11677 IPA_Emulation.ttcnpp:653 match_list result: -1
14:44:48.458179 11677 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Decoded @Osmocom_CTRL_Types.CtrlMessage: {
    resp := {
        verb := "GET_REPLY",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
14:44:48.458210 11677 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
14:44:48.458252 9884 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
14:44:48.458281 9884 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:44:48.458305 9884 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "860810752",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
14:44:48.458325 9884 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
14:44:48.458346 9884 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:44:48.458365 9884 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:44:48.634985 11676 M3UA_Emulation.ttcn:560 Start timer T_Timer: 2 s
14:44:48.635468 11676 M3UA_Emulation.ttcn:561 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP_RESULT : {
    client_id := 8,
    error_status := false,
    error_message := omit
} id 1
14:44:48.635717 11676 M3UA_Emulation.ttcn:562 Matching on port SCTP_PORT succeeded:  matched
14:44:48.635891 11676 M3UA_Emulation.ttcn:562 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP_RESULT : {
    client_id := 8,
    error_status := false,
    error_message := omit
} id 1
14:44:48.636024 11676 M3UA_Emulation.ttcn:562 Message with id 1 was extracted from the queue of SCTP_PORT.
14:44:48.636139 11676 M3UA_Emulation.ttcn:569 SCTP_ConnectResult -> connection established from: "127.0.0.1":23908 to server: "127.0.0.1":2905 association #8
14:44:48.636273 11676 M3UA_Emulation.ttcn:579 Stop timer T_Timer: 2 s
14:44:48.636343 11676 M3UA_Emulation.ttcn:537 Start timer T_Assoc_restart: 60 s
14:44:48.636460 11676 M3UA_Emulation.ttcn:542 Start timer T_ASPUP_resend: 2 s
14:44:48.636484 11676 M3UA_Emulation.ttcn:543 Start timer T_ASPAC_resend: 2 s
14:44:48.636868 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE : {
    client_id := 8,
    sac_state := SCTP_COMM_UP (0)
} id 2
14:44:48.636960 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT succeeded:  matched
14:44:48.636989 11676 M3UA_Emulation.ttcn:668 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE : {
    client_id := 8,
    sac_state := SCTP_COMM_UP (0)
} id 2
14:44:48.637011 11676 M3UA_Emulation.ttcn:668 Message with id 2 was extracted from the queue of SCTP_PORT.
14:44:48.637547 11676 M3UA_Emulation.ttcn:959 enc_PDU_M3UA(): Encoding @M3UA_Types.PDU_M3UA: {
    m3UA_ASPUP := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0301'O,
        messageLength := 0,
        messageParameters := {
            aSP_Identifier := omit,
            info_String := omit
        }
    }
}
14:44:48.637910 11676 M3UA_Emulation.ttcn:959 enc_PDU_M3UA(): Stream after encoding: '0100030100000008'O
14:44:48.638086 11676 M3UA_Emulation.ttcn:959 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030100000008'O
}
14:44:48.638547 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030400000008'O
} id 3
14:44:48.638647 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.638707 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.638733 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030400000008'O
} id 3
14:44:48.638754 11676 M3UA_Emulation.ttcn:711 Message with id 3 was extracted from the queue of SCTP_PORT.
14:44:48.638830 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100030400000008'O
14:44:48.639083 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_ASPUP_Ack := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0304'O,
        messageLength := 8,
        messageParameters := {
            info_String := omit
        }
    }
}
14:44:48.639514 11676 M3UA_Emulation.ttcn:1189 enc_PDU_M3UA(): Encoding @M3UA_Types.PDU_M3UA: {
    m3UA_ASPAC := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0401'O,
        messageLength := 0,
        messageParameters := {
            traffic_Mode_Type := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
14:44:48.639684 11676 M3UA_Emulation.ttcn:1189 enc_PDU_M3UA(): Stream after encoding: '01000401000000100006000800000006'O
14:44:48.640028 11676 M3UA_Emulation.ttcn:1189 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000401000000100006000800000006'O
}
14:44:48.640122 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030300000008'O
} id 4
14:44:48.640147 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.640183 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.640198 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030300000008'O
} id 4
14:44:48.640213 11676 M3UA_Emulation.ttcn:711 Message with id 4 was extracted from the queue of SCTP_PORT.
14:44:48.640227 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100030300000008'O
14:44:48.640280 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_BEAT := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0303'O,
        messageLength := 8,
        messageParameters := {
            heartbeat_Data := omit
        }
    }
}
14:44:48.640347 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100020006000800000006'O
} id 5
14:44:48.640432 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.640447 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.640551 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100020006000800000006'O
} id 5
14:44:48.640636 11676 M3UA_Emulation.ttcn:711 Message with id 5 was extracted from the queue of SCTP_PORT.
14:44:48.640650 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100000100000018000D0008000100020006000800000006'O
14:44:48.640770 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_NOTIFY := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0001'O,
        messageLength := 24,
        messageParameters := {
            status := {
                tag := '000D'O,
                lengthInd := 8,
                statusType := '0001'O,
                statusInfo := '0002'O
            },
            aSP_Identifier := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
14:44:48.640836 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000403000000100006000800000006'O
} id 6
14:44:48.640849 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.640861 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.640873 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000403000000100006000800000006'O
} id 6
14:44:48.640884 11676 M3UA_Emulation.ttcn:711 Message with id 6 was extracted from the queue of SCTP_PORT.
14:44:48.640896 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '01000403000000100006000800000006'O
14:44:48.640943 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_ASPAC_Ack := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0403'O,
        messageLength := 16,
        messageParameters := {
            traffic_Mode_Type := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
14:44:48.641021 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100030006000800000006'O
} id 7
14:44:48.641036 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.641048 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.641060 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100030006000800000006'O
} id 7
14:44:48.641071 11676 M3UA_Emulation.ttcn:711 Message with id 7 was extracted from the queue of SCTP_PORT.
14:44:48.641083 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100000100000018000D0008000100030006000800000006'O
14:44:48.641098 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_NOTIFY := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0001'O,
        messageLength := 24,
        messageParameters := {
            status := {
                tag := '000D'O,
                lengthInd := 8,
                statusType := '0001'O,
                statusInfo := '0003'O
            },
            aSP_Identifier := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
14:44:48.641119 11676 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
} id 8
14:44:48.641132 11676 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
14:44:48.641142 11676 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
14:44:48.641155 11676 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
} id 8
14:44:48.641166 11676 M3UA_Emulation.ttcn:711 Message with id 8 was extracted from the queue of SCTP_PORT.
14:44:48.641177 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
14:44:48.641234 11676 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_DUNA := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0201'O,
        messageLength := 48,
        messageParameters := {
            network_Appearance := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            affected_Point_Codes := {
                tag := '0012'O,
                lengthInd := 12,
                pointCodes := {
                    {
                        mask := '00'O,
                        affected_Point_Code := '000002'O
                    },
                    {
                        mask := '00'O,
                        affected_Point_Code := '000003'O
                    }
                }
            },
            info_String := {
                tag := '0004'O,
                lengthInd := 18,
                infoString := '5246433436363620342E352E3100'O
            }
        }
    }
}
14:44:49.458468 9884 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:44:49.458665 9884 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:44:49.462252 11680 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
14:44:49.462425 11680 - TTCN-3 Parallel Test Component started on 8735d0ffe6e2. Component reference: IPA-BTS0-TRX0-RSL-IPA(258), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
14:44:49.462536 11680 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
14:44:49.462676 11680 - Connected to MC.
14:44:49.462829 11680 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_si2_ncc_permitted.
14:44:49.462933 9884 BSC_Tests.ttcn:951 PTC was created. Component reference: 258, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:44:49.463003 9884 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
14:44:49.463040 9884 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
14:44:49.463068 9884 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(258):IPA_PORT to system:IPA_CODEC_PT.
14:44:49.464053 11680 - Port IPA_PORT was started.
14:44:49.464078 11680 - Port CFG_PORT was started.
14:44:49.464090 11680 - Port MTP3_SP_PORT was started.
14:44:49.464102 11680 - Port IPA_MGCP_PORT was started.
14:44:49.464113 11680 - Port IPA_RSL_PORT was started.
14:44:49.464123 11680 - Port IPA_OML_PORT was started.
14:44:49.464134 11680 - Port IPA_CTRL_PORT was started.
14:44:49.464144 11680 - Port IPA_SP_PORT was started.
14:44:49.464155 11680 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
14:44:49.464190 11680 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
14:44:49.464304 9884 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(258):IPA_PORT to system:IPA_CODEC_PT finished.
14:44:49.464341 9884 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
14:44:49.464686 9884 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-28728b6e.
14:44:49.464759 11680 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
14:44:49.464821 9884 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT.
14:44:49.464876 9884 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
14:44:49.464905 9884 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
14:44:49.465144 9884 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-4b68ab76.
14:44:49.465213 11680 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
14:44:49.465269 9884 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT.
14:44:49.465329 9884 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
14:44:49.465353 9884 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(258).
14:44:49.465401 9884 BSC_Tests.ttcn:969 Function was started.
14:44:49.465424 9884 BSC_Tests.ttcn:976 Start timer T: 10 s
14:44:49.465505 11680 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
14:44:49.465678 11680 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
14:44:49.466493 11680 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Encoding @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
14:44:49.466602 11680 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Stream after encoding: '06'O
14:44:49.466773 11680 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
14:44:49.466866 11680 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
14:44:49.466933 11680 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '06'O
}
14:44:49.466974 11680 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0001FE06'O
14:44:49.467033 11680 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
14:44:49.467359 11680 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
14:44:49.467433 9884 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
14:44:49.467465 9884 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
14:44:49.467491 9884 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
14:44:49.467513 9884 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
14:44:49.467535 9884 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
14:44:49.468050 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
14:44:49.468071 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0011FE0401080107010201030104010501010100'O
14:44:49.468173 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 17,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '0401080107010201030104010501010100'O
}
14:44:49.468196 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
14:44:49.468220 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
14:44:49.468238 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0001FE06'O
14:44:49.468251 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '06'O
}
14:44:49.468264 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
14:44:49.468333 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
14:44:49.468361 11680 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
14:44:49.468378 11680 IPA_Emulation.ttcnpp:774 Message with id 1 was extracted from the queue of IPA_PORT.
14:44:49.468391 11680 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Stream before decoding: '0401080107010201030104010501010100'O
14:44:49.468423 11680 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Decoded @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
14:44:49.468444 11680 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
14:44:49.468618 11680 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Encoding @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
14:44:49.468665 11680 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Stream after encoding: '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
14:44:49.468684 11680 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
14:44:49.468741 11680 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
14:44:49.468755 11680 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
14:44:49.468774 11680 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
14:44:49.468790 11680 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
14:44:49.468830 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
14:44:49.468846 11680 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
14:44:49.468859 11680 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
14:44:49.468871 11680 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Stream before decoding: '06'O
14:44:49.468884 11680 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Decoded @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
14:44:49.468896 11680 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
14:44:49.468914 11680 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
14:44:49.468942 9884 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
14:44:49.468975 9884 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
14:44:49.468997 9884 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
14:44:49.469018 9884 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
14:44:49.469037 9884 BSC_Tests.ttcn:979 Stop timer T: 10 s
14:44:49.469061 9884 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:44:49.469086 9884 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.184819.
14:44:49.469122 9884 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
14:44:49.469149 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
14:44:49.469153 9884 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:44:49.469163 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
14:44:49.469172 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
14:44:49.469178 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
}
14:44:49.469197 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
14:44:49.469221 11677 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
14:44:49.469238 11677 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
14:44:49.469251 11677 IPA_Emulation.ttcnpp:921 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
14:44:49.469259 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.469264 11677 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Encoding @Osmocom_CTRL_Types.CtrlMessage: {
    cmd := {
        verb := "GET",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
14:44:49.469275 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.469279 11677 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Stream after encoding: "GET 184818861 bts.0.oml-connection-state"
14:44:49.469289 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
14:44:49.469302 11680 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
14:44:49.469305 11677 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 184818861 bts.0.oml-connection-state")
}
14:44:49.469320 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '47455420313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 184818861 bts.0.oml-connection-state")
}
14:44:49.469343 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0029EE0047455420313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
14:44:49.469360 11677 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
14:44:49.469361 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
14:44:49.469478 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 44965,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 2
14:44:49.469493 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0039EE004745545F5245504C5920313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
14:44:49.469510 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 57,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '4745545F5245504C5920313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 184818861 bts.0.oml-connection-state connected")
}
14:44:49.469538 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 184818861 bts.0.oml-connection-state connected")
} id 2
14:44:49.469552 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.469567 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313834383138383631206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 184818861 bts.0.oml-connection-state connected")
} id 2
14:44:49.469580 11677 IPA_Emulation.ttcnpp:790 Message with id 2 was extracted from the queue of IPA_PORT.
14:44:49.469592 11677 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Stream before decoding: "GET_REPLY 184818861 bts.0.oml-connection-state connected"
14:44:49.469609 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 184818861 bts.0.oml-connection-state connected
14:44:49.469621 11677 IPA_Emulation.ttcnpp:653 match_begin token: null_match
14:44:49.469633 11677 IPA_Emulation.ttcnpp:653 match_begin result: 0
14:44:49.469652 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 184818861 bts.0.oml-connection-state connected
14:44:49.469664 11677 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET)|(SET)))"
14:44:49.469677 11677 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
14:44:49.469689 11677 IPA_Emulation.ttcnpp:653 match_begin result: 3
14:44:49.469701 11677 IPA_Emulation.ttcnpp:653 match_begin data: _REPLY 184818861 bts.0.oml-connection-state connected
14:44:49.469712 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:49.469725 11677 IPA_Emulation.ttcnpp:653 match_begin result: -1
14:44:49.469740 11677 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 184818861 bts.0.oml-connection-state connected
14:44:49.469752 11677 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET_REPLY)|(SET_REPLY)))"
14:44:49.469752 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_1 (1)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '5506198FB38000000000000000000000000000E504002B'O
                }
            }
        }
    }
}
14:44:49.469765 11677 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
14:44:49.469777 11677 IPA_Emulation.ttcnpp:653 match_begin result: 9
14:44:49.469789 11677 IPA_Emulation.ttcnpp:653 match_begin data:  184818861 bts.0.oml-connection-state connected
14:44:49.469800 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:49.469811 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:49.469823 11677 IPA_Emulation.ttcnpp:653 match_first data: 184818861 bts.0.oml-connection-state connected
14:44:49.469834 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:49.469845 11677 IPA_Emulation.ttcnpp:653 match_first result: 9
14:44:49.469857 11677 IPA_Emulation.ttcnpp:653 match_list data: 184818861 bts.0.oml-connection-state connected
14:44:49.469868 11677 IPA_Emulation.ttcnpp:653 match_list result: 9
14:44:49.469880 11677 IPA_Emulation.ttcnpp:653 match_begin data:  bts.0.oml-connection-state connected
14:44:49.469892 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:49.469904 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:49.469915 11677 IPA_Emulation.ttcnpp:653 match_first data: bts.0.oml-connection-state connected
14:44:49.469927 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:49.469939 11677 IPA_Emulation.ttcnpp:653 match_first result: 26
14:44:49.469950 11677 IPA_Emulation.ttcnpp:653 match_list data: bts.0.oml-connection-state connected
14:44:49.469961 11677 IPA_Emulation.ttcnpp:653 match_list result: 26
14:44:49.469973 11677 IPA_Emulation.ttcnpp:653 match_begin data:  connected
14:44:49.469984 11677 IPA_Emulation.ttcnpp:653 match_begin token: " "
14:44:49.469995 11677 IPA_Emulation.ttcnpp:653 match_begin result: 1
14:44:49.470007 11677 IPA_Emulation.ttcnpp:653 match_first data: connected
14:44:49.470018 11677 IPA_Emulation.ttcnpp:653 match_first token: " "
14:44:49.470031 11677 IPA_Emulation.ttcnpp:653 match_first result: -1
14:44:49.470042 11677 IPA_Emulation.ttcnpp:653 match_list data: connected
14:44:49.470053 11677 IPA_Emulation.ttcnpp:653 match_list result: -1
14:44:49.470065 11677 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Decoded @Osmocom_CTRL_Types.CtrlMessage: {
    resp := {
        verb := "GET_REPLY",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
14:44:49.470081 11677 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
14:44:49.470108 9884 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
14:44:49.470138 9884 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:44:49.470163 9884 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "184818861",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
14:44:49.470184 9884 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
14:44:49.470206 9884 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:44:49.470226 9884 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:44:49.470544 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
14:44:49.470682 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
14:44:49.470693 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
14:44:49.470698 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E02271759061A00000000000000000000000000000000E0E50400'O
14:44:49.470714 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
}
14:44:49.470731 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
14:44:49.470745 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
14:44:49.470757 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0006000C1101801E0A'O
14:44:49.470770 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 6,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0A'O
}
14:44:49.470783 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
14:44:49.470796 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
14:44:49.470808 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
14:44:49.470822 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
}
14:44:49.470836 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
14:44:49.470850 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
14:44:49.470862 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
14:44:49.470875 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
}
14:44:49.470890 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
14:44:49.470905 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
14:44:49.470916 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
14:44:49.470929 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
}
14:44:49.470944 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
14:44:49.470957 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
14:44:49.470969 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
14:44:49.470983 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
}
14:44:49.470997 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
14:44:49.471010 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
14:44:49.471022 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
14:44:49.471035 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
}
14:44:49.471049 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
14:44:49.471062 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
14:44:49.471074 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001A00101A1E050B001349061D10000000000000000000000000000000'O
14:44:49.471087 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 26,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E050B001349061D10000000000000000000000000000000'O
}
14:44:49.471100 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
14:44:49.471113 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
14:44:49.471126 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '000400101A1E0D'O
14:44:49.471138 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 4,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E0D'O
}
14:44:49.471151 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
14:44:49.471164 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471177 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471190 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
14:44:49.471202 11680 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
14:44:49.471214 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
14:44:49.471232 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2 (2)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '59061A00000000000000000000000000000000E0E50400'O
                }
            }
        }
    }
}
14:44:49.471292 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
}
14:44:49.471312 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471326 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471328 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
} id 4
14:44:49.471339 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
14:44:49.471352 11680 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
14:44:49.471364 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0A'O
14:44:49.471379 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
            }
        }
    }
}
14:44:49.471401 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
14:44:49.471418 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471430 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471432 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
14:44:49.471443 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
14:44:49.471456 11680 IPA_Emulation.ttcnpp:790 Message with id 6 was extracted from the queue of IPA_PORT.
14:44:49.471467 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
14:44:49.471483 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                }
            }
        }
    }
}
14:44:49.471509 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
14:44:49.471524 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471537 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471540 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
14:44:49.471550 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
14:44:49.471560 11680 IPA_Emulation.ttcnpp:790 Message with id 7 was extracted from the queue of IPA_PORT.
14:44:49.471572 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
14:44:49.471587 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                }
            }
        }
    }
}
14:44:49.471610 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
14:44:49.471627 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471639 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471642 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
14:44:49.471652 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
14:44:49.471665 11680 IPA_Emulation.ttcnpp:790 Message with id 8 was extracted from the queue of IPA_PORT.
14:44:49.471682 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
14:44:49.471698 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_3 (3)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                }
            }
        }
    }
}
14:44:49.471721 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
14:44:49.471736 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471748 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471751 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
14:44:49.471761 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
14:44:49.471771 11680 IPA_Emulation.ttcnpp:790 Message with id 9 was extracted from the queue of IPA_PORT.
14:44:49.471783 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
14:44:49.471797 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_4 (4)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                }
            }
        }
    }
}
14:44:49.471821 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
14:44:49.471836 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471849 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471851 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
14:44:49.471862 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
14:44:49.471875 11680 IPA_Emulation.ttcnpp:790 Message with id 10 was extracted from the queue of IPA_PORT.
14:44:49.471887 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
14:44:49.471903 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_13 (40)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                }
            }
        }
    }
}
14:44:49.471924 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
14:44:49.471939 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.471951 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.471954 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
14:44:49.471964 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
14:44:49.471975 11680 IPA_Emulation.ttcnpp:790 Message with id 11 was extracted from the queue of IPA_PORT.
14:44:49.471987 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E050B001349061D10000000000000000000000000000000'O
14:44:49.472015 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5 (5)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 19,
                    payload := '49061D10000000000000000000000000000000'O
                }
            }
        }
    }
}
14:44:49.472069 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
14:44:49.472086 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.472099 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.472100 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
14:44:49.472110 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
14:44:49.472124 11680 IPA_Emulation.ttcnpp:790 Message with id 12 was extracted from the queue of IPA_PORT.
14:44:49.472136 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E0D'O
14:44:49.472149 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
            }
        }
    }
}
14:44:49.472166 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
14:44:49.472189 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
14:44:49.472192 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
14:44:49.472202 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
14:44:49.472216 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 26,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E0E0B00134906069E050020000000000000000000000000'O
}
14:44:49.472231 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
14:44:49.472244 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197E02B'O
} id 14
14:44:49.472256 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001400101A1E060B000D2D061E000000F110000197E02B'O
14:44:49.472269 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 20,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E060B000D2D061E000000F110000197E02B'O
}
14:44:49.472283 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197E02B'O
} id 14
14:44:49.472297 11680 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
14:44:49.472309 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
14:44:49.472323 11680 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 63,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
}
14:44:49.472340 11680 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
14:44:49.472352 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.472366 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.472378 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
14:44:49.472390 11680 IPA_Emulation.ttcnpp:790 Message with id 13 was extracted from the queue of IPA_PORT.
14:44:49.472403 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E0E0B00134906069E050020000000000000000000000000'O
14:44:49.472417 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 19,
                    payload := '4906069E050020000000000000000000000000'O
                }
            }
        }
    }
}
14:44:49.472437 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
14:44:49.472452 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.472463 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.472465 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
14:44:49.472476 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197E02B'O
} id 14
14:44:49.472488 11680 IPA_Emulation.ttcnpp:790 Message with id 14 was extracted from the queue of IPA_PORT.
14:44:49.472500 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E060B000D2D061E000000F110000197E02B'O
14:44:49.472513 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_6 (6)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 13,
                    payload := '2D061E000000F110000197E02B'O
                }
            }
        }
    }
}
14:44:49.472532 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197E02B'O
                    }
                }
            }
        }
    }
}
14:44:49.472545 11680 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
14:44:49.472557 11680 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
14:44:49.472558 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197E02B'O
                    }
                }
            }
        }
    }
} id 14
14:44:49.472570 11680 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
14:44:49.472583 11680 IPA_Emulation.ttcnpp:790 Message with id 15 was extracted from the queue of IPA_PORT.
14:44:49.472596 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
14:44:49.472646 11680 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
    ies := {
        {
            iei := RSL_IE_MS_POWER (13),
            body := {
                ms_power := {
                    reserved := 0,
                    fpc_epc := false,
                    power_level := 0
                }
            }
        },
        {
            iei := RSL_IE_BS_POWER (4),
            body := {
                bs_power := {
                    reserved := 0,
                    epc := false,
                    fpc := false,
                    power_level := 0
                }
            }
        },
        {
            iei := RSL_IE_MS_POWER_PARAM (31),
            body := {
                ms_power_params := {
                    len := 55,
                    params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                }
            }
        }
    }
}
14:44:49.472761 11680 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
14:44:49.472800 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
14:44:50.470414 9884 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:44:50.470536 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:50.470592 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.470722 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 38
14:44:50.470760 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.470785 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.470821 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.470835 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 38
14:44:50.470850 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 38 was extracted from the queue of BSCVTY.
14:44:50.470863 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.470877 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
14:44:50.470895 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.470978 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 39
14:44:50.470998 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.471017 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.471039 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.471053 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 39
14:44:50.471066 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 39 was extracted from the queue of BSCVTY.
14:44:50.471079 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.471092 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
14:44:50.471109 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.471137 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 40
14:44:50.471157 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.471175 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.471198 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.471211 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 40
14:44:50.471225 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 40 was extracted from the queue of BSCVTY.
14:44:50.471238 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.471252 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:44:50.471267 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.471306 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 41
14:44:50.471324 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.471343 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.471364 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.471378 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 41
14:44:50.471391 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 41 was extracted from the queue of BSCVTY.
14:44:50.471404 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.471417 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:44:50.471434 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.471451 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 42
14:44:50.471470 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.471488 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:50.471501 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 42
14:44:50.471514 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 42 was extracted from the queue of BSCVTY.
14:44:50.471528 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.471542 9884 Osmocom_VTY_Functions.ttcn:338 "TC_si2_ncc_permitted() start"
14:44:50.471567 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_si2_ncc_permitted() start"
14:44:50.471631 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.471696 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 43
14:44:50.471819 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.471888 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:50.471903 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 43
14:44:50.471916 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 43 was extracted from the queue of BSCVTY.
14:44:50.471929 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.471942 9884 BSC_Tests.ttcn:3143 Start timer T: 5 s
14:44:50.472030 9884 BSC_Tests.ttcn:3147 Matching on port IPA_RSL[0][0] .rsl.ies{
    {
        iei := RSL_IE_CHAN_NR (1),
        body := {
            chan_nr := {
                u := {
                    ch0 := RSL_CHAN_NR_BCCH (16)
                },
                tn := 0
            }
        }
    },
    {
        iei := RSL_IE_SYSINFO_TYPE (30),
        body := {
            sysinfo_type := RSL_SYSTEM_INFO_1 (1)
        }
    },
    {
        iei := RSL_IE_FULL_BCCH_INFO (39),
        body := {
            other := {
                len := 23,
                payload := '5506198FB38000000000000000000000000000E504002B'O
            }
        }
    }
} with {
    {
        iei := ?,
        body := {
            chan_nr := {
                u := {
                    ch0 := RSL_CHAN_NR_BCCH (16)
                },
                tn := 0
            }
        }
    },
    {
        iei := ?,
        body := {
            sysinfo_type := RSL_SYSTEM_INFO_2 (2)
        }
    },
    {
        iei := ?,
        body := {
            other := {
                len := ?,
                payload := ?
            }
        }
    },
    *
} unmatched: First message in the queue does not match the template: 
14:44:50.472048 9884 BSC_Tests.ttcn:3162 Matching on port IPA_RSL[0][0] succeeded.
14:44:50.472065 9884 BSC_Tests.ttcn:3162 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_RSL_Unitdata: {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
14:44:50.472082 9884 BSC_Tests.ttcn:3162 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
14:44:50.472100 9884 BSC_Tests.ttcn:3147 Matching on port IPA_RSL[0][0] succeeded:  matched
14:44:50.472114 9884 BSC_Tests.ttcn:3147 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
} id 4
14:44:50.472130 9884 BSC_Tests.ttcn:3147 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
14:44:50.472173 9884 BSC_Tests.ttcn:3149 dec_SystemInformation(): Stream before decoding: '59061A00000000000000000000000000000000E0E50400'O
14:44:50.472206 9884 BSC_Tests.ttcn:3149 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: {
    header := {
        l2_plen := {
            l2_plen := 22,
            zero_one := '01'B
        },
        skip_indicator := 0,
        rr_protocol_discriminator := 6,
        message_type := SYSTEM_INFORMATION_TYPE_2 (26)
    },
    payload := {
        si2 := {
            bcch_freq_list := '00000000000000000000000000000000'O,
            ncc_permitted := '11100000'B,
            rach_control := {
                max_retrans := RACH_MAX_RETRANS_7 (3),
                tx_integer := '1001'B,
                cell_barr_access := false,
                re_not_allowed := true,
                acc := '0000010000000000'B
            }
        }
    }
}
14:44:50.472241 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:44:50.472261 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.472346 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 44
14:44:50.472370 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.472390 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.472414 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.472428 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 44
14:44:50.472441 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 44 was extracted from the queue of BSCVTY.
14:44:50.472454 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.472467 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
14:44:50.472483 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.472557 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 45
14:44:50.472576 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.472596 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.472617 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.472631 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 45
14:44:50.472643 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 45 was extracted from the queue of BSCVTY.
14:44:50.472657 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.472670 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
14:44:50.472685 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.472759 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 46
14:44:50.472778 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.472795 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.472816 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.472829 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 46
14:44:50.472844 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 46 was extracted from the queue of BSCVTY.
14:44:50.472857 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.472870 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "ncc-permitted all"
14:44:50.472885 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.472914 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 47
14:44:50.472932 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.472949 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.472970 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:44:50.472982 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 47
14:44:50.472995 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 47 was extracted from the queue of BSCVTY.
14:44:50.473007 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.473020 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:44:50.473035 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.473051 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 48
14:44:50.473069 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.473087 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:50.473099 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 48
14:44:50.473111 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 48 was extracted from the queue of BSCVTY.
14:44:50.473124 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.473147 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
14:44:50.473162 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:44:50.473373 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" id 49
14:44:50.473387 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 50
14:44:50.473406 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.473425 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:44:50.473444 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:44:50.473460 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:44:50.473474 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" with ? matched
14:44:50.473487 9884 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1466015 bytes in 1340 blocks)" id 49
14:44:50.473501 9884 Osmocom_VTY_Functions.ttcn:85 Message with id 49 was extracted from the queue of BSCVTY.
14:44:50.473518 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:44:50.473535 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:44:50.473548 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 50
14:44:50.473561 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 50 was extracted from the queue of BSCVTY.
14:44:50.473573 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:44:50.473586 9884 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
14:44:50.473605 9884 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
14:44:50.473622 9884 BSC_Tests.ttcn:888 Stopping all components.
14:44:50.473666 11672 StatsD_Checker.ttcnpp:143 Kill was requested from MC.
14:44:50.473666 11673 SCCP_Emulation.ttcn:5439 Stopping test component execution.
14:44:50.473668 11675 SCCP_Emulation.ttcn:5439 Stop was requested from MC.
14:44:50.473679 11677 IPA_Emulation.ttcnpp:772 Kill was requested from MC.
14:44:50.473688 11674 M3UA_Emulation.ttcn:596 Stopping test component execution.
14:44:50.473695 11678 MGCP_Emulation.ttcn:301 Stop was requested from MC.
14:44:50.473695 11680 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
14:44:50.473749 11676 M3UA_Emulation.ttcn:596 Stop was requested from MC.
14:44:50.473770 11675 SCCP_Emulation.ttcn:5439 Stopping test component execution.
14:44:50.473791 11672 StatsD_Checker.ttcnpp:143 Terminating test component execution.
14:44:50.473799 11680 IPA_Emulation.ttcnpp:772 Stopping test component execution.
14:44:50.473803 11677 IPA_Emulation.ttcnpp:772 Terminating test component execution.
14:44:50.473861 11676 M3UA_Emulation.ttcn:596 Stopping test component execution.
14:44:50.473874 11678 MGCP_Emulation.ttcn:301 Stopping test component execution.
14:44:50.474114 11672 - Function main was stopped. PTC terminates.
14:44:50.474121 11673 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
14:44:50.474149 11680 - Function main_client was stopped. PTC remains alive and is waiting for next start.
14:44:50.474168 11675 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
14:44:50.474195 11672 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
14:44:50.474298 11674 - Function f_M3UA_Emulation was stopped. PTC remains alive and is waiting for next start.
14:44:50.474305 11672 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
14:44:50.474365 11672 - Port STATSVTY was unmapped from system:STATSVTY.
14:44:50.474379 11677 - Function main_client was stopped. PTC terminates.
14:44:50.474411 11676 - Function f_M3UA_Emulation was stopped. PTC remains alive and is waiting for next start.
14:44:50.474430 11672 - Port STATSVTY was stopped.
14:44:50.474440 11678 - Function main was stopped. PTC remains alive and is waiting for next start.
14:44:50.474451 11672 - Port STATSD_PROC was stopped.
14:44:50.474462 11672 - Removing unterminated mapping between port STATS and system:STATS.
14:44:50.474471 11677 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
14:44:50.474497 11677 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
14:44:50.474657 11672 - Port STATS was unmapped from system:STATS.
14:44:50.474679 11672 - Port STATS was stopped.
14:44:50.474691 11672 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.474707 11672 - Final verdict of PTC: none
14:44:50.474745 11672 - Disconnected from MC.
14:44:50.474761 11672 - TTCN-3 Parallel Test Component finished.
14:44:50.474831 11677 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
14:44:50.474867 11677 - Port IPA_PORT was stopped.
14:44:50.474888 11677 - Port CFG_PORT was stopped.
14:44:50.474906 11677 - Port MTP3_SP_PORT was stopped.
14:44:50.474925 11677 - Port IPA_MGCP_PORT was stopped.
14:44:50.474943 11677 - Port IPA_RSL_PORT was stopped.
14:44:50.474961 11677 - Port IPA_OML_PORT was stopped.
14:44:50.474979 11677 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
14:44:50.475010 11677 - Port IPA_CTRL_PORT was stopped.
14:44:50.475015 9884 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT was closed unexpectedly by the peer.
14:44:50.475030 11677 - Port IPA_SP_PORT was stopped.
14:44:50.475033 9884 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT.
14:44:50.475050 11677 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.475120 11677 - Final verdict of PTC: none
14:44:50.475128 9884 BSC_Tests.ttcn:888 All components were stopped.
14:44:50.475143 9884 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
14:44:50.475158 9884 BSC_Tests.ttcn:890 Stopping test component execution.
14:44:50.475173 11677 - Disconnected from MC.
14:44:50.475184 9884 BSC_Tests.ttcn:3174 Test case TC_si2_ncc_permitted was stopped.
14:44:50.475196 11677 - TTCN-3 Parallel Test Component finished.
14:44:50.475199 9884 BSC_Tests.ttcn:3174 Terminating component type BSC_Tests.test_CT.
14:44:50.475212 9884 BSC_Tests.ttcn:3174 Default with id 1 (altstep as_Tguard) was deactivated.
14:44:50.475226 9884 BSC_Tests.ttcn:3174 Stop timer T_guard: 30 s
14:44:50.475241 9884 BSC_Tests.ttcn:3174 Port IPA_CTRL was stopped.
14:44:50.475254 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[0] was stopped.
14:44:50.475266 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[1] was stopped.
14:44:50.475323 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[2] was stopped.
14:44:50.475358 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT.
14:44:50.475401 9884 BSC_Tests.ttcn:3174 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475402 11680 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
14:44:50.475445 11680 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
14:44:50.475446 9884 BSC_Tests.ttcn:3174 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475469 9884 BSC_Tests.ttcn:3174 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475490 9884 BSC_Tests.ttcn:3174 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475511 9884 BSC_Tests.ttcn:3174 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475531 9884 BSC_Tests.ttcn:3174 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475552 9884 BSC_Tests.ttcn:3174 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475572 9884 BSC_Tests.ttcn:3174 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475592 9884 BSC_Tests.ttcn:3174 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475612 9884 BSC_Tests.ttcn:3174 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475632 9884 BSC_Tests.ttcn:3174 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
14:44:50.475652 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][0] was stopped.
14:44:50.475671 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][1] was stopped.
14:44:50.475707 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][2] was stopped.
14:44:50.475727 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][3] was stopped.
14:44:50.475746 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][0] was stopped.
14:44:50.475765 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][1] was stopped.
14:44:50.475784 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][2] was stopped.
14:44:50.475802 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][3] was stopped.
14:44:50.475821 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][0] was stopped.
14:44:50.475840 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][1] was stopped.
14:44:50.475859 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][2] was stopped.
14:44:50.475885 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][3] was stopped.
14:44:50.475905 9884 BSC_Tests.ttcn:3174 Port IPA was stopped.
14:44:50.475925 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CTRL was stopped.
14:44:50.475943 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT.
14:44:50.475975 11680 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
14:44:50.475975 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][0] was stopped.
14:44:50.476011 11680 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
14:44:50.476021 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][1] was stopped.
14:44:50.476041 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][2] was stopped.
14:44:50.476060 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][3] was stopped.
14:44:50.476079 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][0] was stopped.
14:44:50.476097 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][1] was stopped.
14:44:50.476116 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][2] was stopped.
14:44:50.476134 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][3] was stopped.
14:44:50.476153 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][0] was stopped.
14:44:50.476172 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][1] was stopped.
14:44:50.476190 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][2] was stopped.
14:44:50.476210 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][3] was stopped.
14:44:50.476229 9884 BSC_Tests.ttcn:3174 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
14:44:50.476272 9884 BSC_Tests.ttcn:3174 Port BSCVTY was unmapped from system:BSCVTY.
14:44:50.476299 9884 BSC_Tests.ttcn:3174 Port BSCVTY was stopped.
14:44:50.476319 9884 BSC_Tests.ttcn:3174 Port STPVTY was stopped.
14:44:50.476338 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
14:44:50.476357 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
14:44:50.476375 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
14:44:50.476395 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT.
14:44:50.476428 9884 BSC_Tests.ttcn:3174 Port BSSAP was stopped.
14:44:50.476464 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT.
14:44:50.476495 9884 BSC_Tests.ttcn:3174 Port BSSAP_LE was stopped.
14:44:50.476503 11675 - Connection of port SCCP_SP_PORT to mtc:BSSAP_LE was closed unexpectedly by the peer.
14:44:50.476528 9884 BSC_Tests.ttcn:3174 Component type BSC_Tests.test_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.476537 11675 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP_LE.
14:44:50.476550 9884 BSC_Tests.ttcn:3174 Waiting for PTCs to finish.
14:44:50.476582 11673 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476585 11675 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476591 11680 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476594 11676 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476595 11674 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476602 11673 - Terminating component type SCCP_Emulation.SCCP_CT.
14:44:50.476611 11678 - Kill was requested from MC. Terminating idle PTC.
14:44:50.476611 11680 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
14:44:50.476621 11676 - Terminating component type M3UA_Emulation.M3UA_CT.
14:44:50.476622 11680 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
14:44:50.476626 11673 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.476626 11675 - Terminating component type SCCP_Emulation.SCCP_CT.
14:44:50.476628 11674 - Terminating component type M3UA_Emulation.M3UA_CT.
14:44:50.476668 11673 - Final verdict of PTC: none
14:44:50.476669 11676 - Stop timer T_ASPUP_resend: 2 s
14:44:50.476679 11678 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
14:44:50.476682 11675 - Port SCCP_SP_PORT was stopped.
14:44:50.476692 11676 - Stop timer T_ASPAC_resend: 2 s
14:44:50.476701 11678 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
14:44:50.476703 11675 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtSMLC-M3UA(255):MTP3_SP_PORT.
14:44:50.476715 11676 - Stop timer T_Assoc_restart: 60 s
14:44:50.476758 11676 - Removing unterminated connection between port MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT.
14:44:50.476770 11675 - Port MTP3_SCCP_PORT was stopped.
14:44:50.476820 11675 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.476833 11680 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
14:44:50.476853 11674 - Component type M3UA_Emulation.M3UA_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.476857 11675 - Final verdict of PTC: none
14:44:50.476886 11676 - Port MTP3_SP_PORT was stopped.
14:44:50.476891 11674 - Final verdict of PTC: none
14:44:50.476924 11675 - Disconnected from MC.
14:44:50.476974 11675 - TTCN-3 Parallel Test Component finished.
14:44:50.477003 11676 - Removing unterminated mapping between port SCTP_PORT and system:sctp.
14:44:50.477113 11678 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
14:44:50.477144 11678 - Port MGCP was stopped.
14:44:50.477162 11678 - Port MGCP_CLIENT was stopped.
14:44:50.477224 11678 - Port MGCP_CLIENT_MULTI was stopped.
14:44:50.477253 11676 - Port SCTP_PORT was unmapped from system:sctp.
14:44:50.477259 11680 - Port IPA_PORT was stopped.
14:44:50.477321 11678 - Port MGCP_PROC was stopped.
14:44:50.477335 11676 - Port SCTP_PORT was stopped.
14:44:50.477336 11680 - Port CFG_PORT was stopped.
14:44:50.477366 11678 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.477377 11680 - Port MTP3_SP_PORT was stopped.
14:44:50.477405 11678 - Final verdict of PTC: none
14:44:50.477449 11676 - Component type M3UA_Emulation.M3UA_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.477454 11680 - Port IPA_MGCP_PORT was stopped.
14:44:50.477482 11680 - Port IPA_RSL_PORT was stopped.
14:44:50.477504 11676 - Final verdict of PTC: none
14:44:50.477519 11680 - Port IPA_OML_PORT was stopped.
14:44:50.477538 11680 - Port IPA_CTRL_PORT was stopped.
14:44:50.477544 11678 - Disconnected from MC.
14:44:50.477559 11680 - Port IPA_SP_PORT was stopped.
14:44:50.477586 11678 - TTCN-3 Parallel Test Component finished.
14:44:50.477590 11676 - Disconnected from MC.
14:44:50.477590 11680 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
14:44:50.477686 11680 - Final verdict of PTC: none
14:44:50.477711 11676 - TTCN-3 Parallel Test Component finished.
14:44:50.477777 11680 - Disconnected from MC.
14:44:50.477786 9884 BSC_Tests.ttcn:3174 Setting final verdict of the test case.
14:44:50.477859 11680 - TTCN-3 Parallel Test Component finished.
14:44:50.478319 9884 BSC_Tests.ttcn:3174 Local verdict of MTC: pass
14:44:50.478403 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-STATS(251): none (pass -> pass)
14:44:50.478488 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-SCCP(252): none (pass -> pass)
14:44:50.478561 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-M3UA(253): none (pass -> pass)
14:44:50.478594 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtSMLC-SCCP(254): none (pass -> pass)
14:44:50.478670 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtSMLC-M3UA(255): none (pass -> pass)
14:44:50.478715 9884 BSC_Tests.ttcn:3174 Local verdict of PTC IPA-CTRL-CLI-IPA(256): none (pass -> pass)
14:44:50.478792 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMGW-MGCP-0(257): none (pass -> pass)
14:44:50.478848 9884 BSC_Tests.ttcn:3174 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(258): none (pass -> pass)
14:44:50.478896 9884 BSC_Tests.ttcn:3174 Test case TC_si2_ncc_permitted finished. Verdict: pass
14:44:50.478940 9884 BSC_Tests.ttcn:3174 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2_ncc_permitted pass'.
14:44:55.743630 9884 BSC_Tests.ttcn:3174 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2_ncc_permitted pass' was executed successfully (exit status: 0).
14:44:55.743796 9884 BSC_Tests.ttcn:1399 Switching to log file `BSC_Tests-TC_chan_act_noreply-8735d0ffe6e2-mtc-9884.log'
