-- 3GPP TS 38.413 V17.5.0 (2023-06)
-- 9.4.3	Elementary Procedure Definitions
-- **************************************************************
--
-- Elementary Procedure definitions
--
-- **************************************************************

NGAP-PDU-Descriptions  {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Descriptions (0)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	Criticality,
	ProcedureCode
FROM NGAP-CommonDataTypes

	AMFConfigurationUpdate,
	AMFConfigurationUpdateAcknowledge,
	AMFConfigurationUpdateFailure,
	AMFCPRelocationIndication,
	AMFStatusIndication,
	BroadcastSessionModificationFailure,
	BroadcastSessionModificationRequest,
	BroadcastSessionModificationResponse,
	BroadcastSessionReleaseRequest,
	BroadcastSessionReleaseRequired,
	BroadcastSessionReleaseResponse,
	BroadcastSessionSetupFailure,
	BroadcastSessionSetupRequest,
	BroadcastSessionSetupResponse,
	CellTrafficTrace,
	ConnectionEstablishmentIndication,
	DeactivateTrace,
	DistributionReleaseRequest,
	DistributionReleaseResponse,
	DistributionSetupFailure,
	DistributionSetupRequest,
	DistributionSetupResponse,
	DownlinkNASTransport,
	DownlinkNonUEAssociatedNRPPaTransport,
	DownlinkRANConfigurationTransfer,
	DownlinkRANEarlyStatusTransfer,
	DownlinkRANStatusTransfer,
	DownlinkUEAssociatedNRPPaTransport,
	ErrorIndication,
	HandoverCancel,
	HandoverCancelAcknowledge,
	HandoverCommand,
	HandoverFailure,
	HandoverNotify,
	HandoverPreparationFailure,
	HandoverRequest,
	HandoverRequestAcknowledge,
	HandoverRequired,
	HandoverSuccess,
	InitialContextSetupFailure,
	InitialContextSetupRequest,
	InitialContextSetupResponse,
	InitialUEMessage,
	LocationReport,
	LocationReportingControl,
	LocationReportingFailureIndication,
	MulticastSessionActivationFailure,
	MulticastSessionActivationRequest,
	MulticastSessionActivationResponse,
	MulticastSessionDeactivationRequest,
	MulticastSessionDeactivationResponse,
	MulticastSessionUpdateFailure,
	MulticastSessionUpdateRequest,
	MulticastSessionUpdateResponse,
	MulticastGroupPaging,
	NASNonDeliveryIndication,
	NGReset,
	NGResetAcknowledge,
	NGSetupFailure,
	NGSetupRequest,
	NGSetupResponse,
	OverloadStart,
	OverloadStop,
	Paging,
	PathSwitchRequest,
	PathSwitchRequestAcknowledge,
	PathSwitchRequestFailure,
	PDUSessionResourceModifyConfirm,
	PDUSessionResourceModifyIndication,
	PDUSessionResourceModifyRequest,
	PDUSessionResourceModifyResponse,
	PDUSessionResourceNotify,
	PDUSessionResourceReleaseCommand,
	PDUSessionResourceReleaseResponse,
	PDUSessionResourceSetupRequest,
	PDUSessionResourceSetupResponse,
	PrivateMessage,
	PWSCancelRequest,
	PWSCancelResponse,
	PWSFailureIndication,
	PWSRestartIndication,
	RANConfigurationUpdate,
	RANConfigurationUpdateAcknowledge,
	RANConfigurationUpdateFailure,
	RANCPRelocationIndication,
	RerouteNASRequest,
	RetrieveUEInformation,
	RRCInactiveTransitionReport,
	SecondaryRATDataUsageReport,
	TraceFailureIndication,
	TraceStart,
	UEContextModificationFailure,
	UEContextModificationRequest,
	UEContextModificationResponse,
	UEContextReleaseCommand,
	UEContextReleaseComplete,
	UEContextReleaseRequest,
	UEContextResumeRequest,
	UEContextResumeResponse,
	UEContextResumeFailure,
	UEContextSuspendRequest,
	UEContextSuspendResponse,
	UEContextSuspendFailure,
	UEInformationTransfer,
	UERadioCapabilityCheckRequest,
	UERadioCapabilityCheckResponse,
	UERadioCapabilityIDMappingRequest,
	UERadioCapabilityIDMappingResponse,
	UERadioCapabilityInfoIndication,
	UETNLABindingReleaseRequest,
	UplinkNASTransport,
	UplinkNonUEAssociatedNRPPaTransport,
	UplinkRANConfigurationTransfer,
	UplinkRANEarlyStatusTransfer,
	UplinkRANStatusTransfer,
	UplinkUEAssociatedNRPPaTransport,
	WriteReplaceWarningRequest,
	WriteReplaceWarningResponse,
	UplinkRIMInformationTransfer,
	DownlinkRIMInformationTransfer

FROM NGAP-PDU-Contents

	id-AMFConfigurationUpdate,
	id-AMFCPRelocationIndication,
	id-AMFStatusIndication,
	id-BroadcastSessionModification,
	id-BroadcastSessionRelease,
	id-BroadcastSessionReleaseRequired,
	id-BroadcastSessionSetup,
	id-CellTrafficTrace,
	id-ConnectionEstablishmentIndication,
	id-DeactivateTrace,
	id-DistributionSetup,
	id-DistributionRelease,
	id-DownlinkNASTransport,
	id-DownlinkNonUEAssociatedNRPPaTransport,
	id-DownlinkRANConfigurationTransfer,
	id-DownlinkRANEarlyStatusTransfer,
	id-DownlinkRANStatusTransfer,
	id-DownlinkUEAssociatedNRPPaTransport,
	id-ErrorIndication,
	id-HandoverCancel,
	id-HandoverNotification,
	id-HandoverPreparation,
	id-HandoverResourceAllocation,
	id-HandoverSuccess,
	id-InitialContextSetup,
	id-InitialUEMessage,
	id-LocationReport,
	id-LocationReportingControl,
	id-LocationReportingFailureIndication,
	id-MulticastSessionActivation,
	id-MulticastSessionDeactivation,
	id-MulticastSessionUpdate,
	id-MulticastGroupPaging,
	id-NASNonDeliveryIndication,
	id-NGReset,
	id-NGSetup,
	id-OverloadStart,
	id-OverloadStop,
	id-Paging,
	id-PathSwitchRequest,
	id-PDUSessionResourceModify,
	id-PDUSessionResourceModifyIndication,
	id-PDUSessionResourceNotify,
	id-PDUSessionResourceRelease,
	id-PDUSessionResourceSetup,
	id-PrivateMessage,
	id-PWSCancel,
	id-PWSFailureIndication,
	id-PWSRestartIndication,
	id-RANConfigurationUpdate,
	id-RANCPRelocationIndication,
	id-RerouteNASRequest,
	id-RetrieveUEInformation,
	id-RRCInactiveTransitionReport,
	id-SecondaryRATDataUsageReport,
	id-TraceFailureIndication,
	id-TraceStart,
	id-UEContextModification,
	id-UEContextRelease,
	id-UEContextReleaseRequest,
	id-UEContextResume,
	id-UEContextSuspend,
	id-UEInformationTransfer,
	id-UERadioCapabilityCheck,
	id-UERadioCapabilityIDMapping,
	id-UERadioCapabilityInfoIndication,
	id-UETNLABindingRelease,
	id-UplinkNASTransport,
	id-UplinkNonUEAssociatedNRPPaTransport,
	id-UplinkRANConfigurationTransfer,
	id-UplinkRANEarlyStatusTransfer,
	id-UplinkRANStatusTransfer,
	id-UplinkUEAssociatedNRPPaTransport,
	id-WriteReplaceWarning,
	id-UplinkRIMInformationTransfer,
	id-DownlinkRIMInformationTransfer

FROM NGAP-Constants;

-- **************************************************************
--
-- Interface Elementary Procedure Class
--
-- **************************************************************

NGAP-ELEMENTARY-PROCEDURE ::= CLASS {
	&InitiatingMessage				,
	&SuccessfulOutcome							OPTIONAL,
	&UnsuccessfulOutcome						OPTIONAL,
	&procedureCode				ProcedureCode	UNIQUE,
	&criticality				Criticality	DEFAULT ignore
}

WITH SYNTAX {
	INITIATING MESSAGE			&InitiatingMessage
	[SUCCESSFUL OUTCOME			&SuccessfulOutcome]
	[UNSUCCESSFUL OUTCOME		&UnsuccessfulOutcome]
	PROCEDURE CODE				&procedureCode
	[CRITICALITY				&criticality]
}

-- **************************************************************
--
-- Interface PDU Definition
--
-- **************************************************************

NGAP-PDU ::= CHOICE {
	initiatingMessage			InitiatingMessage,
	successfulOutcome			SuccessfulOutcome,
	unsuccessfulOutcome			UnsuccessfulOutcome,
	...
}

InitiatingMessage ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&InitiatingMessage	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

SuccessfulOutcome ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

UnsuccessfulOutcome ::= SEQUENCE {
	procedureCode	NGAP-ELEMENTARY-PROCEDURE.&procedureCode		({NGAP-ELEMENTARY-PROCEDURES}),
	criticality		NGAP-ELEMENTARY-PROCEDURE.&criticality			({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode}),
	value			NGAP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome	({NGAP-ELEMENTARY-PROCEDURES}{@procedureCode})
}

-- **************************************************************
--
-- Interface Elementary Procedure List
--
-- **************************************************************

NGAP-ELEMENTARY-PROCEDURES NGAP-ELEMENTARY-PROCEDURE ::= {
	NGAP-ELEMENTARY-PROCEDURES-CLASS-1			|
	NGAP-ELEMENTARY-PROCEDURES-CLASS-2,
	...
}

NGAP-ELEMENTARY-PROCEDURES-CLASS-1 NGAP-ELEMENTARY-PROCEDURE ::= {
	aMFConfigurationUpdate			|
	broadcastSessionModification	|
	broadcastSessionRelease			|
	broadcastSessionSetup			|
	distributionSetup				|
	distributionRelease				|
	handoverCancel					|
	handoverPreparation				|
	handoverResourceAllocation		|
	initialContextSetup				|
	multicastSessionActivation					|
	multicastSessionDeactivation				|
	multicastSessionUpdate			|
	nGReset							|
	nGSetup							|
	pathSwitchRequest				|
	pDUSessionResourceModify		|
	pDUSessionResourceModifyIndication			|
	pDUSessionResourceRelease		|
	pDUSessionResourceSetup			|
	pWSCancel						|
	rANConfigurationUpdate			|
	uEContextModification			|
	uEContextRelease				|
	uEContextResume								|
	uEContextSuspend							|
	uERadioCapabilityCheck			|
	uERadioCapabilityIDMapping		|
	writeReplaceWarning,
	...
}

NGAP-ELEMENTARY-PROCEDURES-CLASS-2 NGAP-ELEMENTARY-PROCEDURE ::= {
	aMFCPRelocationIndication		|
	aMFStatusIndication				|
	broadcastSessionReleaseRequired	|
	cellTrafficTrace				|
	connectionEstablishmentIndication	|
	deactivateTrace					|
	downlinkNASTransport			|
	downlinkNonUEAssociatedNRPPaTransport	|
	downlinkRANConfigurationTransfer	|
	downlinkRANEarlyStatusTransfer	|
	downlinkRANStatusTransfer		|
	downlinkRIMInformationTransfer	|
	downlinkUEAssociatedNRPPaTransport	|
	errorIndication					|
	handoverNotification			|
	handoverSuccess								|
	initialUEMessage				|
	locationReport					|
	locationReportingControl		|
	locationReportingFailureIndication	|
	multicastGroupPaging			|
	nASNonDeliveryIndication		|
	overloadStart					|
	overloadStop					|
	paging							|
	pDUSessionResourceNotify		|
	privateMessage					|
	pWSFailureIndication						|
	pWSRestartIndication			|
	rANCPRelocationIndication		|
	rerouteNASRequest				|
	retrieveUEInformation						|
	rRCInactiveTransitionReport					|
	secondaryRATDataUsageReport		|
	traceFailureIndication			|
	traceStart						|
	uEContextReleaseRequest			|
	uEInformationTransfer						|
	uERadioCapabilityInfoIndication	|
	uETNLABindingRelease			|
	uplinkNASTransport				|
	uplinkNonUEAssociatedNRPPaTransport	|
	uplinkRANConfigurationTransfer	|
	uplinkRANEarlyStatusTransfer				|
	uplinkRANStatusTransfer			|
	uplinkRIMInformationTransfer				|
	uplinkUEAssociatedNRPPaTransport,
	...

}

-- **************************************************************
--
-- Interface Elementary Procedures
--
-- **************************************************************

aMFConfigurationUpdate NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		AMFConfigurationUpdate
	SUCCESSFUL OUTCOME		AMFConfigurationUpdateAcknowledge
	UNSUCCESSFUL OUTCOME	AMFConfigurationUpdateFailure
	PROCEDURE CODE			id-AMFConfigurationUpdate
	CRITICALITY				reject
}

aMFCPRelocationIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		AMFCPRelocationIndication
	PROCEDURE CODE			id-AMFCPRelocationIndication
	CRITICALITY				reject
}

aMFStatusIndication NGAP-ELEMENTARY-PROCEDURE ::={
	INITIATING MESSAGE		AMFStatusIndication
	PROCEDURE CODE			id-AMFStatusIndication
	CRITICALITY				ignore
}

broadcastSessionModification NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		BroadcastSessionModificationRequest
	SUCCESSFUL OUTCOME		BroadcastSessionModificationResponse
	UNSUCCESSFUL OUTCOME	BroadcastSessionModificationFailure
	PROCEDURE CODE			id-BroadcastSessionModification
	CRITICALITY				reject
}

broadcastSessionRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		BroadcastSessionReleaseRequest
	SUCCESSFUL OUTCOME		BroadcastSessionReleaseResponse
	PROCEDURE CODE			id-BroadcastSessionRelease
	CRITICALITY				reject
}

broadcastSessionReleaseRequired NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		BroadcastSessionReleaseRequired
	PROCEDURE CODE			id-BroadcastSessionReleaseRequired
	CRITICALITY				reject
}

broadcastSessionSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		BroadcastSessionSetupRequest
	SUCCESSFUL OUTCOME		BroadcastSessionSetupResponse
	UNSUCCESSFUL OUTCOME	BroadcastSessionSetupFailure
	PROCEDURE CODE			id-BroadcastSessionSetup
	CRITICALITY				reject
}

cellTrafficTrace NGAP-ELEMENTARY-PROCEDURE ::={
	INITIATING MESSAGE		CellTrafficTrace
	PROCEDURE CODE			id-CellTrafficTrace
	CRITICALITY				ignore
}

connectionEstablishmentIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		ConnectionEstablishmentIndication
	PROCEDURE CODE			id-ConnectionEstablishmentIndication
	CRITICALITY				reject
}

deactivateTrace NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DeactivateTrace
	PROCEDURE CODE			id-DeactivateTrace
	CRITICALITY				ignore
}

distributionSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DistributionSetupRequest
	SUCCESSFUL OUTCOME		DistributionSetupResponse
	UNSUCCESSFUL OUTCOME	DistributionSetupFailure
	PROCEDURE CODE			id-DistributionSetup
	CRITICALITY				reject
}

distributionRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DistributionReleaseRequest
	SUCCESSFUL OUTCOME		DistributionReleaseResponse
	PROCEDURE CODE			id-DistributionRelease
	CRITICALITY				reject
}

downlinkNASTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkNASTransport
	PROCEDURE CODE			id-DownlinkNASTransport
	CRITICALITY				ignore
}

downlinkNonUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkNonUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-DownlinkNonUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

downlinkRANConfigurationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRANConfigurationTransfer
	PROCEDURE CODE			id-DownlinkRANConfigurationTransfer
	CRITICALITY				ignore
}

downlinkRANEarlyStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRANEarlyStatusTransfer
	PROCEDURE CODE			id-DownlinkRANEarlyStatusTransfer
	CRITICALITY				ignore
}

downlinkRANStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRANStatusTransfer
	PROCEDURE CODE			id-DownlinkRANStatusTransfer
	CRITICALITY				ignore
}

downlinkUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-DownlinkUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

errorIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		ErrorIndication
	PROCEDURE CODE			id-ErrorIndication
	CRITICALITY				ignore
}

handoverCancel NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverCancel
	SUCCESSFUL OUTCOME		HandoverCancelAcknowledge
	PROCEDURE CODE			id-HandoverCancel
	CRITICALITY				reject
}

handoverNotification NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverNotify
	PROCEDURE CODE			id-HandoverNotification
	CRITICALITY				ignore
}

handoverPreparation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverRequired
	SUCCESSFUL OUTCOME		HandoverCommand
	UNSUCCESSFUL OUTCOME	HandoverPreparationFailure
	PROCEDURE CODE			id-HandoverPreparation
	CRITICALITY				reject
}

handoverResourceAllocation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverRequest
	SUCCESSFUL OUTCOME		HandoverRequestAcknowledge
	UNSUCCESSFUL OUTCOME	HandoverFailure
	PROCEDURE CODE			id-HandoverResourceAllocation
	CRITICALITY				reject
}

handoverSuccess NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		HandoverSuccess
	PROCEDURE CODE			id-HandoverSuccess
	CRITICALITY				ignore
}

initialContextSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		InitialContextSetupRequest
	SUCCESSFUL OUTCOME		InitialContextSetupResponse
	UNSUCCESSFUL OUTCOME	InitialContextSetupFailure
	PROCEDURE CODE			id-InitialContextSetup
	CRITICALITY				reject
}

initialUEMessage NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		InitialUEMessage
	PROCEDURE CODE			id-InitialUEMessage
	CRITICALITY				ignore
}

locationReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReport
	PROCEDURE CODE			id-LocationReport
	CRITICALITY				ignore
}

locationReportingControl NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReportingControl
	PROCEDURE CODE			id-LocationReportingControl
	CRITICALITY				ignore
}

locationReportingFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		LocationReportingFailureIndication
	PROCEDURE CODE			id-LocationReportingFailureIndication
	CRITICALITY				ignore
}

multicastSessionActivation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		MulticastSessionActivationRequest
	SUCCESSFUL OUTCOME		MulticastSessionActivationResponse
	UNSUCCESSFUL OUTCOME	MulticastSessionActivationFailure
	PROCEDURE CODE			id-MulticastSessionActivation
	CRITICALITY				reject
}

multicastSessionDeactivation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		MulticastSessionDeactivationRequest
	SUCCESSFUL OUTCOME		MulticastSessionDeactivationResponse
	PROCEDURE CODE			id-MulticastSessionDeactivation
	CRITICALITY				reject
}

multicastSessionUpdate NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		MulticastSessionUpdateRequest
	SUCCESSFUL OUTCOME		MulticastSessionUpdateResponse
	UNSUCCESSFUL OUTCOME	MulticastSessionUpdateFailure
	PROCEDURE CODE			id-MulticastSessionUpdate
	CRITICALITY				reject
}

multicastGroupPaging 		NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		MulticastGroupPaging
	PROCEDURE CODE			id-MulticastGroupPaging
	CRITICALITY				ignore
}

nASNonDeliveryIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NASNonDeliveryIndication
	PROCEDURE CODE			id-NASNonDeliveryIndication
	CRITICALITY				ignore
}

nGReset NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NGReset
	SUCCESSFUL OUTCOME		NGResetAcknowledge
	PROCEDURE CODE			id-NGReset
	CRITICALITY				reject
}

nGSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		NGSetupRequest
	SUCCESSFUL OUTCOME		NGSetupResponse
	UNSUCCESSFUL OUTCOME	NGSetupFailure
	PROCEDURE CODE			id-NGSetup
	CRITICALITY				reject
}

overloadStart NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		OverloadStart
	PROCEDURE CODE			id-OverloadStart
	CRITICALITY				ignore
}

overloadStop NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		OverloadStop
	PROCEDURE CODE			id-OverloadStop
	CRITICALITY				reject
}

paging NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		Paging
	PROCEDURE CODE			id-Paging
	CRITICALITY				ignore
}

pathSwitchRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PathSwitchRequest
	SUCCESSFUL OUTCOME		PathSwitchRequestAcknowledge
	UNSUCCESSFUL OUTCOME	PathSwitchRequestFailure
	PROCEDURE CODE			id-PathSwitchRequest
	CRITICALITY				reject
}

pDUSessionResourceModify NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceModifyRequest
	SUCCESSFUL OUTCOME		PDUSessionResourceModifyResponse
	PROCEDURE CODE			id-PDUSessionResourceModify
	CRITICALITY				reject
}

pDUSessionResourceModifyIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceModifyIndication
	SUCCESSFUL OUTCOME		PDUSessionResourceModifyConfirm
	PROCEDURE CODE			id-PDUSessionResourceModifyIndication
	CRITICALITY				reject
}

pDUSessionResourceNotify NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceNotify
	PROCEDURE CODE			id-PDUSessionResourceNotify
	CRITICALITY				ignore
}

pDUSessionResourceRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceReleaseCommand
	SUCCESSFUL OUTCOME		PDUSessionResourceReleaseResponse
	PROCEDURE CODE			id-PDUSessionResourceRelease
	CRITICALITY				reject
}

pDUSessionResourceSetup NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PDUSessionResourceSetupRequest
	SUCCESSFUL OUTCOME		PDUSessionResourceSetupResponse
	PROCEDURE CODE			id-PDUSessionResourceSetup
	CRITICALITY				reject
}

privateMessage NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PrivateMessage
	PROCEDURE CODE			id-PrivateMessage
	CRITICALITY				ignore
}

pWSCancel NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSCancelRequest
	SUCCESSFUL OUTCOME		PWSCancelResponse
	PROCEDURE CODE			id-PWSCancel
	CRITICALITY				reject
}

pWSFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSFailureIndication
	PROCEDURE CODE			id-PWSFailureIndication
	CRITICALITY				ignore
}

pWSRestartIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		PWSRestartIndication
	PROCEDURE CODE			id-PWSRestartIndication
	CRITICALITY				ignore
}

rANConfigurationUpdate NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RANConfigurationUpdate
	SUCCESSFUL OUTCOME		RANConfigurationUpdateAcknowledge
	UNSUCCESSFUL OUTCOME	RANConfigurationUpdateFailure
	PROCEDURE CODE			id-RANConfigurationUpdate
	CRITICALITY				reject
}

rANCPRelocationIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RANCPRelocationIndication
	PROCEDURE CODE			id-RANCPRelocationIndication
	CRITICALITY				reject
}

rerouteNASRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RerouteNASRequest
	PROCEDURE CODE			id-RerouteNASRequest
	CRITICALITY				reject
}


retrieveUEInformation NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RetrieveUEInformation
	PROCEDURE CODE			id-RetrieveUEInformation
	CRITICALITY				reject
}

rRCInactiveTransitionReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		RRCInactiveTransitionReport
	PROCEDURE CODE			id-RRCInactiveTransitionReport
	CRITICALITY				ignore
}

secondaryRATDataUsageReport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		SecondaryRATDataUsageReport
	PROCEDURE CODE			id-SecondaryRATDataUsageReport
	CRITICALITY				ignore
}

traceFailureIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		TraceFailureIndication
	PROCEDURE CODE			id-TraceFailureIndication
	CRITICALITY				ignore
}

traceStart NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		TraceStart
	PROCEDURE CODE			id-TraceStart
	CRITICALITY				ignore
}

uEContextModification NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextModificationRequest
	SUCCESSFUL OUTCOME		UEContextModificationResponse
	UNSUCCESSFUL OUTCOME	UEContextModificationFailure
	PROCEDURE CODE			id-UEContextModification
	CRITICALITY				reject
}

uEContextRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextReleaseCommand
	SUCCESSFUL OUTCOME		UEContextReleaseComplete
	PROCEDURE CODE			id-UEContextRelease
	CRITICALITY				reject
}

uEContextReleaseRequest NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextReleaseRequest
	PROCEDURE CODE			id-UEContextReleaseRequest
	CRITICALITY				ignore
}

uEContextResume NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextResumeRequest
	SUCCESSFUL OUTCOME		UEContextResumeResponse
	UNSUCCESSFUL OUTCOME	UEContextResumeFailure
	PROCEDURE CODE			id-UEContextResume
	CRITICALITY				reject
}

uEContextSuspend NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEContextSuspendRequest
	SUCCESSFUL OUTCOME		UEContextSuspendResponse
	UNSUCCESSFUL OUTCOME	UEContextSuspendFailure
	PROCEDURE CODE			id-UEContextSuspend
	CRITICALITY				reject
}

uEInformationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UEInformationTransfer
	PROCEDURE CODE			id-UEInformationTransfer
	CRITICALITY				reject
}

uERadioCapabilityCheck NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UERadioCapabilityCheckRequest
	SUCCESSFUL OUTCOME		UERadioCapabilityCheckResponse
	PROCEDURE CODE			id-UERadioCapabilityCheck
	CRITICALITY				reject
}

uERadioCapabilityIDMapping NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UERadioCapabilityIDMappingRequest
	SUCCESSFUL OUTCOME		UERadioCapabilityIDMappingResponse
	PROCEDURE CODE			id-UERadioCapabilityIDMapping
	CRITICALITY				reject
}

uERadioCapabilityInfoIndication NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UERadioCapabilityInfoIndication
	PROCEDURE CODE			id-UERadioCapabilityInfoIndication
	CRITICALITY				ignore
}

uETNLABindingRelease NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UETNLABindingReleaseRequest
	PROCEDURE CODE			id-UETNLABindingRelease
	CRITICALITY				ignore
}

uplinkNASTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkNASTransport
	PROCEDURE CODE			id-UplinkNASTransport
	CRITICALITY				ignore
}

uplinkNonUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkNonUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-UplinkNonUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

uplinkRANConfigurationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRANConfigurationTransfer
	PROCEDURE CODE			id-UplinkRANConfigurationTransfer
	CRITICALITY				ignore
}

uplinkRANEarlyStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRANEarlyStatusTransfer
	PROCEDURE CODE			id-UplinkRANEarlyStatusTransfer
	CRITICALITY				reject
}

uplinkRANStatusTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRANStatusTransfer
	PROCEDURE CODE			id-UplinkRANStatusTransfer
	CRITICALITY				ignore
}

uplinkUEAssociatedNRPPaTransport NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkUEAssociatedNRPPaTransport
	PROCEDURE CODE			id-UplinkUEAssociatedNRPPaTransport
	CRITICALITY				ignore
}

writeReplaceWarning NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		WriteReplaceWarningRequest
	SUCCESSFUL OUTCOME		WriteReplaceWarningResponse
	PROCEDURE CODE			id-WriteReplaceWarning
	CRITICALITY				reject
}

uplinkRIMInformationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		UplinkRIMInformationTransfer
	PROCEDURE CODE			id-UplinkRIMInformationTransfer
	CRITICALITY				ignore
}

downlinkRIMInformationTransfer NGAP-ELEMENTARY-PROCEDURE ::= {
	INITIATING MESSAGE		DownlinkRIMInformationTransfer
	PROCEDURE CODE			id-DownlinkRIMInformationTransfer
	CRITICALITY				ignore
}

END
