-- 3GPP TS 38.413 V17.5.0 (2023-06)
-- 9.4.5	Information Element Definitions
-- **************************************************************
--
-- Information Element Definitions
--
-- **************************************************************

NGAP-IEs {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

	id-AdditionalDLForwardingUPTNLInformation,
	id-AdditionalULForwardingUPTNLInformation,
	id-AdditionalDLQosFlowPerTNLInformation,
	id-AdditionalDLUPTNLInformationForHOList,
	id-AdditionalNGU-UP-TNLInformation,
	id-AdditionalRedundantDL-NGU-UP-TNLInformation,
	id-AdditionalRedundantDLQosFlowPerTNLInformation,
	id-AdditionalRedundantNGU-UP-TNLInformation,
	id-AdditionalRedundantUL-NGU-UP-TNLInformation,
	id-AdditionalUL-NGU-UP-TNLInformation,
	id-AlternativeQoSParaSetList,
	id-BurstArrivalTimeDownlink,
	id-Cause,
	id-CNPacketDelayBudgetDL,
	id-CNPacketDelayBudgetUL,
	id-CNTypeRestrictionsForEquivalent,
	id-CNTypeRestrictionsForServing,
	id-CommonNetworkInstance,
	id-ConfiguredTACIndication,
	id-CurrentQoSParaSetIndex,
	id-DAPSRequestInfo,
	id-DAPSResponseInfoList,
	id-DataForwardingNotPossible,
	id-DataForwardingResponseERABList,
	id-DirectForwardingPathAvailability,
	id-DL-NGU-UP-TNLInformation,
	id-EndpointIPAddressAndPort,
	id-EnergySavingIndication,
	id-ExtendedPacketDelayBudget,
	id-ExtendedRATRestrictionInformation,
	id-ExtendedReportIntervalMDT,
	id-ExtendedSliceSupportList,
	id-ExtendedTAISliceSupportList,
	id-ExtendedUEIdentityIndexValue,
	id-EUTRA-PagingeDRXInformation,
	id-GlobalCable-ID,
	id-GlobalRANNodeID,
	id-GlobalTNGF-ID,
 	id-GlobalTWIF-ID,
	id-GlobalW-AGF-ID,
	id-GUAMIType,
id-HashedUEIdentityIndexValue,
	id-IncludeBeamMeasurementsIndication,
	id-IntersystemSONInformationRequest,
	id-IntersystemSONInformationReply,
	id-IntersystemResourceStatusUpdate,
	id-LastEUTRAN-PLMNIdentity,
	id-LastVisitedPSCellList,
	id-LocationReportingAdditionalInfo,
	id-M4ReportAmount,
	id-M5ReportAmount,
	id-M6ReportAmount,
	id-ExcessPacketDelayThresholdConfiguration,
	id-M7ReportAmount,
	id-MaximumIntegrityProtectedDataRate-DL,
	id-MBS-AreaSessionID,
	id-MBS-QoSFlowsToBeSetupList,
	id-MBS-QoSFlowsToBeSetupModList,
	id-MBS-QoSFlowToReleaseList,
	id-MBS-ServiceArea,
	id-MBS-SessionFSAIDList,
	id-MBS-SessionID,
	id-MBS-ActiveSessionInformation-SourcetoTargetList,
	id-MBS-ActiveSessionInformation-TargettoSourceList,
	id-MBS-SessionTNLInfo5GC,
	id-MBS-SupportIndicator,
	id-MBSSessionFailedtoSetupList,
	id-MBSSessionFailedtoSetuporModifyList,
	id-MBSSessionSetupResponseList,
	id-MBSSessionSetuporModifyResponseList,
	id-MBSSessionToReleaseList,
	id-MBSSessionSetupRequestList,
	id-MBSSessionSetuporModifyRequestList,
	id-MDTConfiguration,
	id-MicoAllPLMN,
	id-NetworkInstance,
	id-NGAPIESupportInformationRequestList,
	id-NGAPIESupportInformationResponseList,
	id-NID,
	id-NR-CGI,
	id-NRNTNTAIInformation,
	id-NPN-MobilityInformation,
	id-NPN-PagingAssistanceInformation,
	id-NPN-Support,
	id-NR-PagingeDRXInformation,
	id-OldAssociatedQosFlowList-ULendmarkerexpected,
	id-OnboardingSupport,
	id-PagingAssisDataforCEcapabUE,
	id-PagingCauseIndicationForVoiceService,
	id-PDUSessionAggregateMaximumBitRate,
	id-PduSessionExpectedUEActivityBehaviour,
	id-PDUSessionPairID,
	id-PDUSessionResourceFailedToSetupListCxtFail,
	id-PDUSessionResourceReleaseResponseTransfer,
	id-PDUSessionType,
	id-PEIPSassistanceInformation,
	id-PSCellInformation,
	id-QMCConfigInfo,
	id-QosFlowAddOrModifyRequestList,
	id-QosFlowFailedToSetupList,
	id-QosFlowFeedbackList,
	id-QosFlowParametersList,
	id-QosFlowSetupRequestList,
	id-QosFlowToReleaseList,
	id-QosMonitoringRequest,
	id-QosMonitoringReportingFrequency,
	id-SuccessfulHandoverReportList,
	id-UEContextReferenceAtSource,
	id-RAT-Information,
	id-RedundantCommonNetworkInstance,
	id-RedundantDL-NGU-TNLInformationReused,
	id-RedundantDL-NGU-UP-TNLInformation,
	id-RedundantDLQosFlowPerTNLInformation,
	id-RedundantPDUSessionInformation,
	id-RedundantQosFlowIndicator,
	id-RedundantUL-NGU-UP-TNLInformation,
	id-SCTP-TLAs,
	id-SecondaryRATUsageInformation,
	id-SecurityIndication,
	id-SecurityResult,
	id-SgNB-UE-X2AP-ID,
	id-S-NSSAI,
	id-SONInformationReport,
	id-SourceNodeID,
	id-SourceNodeTNLAddrInfo,
	id-SourceTNLAddrInfo,
	id-SurvivalTime,
	id-TNLAssociationTransportLayerAddressNGRAN,
	id-TAINSAGSupportList,
	id-TargetHomeENB-ID,
	id-TargetRNC-ID,
	id-TraceCollectionEntityURI,
	id-TSCTrafficCharacteristics,
	id-UEHistoryInformationFromTheUE,
	id-UERadioCapabilityForPaging,
	id-UERadioCapabilityForPagingOfNB-IoT,
	id-UL-NGU-UP-TNLInformation,
	id-UL-NGU-UP-TNLModifyList,
	id-ULForwarding,
	id-ULForwardingUP-TNLInformation,
	id-UsedRSNInformation,
	id-UserLocationInformationTNGF,
	id-UserLocationInformationTWIF,
	id-UserLocationInformationW-AGF,
	id-EarlyMeasurement,
	id-BeamMeasurementsReportConfiguration,
	id-TAI,
	id-HFCNode-ID-new,
	id-GlobalCable-ID-new,
	maxnoofAllowedAreas,
	maxnoofAllowedCAGsperPLMN,
	maxnoofAllowedS-NSSAIs,
	maxnoofBluetoothName,
	maxnoofBPLMNs,
	maxnoofCAGSperCell,
	maxnoofCandidateCells,
	maxnoofCellIDforMDT,
	maxnoofCellIDforQMC,
	maxnoofCellIDforWarning,
	maxnoofCellinAoI,
	maxnoofCellinEAI,
	maxnoofCellsforMBS,
	maxnoofCellsingNB,
	maxnoofCellsinngeNB,
	maxnoofCellsinNGRANNode,
	maxnoofCellinTAI,
	maxnoofCellsinUEHistoryInfo,
	maxnoofCellsUEMovingTrajectory,
	maxnoofDRBs,
	maxnoofEmergencyAreaID,
	maxnoofEAIforRestart,
	maxnoofEPLMNs,
	maxnoofEPLMNsPlusOne,
	maxnoofE-RABs,
	maxnoofErrors,
	maxnoofExtSliceItems,
	maxnoofForbTACs,
	maxnoofFreqforMDT,
	maxnoofMBSFSAs,
	maxnoofMBSQoSFlows,
	maxnoofMBSServiceAreaInformation,
	maxnoofMBSAreaSessionIDs,
	maxnoofMBSSessions,
	maxnoofMBSSessionsofUE,
	maxnoofMDTPLMNs,
	maxnoofMRBs,
	maxnoofMultiConnectivity,
	maxnoofMultiConnectivityMinusOne,
	maxnoofNeighPCIforMDT,
	maxnoofNGAPIESupportInfo,
	maxnoofNGConnectionsToReset,
	maxNRARFCN,
	maxnoofNRCellBands,
	maxnoofNSAGs,
	maxnoofPagingAreas,
	maxnoofPC5QoSFlows,
	maxnoofPDUSessions,
	maxnoofPLMNs,
	maxnoofPLMNforQMC,
	maxnoofQosFlows,
	maxnoofQosParaSets,
	maxnoofRANNodeinAoI,
	maxnoofRecommendedCells,
	maxnoofRecommendedRANNodes,
	maxnoofAoI,
	maxnoofPSCellsPerPrimaryCellinUEHistoryInfo,
	maxnoofReportedCells,
	maxnoofSensorName,
	maxnoofServedGUAMIs,
	maxnoofSliceItems,
	maxnoofSNSSAIforQMC,
	maxnoofSuccessfulHOReports,
	maxnoofTACs,
	maxnoofTACsinNTN,
	maxnoofTAforMDT,
	maxnoofTAforQMC,
	maxnoofTAIforInactive,
	maxnoofTAIforMBS,
	maxnoofTAIforPaging,
	maxnoofTAIforRestart,
	maxnoofTAIforWarning,
	maxnoofTAIinAoI,
	maxnoofTargetS-NSSAIs,
	maxnoofTimePeriods,
	maxnoofTNLAssociations,
	maxnoofUEAppLayerMeas,
	maxnoofUEsforPaging,
	maxnoofWLANName,
	maxnoofXnExtTLAs,
	maxnoofXnGTP-TLAs,
	maxnoofXnTLAs,
	maxnoofThresholdsForExcessPacketDelay

FROM NGAP-Constants

	Criticality,
	ProcedureCode,
	ProtocolIE-ID,
	TriggeringMessage
FROM NGAP-CommonDataTypes

	ProtocolExtensionContainer{},
	ProtocolIE-Container{},
	NGAP-PROTOCOL-EXTENSION,
	ProtocolIE-SingleContainer{},
	NGAP-PROTOCOL-IES
FROM NGAP-Containers;

-- A

AdditionalDLUPTNLInformationForHOList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF AdditionalDLUPTNLInformationForHOItem

AdditionalDLUPTNLInformationForHOItem ::= SEQUENCE {
	additionalDL-NGU-UP-TNLInformation				UPTransportLayerInformation,
	additionalQosFlowSetupResponseList				QosFlowListWithDataForwarding,
	additionalDLForwardingUPTNLInformation			UPTransportLayerInformation 							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { AdditionalDLUPTNLInformationForHOItem-ExtIEs} }	OPTIONAL,
	...
}

AdditionalDLUPTNLInformationForHOItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalRedundantDL-NGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformation		PRESENCE optional		},
	...
}

AdditionalQosFlowInformation ::= ENUMERATED {
	more-likely,
	...
}

AllocationAndRetentionPriority ::= SEQUENCE {
	priorityLevelARP				PriorityLevelARP,
	pre-emptionCapability			Pre-emptionCapability,
	pre-emptionVulnerability		Pre-emptionVulnerability,
	iE-Extensions		ProtocolExtensionContainer { {AllocationAndRetentionPriority-ExtIEs} } OPTIONAL,
	...
}

AllocationAndRetentionPriority-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Allowed-CAG-List-per-PLMN ::= SEQUENCE (SIZE(1..maxnoofAllowedCAGsperPLMN)) OF CAG-ID

AllowedNSSAI ::= SEQUENCE (SIZE(1..maxnoofAllowedS-NSSAIs)) OF AllowedNSSAI-Item

AllowedNSSAI-Item ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {AllowedNSSAI-Item-ExtIEs} } OPTIONAL,
	...
}

AllowedNSSAI-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Allowed-PNI-NPN-List ::= SEQUENCE (SIZE(1..maxnoofEPLMNsPlusOne)) OF Allowed-PNI-NPN-Item

Allowed-PNI-NPN-Item ::= SEQUENCE {
	pLMNIdentity				PLMNIdentity,
	pNI-NPN-restricted			ENUMERATED {restricted, not-restricted, ...},
	allowed-CAG-List-per-PLMN	Allowed-CAG-List-per-PLMN,
	iE-Extensions			ProtocolExtensionContainer { {Allowed-PNI-NPN-Item-ExtIEs} } OPTIONAL,
	...
}

Allowed-PNI-NPN-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AllowedTACs ::= SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC

AlternativeQoSParaSetIndex ::= INTEGER (1..8, ...)

AlternativeQoSParaSetNotifyIndex ::= INTEGER (0..8, ...)

AlternativeQoSParaSetList ::= SEQUENCE (SIZE(1..maxnoofQosParaSets)) OF AlternativeQoSParaSetItem

AlternativeQoSParaSetItem ::= SEQUENCE {
	alternativeQoSParaSetIndex			AlternativeQoSParaSetIndex,
	guaranteedFlowBitRateDL				BitRate												OPTIONAL,
	guaranteedFlowBitRateUL				BitRate												OPTIONAL,
	packetDelayBudget					PacketDelayBudget									OPTIONAL,
	packetErrorRate						PacketErrorRate										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AlternativeQoSParaSetItem-ExtIEs} }	OPTIONAL,
	...
}

AlternativeQoSParaSetItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMFName ::= PrintableString (SIZE(1..150, ...))

AMFNameVisibleString ::= VisibleString (SIZE(1..150, ...))

AMFNameUTF8String ::= UTF8String (SIZE(1..150, ...))

AMFPagingTarget ::= CHOICE {
	globalRANNodeID			GlobalRANNodeID,
	tAI						TAI,
	choice-Extensions		ProtocolIE-SingleContainer { {AMFPagingTarget-ExtIEs} }
}

AMFPagingTarget-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

AMFPointer ::= BIT STRING (SIZE(6))

AMFRegionID ::= BIT STRING (SIZE(8))

AMFSetID ::= BIT STRING (SIZE(10))

AMF-TNLAssociationSetupList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationSetupItem

AMF-TNLAssociationSetupItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationSetupItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationSetupItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-TNLAssociationToAddList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToAddItem

AMF-TNLAssociationToAddItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	tNLAssociationUsage				TNLAssociationUsage										OPTIONAL,
	tNLAddressWeightFactor			TNLAddressWeightFactor,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToAddItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToAddItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-TNLAssociationToRemoveList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToRemoveItem

AMF-TNLAssociationToRemoveItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToRemoveItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToRemoveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-TNLAssociationTransportLayerAddressNGRAN	CRITICALITY reject	EXTENSION CPTransportLayerInformation	PRESENCE optional},
	...
}

AMF-TNLAssociationToUpdateList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF AMF-TNLAssociationToUpdateItem

AMF-TNLAssociationToUpdateItem ::= SEQUENCE {
	aMF-TNLAssociationAddress		CPTransportLayerInformation,
	tNLAssociationUsage				TNLAssociationUsage											OPTIONAL,
	tNLAddressWeightFactor			TNLAddressWeightFactor										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AMF-TNLAssociationToUpdateItem-ExtIEs} }	OPTIONAL,
	...
}

AMF-TNLAssociationToUpdateItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AMF-UE-NGAP-ID ::= INTEGER (0..1099511627775)

AreaOfInterest ::= SEQUENCE {
	areaOfInterestTAIList			AreaOfInterestTAIList						OPTIONAL,
	areaOfInterestCellList			AreaOfInterestCellList						OPTIONAL,
 	areaOfInterestRANNodeList		AreaOfInterestRANNodeList					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterest-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterest-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestCellList ::= SEQUENCE (SIZE(1..maxnoofCellinAoI)) OF AreaOfInterestCellItem

AreaOfInterestCellItem ::= SEQUENCE {
	nGRAN-CGI			NGRAN-CGI,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestCellItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestList ::= SEQUENCE (SIZE(1..maxnoofAoI)) OF AreaOfInterestItem

AreaOfInterestItem ::= SEQUENCE {
	areaOfInterest						AreaOfInterest,
	locationReportingReferenceID		LocationReportingReferenceID,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestRANNodeList ::= SEQUENCE (SIZE(1..maxnoofRANNodeinAoI)) OF AreaOfInterestRANNodeItem

AreaOfInterestRANNodeItem ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestRANNodeItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestRANNodeItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaOfInterestTAIList ::= SEQUENCE (SIZE(1..maxnoofTAIinAoI)) OF AreaOfInterestTAIItem

AreaOfInterestTAIItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {AreaOfInterestTAIItem-ExtIEs} }	OPTIONAL,
	...
}

AreaOfInterestTAIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssistanceDataForPaging ::= SEQUENCE {
	assistanceDataForRecommendedCells		AssistanceDataForRecommendedCells			OPTIONAL,
	pagingAttemptInformation				PagingAttemptInformation					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AssistanceDataForPaging-ExtIEs} } OPTIONAL,
	...
}

AssistanceDataForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-NPN-PagingAssistanceInformation		CRITICALITY ignore	EXTENSION NPN-PagingAssistanceInformation			PRESENCE optional	}|
	{ ID id-PagingAssisDataforCEcapabUE			CRITICALITY ignore	EXTENSION PagingAssisDataforCEcapabUE				PRESENCE optional	},
	...
}

AssistanceDataForRecommendedCells ::= SEQUENCE {
	recommendedCellsForPaging		RecommendedCellsForPaging,
	iE-Extensions		ProtocolExtensionContainer { {AssistanceDataForRecommendedCells-ExtIEs} }	OPTIONAL,
	...
}

AssistanceDataForRecommendedCells-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssociatedMBSQosFlowSetupRequestList ::= SEQUENCE (SIZE(1..maxnoofMBSQoSFlows)) OF AssociatedMBSQosFlowSetupRequestItem

AssociatedMBSQosFlowSetupRequestItem ::= SEQUENCE {
	mBS-QosFlowIdentifier				QosFlowIdentifier,
	associatedUnicastQosFlowIdentifier	QosFlowIdentifier,
	iE-Extensions						ProtocolExtensionContainer { { AssociatedMBSQosFlowSetupRequestItem-ExtIEs} }	OPTIONAL,
	...
}

AssociatedMBSQosFlowSetupRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssociatedMBSQosFlowSetuporModifyRequestList ::= SEQUENCE (SIZE(1..maxnoofMBSQoSFlows)) OF AssociatedMBSQosFlowSetuporModifyRequestItem

AssociatedMBSQosFlowSetuporModifyRequestItem ::= SEQUENCE {
	mBS-QosFlowIdentifier				QosFlowIdentifier,
	associatedUnicastQosFlowIdentifier	QosFlowIdentifier,
	iE-Extensions						ProtocolExtensionContainer { { AssociatedMBSQosFlowSetuporModifyRequestItem-ExtIEs} }	OPTIONAL,
	...
}

AssociatedMBSQosFlowSetuporModifyRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AssociatedQosFlowList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF AssociatedQosFlowItem

AssociatedQosFlowItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowMappingIndication		ENUMERATED {ul, dl, ...}							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {AssociatedQosFlowItem-ExtIEs} }	OPTIONAL,
	...
}

AssociatedQosFlowItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CurrentQoSParaSetIndex	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetIndex	PRESENCE optional	},
	...
}

AuthenticatedIndication ::= ENUMERATED {true, ...}

AveragingWindow ::= INTEGER (0..4095, ...)

AreaScopeOfMDT-NR ::= CHOICE {
	cellBased					CellBasedMDT-NR,
	tABased						TABasedMDT,
	pLMNWide					NULL,
	tAIBased					TAIBasedMDT,
	choice-Extensions		ProtocolIE-SingleContainer { {AreaScopeOfMDT-NR-ExtIEs} }
}

AreaScopeOfMDT-NR-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

AreaScopeOfMDT-EUTRA ::= CHOICE {
	cellBased					CellBasedMDT-EUTRA,
	tABased						TABasedMDT,
	pLMNWide					NULL,
	tAIBased					TAIBasedMDT,
	choice-Extensions		ProtocolIE-SingleContainer { {AreaScopeOfMDT-EUTRA-ExtIEs} }
}

AreaScopeOfMDT-EUTRA-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

AreaScopeOfNeighCellsList ::= SEQUENCE (SIZE(1..maxnoofFreqforMDT)) OF AreaScopeOfNeighCellsItem
AreaScopeOfNeighCellsItem ::= SEQUENCE {
	nrFrequencyInfo				NRFrequencyInfo,
	pciListForMDT				PCIListForMDT												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { AreaScopeOfNeighCellsItem-ExtIEs} }	OPTIONAL,
	...
}

AreaScopeOfNeighCellsItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

AreaScopeOfQMC ::= CHOICE {
	cellBased				CellBasedQMC,
	tABased					TABasedQMC,
	tAIBased					TAIBasedQMC,
	pLMNAreaBased			PLMNAreaBasedQMC,
	choice-Extensions		ProtocolIE-SingleContainer { { AreaScopeOfQMC-ExtIEs} }
}

AreaScopeOfQMC-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

AvailableRANVisibleQoEMetrics ::= SEQUENCE {
	applicationLayerBufferLevelList		ENUMERATED {true, ...}		OPTIONAL,
	playoutDelayForMediaStartup			ENUMERATED {true, ...}		OPTIONAL,
	iE-Extensions				ProtocolExtensionContainer { { AvailableRANVisibleQoEMetrics-ExtIEs} }	OPTIONAL,
	...
}

AvailableRANVisibleQoEMetrics-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


-- B

BeamMeasurementsReportConfiguration ::= SEQUENCE {
	beamMeasurementsReportQuantity			BeamMeasurementsReportQuantity 	OPTIONAL,
	maxNrofRS-IndexesToReport               MaxNrofRS-IndexesToReport		OPTIONAL,
	iE-Extensions							ProtocolExtensionContainer { { BeamMeasurementsReportConfiguration-ExtIEs} } OPTIONAL,
	...
}

BeamMeasurementsReportConfiguration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

BeamMeasurementsReportQuantity ::= SEQUENCE {
    rSRP						ENUMERATED {true, ...},
    rSRQ						ENUMERATED {true, ...},
    sINR						ENUMERATED {true, ...},
	iE-Extensions			ProtocolExtensionContainer { { BeamMeasurementsReportQuantity-ExtIEs} } OPTIONAL,
	...
}

BeamMeasurementsReportQuantity-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

BitRate	::= INTEGER (0..4000000000000, ...)

BroadcastCancelledAreaList ::= CHOICE {
	cellIDCancelledEUTRA				CellIDCancelledEUTRA,
	tAICancelledEUTRA					TAICancelledEUTRA,
	emergencyAreaIDCancelledEUTRA		EmergencyAreaIDCancelledEUTRA,
	cellIDCancelledNR					CellIDCancelledNR,
	tAICancelledNR						TAICancelledNR,
	emergencyAreaIDCancelledNR			EmergencyAreaIDCancelledNR,
	choice-Extensions		ProtocolIE-SingleContainer { {BroadcastCancelledAreaList-ExtIEs} }
}

BroadcastCancelledAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

BroadcastCompletedAreaList ::= CHOICE {
	cellIDBroadcastEUTRA				CellIDBroadcastEUTRA,
	tAIBroadcastEUTRA					TAIBroadcastEUTRA,
	emergencyAreaIDBroadcastEUTRA		EmergencyAreaIDBroadcastEUTRA,
	cellIDBroadcastNR					CellIDBroadcastNR,
	tAIBroadcastNR						TAIBroadcastNR,
	emergencyAreaIDBroadcastNR			EmergencyAreaIDBroadcastNR,
	choice-Extensions		ProtocolIE-SingleContainer { {BroadcastCompletedAreaList-ExtIEs} }
}

BroadcastCompletedAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

BroadcastPLMNList ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF BroadcastPLMNItem

BroadcastPLMNItem ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	tAISliceSupportList		SliceSupportList,
	iE-Extensions		ProtocolExtensionContainer { {BroadcastPLMNItem-ExtIEs} } OPTIONAL,
	...
}

BroadcastPLMNItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-NPN-Support					CRITICALITY reject	EXTENSION NPN-Support				PRESENCE optional}|
	{ID id-ExtendedTAISliceSupportList	CRITICALITY reject	EXTENSION ExtendedSliceSupportList 	PRESENCE optional}|
	{ID id-TAINSAGSupportList			CRITICALITY ignore	EXTENSION TAINSAGSupportList		PRESENCE optional},
	...
}

BluetoothMeasurementConfiguration ::= SEQUENCE {
	bluetoothMeasConfig				BluetoothMeasConfig,
	bluetoothMeasConfigNameList		BluetoothMeasConfigNameList											OPTIONAL,
	bt-rssi							ENUMERATED {true, ...}												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { BluetoothMeasurementConfiguration-ExtIEs } } 	OPTIONAL,
	...
}

BluetoothMeasurementConfiguration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

BluetoothMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofBluetoothName)) OF BluetoothMeasConfigNameItem

BluetoothMeasConfigNameItem ::= SEQUENCE {
	bluetoothName		BluetoothName,
	iE-Extensions		ProtocolExtensionContainer { { BluetoothMeasConfigNameItem-ExtIEs } } 	OPTIONAL,
	...
}

BluetoothMeasConfigNameItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

BluetoothMeasConfig::= ENUMERATED {setup,...}

BluetoothName ::= OCTET STRING (SIZE (1..248))

BurstArrivalTime ::= OCTET STRING

-- C

CAG-ID ::= BIT STRING (SIZE(32))

CancelAllWarningMessages ::= ENUMERATED {
	true,
	...
}

CancelledCellsInEAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CancelledCellsInEAI-EUTRA-Item

CancelledCellsInEAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInEAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInEAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInEAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CancelledCellsInEAI-NR-Item

CancelledCellsInEAI-NR-Item ::= SEQUENCE {
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInEAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInEAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInTAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CancelledCellsInTAI-EUTRA-Item

CancelledCellsInTAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInTAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInTAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CancelledCellsInTAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CancelledCellsInTAI-NR-Item

CancelledCellsInTAI-NR-Item ::= SEQUENCE{
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CancelledCellsInTAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CancelledCellsInTAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CandidateCellList ::= SEQUENCE (SIZE(1.. maxnoofCandidateCells)) OF CandidateCellItem

CandidateCellItem ::= SEQUENCE{
	candidateCell		CandidateCell,
	iE-Extensions		ProtocolExtensionContainer { {CandidateCellItem-ExtIEs} } OPTIONAL,
	...
}

CandidateCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CandidateCell::= CHOICE {
	candidateCGI			CandidateCellID,
	candidatePCI			CandidatePCI,
	choice-Extensions		ProtocolIE-SingleContainer { { CandidateCell-ExtIEs} }
}

CandidateCell-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}


CandidateCellID::= SEQUENCE {
	candidateCellID			NR-CGI,
	iE-Extensions			ProtocolExtensionContainer { { CandidateCellID-ExtIEs} }			OPTIONAL,
	...
}

CandidateCellID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CandidatePCI::= SEQUENCE {
	candidatePCI			INTEGER (0..1007, ...),
	candidateNRARFCN		INTEGER (0..maxNRARFCN),
	iE-Extensions			ProtocolExtensionContainer { { CandidatePCI-ExtIEs} }			OPTIONAL,
	...
}

CandidatePCI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Cause ::= CHOICE {
	radioNetwork		CauseRadioNetwork,
	transport			CauseTransport,
	nas					CauseNas,
	protocol			CauseProtocol,
	misc				CauseMisc,
	choice-Extensions		ProtocolIE-SingleContainer { {Cause-ExtIEs} }
}

Cause-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

CauseMisc ::= ENUMERATED {
	control-processing-overload,
	not-enough-user-plane-processing-resources,
	hardware-failure,
	om-intervention,
	unknown-PLMN-or-SNPN,
	unspecified,
	...
}

CauseNas ::= ENUMERATED {
	normal-release,
	authentication-failure,
	deregister,
	unspecified,
	...,
	uE-not-in-PLMN-serving-area
}

CauseProtocol ::= ENUMERATED {
	transfer-syntax-error,
	abstract-syntax-error-reject,
	abstract-syntax-error-ignore-and-notify,
	message-not-compatible-with-receiver-state,
	semantic-error,
	abstract-syntax-error-falsely-constructed-message,
	unspecified,
	...
}

CauseRadioNetwork ::= ENUMERATED {
	unspecified,
	txnrelocoverall-expiry,
	successful-handover,
	release-due-to-ngran-generated-reason,
	release-due-to-5gc-generated-reason,
	handover-cancelled,
	partial-handover,
	ho-failure-in-target-5GC-ngran-node-or-target-system,
	ho-target-not-allowed,
	tngrelocoverall-expiry,
	tngrelocprep-expiry,
	cell-not-available,
	unknown-targetID,
	no-radio-resources-available-in-target-cell,
	unknown-local-UE-NGAP-ID,
	inconsistent-remote-UE-NGAP-ID,
	handover-desirable-for-radio-reason,
	time-critical-handover,
	resource-optimisation-handover,
	reduce-load-in-serving-cell,
	user-inactivity,
	radio-connection-with-ue-lost,
	radio-resources-not-available,
	invalid-qos-combination,
	failure-in-radio-interface-procedure,
	interaction-with-other-procedure,
	unknown-PDU-session-ID,
	unkown-qos-flow-ID,
	multiple-PDU-session-ID-instances,
	multiple-qos-flow-ID-instances,
	encryption-and-or-integrity-protection-algorithms-not-supported,
	ng-intra-system-handover-triggered,
	ng-inter-system-handover-triggered,
	xn-handover-triggered,
	not-supported-5QI-value,
	ue-context-transfer,
	ims-voice-eps-fallback-or-rat-fallback-triggered,
	up-integrity-protection-not-possible,
	up-confidentiality-protection-not-possible,
	slice-not-supported,
	ue-in-rrc-inactive-state-not-reachable,
	redirection,
	resources-not-available-for-the-slice,
	ue-max-integrity-protected-data-rate-reason,
	release-due-to-cn-detected-mobility,
	...,
	n26-interface-not-available,
	release-due-to-pre-emption,
	multiple-location-reporting-reference-ID-instances,
	rsn-not-available-for-the-up,
	npn-access-denied,
	cag-only-access-denied,
	insufficient-ue-capabilities,
	redcap-ue-not-supported,
	unknown-MBS-Session-ID,
	indicated-MBS-session-area-information-not-served-by-the-gNB,
	inconsistent-slice-info-for-the-session,
	misaligned-association-for-multicast-unicast
}

CauseTransport ::= ENUMERATED {
	transport-resource-unavailable,
	unspecified,
	...
}

Cell-CAGInformation ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	cellCAGList			CellCAGList,
	iE-Extensions		ProtocolExtensionContainer { {Cell-CAGInformation-ExtIEs} } OPTIONAL,
	...
}

Cell-CAGInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


CellCAGList ::= SEQUENCE (SIZE(1..maxnoofCAGSperCell)) OF CAG-ID

CellIDBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDBroadcastEUTRA-Item

CellIDBroadcastEUTRA-Item ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CellIDBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDBroadcastNR-Item

CellIDBroadcastNR-Item ::= SEQUENCE {
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CellIDBroadcastNR-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDCancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDCancelledEUTRA-Item

CellIDCancelledEUTRA-Item ::= SEQUENCE {
	eUTRA-CGI				EUTRA-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CellIDCancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDCancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDCancelledNR ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF CellIDCancelledNR-Item

CellIDCancelledNR-Item ::= SEQUENCE {
	nR-CGI					NR-CGI,
	numberOfBroadcasts		NumberOfBroadcasts,
	iE-Extensions		ProtocolExtensionContainer { {CellIDCancelledNR-Item-ExtIEs} } OPTIONAL,
	...
}

CellIDCancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIDListForRestart ::= CHOICE {
	eUTRA-CGIListforRestart		EUTRA-CGIList,
	nR-CGIListforRestart		NR-CGIList,
	choice-Extensions		ProtocolIE-SingleContainer { {CellIDListForRestart-ExtIEs} }
}

CellIDListForRestart-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

CellSize ::= ENUMERATED {verysmall, small, medium, large, ...}


CellType ::= SEQUENCE {
	cellSize		CellSize,
	iE-Extensions		ProtocolExtensionContainer { {CellType-ExtIEs} }	OPTIONAL,
	...
}

CellType-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CEmodeBSupport-Indicator ::= ENUMERATED {supported,...}


CEmodeBrestricted ::= ENUMERATED {
	restricted,
	not-restricted,
	...
}

CNAssistedRANTuning ::= SEQUENCE {
	expectedUEBehaviour					ExpectedUEBehaviour							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {CNAssistedRANTuning-ExtIEs} }	OPTIONAL,
	...
}

CNAssistedRANTuning-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CNsubgroupID ::= INTEGER (0..7, ...)

CNTypeRestrictionsForEquivalent ::= SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF CNTypeRestrictionsForEquivalentItem

CNTypeRestrictionsForEquivalentItem ::= SEQUENCE {
	plmnIdentity		PLMNIdentity,
	cn-Type				ENUMERATED {epc-forbidden, fiveGC-forbidden, ...},
	iE-Extensions		ProtocolExtensionContainer { {CNTypeRestrictionsForEquivalentItem-ExtIEs} }		OPTIONAL,
	...
}

CNTypeRestrictionsForEquivalentItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::={
	...
}

CNTypeRestrictionsForServing ::= ENUMERATED {
	epc-forbidden,
	...
}

CommonNetworkInstance ::= OCTET STRING

CompletedCellsInEAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CompletedCellsInEAI-EUTRA-Item

CompletedCellsInEAI-EUTRA-Item ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInEAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInEAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInEAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CompletedCellsInEAI-NR-Item

CompletedCellsInEAI-NR-Item ::= SEQUENCE {
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInEAI-NR-Item-ExtIEs} }	OPTIONAL,
	...
}

CompletedCellsInEAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInTAI-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CompletedCellsInTAI-EUTRA-Item

CompletedCellsInTAI-EUTRA-Item ::= SEQUENCE{
	eUTRA-CGI			EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInTAI-EUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInTAI-EUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompletedCellsInTAI-NR ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CompletedCellsInTAI-NR-Item

CompletedCellsInTAI-NR-Item ::= SEQUENCE{
	nR-CGI				NR-CGI,
	iE-Extensions		ProtocolExtensionContainer { {CompletedCellsInTAI-NR-Item-ExtIEs} } OPTIONAL,
	...
}

CompletedCellsInTAI-NR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ConcurrentWarningMessageInd ::= ENUMERATED {
	true,
	...
}

ConfidentialityProtectionIndication ::= ENUMERATED {
	required,
	preferred,
	not-needed,
	...
}

ConfidentialityProtectionResult ::= ENUMERATED {
	performed,
	not-performed,
	...
}

ConfiguredTACIndication ::= ENUMERATED {
	true,
	...
}

CoreNetworkAssistanceInformationForInactive ::= SEQUENCE {
	uEIdentityIndexValue				UEIdentityIndexValue,
	uESpecificDRX						PagingDRX																	OPTIONAL,
	periodicRegistrationUpdateTimer		PeriodicRegistrationUpdateTimer,
	mICOModeIndication					MICOModeIndication															OPTIONAL,
	tAIListForInactive					TAIListForInactive,
	expectedUEBehaviour					ExpectedUEBehaviour															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {CoreNetworkAssistanceInformationForInactive-ExtIEs} }	OPTIONAL,
	...
}

CoreNetworkAssistanceInformationForInactive-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-EUTRA-PagingeDRXInformation					CRITICALITY ignore	EXTENSION EUTRA-PagingeDRXInformation					PRESENCE optional	}|
	{ ID id-ExtendedUEIdentityIndexValue				CRITICALITY ignore	EXTENSION ExtendedUEIdentityIndexValue					PRESENCE optional	}|
	{ ID id-UERadioCapabilityForPaging					CRITICALITY ignore	EXTENSION UERadioCapabilityForPaging						PRESENCE optional	}|
	{ ID id-MicoAllPLMN									CRITICALITY ignore	EXTENSION MicoAllPLMN											PRESENCE optional	}|
	{ ID id-NR-PagingeDRXInformation					CRITICALITY ignore	EXTENSION NR-PagingeDRXInformation						PRESENCE optional	}|
	{ ID id-PagingCauseIndicationForVoiceService		CRITICALITY ignore	EXTENSION PagingCauseIndicationForVoiceService		PRESENCE optional	}|
	{ ID id-PEIPSassistanceInformation					CRITICALITY ignore	EXTENSION PEIPSassistanceInformation						PRESENCE optional	}|
	{ ID id-HashedUEIdentityIndexValue					CRITICALITY ignore	EXTENSION HashedUEIdentityIndexValue						PRESENCE optional	},
	...
}

COUNTValueForPDCP-SN12 ::= SEQUENCE {
	pDCP-SN12			INTEGER (0..4095),
	hFN-PDCP-SN12		INTEGER (0..1048575),
	iE-Extensions		ProtocolExtensionContainer { {COUNTValueForPDCP-SN12-ExtIEs} }	OPTIONAL,
	...
}

COUNTValueForPDCP-SN12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

COUNTValueForPDCP-SN18 ::= SEQUENCE {
	pDCP-SN18			INTEGER (0..262143),
	hFN-PDCP-SN18		INTEGER (0..16383),
	iE-Extensions		ProtocolExtensionContainer { {COUNTValueForPDCP-SN18-ExtIEs} }	OPTIONAL,
	...
}

COUNTValueForPDCP-SN18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CoverageEnhancementLevel ::= OCTET STRING

CPTransportLayerInformation ::= CHOICE {
	endpointIPAddress		TransportLayerAddress,
	choice-Extensions		ProtocolIE-SingleContainer { {CPTransportLayerInformation-ExtIEs} }
}

CPTransportLayerInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-EndpointIPAddressAndPort		CRITICALITY reject	TYPE EndpointIPAddressAndPort		PRESENCE mandatory	},
	...
}

CriticalityDiagnostics ::= SEQUENCE {
	procedureCode					ProcedureCode											OPTIONAL,
	triggeringMessage				TriggeringMessage										OPTIONAL,
	procedureCriticality			Criticality												OPTIONAL,
	iEsCriticalityDiagnostics		CriticalityDiagnostics-IE-List							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer {{CriticalityDiagnostics-ExtIEs}}		OPTIONAL,
	...
}

CriticalityDiagnostics-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE(1..maxnoofErrors)) OF CriticalityDiagnostics-IE-Item

CriticalityDiagnostics-IE-Item ::= SEQUENCE {
	iECriticality		Criticality,
	iE-ID				ProtocolIE-ID,
	typeOfError			TypeOfError,
	iE-Extensions		ProtocolExtensionContainer {{CriticalityDiagnostics-IE-Item-ExtIEs}} OPTIONAL,
	...
}

CriticalityDiagnostics-IE-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellBasedMDT-NR::= SEQUENCE {
	cellIdListforMDT	CellIdListforMDT-NR,
	iE-Extensions		ProtocolExtensionContainer { {CellBasedMDT-NR-ExtIEs} } OPTIONAL,
	...
}

CellBasedMDT-NR-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIdListforMDT-NR ::= SEQUENCE (SIZE(1..maxnoofCellIDforMDT)) OF NR-CGI


CellBasedMDT-EUTRA::= SEQUENCE {
	cellIdListforMDT	CellIdListforMDT-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {CellBasedMDT-EUTRA-ExtIEs} } OPTIONAL,
	...
}

CellBasedMDT-EUTRA-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellBasedQMC ::= SEQUENCE {
	cellIdListforQMC 	CellIdListforQMC,
	iE-Extensions		ProtocolExtensionContainer { {CellBasedQMC-ExtIEs} } OPTIONAL,
	...
}

CellBasedQMC-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellIdListforQMC ::= SEQUENCE (SIZE(1..maxnoofCellIDforQMC)) OF NGRAN-CGI

CellIdListforMDT-EUTRA ::= SEQUENCE (SIZE(1..maxnoofCellIDforMDT)) OF EUTRA-CGI


-- D

DataCodingScheme ::= BIT STRING (SIZE(8))

DataForwardingAccepted ::= ENUMERATED {
	data-forwarding-accepted,
	...
}

DataForwardingNotPossible ::= ENUMERATED {
	data-forwarding-not-possible,
	...
}

DataForwardingResponseDRBList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DataForwardingResponseDRBItem

DataForwardingResponseDRBItem ::= SEQUENCE {
	dRB-ID								DRB-ID,
	dLForwardingUP-TNLInformation		UPTransportLayerInformation								OPTIONAL,
	uLForwardingUP-TNLInformation		UPTransportLayerInformation								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer {{DataForwardingResponseDRBItem-ExtIEs}}		OPTIONAL,
	...
}

DataForwardingResponseDRBItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DAPSRequestInfo ::= SEQUENCE {
	dAPSIndicator				ENUMERATED {daps-ho-required, ...},
	iE-Extensions				ProtocolExtensionContainer { {DAPSRequestInfo-ExtIEs} } OPTIONAL,
	...
}

DAPSRequestInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DAPSResponseInfoList ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DAPSResponseInfoItem

DAPSResponseInfoItem ::= SEQUENCE {
	dRB-ID				DRB-ID,
	dAPSResponseInfo		DAPSResponseInfo,
	iE-Extension			ProtocolExtensionContainer { {DAPSResponseInfoItem-ExtIEs} }		OPTIONAL,
	...
}

DAPSResponseInfoItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DAPSResponseInfo ::= SEQUENCE {
	dapsresponseindicator		ENUMERATED {daps-ho-accepted, daps-ho-not-accepted, ...},
	iE-Extensions			ProtocolExtensionContainer { { DAPSResponseInfo-ExtIEs} } 	OPTIONAL,
	...
}

DAPSResponseInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


DataForwardingResponseERABList ::= SEQUENCE (SIZE(1..maxnoofE-RABs)) OF DataForwardingResponseERABListItem

DataForwardingResponseERABListItem ::= SEQUENCE {
	e-RAB-ID							E-RAB-ID,
	dLForwardingUP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {DataForwardingResponseERABListItem-ExtIEs} }	OPTIONAL,
	...
}

DataForwardingResponseERABListItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DelayCritical ::= ENUMERATED {
	delay-critical,
	non-delay-critical,
	...
}

DL-CP-SecurityInformation ::= SEQUENCE {
	dl-NAS-MAC				DL-NAS-MAC,
	iE-Extensions			ProtocolExtensionContainer { { DL-CP-SecurityInformation-ExtIEs} }	OPTIONAL,
	...
}

DL-CP-SecurityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DL-NAS-MAC ::= BIT STRING (SIZE (16))

DLForwarding ::= ENUMERATED {
	dl-forwarding-proposed,
	...
}

DL-NGU-TNLInformationReused ::= ENUMERATED {
	true,
	...
}

DirectForwardingPathAvailability ::= ENUMERATED {
	direct-path-available,
	...
}

DRB-ID ::= INTEGER (1..32, ...)

DRBsSubjectToStatusTransferList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsSubjectToStatusTransferItem

DRBsSubjectToStatusTransferItem ::= SEQUENCE {
	dRB-ID				DRB-ID,
	dRBStatusUL			DRBStatusUL,
	dRBStatusDL			DRBStatusDL,
	iE-Extension		ProtocolExtensionContainer { {DRBsSubjectToStatusTransferItem-ExtIEs} }	OPTIONAL,
	...
}

DRBsSubjectToStatusTransferItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-OldAssociatedQosFlowList-ULendmarkerexpected	CRITICALITY ignore EXTENSION AssociatedQosFlowList	 PRESENCE optional },
	...
}

DRBStatusDL ::= CHOICE {
	dRBStatusDL12			DRBStatusDL12,
	dRBStatusDL18			DRBStatusDL18,
	choice-Extensions		ProtocolIE-SingleContainer { {DRBStatusDL-ExtIEs} }
}

DRBStatusDL-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

DRBStatusDL12 ::= SEQUENCE {
	dL-COUNTValue		COUNTValueForPDCP-SN12,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusDL12-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusDL12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusDL18 ::= SEQUENCE {
	dL-COUNTValue		COUNTValueForPDCP-SN18,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusDL18-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusDL18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusUL ::= CHOICE {
	dRBStatusUL12			DRBStatusUL12,
	dRBStatusUL18			DRBStatusUL18,
	choice-Extensions		ProtocolIE-SingleContainer { {DRBStatusUL-ExtIEs} }
}

DRBStatusUL-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

DRBStatusUL12 ::= SEQUENCE {
	uL-COUNTValue					COUNTValueForPDCP-SN12,
	receiveStatusOfUL-PDCP-SDUs		BIT STRING (SIZE(1..2048))						OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusUL12-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusUL12-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBStatusUL18 ::= SEQUENCE {
	uL-COUNTValue					COUNTValueForPDCP-SN18,
	receiveStatusOfUL-PDCP-SDUs		BIT STRING (SIZE(1..131072))					OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {DRBStatusUL18-ExtIEs} }		OPTIONAL,
	...
}

DRBStatusUL18-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBsToQosFlowsMappingList ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBsToQosFlowsMappingItem

DRBsToQosFlowsMappingItem ::= SEQUENCE {
	dRB-ID								DRB-ID,
	associatedQosFlowList				AssociatedQosFlowList,
	iE-Extensions		ProtocolExtensionContainer { {DRBsToQosFlowsMappingItem-ExtIEs} }		OPTIONAL,
	...
}

DRBsToQosFlowsMappingItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-DAPSRequestInfo	CRITICALITY ignore	EXTENSION DAPSRequestInfo	PRESENCE optional  },
	...
}

Dynamic5QIDescriptor ::= SEQUENCE {
	priorityLevelQos			PriorityLevelQos,
	packetDelayBudget			PacketDelayBudget,
	packetErrorRate				PacketErrorRate,
	fiveQI						FiveQI													OPTIONAL,
	delayCritical				DelayCritical											OPTIONAL,
-- The above IE shall be present in case of GBR QoS flow
	averagingWindow				AveragingWindow											OPTIONAL,
-- The above IE shall be present in case of GBR QoS flow
	maximumDataBurstVolume		MaximumDataBurstVolume									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {Dynamic5QIDescriptor-ExtIEs} }	OPTIONAL,
	...
}

Dynamic5QIDescriptor-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-ExtendedPacketDelayBudget	CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional		}|
	{ ID id-CNPacketDelayBudgetDL		CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional		}|
	{ ID id-CNPacketDelayBudgetUL		CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional		},
	...
}

-- E

EarlyMeasurement ::= ENUMERATED {true, ...}

EarlyStatusTransfer-TransparentContainer ::= SEQUENCE {
	procedureStage			ProcedureStageChoice,
	iE-Extensions			ProtocolExtensionContainer { {EarlyStatusTransfer-TransparentContainer-ExtIEs} }	OPTIONAL,
	...
}

EarlyStatusTransfer-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ProcedureStageChoice ::= CHOICE {
	first-dl-count			FirstDLCount,
	choice-Extensions		ProtocolIE-SingleContainer { {ProcedureStageChoice-ExtIEs} }
}

ProcedureStageChoice-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

FirstDLCount ::= SEQUENCE {
	dRBsSubjectToEarlyStatusTransfer		DRBsSubjectToEarlyStatusTransfer-List,
	iE-Extension		ProtocolExtensionContainer { {FirstDLCount-ExtIEs} }		OPTIONAL,
	...
}

FirstDLCount-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

DRBsSubjectToEarlyStatusTransfer-List ::= SEQUENCE (SIZE (1.. maxnoofDRBs)) OF DRBsSubjectToEarlyStatusTransfer-Item

DRBsSubjectToEarlyStatusTransfer-Item ::= SEQUENCE {
	dRB-ID				DRB-ID,
	firstDLCOUNT		DRBStatusDL,
	iE-Extension		ProtocolExtensionContainer { { DRBsSubjectToEarlyStatusTransfer-Item-ExtIEs} }	OPTIONAL,
	...
}

DRBsSubjectToEarlyStatusTransfer-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


EDT-Session ::= ENUMERATED {
	true,
	...
}

EmergencyAreaID ::= OCTET STRING (SIZE(3))

EmergencyAreaIDBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDBroadcastEUTRA-Item

EmergencyAreaIDBroadcastEUTRA-Item ::= SEQUENCE {
	emergencyAreaID					EmergencyAreaID,
	completedCellsInEAI-EUTRA		CompletedCellsInEAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

EmergencyAreaIDBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDBroadcastNR-Item

EmergencyAreaIDBroadcastNR-Item ::= SEQUENCE {
	emergencyAreaID				EmergencyAreaID,
	completedCellsInEAI-NR		CompletedCellsInEAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDBroadcastNR-Item-ExtIEs} }	OPTIONAL,
	...
}

EmergencyAreaIDBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDCancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDCancelledEUTRA-Item

EmergencyAreaIDCancelledEUTRA-Item ::= SEQUENCE {
	emergencyAreaID					EmergencyAreaID,
	cancelledCellsInEAI-EUTRA		CancelledCellsInEAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDCancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

EmergencyAreaIDCancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDCancelledNR ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaIDCancelledNR-Item

EmergencyAreaIDCancelledNR-Item ::= SEQUENCE {
	emergencyAreaID				EmergencyAreaID,
	cancelledCellsInEAI-NR		CancelledCellsInEAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyAreaIDCancelledNR-Item-ExtIEs} }	OPTIONAL,
	...
}

EmergencyAreaIDCancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyAreaIDList ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaID

EmergencyAreaIDListForRestart ::= SEQUENCE (SIZE(1..maxnoofEAIforRestart)) OF EmergencyAreaID

EmergencyFallbackIndicator ::= SEQUENCE {
	emergencyFallbackRequestIndicator		EmergencyFallbackRequestIndicator,
	emergencyServiceTargetCN				EmergencyServiceTargetCN						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {EmergencyFallbackIndicator-ExtIEs} }	OPTIONAL,
	...
}

EmergencyFallbackIndicator-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EmergencyFallbackRequestIndicator ::= ENUMERATED {
	emergency-fallback-requested,
	...
}

EmergencyServiceTargetCN ::= ENUMERATED {
	fiveGC,
	epc,
	...
}

ENB-ID ::= CHOICE {
	macroENB-ID				BIT STRING (SIZE(20)),
	homeENB-ID				BIT STRING (SIZE(28)),
	short-macroENB-ID 		BIT STRING (SIZE(18)),
	long-macroENB-ID		BIT STRING (SIZE(21)),
	choice-Extensions		ProtocolIE-SingleContainer { { ENB-ID-ExtIEs} }
}

ENB-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}


Enhanced-CoverageRestriction ::= ENUMERATED {restricted, ... }


Extended-ConnectedTime ::= INTEGER (0..255)

EN-DCSONConfigurationTransfer ::= OCTET STRING

EndpointIPAddressAndPort ::=SEQUENCE {
	endpointIPAddress TransportLayerAddress,
	portNumber			PortNumber,
	iE-Extensions		ProtocolExtensionContainer { { EndpointIPAddressAndPort-ExtIEs} } OPTIONAL
}

EndIndication ::= ENUMERATED {
	no-further-data,
	further-data-exists,
	...
}

EndpointIPAddressAndPort-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EquivalentPLMNs ::= SEQUENCE (SIZE(1..maxnoofEPLMNs)) OF PLMNIdentity

EPS-TAC ::= OCTET STRING (SIZE(2))

EPS-TAI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	ePS-TAC				EPS-TAC,
	iE-Extensions		ProtocolExtensionContainer { {EPS-TAI-ExtIEs} } OPTIONAL,
	...
}

EPS-TAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

E-RAB-ID ::= INTEGER (0..15, ...)

E-RABInformationList ::= SEQUENCE (SIZE(1..maxnoofE-RABs)) OF E-RABInformationItem

E-RABInformationItem ::= SEQUENCE {
	e-RAB-ID			E-RAB-ID,
	dLForwarding		DLForwarding													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {E-RABInformationItem-ExtIEs} }	OPTIONAL,
	...
}

E-RABInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-SourceTNLAddrInfo		CRITICALITY ignore	EXTENSION TransportLayerAddress	PRESENCE optional}|
	{ID id-SourceNodeTNLAddrInfo	CRITICALITY ignore	EXTENSION TransportLayerAddress	PRESENCE optional},
	...
}

EUTRACellIdentity ::= BIT STRING (SIZE(28))

EUTRA-CGI ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	eUTRACellIdentity		EUTRACellIdentity,
	iE-Extensions		ProtocolExtensionContainer { {EUTRA-CGI-ExtIEs} } OPTIONAL,
	...
}

EUTRA-CGI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRA-CGIList ::= SEQUENCE (SIZE(1..maxnoofCellsinngeNB)) OF EUTRA-CGI

EUTRA-CGIListForWarning ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF EUTRA-CGI

EUTRA-PagingeDRXInformation ::= SEQUENCE {
	eUTRA-paging-eDRX-Cycle		EUTRA-Paging-eDRX-Cycle,
	eUTRA-paging-Time-Window	EUTRA-Paging-Time-Window					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {EUTRA-PagingeDRXInformation-ExtIEs} }	OPTIONAL,
	...
}

EUTRA-PagingeDRXInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRA-Paging-eDRX-Cycle ::= ENUMERATED {
	hfhalf, hf1, hf2, hf4, hf6,
	hf8, hf10, hf12, hf14, hf16,
	hf32, hf64, hf128, hf256,
	...
}

EUTRA-Paging-Time-Window ::= ENUMERATED {
	s1, s2, s3, s4, s5,
	s6, s7, s8, s9, s10,
	s11, s12, s13, s14, s15, s16,
	...
}

EUTRAencryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

EUTRAintegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

EventType ::= ENUMERATED {
	direct,
	change-of-serve-cell,
	ue-presence-in-area-of-interest,
	stop-change-of-serve-cell,
	stop-ue-presence-in-area-of-interest,
	cancel-location-reporting-for-the-ue,
	...
}

ExcessPacketDelayThresholdConfiguration ::= SEQUENCE (SIZE(1..maxnoofThresholdsForExcessPacketDelay)) OF ExcessPacketDelayThresholdItem

ExcessPacketDelayThresholdItem ::= SEQUENCE {
	fiveQi		FiveQI,
	excessPacketDelayThresholdValue			ExcessPacketDelayThresholdValue,
	iE-Extensions		ProtocolExtensionContainer { { ExcessPacketDelayThresholdItem-ExtIEs} }	OPTIONAL,
	...
}

ExcessPacketDelayThresholdItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExcessPacketDelayThresholdValue ::= ENUMERATED {
ms0dot25, ms0dot5, ms1, ms2, ms4, ms5, ms10, ms20, ms30, ms40, ms50, ms60, ms70, ms80, ms90, ms100, ms150, ms300, ms500,
	...
}

ExpectedActivityPeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedHOInterval ::= ENUMERATED {
	sec15, sec30, sec60, sec90, sec120, sec180, long-time,
	...
}

ExpectedIdlePeriod ::= INTEGER (1..30|40|50|60|80|100|120|150|180|181, ...)

ExpectedUEActivityBehaviour ::= SEQUENCE {
	expectedActivityPeriod						ExpectedActivityPeriod						OPTIONAL,
	expectedIdlePeriod							ExpectedIdlePeriod							OPTIONAL,
	sourceOfUEActivityBehaviourInformation		SourceOfUEActivityBehaviourInformation		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEActivityBehaviour-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEActivityBehaviour-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExpectedUEBehaviour ::= SEQUENCE {
	expectedUEActivityBehaviour		ExpectedUEActivityBehaviour 					OPTIONAL,
	expectedHOInterval				ExpectedHOInterval		 						OPTIONAL,
	expectedUEMobility				ExpectedUEMobility								OPTIONAL,
	expectedUEMovingTrajectory		ExpectedUEMovingTrajectory						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEBehaviour-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEBehaviour-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExpectedUEMobility ::= ENUMERATED {
	stationary,
	mobile,
	...
}

ExpectedUEMovingTrajectory ::= SEQUENCE (SIZE(1..maxnoofCellsUEMovingTrajectory)) OF ExpectedUEMovingTrajectoryItem

ExpectedUEMovingTrajectoryItem ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	timeStayedInCell		INTEGER (0..4095)													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ExpectedUEMovingTrajectoryItem-ExtIEs} }	OPTIONAL,
	...
}

ExpectedUEMovingTrajectoryItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Extended-AMFName	 ::= SEQUENCE {
	aMFNameVisibleString		AMFNameVisibleString				OPTIONAL,
	aMFNameUTF8String			AMFNameUTF8String					OPTIONAL,
	iE-Extensions				ProtocolExtensionContainer { { Extended-AMFName-ExtIEs } } OPTIONAL,
	...
}

Extended-AMFName-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExtendedPacketDelayBudget ::= INTEGER (1..65535, ..., 65536..109999)


Extended-RANNodeName	 ::= SEQUENCE {
	rANNodeNameVisibleString		RANNodeNameVisibleString					OPTIONAL,
	rANNodeNameUTF8String			RANNodeNameUTF8String						OPTIONAL,
	iE-Extensions					ProtocolExtensionContainer { { Extended-RANNodeName-ExtIEs } } OPTIONAL,	...
}

Extended-RANNodeName-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExtendedRATRestrictionInformation ::= SEQUENCE {
	primaryRATRestriction		BIT STRING (SIZE(8, ...)),
	secondaryRATRestriction		BIT STRING (SIZE(8, ...)),
	iE-Extensions		ProtocolExtensionContainer { {ExtendedRATRestrictionInformation-ExtIEs} }	OPTIONAL,
	...
}

ExtendedRATRestrictionInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ExtendedRNC-ID					::= INTEGER (4096..65535)

ExtendedSliceSupportList ::= SEQUENCE (SIZE(1..maxnoofExtSliceItems)) OF SliceSupportItem

ExtendedUEIdentityIndexValue ::= BIT STRING (SIZE(16))

EventTrigger::= CHOICE {
	outOfCoverage				ENUMERATED {true, ...},
	eventL1LoggedMDTConfig		EventL1LoggedMDTConfig,
	choice-Extensions		ProtocolIE-SingleContainer { { EventTrigger-ExtIEs} }
}

EventTrigger-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

EventL1LoggedMDTConfig ::= SEQUENCE {
	l1Threshold					MeasurementThresholdL1LoggedMDT,
	hysteresis					Hysteresis,
	timeToTrigger				TimeToTrigger,
	iE-Extensions				ProtocolExtensionContainer { { EventL1LoggedMDTConfig-ExtIEs} } OPTIONAL,
	...
}

EventL1LoggedMDTConfig-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MeasurementThresholdL1LoggedMDT ::= CHOICE {
	threshold-RSRP				Threshold-RSRP,
	threshold-RSRQ				Threshold-RSRQ,
	choice-Extensions		ProtocolIE-SingleContainer { { MeasurementThresholdL1LoggedMDT-ExtIEs} }
}

MeasurementThresholdL1LoggedMDT-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

-- F

FailureIndication ::= SEQUENCE {
	uERLFReportContainer 	UERLFReportContainer,
	iE-Extensions		ProtocolExtensionContainer { { FailureIndication-ExtIEs} }	OPTIONAL,
	...
}

FailureIndication-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveG-ProSeAuthorized ::= SEQUENCE {
	fiveGProSeDirectDiscovery				FiveGProSeDirectDiscovery						OPTIONAL,
	fiveGProSeDirectCommunication			FiveGProSeDirectCommunication					OPTIONAL,
	fiveGProSeLayer2UEtoNetworkRelay			FiveGProSeLayer2UEtoNetworkRelay					OPTIONAL,
	fiveGProSeLayer3UEtoNetworkRelay			FiveGProSeLayer3UEtoNetworkRelay					OPTIONAL,
	fiveGProSeLayer2RemoteUE					FiveGProSeLayer2RemoteUE							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {FiveG-ProSeAuthorized-ExtIEs} }		OPTIONAL,
	...
}

FiveG-ProSeAuthorized-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveGProSeDirectDiscovery ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

FiveGProSeDirectCommunication ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

FiveGProSeLayer2UEtoNetworkRelay ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

FiveGProSeLayer3UEtoNetworkRelay ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

FiveGProSeLayer2RemoteUE ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}



FiveG-ProSePC5QoSParameters ::= SEQUENCE {
	fiveGProSepc5QoSFlowList					FiveGProSePC5QoSFlowList,
	fiveGProSepc5LinkAggregateBitRates		BitRate												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { FiveG-ProSePC5QoSParameters-ExtIEs} }	OPTIONAL,
	...
}

FiveG-ProSePC5QoSParameters-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveGProSePC5QoSFlowList ::= SEQUENCE (SIZE(1..maxnoofPC5QoSFlows)) OF FiveGProSePC5QoSFlowItem

FiveGProSePC5QoSFlowItem ::= SEQUENCE {
	fiveGproSepQI				FiveQI,
	fiveGproSepc5FlowBitRates	FiveGProSePC5FlowBitRates				OPTIONAL,
	fiveGproSerange				Range									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { FiveGProSePC5QoSFlowItem-ExtIEs} }	OPTIONAL,
	...
}

FiveGProSePC5QoSFlowItem-ExtIEs  NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveGProSePC5FlowBitRates ::= SEQUENCE {
	fiveGproSeguaranteedFlowBitRate		BitRate,
	fiveGproSemaximumFlowBitRate		BitRate,
	iE-Extensions		ProtocolExtensionContainer { { FiveGProSePC5FlowBitRates-ExtIEs} }	OPTIONAL,
	...
}

FiveGProSePC5FlowBitRates-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


FiveG-S-TMSI ::= SEQUENCE {
	aMFSetID			AMFSetID,
	aMFPointer			AMFPointer,
	fiveG-TMSI			FiveG-TMSI,
	iE-Extensions		ProtocolExtensionContainer { {FiveG-S-TMSI-ExtIEs} }	OPTIONAL,
	...
}

FiveG-S-TMSI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FiveG-TMSI ::= OCTET STRING (SIZE(4))

FiveQI ::= INTEGER (0..255, ...)

ForbiddenAreaInformation ::= SEQUENCE (SIZE(1.. maxnoofEPLMNsPlusOne)) OF ForbiddenAreaInformation-Item

ForbiddenAreaInformation-Item ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	forbiddenTACs		ForbiddenTACs,
	iE-Extensions		ProtocolExtensionContainer { {ForbiddenAreaInformation-Item-ExtIEs} } OPTIONAL,
	...
}

ForbiddenAreaInformation-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ForbiddenTACs ::= SEQUENCE (SIZE(1..maxnoofForbTACs)) OF TAC

FromEUTRANtoNGRAN ::= SEQUENCE {
	sourceeNBID				IntersystemSONeNBID,
	targetNGRANnodeID		IntersystemSONNGRANnodeID,
	iE-Extensions			ProtocolExtensionContainer { { FromEUTRANtoNGRAN-ExtIEs} }			OPTIONAL
}

FromEUTRANtoNGRAN-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

FromNGRANtoEUTRAN ::= SEQUENCE {
	sourceNGRANnodeID		IntersystemSONNGRANnodeID,
	targeteNBID				IntersystemSONeNBID,
	iE-Extensions			ProtocolExtensionContainer { { FromNGRANtoEUTRAN-ExtIEs} }			OPTIONAL
}

FromNGRANtoEUTRAN-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- G

GBR-QosInformation ::= SEQUENCE {
	maximumFlowBitRateDL		BitRate,
	maximumFlowBitRateUL		BitRate,
	guaranteedFlowBitRateDL		BitRate,
	guaranteedFlowBitRateUL		BitRate,
	notificationControl			NotificationControl									OPTIONAL,
	maximumPacketLossRateDL		PacketLossRate										OPTIONAL,
	maximumPacketLossRateUL		PacketLossRate										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {GBR-QosInformation-ExtIEs} }	OPTIONAL,
	...
}

GBR-QosInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AlternativeQoSParaSetList	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetList	PRESENCE optional	},
	...
}

GlobalCable-ID ::= OCTET STRING

GlobalCable-ID-new ::= SEQUENCE {
	globalCable-ID			GlobalCable-ID,
	tAI						TAI,
	iE-Extensions			ProtocolExtensionContainer { { GlobalCable-ID-new-ExtIEs} }		OPTIONAL,
	...
}

GlobalCable-ID-new-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalENB-ID ::= SEQUENCE {
	pLMNidentity			PLMNIdentity,
	eNB-ID					ENB-ID,
	iE-Extensions			ProtocolExtensionContainer { {GlobalENB-ID-ExtIEs} }		OPTIONAL,
	...
}

GlobalENB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


GlobalGNB-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	gNB-ID				GNB-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalGNB-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalGNB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalN3IWF-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	n3IWF-ID			N3IWF-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalN3IWF-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalN3IWF-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalLine-ID ::= SEQUENCE {
	globalLineIdentity		GlobalLineIdentity,
	lineType			LineType									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {GlobalLine-ID-ExtIEs} } 		OPTIONAL,
	...
}

GlobalLine-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-TAI				CRITICALITY ignore	EXTENSION TAI							PRESENCE optional	},
	...
}

GlobalLineIdentity ::= OCTET STRING

GlobalNgENB-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	ngENB-ID			NgENB-ID,
	iE-Extensions		ProtocolExtensionContainer { {GlobalNgENB-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalNgENB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GlobalRANNodeID ::= CHOICE {
	globalGNB-ID			GlobalGNB-ID,
	globalNgENB-ID			GlobalNgENB-ID,
	globalN3IWF-ID			GlobalN3IWF-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {GlobalRANNodeID-ExtIEs} }
}

GlobalRANNodeID-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GlobalTNGF-ID		CRITICALITY reject	TYPE GlobalTNGF-ID		PRESENCE mandatory	}|
	{ ID id-GlobalTWIF-ID		CRITICALITY reject	TYPE GlobalTWIF-ID			PRESENCE mandatory 	}|
	{ ID id-GlobalW-AGF-ID		CRITICALITY reject	TYPE GlobalW-AGF-ID			PRESENCE mandatory 	},
	...
}

GlobalTNGF-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	tNGF-ID				TNGF-ID,
	iE-Extensions		ProtocolExtensionContainer { { GlobalTNGF-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalTNGF-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


GlobalTWIF-ID ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	tWIF-ID				TWIF-ID,
	iE-Extensions		ProtocolExtensionContainer { { GlobalTWIF-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalTWIF-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


GlobalW-AGF-ID ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	w-AGF-ID				W-AGF-ID,
	iE-Extensions			ProtocolExtensionContainer { { GlobalW-AGF-ID-ExtIEs} } OPTIONAL,
	...
}

GlobalW-AGF-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GNB-ID ::= CHOICE {
	gNB-ID		BIT STRING (SIZE(22..32)),
	choice-Extensions		ProtocolIE-SingleContainer { {GNB-ID-ExtIEs} }
}

GNB-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

GTP-TEID ::= OCTET STRING (SIZE(4))

GTPTunnel ::= SEQUENCE {
	transportLayerAddress		TransportLayerAddress,
	gTP-TEID					GTP-TEID,
	iE-Extensions		ProtocolExtensionContainer { {GTPTunnel-ExtIEs} } OPTIONAL,
	...
}

GTPTunnel-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GUAMI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	aMFRegionID			AMFRegionID,
	aMFSetID			AMFSetID,
	aMFPointer			AMFPointer,
	iE-Extensions		ProtocolExtensionContainer { {GUAMI-ExtIEs} } OPTIONAL,
	...
}

GUAMI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GUAMIType ::= ENUMERATED {native, mapped, ...}

-- H

HandoverCommandTransfer ::= SEQUENCE {
	dLForwardingUP-TNLInformation		UPTransportLayerInformation						OPTIONAL,
	qosFlowToBeForwardedList			QosFlowToBeForwardedList						OPTIONAL,
	dataForwardingResponseDRBList		DataForwardingResponseDRBList					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverCommandTransfer-ExtIEs} } OPTIONAL,
	...
}

HandoverCommandTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLForwardingUPTNLInformation		CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList			PRESENCE optional		}|
	{ ID id-ULForwardingUP-TNLInformation				CRITICALITY reject	EXTENSION UPTransportLayerInformation			PRESENCE optional		}|
	{ ID id-AdditionalULForwardingUPTNLInformation		CRITICALITY reject	EXTENSION UPTransportLayerInformationList		PRESENCE optional		}|
	{ ID id-DataForwardingResponseERABList				CRITICALITY ignore	EXTENSION DataForwardingResponseERABList		PRESENCE optional		}|
	{ ID id-QosFlowFailedToSetupList					CRITICALITY ignore	EXTENSION QosFlowListWithCause						PRESENCE optional		},
	...
}

HandoverFlag ::= ENUMERATED {
	handover-preparation,
	...
}

HandoverPreparationUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {HandoverPreparationUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverPreparationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverRequestAcknowledgeTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation			UPTransportLayerInformation,
	dLForwardingUP-TNLInformation		UPTransportLayerInformation										OPTIONAL,
	securityResult						SecurityResult													OPTIONAL,
	qosFlowSetupResponseList			QosFlowListWithDataForwarding,
	qosFlowFailedToSetupList			QosFlowListWithCause											OPTIONAL,
	dataForwardingResponseDRBList		DataForwardingResponseDRBList									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverRequestAcknowledgeTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverRequestAcknowledgeTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLUPTNLInformationForHOList		CRITICALITY ignore	EXTENSION AdditionalDLUPTNLInformationForHOList		PRESENCE optional	}|
	{ ID id-ULForwardingUP-TNLInformation				CRITICALITY reject	EXTENSION UPTransportLayerInformation					PRESENCE optional	}|
	{ ID id-AdditionalULForwardingUPTNLInformation		CRITICALITY reject	EXTENSION UPTransportLayerInformationList				PRESENCE optional	}|
	{ ID id-DataForwardingResponseERABList				CRITICALITY ignore	EXTENSION DataForwardingResponseERABList 				PRESENCE optional	}|
	{ ID id-RedundantDL-NGU-UP-TNLInformation			CRITICALITY ignore	EXTENSION UPTransportLayerInformation 					PRESENCE optional	}|
	{ ID id-UsedRSNInformation							CRITICALITY ignore	EXTENSION RedundantPDUSessionInformation				PRESENCE optional	}|
	{ ID id-GlobalRANNodeID 								CRITICALITY ignore	EXTENSION GlobalRANNodeID									PRESENCE optional	}|
	{ ID id-MBS-SupportIndicator						CRITICALITY ignore	EXTENSION MBS-SupportIndicator								PRESENCE optional	},
	...
}

HandoverRequiredTransfer ::= SEQUENCE {
	directForwardingPathAvailability		DirectForwardingPathAvailability				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverRequiredTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverRequiredTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverResourceAllocationUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																	OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {HandoverResourceAllocationUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

HandoverResourceAllocationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HandoverType ::= ENUMERATED {
	intra5gs,
	fivegs-to-eps,
	eps-to-5gs,
	...,
	fivegs-to-utran
}

HashedUEIdentityIndexValue ::= BIT STRING (SIZE(13, ...))


HFCNode-ID ::= OCTET STRING

HFCNode-ID-new ::= SEQUENCE {
	hFCNode-ID			HFCNode-ID,
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { { HFCNode-ID-new-ExtIEs} }	OPTIONAL,
	...
}

HFCNode-ID-new-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

HOReport::= SEQUENCE {
	handoverReportType			ENUMERATED {ho-too-early, ho-to-wrong-cell, intersystem-ping-pong, ...},
	handoverCause				Cause,
	sourcecellCGI				NGRAN-CGI,
	targetcellCGI				NGRAN-CGI,
	reestablishmentcellCGI		NGRAN-CGI									OPTIONAL,
	-- The above IE shall be present if the Handover Report Type IE is set to the value "HO to wrong cell" --
	sourcecellC-RNTI			BIT STRING (SIZE(16))						OPTIONAL,
	targetcellinE-UTRAN			EUTRA-CGI									OPTIONAL,
	-- The above IE shall be present if the Handover Report Type IE is set to the value "Inter System ping-pong" --
	mobilityInformation			MobilityInformation							OPTIONAL,
	uERLFReportContainer		UERLFReportContainer						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { HOReport-ExtIEs} }	OPTIONAL,
	...
}

HOReport-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


Hysteresis ::=                      INTEGER (0..30)

-- I

IAB-Authorized ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

IAB-Supported ::= ENUMERATED {
	true,
	...
}

IABNodeIndication ::= ENUMERATED {
	true,
	...
}

IMSVoiceSupportIndicator ::= ENUMERATED {
	supported,
	not-supported,
	...
}

IndexToRFSP ::= INTEGER (1..256, ...)

InfoOnRecommendedCellsAndRANNodesForPaging ::= SEQUENCE {
	recommendedCellsForPaging		RecommendedCellsForPaging,
	recommendRANNodesForPaging		RecommendedRANNodesForPaging,
	iE-Extensions		ProtocolExtensionContainer { {InfoOnRecommendedCellsAndRANNodesForPaging-ExtIEs} }	OPTIONAL,
	...
}

InfoOnRecommendedCellsAndRANNodesForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


IntegrityProtectionIndication ::= ENUMERATED {
	required,
	preferred,
	not-needed,
	...
}

IntegrityProtectionResult ::= ENUMERATED {
	performed,
	not-performed,
	...
}

IntendedNumberOfPagingAttempts ::= INTEGER (1..16, ...)

InterfacesToTrace ::= BIT STRING (SIZE(8))

ImmediateMDTNr ::= SEQUENCE {
	measurementsToActivate					MeasurementsToActivate,
	m1Configuration							M1Configuration						OPTIONAL,
-- The above IE shall be present if the Measurements to Activate IE has the first bit set to “1”
	m4Configuration							M4Configuration						OPTIONAL,
-- The above IE shall be present if the Measurements to Activate IE has the third bit set to “1”
	m5Configuration							M5Configuration						OPTIONAL,
-- The above IE shall be present if the Measurements to Activate IE has the fourth bit set to “1”
	m6Configuration							M6Configuration						OPTIONAL,
-- The above IE shall be present if the Measurements to Activate IE has the fifth bit set to “1”
	m7Configuration							M7Configuration						OPTIONAL,
-- The above IE shall be present if the Measurements to Activate IE has the sixth bit set to “1”
	bluetoothMeasurementConfiguration		BluetoothMeasurementConfiguration	OPTIONAL,
	wLANMeasurementConfiguration			WLANMeasurementConfiguration 		OPTIONAL,
	mDT-Location-Info 						MDT-Location-Info 					OPTIONAL,
	sensorMeasurementConfiguration			SensorMeasurementConfiguration		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { ImmediateMDTNr-ExtIEs} } OPTIONAL,
	...
}

ImmediateMDTNr-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

InterSystemFailureIndication ::= SEQUENCE {
	uERLFReportContainer		UERLFReportContainer	OPTIONAL,
	iE-Extensions			ProtocolExtensionContainer { { InterSystemFailureIndication-ExtIEs} }			OPTIONAL,
	...
}

InterSystemFailureIndication-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

IntersystemSONConfigurationTransfer ::= SEQUENCE {
	transferType				IntersystemSONTransferType,
	intersystemSONInformation	IntersystemSONInformation,
	iE-Extensions			ProtocolExtensionContainer { { IntersystemSONConfigurationTransfer-ExtIEs} }			OPTIONAL,
	...
}

IntersystemSONConfigurationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

IntersystemSONTransferType ::= CHOICE {
	fromEUTRANtoNGRAN				FromEUTRANtoNGRAN,
	fromNGRANtoEUTRAN				FromNGRANtoEUTRAN,
	choice-Extensions		ProtocolIE-SingleContainer { { IntersystemSONTransferType-ExtIEs} }
}
IntersystemSONTransferType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

IntersystemSONeNBID ::= SEQUENCE {
	globaleNBID				GlobalENB-ID,
	selectedEPSTAI			EPS-TAI,
	iE-Extensions			ProtocolExtensionContainer { { IntersystemSONeNBID-ExtIEs} }			OPTIONAL,
	...
}

IntersystemSONeNBID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

IntersystemSONNGRANnodeID ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { { IntersystemSONNGRANnodeID-ExtIEs} }			OPTIONAL,
	...
}

IntersystemSONNGRANnodeID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

IntersystemSONInformation ::= CHOICE {
	intersystemSONInformationReport 	IntersystemSONInformationReport,
	choice-Extensions		ProtocolIE-SingleContainer { { IntersystemSONInformation-ExtIEs} }
}

IntersystemSONInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-IntersystemSONInformationRequest		CRITICALITY ignore	TYPE IntersystemSONInformationRequest			PRESENCE mandatory }|
	{ ID id-IntersystemSONInformationReply			CRITICALITY ignore	TYPE IntersystemSONInformationReply			PRESENCE mandatory },
	...
}

-- --------------------------------------------------------------------
-- INTER SYSTEM SON INFORMATION REQUEST
-- --------------------------------------------------------------------

IntersystemSONInformationRequest ::= CHOICE {
	nGRAN-CellActivation		IntersystemCellActivationRequest,
	resourceStatus				IntersystemResourceStatusRequest,
	choice-Extensions		ProtocolIE-SingleContainer { { IntersystemSONInformationRequest-ExtIEs} }
}

IntersystemSONInformationRequest-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

IntersystemCellActivationRequest ::= SEQUENCE {
	activationID			INTEGER (0..16384, ...),
	cellsToActivateList		CellsToActivateList,
	iE-Extensions		ProtocolExtensionContainer { { IntersystemCellActivationRequest-ExtIEs} } OPTIONAL,
	...
}

IntersystemCellActivationRequest-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CellsToActivateList ::= SEQUENCE (SIZE(1..maxnoofCellsinNGRANNode)) OF NGRAN-CGI


-- --------------------------------------------------------------------
-- Inter System Resource Status Request
-- --------------------------------------------------------------------

IntersystemResourceStatusRequest ::= SEQUENCE {
	reportingSystem				ReportingSystem,
	reportCharacteristics		ReportCharacteristics,
	reportType					ReportType,
	iE-Extensions		ProtocolExtensionContainer { { IntersystemResourceStatusRequest-ExtIEs} }	OPTIONAL,
	...
}

IntersystemResourceStatusRequest-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ReportingSystem ::= CHOICE {
	eUTRAN			EUTRAN-ReportingSystemIEs,
	nGRAN			NGRAN-ReportingSystemIEs,
	noReporting		NULL,
	choice-Extensions		ProtocolIE-SingleContainer { { ReportingSystem-ExtIEs}}
}

ReportingSystem-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

EUTRAN-ReportingSystemIEs::= SEQUENCE {
	eUTRAN-CellToReportList				EUTRAN-CellToReportList,
	iE-Extensions		ProtocolExtensionContainer { {EUTRAN-ReportingSystemIEs-ExtIEs} } OPTIONAL,
	...
}

EUTRAN-ReportingSystemIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGRAN-ReportingSystemIEs ::= SEQUENCE {
	nGRAN-CellToReportList				NGRAN-CellToReportList,
	iE-Extensions		ProtocolExtensionContainer { {NGRAN-ReportingSystemIEs-ExtIEs} } OPTIONAL,
	...
}

NGRAN-ReportingSystemIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRAN-CellToReportList ::= SEQUENCE (SIZE(1..maxnoofReportedCells)) OF EUTRAN-CellToReportItem

EUTRAN-CellToReportItem::= SEQUENCE {
	eCGI				EUTRA-CGI,
	iE-Extensions		ProtocolExtensionContainer { {EUTRAN-CellToReportItem-ExtIEs} } OPTIONAL,
	...
}

EUTRAN-CellToReportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


NGRAN-CellToReportList ::= SEQUENCE (SIZE(1.. maxnoofReportedCells)) OF NGRAN-CellToReportItem

NGRAN-CellToReportItem::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	iE-Extensions		ProtocolExtensionContainer { {NGRAN-CellToReportItem-ExtIEs} } OPTIONAL,
	...
}

NGRAN-CellToReportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ReportCharacteristics ::=  BIT STRING(SIZE(32))

ReportType ::= CHOICE {
	eventBasedReporting		EventBasedReportingIEs,
	periodicReporting		PeriodicReportingIEs,
	choice-Extensions		ProtocolIE-SingleContainer { { ReportType-ExtIEs}}
}

ReportType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

EventBasedReportingIEs ::= SEQUENCE {
	intersystemResourceThresholdLow				IntersystemResourceThreshold,
	intersystemResourceThresholdHigh				IntersystemResourceThreshold,
	numberOfMeasurementReportingLevels				NumberOfMeasurementReportingLevels,
	iE-Extensions		ProtocolExtensionContainer { {EventBasedReportingIEs-ExtIEs} } OPTIONAL,
	...
}
EventBasedReportingIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

IntersystemResourceThreshold ::= INTEGER(0..100)

NumberOfMeasurementReportingLevels ::= ENUMERATED {n2, n3, n4, n5, n10, ...}

PeriodicReportingIEs ::= SEQUENCE {
	reportingPeriodicity			ReportingPeriodicity,
	iE-Extensions		ProtocolExtensionContainer { {PeriodicReportingIEs-ExtIEs} } OPTIONAL,
	...
}

PeriodicReportingIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ReportingPeriodicity ::= ENUMERATED {
	stop,
	single,
	ms1000,
	ms2000,
	ms5000,
	ms10000,
	...
}


-- --------------------------------------------------------------------
-- INTER SYSTEM SON INFORMATION REPLY
-- --------------------------------------------------------------------

IntersystemSONInformationReply ::= CHOICE {
	nGRAN-CellActivation		IntersystemCellActivationReply,
	resourceStatus				IntersystemResourceStatusReply,
	choice-Extensions		ProtocolIE-SingleContainer { { IntersystemSONInformationReply-ExtIEs} }
}

IntersystemSONInformationReply-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

IntersystemCellActivationReply ::= SEQUENCE {
	activatedCellList		ActivatedCellList,
	activation-ID			INTEGER(0..16384, ...),
	iE-Extensions			ProtocolExtensionContainer { { IntersystemCellActivationReply-ExtIEs} } OPTIONAL,
	...
}

IntersystemCellActivationReply-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ActivatedCellList ::= SEQUENCE (SIZE(1..maxnoofCellsinNGRANNode)) OF NGRAN-CGI


-- --------------------------------------------------------------------
-- Inter System Resource Status Reply
-- --------------------------------------------------------------------

IntersystemResourceStatusReply ::= SEQUENCE {
	reportingsystem				ReportingSystem,
	iE-Extensions		ProtocolExtensionContainer { { IntersystemResourceStatusReply-ExtIEs} }		OPTIONAL,
	...
}

IntersystemResourceStatusReply-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


-- --------------------------------------------------------------------
-- INTER SYSTEM SON INFORMATION REPORT
-- --------------------------------------------------------------------

IntersystemSONInformationReport::= CHOICE {
	hOReportInformation				InterSystemHOReport,
	failureIndicationInformation	InterSystemFailureIndication,
	choice-Extensions		ProtocolIE-SingleContainer { { IntersystemSONInformationReport-ExtIEs} }
}

IntersystemSONInformationReport-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-EnergySavingIndication				CRITICALITY ignore	TYPE IntersystemCellStateIndication						PRESENCE mandatory }|
	{ ID id-IntersystemResourceStatusUpdate		CRITICALITY ignore	TYPE IntersystemResourceStatusReport					PRESENCE mandatory },
	...
}

IntersystemCellStateIndication ::= SEQUENCE {
	notificationCellList	NotificationCellList,
	iE-Extensions		ProtocolExtensionContainer { { IntersystemCellStateIndication-ExtIEs} } OPTIONAL,
	...
}

IntersystemCellStateIndication-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NotificationCellList ::= SEQUENCE (SIZE(1.. maxnoofCellsinNGRANNode)) OF NotificationCell-Item

NotificationCell-Item ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	notifyFlag				ENUMERATED {activated, deactivated, ...},
	iE-Extensions		ProtocolExtensionContainer { { NotificationCell-Item-ExtIEs} } OPTIONAL,
	...
}

NotificationCell-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- --------------------------------------------------------------------
-- Inter System Resource Status Report
-- --------------------------------------------------------------------

IntersystemResourceStatusReport ::= SEQUENCE {
	reportingSystem		ResourceStatusReportingSystem,
	iE-Extensions					ProtocolExtensionContainer { { IntersystemResourceStatusReport-ExtIEs} }		OPTIONAL,
	...
}

IntersystemResourceStatusReport-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ResourceStatusReportingSystem ::= CHOICE {
	eUTRAN-ReportingStatus		EUTRAN-ReportingStatusIEs,
	nGRAN-ReportingStatus		NGRAN-ReportingStatusIEs,
	choice-Extensions			ProtocolIE-SingleContainer { { ResourceStatusReportingSystem-ExtIEs}}
}

ResourceStatusReportingSystem-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

EUTRAN-ReportingStatusIEs::= SEQUENCE {
	eUTRAN-CellReportList						EUTRAN-CellReportList,
	iE-Extensions		ProtocolExtensionContainer { {EUTRAN-ReportingStatusIEs-ExtIEs} }	OPTIONAL,
	...
}

EUTRAN-ReportingStatusIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRAN-CellReportList ::= SEQUENCE (SIZE(1..maxnoofReportedCells)) OF EUTRAN-CellReportItem

EUTRAN-CellReportItem ::= SEQUENCE {
	eCGI										EUTRA-CGI,
	eUTRAN-CompositeAvailableCapacityGroup		EUTRAN-CompositeAvailableCapacityGroup,
	eUTRAN-NumberOfActiveUEs					EUTRAN-NumberOfActiveUEs					OPTIONAL,
	eUTRAN-NoofRRCConnections					NGRAN-NoofRRCConnections					OPTIONAL,
	eUTRAN-RadioResourceStatus					EUTRAN-RadioResourceStatus					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {EUTRAN-CellReportItem-ExtIEs} }		OPTIONAL,
	...
}

EUTRAN-CellReportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


EUTRAN-CompositeAvailableCapacityGroup	::= SEQUENCE {
	dL-CompositeAvailableCapacity					CompositeAvailableCapacity,
	uL-CompositeAvailableCapacity					CompositeAvailableCapacity,
	iE-Extensions		ProtocolExtensionContainer { { EUTRAN-CompositeAvailableCapacityGroup-ExtIEs} }		OPTIONAL,
	...
}

EUTRAN-CompositeAvailableCapacityGroup-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

CompositeAvailableCapacity ::= SEQUENCE {
	cellCapacityClassValue		INTEGER (1..100, ...)				OPTIONAL,
	capacityValue				INTEGER (0..100),
	iE-Extensions		ProtocolExtensionContainer { {CompositeAvailableCapacity-ExtIEs} } OPTIONAL,
	...
}

CompositeAvailableCapacity-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

EUTRAN-NumberOfActiveUEs ::= INTEGER (0..16777215, ...)

EUTRAN-RadioResourceStatus ::= SEQUENCE {
	dL-GBR-PRB-usage							INTEGER (0..100),
	uL-GBR-PRB-usage							INTEGER (0..100),
	dL-non-GBR-PRB-usage						INTEGER (0..100),
	uL-non-GBR-PRB-usage						INTEGER (0..100),
	dL-Total-PRB-usage							INTEGER (0..100),
	uL-Total-PRB-usage							INTEGER (0..100),
	dL-scheduling-PDCCH-CCE-usage				INTEGER (0..100)	OPTIONAL,
	uL-scheduling-PDCCH-CCE-usage				INTEGER (0..100)	OPTIONAL,
	iE-Extensions								ProtocolExtensionContainer { {EUTRAN-RadioResourceStatus-ExtIEs} } OPTIONAL,
	...
}

EUTRAN-RadioResourceStatus-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGRAN-ReportingStatusIEs ::= SEQUENCE {
	nGRAN-CellReportList						NGRAN-CellReportList,
	iE-Extensions		ProtocolExtensionContainer { {NGRAN-ReportingStatusIEs-ExtIEs} }	OPTIONAL,
	...
}

NGRAN-ReportingStatusIEs-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGRAN-CellReportList ::= SEQUENCE (SIZE(1..maxnoofReportedCells)) OF NGRAN-CellReportItem

NGRAN-CellReportItem ::= SEQUENCE {
	nGRAN-CGI									NGRAN-CGI,
	nGRAN-CompositeAvailableCapacityGroup		EUTRAN-CompositeAvailableCapacityGroup,
	nGRAN-NumberOfActiveUEs						NGRAN-NumberOfActiveUEs						OPTIONAL,
	nGRAN-NoofRRCConnections					NGRAN-NoofRRCConnections					OPTIONAL,
	nGRAN-RadioResourceStatus					NGRAN-RadioResourceStatus					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {NGRAN-CellReportItem-ExtIEs} }		OPTIONAL,
	...
}

NGRAN-CellReportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


NGRAN-NumberOfActiveUEs ::= INTEGER (0..16777215, ...)

NGRAN-NoofRRCConnections ::= INTEGER (1..65536, ...)

NGRAN-RadioResourceStatus	::= SEQUENCE {
	dL-GBR-PRB-usage-for-MIMO				INTEGER (0..100),
	uL-GBR-PRB-usage-for-MIMO				INTEGER (0..100),
	dL-non-GBR-PRB-usage-for-MIMO			INTEGER (0..100),
	uL-non-GBR-PRB-usage-for-MIMO			INTEGER (0..100),
	dL-Total-PRB-usage-for-MIMO				INTEGER (0..100),
	uL-Total-PRB-usage-for-MIMO				INTEGER (0..100),
	iE-Extensions							ProtocolExtensionContainer { { NGRAN-RadioResourceStatus-ExtIEs} }	OPTIONAL,
	...
}

NGRAN-RadioResourceStatus-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

InterSystemHOReport ::= SEQUENCE {
	handoverReportType		InterSystemHandoverReportType,
	iE-Extensions			ProtocolExtensionContainer { { InterSystemHOReport-ExtIEs} }			OPTIONAL,
	...
}

InterSystemHOReport-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

InterSystemHandoverReportType ::= CHOICE {
	tooearlyIntersystemHO				TooearlyIntersystemHO,
	intersystemUnnecessaryHO			IntersystemUnnecessaryHO,
	choice-Extensions		ProtocolIE-SingleContainer { { InterSystemHandoverReportType-ExtIEs} }
}

InterSystemHandoverReportType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

IntersystemUnnecessaryHO ::= SEQUENCE {
	sourcecellID			NGRAN-CGI,
	targetcellID			EUTRA-CGI,
	earlyIRATHO				ENUMERATED {true, false, ...},
	candidateCellList		CandidateCellList,
	iE-Extensions			ProtocolExtensionContainer { { IntersystemUnnecessaryHO-ExtIEs} }			OPTIONAL,
	...
}

IntersystemUnnecessaryHO-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- J
-- K
-- L

LAC	::= OCTET STRING (SIZE (2))

LAI ::= SEQUENCE {
	pLMNidentity		PLMNIdentity,
	lAC					LAC,
	iE-Extensions		ProtocolExtensionContainer { {LAI-ExtIEs} } OPTIONAL,
	...
}

LAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LastVisitedCellInformation ::= CHOICE {
	nGRANCell		LastVisitedNGRANCellInformation,
	eUTRANCell		LastVisitedEUTRANCellInformation,
	uTRANCell		LastVisitedUTRANCellInformation,
	gERANCell		LastVisitedGERANCellInformation,
	choice-Extensions		ProtocolIE-SingleContainer { {LastVisitedCellInformation-ExtIEs} }
}

LastVisitedCellInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

LastVisitedCellItem ::= SEQUENCE {
	lastVisitedCellInformation		LastVisitedCellInformation,
	iE-Extensions		ProtocolExtensionContainer { {LastVisitedCellItem-ExtIEs} }	OPTIONAL,
	...
}

LastVisitedCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LastVisitedEUTRANCellInformation ::= OCTET STRING

LastVisitedGERANCellInformation ::= OCTET STRING

LastVisitedNGRANCellInformation::= SEQUENCE {
	globalCellID								NGRAN-CGI,
	cellType									CellType,
	timeUEStayedInCell							TimeUEStayedInCell,
	timeUEStayedInCellEnhancedGranularity		TimeUEStayedInCellEnhancedGranularity 			OPTIONAL,
	hOCauseValue								Cause		 									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {LastVisitedNGRANCellInformation-ExtIEs} }	OPTIONAL,
	...
}

LastVisitedNGRANCellInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-LastVisitedPSCellList	CRITICALITY ignore	EXTENSION LastVisitedPSCellList	PRESENCE optional },
	...
}

LastVisitedPSCellList ::= SEQUENCE (SIZE(1..maxnoofPSCellsPerPrimaryCellinUEHistoryInfo)) OF LastVisitedPSCellInformation

LastVisitedPSCellInformation ::= SEQUENCE {
	pSCellID			NGRAN-CGI	 			OPTIONAL,
	timeStay			INTEGER (0..40950),
	iE-Extensions		ProtocolExtensionContainer { {LastVisitedPSCellInformation-ExtIEs} }	OPTIONAL,
	...
}

LastVisitedPSCellInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LastVisitedUTRANCellInformation ::= OCTET STRING

LineType ::= ENUMERATED {
	dsl,
	pon,
	...
}


LocationReportingAdditionalInfo ::= ENUMERATED {
	includePSCell,
	...
}

LocationReportingReferenceID ::= INTEGER (1..64, ...)

LocationReportingRequestType ::= SEQUENCE {
	eventType										EventType,
	reportArea										ReportArea,
	areaOfInterestList								AreaOfInterestList								OPTIONAL,
	locationReportingReferenceIDToBeCancelled		LocationReportingReferenceID					OPTIONAL,
-- The above IE shall be present if the event type is set to “stop reporting UE presence in the area of interest”
	iE-Extensions		ProtocolExtensionContainer { {LocationReportingRequestType-ExtIEs} }		OPTIONAL,
	...
}

LocationReportingRequestType-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-LocationReportingAdditionalInfo	CRITICALITY ignore	EXTENSION LocationReportingAdditionalInfo		PRESENCE optional },
	...
}

LoggedMDTNr ::= SEQUENCE {
	loggingInterval						LoggingInterval,
	loggingDuration						LoggingDuration,
	loggedMDTTrigger						LoggedMDTTrigger,
	bluetoothMeasurementConfiguration	BluetoothMeasurementConfiguration	OPTIONAL,
	wLANMeasurementConfiguration		WLANMeasurementConfiguration		OPTIONAL,
	sensorMeasurementConfiguration		SensorMeasurementConfiguration		OPTIONAL,
	areaScopeOfNeighCellsList			AreaScopeOfNeighCellsList			OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {LoggedMDTNr-ExtIEs} } OPTIONAL,
	...
}

LoggedMDTNr-ExtIEs	NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-EarlyMeasurement		CRITICALITY ignore	EXTENSION EarlyMeasurement		PRESENCE optional	},
	...
}

LoggingInterval ::= ENUMERATED {
	ms320, ms640, ms1280, ms2560, ms5120, ms10240, ms20480, ms30720, ms40960, ms61440,
	infinity,
	...
}

LoggingDuration ::= ENUMERATED {m10, m20, m40, m60, m90, m120, ...}

Links-to-log ::= ENUMERATED {
	uplink,
	downlink,
	both-uplink-and-downlink,
	...
}

LoggedMDTTrigger ::= CHOICE{
	periodical			NULL,
	eventTrigger			EventTrigger,
	choice-Extensions		ProtocolIE-SingleContainer { {LoggedMDTTrigger-ExtIEs} }
}

LoggedMDTTrigger-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

LTEM-Indication	::= ENUMERATED {lte-m,...}

LTEUERLFReportContainer ::= OCTET STRING

LTEV2XServicesAuthorized ::= SEQUENCE {
	vehicleUE			VehicleUE															OPTIONAL,
	pedestrianUE 		PedestrianUE														OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {LTEV2XServicesAuthorized-ExtIEs} }	OPTIONAL,
	...
}

LTEV2XServicesAuthorized-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

LTEUESidelinkAggregateMaximumBitrate ::= SEQUENCE {
	uESidelinkAggregateMaximumBitRate		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {LTEUE-Sidelink-Aggregate-MaximumBitrates-ExtIEs} } OPTIONAL,
	...
}

LTEUE-Sidelink-Aggregate-MaximumBitrates-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- M

MaskedIMEISV ::= BIT STRING (SIZE(64))

MaximumDataBurstVolume ::= INTEGER (0..4095, ..., 4096.. 2000000)

MessageIdentifier ::= BIT STRING (SIZE(16))

MaximumIntegrityProtectedDataRate ::= ENUMERATED {
	bitrate64kbs,
	maximum-UE-rate,
	...
}


MBS-AreaSessionID ::= INTEGER (0..65535, ...)

MBS-DataForwardingResponseMRBList ::= SEQUENCE (SIZE(1..maxnoofMRBs)) OF MBS-DataForwardingResponseMRBItem

MBS-DataForwardingResponseMRBItem ::= SEQUENCE {
	mRB-ID 								MRB-ID,
	dL-Forwarding-UPTNLInformation		UPTransportLayerInformation,
	mRB-ProgressInformation				MRB-ProgressInformation			OPTIONAL,
	iE-Extensions						ProtocolExtensionContainer { { MBS-DataForwardingResponseMRBItem-ExtIEs} }	OPTIONAL,
	...
}

MBS-DataForwardingResponseMRBItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-MappingandDataForwardingRequestList ::= SEQUENCE (SIZE(1..maxnoofMRBs)) OF MBS-MappingandDataForwardingRequestItem

MBS-MappingandDataForwardingRequestItem ::= SEQUENCE {
	mRB-ID 								MRB-ID,
	mBS-QoSFlowList						MBS-QoSFlowList,
	mRB-ProgressInformation				MRB-ProgressInformation				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBS-MappingandDataForwardingRequestItem-ExtIEs} }	OPTIONAL,
	...
}

MBS-MappingandDataForwardingRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-QoSFlowList ::= SEQUENCE (SIZE(1..maxnoofMBSQoSFlows)) OF QosFlowIdentifier

MRB-ProgressInformation ::= CHOICE {
	pDCP-SN-Length12				INTEGER (0..4095),
	pDCP-SN-Length18				INTEGER (0..262143),
	choice-Extensions		ProtocolIE-SingleContainer { { MRB-ProgressInformation-ExtIEs} }
}

MRB-ProgressInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MBS-QoSFlowsToBeSetupList ::= SEQUENCE (SIZE(1.. maxnoofMBSQoSFlows)) OF MBS-QoSFlowsToBeSetupItem

MBS-QoSFlowsToBeSetupItem ::= SEQUENCE {
	mBSqosFlowIdentifier				QosFlowIdentifier,
	mBSqosFlowLevelQosParameters		QosFlowLevelQosParameters,
	iE-Extensions						ProtocolExtensionContainer { {MBS-QoSFlowsToBeSetupItem-ExtIEs} }	OPTIONAL,
	...
}

MBS-QoSFlowsToBeSetupItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


MBS-ServiceArea ::= CHOICE {
	locationindependent		MBS-ServiceAreaInformation,
	locationdependent		MBS-ServiceAreaInformationList,
	choice-Extensions		ProtocolIE-SingleContainer { {MBS-ServiceArea-ExtIEs} }
}

MBS-ServiceArea-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MBS-ServiceAreaInformationList ::= SEQUENCE (SIZE(1..maxnoofMBSServiceAreaInformation)) OF MBS-ServiceAreaInformationItem


MBS-ServiceAreaInformationItem ::= SEQUENCE {
	mBS-AreaSessionID				MBS-AreaSessionID,
	mBS-ServiceAreaInformation		MBS-ServiceAreaInformation,
	iE-Extensions					ProtocolExtensionContainer { {MBS-ServiceAreaInformationItem-ExtIEs} }	OPTIONAL,
	...
}

MBS-ServiceAreaInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-ServiceAreaInformation ::= SEQUENCE {
	mBS-ServiceAreaCellList		MBS-ServiceAreaCellList																OPTIONAL,
	mBS-ServiceAreaTAIList		MBS-ServiceAreaTAIList																OPTIONAL,
	iE-Extensions					ProtocolExtensionContainer { {MBS-ServiceAreaInformation-ExtIEs} }	OPTIONAL,
	...
}

MBS-ServiceAreaInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-ServiceAreaCellList ::= SEQUENCE (SIZE(1.. maxnoofCellsforMBS)) OF NR-CGI

MBS-ServiceAreaTAIList ::= SEQUENCE (SIZE(1.. maxnoofTAIforMBS)) OF TAI

MBS-SessionID ::= SEQUENCE {
	tMGI								TMGI,
	nID								NID																			OPTIONAL,
	iE-Extensions					ProtocolExtensionContainer { {MBS-SessionID-ExtIEs} } 		OPTIONAL,
	...
}

MBS-SessionID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionFailedtoSetupList ::= SEQUENCE (SIZE(1.. maxnoofMBSSessions)) OF MBSSessionFailedtoSetupItem

MBSSessionFailedtoSetupItem ::= SEQUENCE {
	mBS-SessionID			MBS-SessionID,
	mBS-AreaSessionID		MBS-AreaSessionID															OPTIONAL,
	cause					Cause,
	iE-Extensions			ProtocolExtensionContainer { { MBSSessionFailedtoSetupItem-ExtIEs} }		OPTIONAL,
	...
}

MBSSessionFailedtoSetupItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-ActiveSessionInformation-SourcetoTargetList ::= SEQUENCE (SIZE(1..maxnoofMBSSessionsofUE)) OF MBS-ActiveSessionInformation-SourcetoTargetItem

MBS-ActiveSessionInformation-SourcetoTargetItem ::= SEQUENCE {
	mBS-SessionID 								MBS-SessionID,
	mBS-AreaSessionID							MBS-AreaSessionID							OPTIONAL,
	mBS-ServiceArea								MBS-ServiceArea								OPTIONAL,
	mBS-QoSFlowsToBeSetupList 					MBS-QoSFlowsToBeSetupList,
	mBS-MappingandDataForwardingRequestList 	MBS-MappingandDataForwardingRequestList		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBS-ActiveSessionInformation-SourcetoTargetItem-ExtIEs} }	OPTIONAL,
	...
}

MBS-ActiveSessionInformation-SourcetoTargetItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-ActiveSessionInformation-TargettoSourceList ::= SEQUENCE (SIZE(1..maxnoofMBSSessionsofUE)) OF MBS-ActiveSessionInformation-TargettoSourceItem

MBS-ActiveSessionInformation-TargettoSourceItem ::= SEQUENCE {
	mBS-SessionID 						MBS-SessionID,
	mBS-DataForwardingResponseMRBList	MBS-DataForwardingResponseMRBList													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBS-ActiveSessionInformation-TargettoSourceItem-ExtIEs} }		OPTIONAL,
	...
}

MBS-ActiveSessionInformation-TargettoSourceItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetupOrModFailureTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBSSessionSetupOrModFailureTransfer-ExtIEs} }	OPTIONAL,
	...
}

MBSSessionSetupOrModFailureTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetupResponseList ::= SEQUENCE (SIZE(1.. maxnoofMBSSessions)) OF MBSSessionSetupResponseItem

MBSSessionSetupResponseItem ::= SEQUENCE {
	mBS-SessionID			MBS-SessionID,
	mBS-AreaSessionID		MBS-AreaSessionID													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBSSessionSetupResponseItem-ExtIEs} }	OPTIONAL,
	...
}

MBSSessionSetupResponseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetupOrModRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MBSSessionSetupOrModRequestTransferIEs} },
	...
}

MBSSessionSetupOrModRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionTNLInfo5GC				CRITICALITY reject	TYPE MBS-SessionTNLInfo5GC				PRESENCE	optional		}|
	{ ID id-MBS-QoSFlowsToBeSetupModList		CRITICALITY reject	TYPE MBS-QoSFlowsToBeSetupList		PRESENCE	mandatory	}|
	{ ID id-MBS-SessionFSAIDList				CRITICALITY ignore	TYPE MBS-SessionFSAIDList				PRESENCE	optional		},
	...
}

MBS-SessionFSAIDList ::= SEQUENCE (SIZE(1.. maxnoofMBSFSAs)) OF MBS-SessionFSAID

MBS-SessionFSAID ::= OCTET STRING (SIZE(3))

MBSSessionReleaseResponseTransfer ::= SEQUENCE {
	mBS-SessionTNLInfoNGRAN		MBS-SessionTNLInfoNGRAN				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {MBSSessionReleaseResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

MBSSessionReleaseResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetupOrModResponseTransfer ::= SEQUENCE {
	mBS-SessionTNLInfoNGRAN 	MBS-SessionTNLInfoNGRAN														OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {MBSSessionSetupOrModResponseTransfer-ExtIEs} }		OPTIONAL,
	...
}

MBSSessionSetupOrModResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-SupportIndicator ::= ENUMERATED {
	true,
	...
}

MBS-SessionTNLInfo5GC ::= CHOICE {
	locationindependent			SharedNGU-MulticastTNLInformation,
	locationdependent			MBS-SessionTNLInfo5GCList,
	choice-Extensions		ProtocolIE-SingleContainer { {MBS-SessionTNLInfo5GC-ExtIEs} }
}

MBS-SessionTNLInfo5GC-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MBS-SessionTNLInfo5GCList ::= SEQUENCE (SIZE(1..maxnoofMBSServiceAreaInformation)) OF MBS-SessionTNLInfo5GCItem

MBS-SessionTNLInfo5GCItem ::= SEQUENCE {
	mBS-AreaSessionID						MBS-AreaSessionID,
	sharedNGU-MulticastTNLInformation		SharedNGU-MulticastTNLInformation,
	iE-Extensions		ProtocolExtensionContainer { {MBS-SessionTNLInfo5GCItem-ExtIEs} } 	OPTIONAL,
	...
}

MBS-SessionTNLInfo5GCItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-SessionTNLInfoNGRAN ::= CHOICE {
	locationindependent			UPTransportLayerInformation,
	locationdependent			MBS-SessionTNLInfoNGRANList,
	choice-Extensions		ProtocolIE-SingleContainer { {MBS-SessionTNLInfoNGRAN-ExtIEs} }
}

MBS-SessionTNLInfoNGRAN-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MBS-SessionTNLInfoNGRANList ::= SEQUENCE (SIZE(1..maxnoofMBSServiceAreaInformation)) OF MBS-SessionTNLInfoNGRANItem

MBS-SessionTNLInfoNGRANItem ::= SEQUENCE {
	mBS-AreaSessionID					MBS-AreaSessionID,
	sharedNGU-UnicastTNLInformation		UPTransportLayerInformation								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {MBS-SessionTNLInfoNGRANItem-ExtIEs} } 	OPTIONAL,
	...
}

MBS-SessionTNLInfoNGRANItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-DistributionReleaseRequestTransfer ::= SEQUENCE {
	mBS-SessionID							MBS-SessionID,
	mBS-AreaSessionID						MBS-AreaSessionID												OPTIONAL,
	sharedNGU-UnicastTNLInformation			UPTransportLayerInformation										OPTIONAL,
	cause									Cause,
	iE-Extensions		ProtocolExtensionContainer { { MBS-DistributionReleaseRequesTransfer-ExtIEs} } 	OPTIONAL,
	...
}

MBS-DistributionReleaseRequesTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-DistributionSetupRequestTransfer ::= SEQUENCE {
	mBS-SessionID							MBS-SessionID,
	mBS-AreaSessionID						MBS-AreaSessionID												OPTIONAL,
	sharedNGU-UnicastTNLInformation			UPTransportLayerInformation										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBS-DistributionSetupRequestTransfer-ExtIEs} } 	OPTIONAL,
	...
}

MBS-DistributionSetupRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-DistributionSetupResponseTransfer ::= SEQUENCE {
	mBS-SessionID								MBS-SessionID,
	mBS-AreaSessionID							MBS-AreaSessionID				OPTIONAL,
	sharedNGU-MulticastTNLInformation			MBS-SessionTNLInfo5GCItem		OPTIONAL,
	mBS-QoSFlowsToBeSetupList					MBS-QoSFlowsToBeSetupList,
	mBSSessionStatus							MBSSessionStatus,
	mBS-ServiceArea								MBS-ServiceArea					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {MBS-DistributionSetupResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

MBS-DistributionSetupResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


MBS-DistributionSetupUnsuccessfulTransfer ::= SEQUENCE {
	mBS-SessionID				MBS-SessionID,
	mBS-AreaSessionID			MBS-AreaSessionID																	OPTIONAL,
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MBS-DistributionSetupUnsuccessfulTransfer-ExtIEs} } 	OPTIONAL,
	...
}

MBS-DistributionSetupUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetupRequestList ::= SEQUENCE (SIZE(1..maxnoofMBSSessions)) OF MBSSessionSetupRequestItem

MBSSessionSetupRequestItem ::= SEQUENCE {
	mBS-SessionID									MBS-SessionID,
	mBS-AreaSessionID								MBS-AreaSessionID																	OPTIONAL,
	associatedMBSQosFlowSetupRequestList			AssociatedMBSQosFlowSetupRequestList												OPTIONAL,
	iE-Extensions									ProtocolExtensionContainer { { MBSSessionSetupRequestItem-ExtIEs} }		OPTIONAL,
	...
}

MBSSessionSetupRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionSetuporModifyRequestList ::= SEQUENCE (SIZE(1..maxnoofMBSSessions)) OF MBSSessionSetuporModifyRequestItem

MBSSessionSetuporModifyRequestItem ::= SEQUENCE {
	mBS-SessionID										MBS-SessionID,
	mBS-AreaSessionID									MBS-AreaSessionID									OPTIONAL,
	associatedMBSQosFlowSetuporModifyRequestList		AssociatedMBSQosFlowSetuporModifyRequestList		OPTIONAL,
	mBS-QosFlowToReleaseList 							QosFlowListWithCause								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer {{MBSSessionSetuporModifyRequestItem-ExtIEs}}			OPTIONAL,
	...
}

MBSSessionSetuporModifyRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


MBSSessionToReleaseList ::= SEQUENCE (SIZE(1..maxnoofMBSSessions)) OF MBSSessionToReleaseItem

MBSSessionToReleaseItem ::= SEQUENCE {
	mBS-SessionID		MBS-SessionID,
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { { MBSSessionToReleaseItem-ExtIEs} }	OPTIONAL,
	...
}

MBSSessionToReleaseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBSSessionStatus ::= ENUMERATED {
	activated,
	deactivated,
	...
}

MicoAllPLMN ::= ENUMERATED {
	true,
	...
}


MICOModeIndication ::= ENUMERATED {
	true,
	...
}

MobilityInformation ::= BIT STRING (SIZE(16))

MobilityRestrictionList ::= SEQUENCE {
	servingPLMN					PLMNIdentity,
	equivalentPLMNs				EquivalentPLMNs											OPTIONAL,
	rATRestrictions				RATRestrictions											OPTIONAL,
	forbiddenAreaInformation	ForbiddenAreaInformation								OPTIONAL,
	serviceAreaInformation		ServiceAreaInformation									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {MobilityRestrictionList-ExtIEs} }	OPTIONAL,
	...
}

MobilityRestrictionList-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-LastEUTRAN-PLMNIdentity				CRITICALITY ignore	EXTENSION PLMNIdentity								PRESENCE optional		}|
	{ ID id-CNTypeRestrictionsForServing		CRITICALITY ignore	EXTENSION CNTypeRestrictionsForServing			PRESENCE optional		}|
	{ ID id-CNTypeRestrictionsForEquivalent		CRITICALITY ignore	EXTENSION CNTypeRestrictionsForEquivalent		PRESENCE optional		}|
	{ ID id-NPN-MobilityInformation				CRITICALITY reject	EXTENSION NPN-MobilityInformation				PRESENCE optional		},
	...
}

MDT-AlignmentInfo ::= CHOICE {
	s-basedMDT				NGRANTraceID,
	choice-Extensions		ProtocolIE-SingleContainer { { MDT-AlignmentInfo-ExtIEs} }
}

MDT-AlignmentInfo-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MDTPLMNList ::= SEQUENCE (SIZE(1..maxnoofMDTPLMNs)) OF PLMNIdentity

MDTPLMNModificationList ::= SEQUENCE (SIZE(0..maxnoofMDTPLMNs)) OF PLMNIdentity

MDT-Configuration ::= SEQUENCE {
	mdt-Config-NR		MDT-Configuration-NR		OPTIONAL,
	mdt-Config-EUTRA	MDT-Configuration-EUTRA		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MDT-Configuration-ExtIEs} } OPTIONAL,
	...
}

MDT-Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MDT-Configuration-NR ::= SEQUENCE {
	mdt-Activation				MDT-Activation,
	areaScopeOfMDT				AreaScopeOfMDT-NR,
	mDTModeNr					MDTModeNr,
	signallingBasedMDTPLMNList 	MDTPLMNList												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MDT-Configuration-NR-ExtIEs} } 	OPTIONAL,
	...
}

MDT-Configuration-NR-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MDT-Configuration-EUTRA ::= SEQUENCE {
	mdt-Activation				MDT-Activation,
	areaScopeOfMDT				AreaScopeOfMDT-EUTRA,
	mDTMode						MDTModeEutra,
	signallingBasedMDTPLMNList 	MDTPLMNList													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MDT-Configuration-EUTRA-ExtIEs} } 	OPTIONAL,
	...
}

MDT-Configuration-EUTRA-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MDT-Activation 	::= ENUMERATED {
	immediate-MDT-only,
	logged-MDT-only,
	immediate-MDT-and-Trace,
	...
}

MDTModeNr ::= CHOICE {
	immediateMDTNr				ImmediateMDTNr,
	loggedMDTNr					LoggedMDTNr,
	choice-Extensions		ProtocolIE-SingleContainer { {MDTModeNr-ExtIEs} }
}

MDTModeNr-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

MDTModeEutra ::= OCTET STRING

MeasurementsToActivate ::= BIT STRING(SIZE(8))

MRB-ID ::= INTEGER (1..512, ...)

MulticastSessionActivationRequestTransfer ::= SEQUENCE {
	mBS-SessionID				MBS-SessionID,
	iE-Extensions				ProtocolExtensionContainer { { MulticastSessionActivationRequestTransfer-ExtIEs} } 	OPTIONAL,
	...
}

MulticastSessionActivationRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MulticastSessionDeactivationRequestTransfer ::= SEQUENCE {
	mBS-SessionID				MBS-SessionID,
	iE-Extensions				ProtocolExtensionContainer { { MulticastSessionDeactivationRequestTransfer-ExtIEs} } 	OPTIONAL,
	...
}

MulticastSessionDeactivationRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MulticastSessionUpdateRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionUpdateRequestTransferIEs} },
	...
}

MulticastSessionUpdateRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID						PRESENCE mandatory	}|
	{ ID id-MBS-ServiceArea						CRITICALITY reject	TYPE MBS-ServiceArea					PRESENCE	optional		}|
	{ ID id-MBS-QoSFlowsToBeSetupModList		CRITICALITY reject	TYPE MBS-QoSFlowsToBeSetupList		PRESENCE	optional		}|
	{ ID id-MBS-QoSFlowToReleaseList			CRITICALITY reject	TYPE QosFlowListWithCause				PRESENCE	optional		}|
	{ ID id-MBS-SessionTNLInfo5GC				CRITICALITY reject	TYPE MBS-SessionTNLInfo5GC				PRESENCE	optional		},
	...
}


MulticastGroupPagingAreaList ::= SEQUENCE (SIZE(1..maxnoofPagingAreas)) OF MulticastGroupPagingAreaItem

MulticastGroupPagingAreaItem ::= SEQUENCE {
	multicastGroupPagingArea		MulticastGroupPagingArea,
	uE-PagingList					UE-PagingList 												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { MulticastGroupPagingAreaItem-ExtIEs} }	OPTIONAL,
	...
}

MulticastGroupPagingAreaItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MBS-AreaTAIList ::= SEQUENCE (SIZE(1..maxnoofTAIforPaging)) OF TAI

MulticastGroupPagingArea ::= SEQUENCE {
	mBS-AreaTAIList		MBS-AreaTAIList,
	iE-Extensions		ProtocolExtensionContainer { { MulticastGroupPagingArea-ExtIEs} } OPTIONAL,
	...
}

MulticastGroupPagingArea-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UE-PagingList ::= SEQUENCE (SIZE(1..maxnoofUEsforPaging)) OF UE-PagingItem

UE-PagingItem ::= SEQUENCE {
	uEIdentityIndexValue		UEIdentityIndexValue,
	pagingDRX					PagingDRX 										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { UE-PagingItem-ExtIEs} }	OPTIONAL,
	...
}

UE-PagingItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

M1Configuration ::= SEQUENCE {
	m1reportingTrigger			M1ReportingTrigger,
	m1thresholdEventA2			M1ThresholdEventA2									OPTIONAL,
--	The above IE shall be present if the M1 Reporting Trigger IE is set to “A2event-triggered” or “A2event-triggered periodic”
	m1periodicReporting			M1PeriodicReporting									OPTIONAL,
--	The above IE shall be present if the M1 Reporting Trigger IE is set to “periodic” or “A2event-triggered periodic”
	iE-Extensions		ProtocolExtensionContainer { { M1Configuration-ExtIEs} } 	OPTIONAL,
	...
}

M1Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-IncludeBeamMeasurementsIndication		CRITICALITY ignore	EXTENSION IncludeBeamMeasurementsIndication		PRESENCE optional			}|
	{ ID id-BeamMeasurementsReportConfiguration		CRITICALITY ignore	EXTENSION BeamMeasurementsReportConfiguration	PRESENCE conditional		},
-- The above IE shall be present if the IncludeBeamMeasurementsIndication IE is set to “true”
	...
}

IncludeBeamMeasurementsIndication ::= ENUMERATED {
	true,
	...
}

MaxNrofRS-IndexesToReport ::= INTEGER (1..64, ...)

M1ReportingTrigger ::= ENUMERATED {
	periodic,
	a2eventtriggered,
	a2eventtriggered-periodic,
	...
}

M1ThresholdEventA2 ::= SEQUENCE {
	m1ThresholdType		M1ThresholdType,
	iE-Extensions		ProtocolExtensionContainer { { M1ThresholdEventA2-ExtIEs} } OPTIONAL,
	...
}

M1ThresholdEventA2-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

M1ThresholdType ::= CHOICE {
	threshold-RSRP				Threshold-RSRP,
	threshold-RSRQ				Threshold-RSRQ,
	threshold-SINR				Threshold-SINR,
	choice-Extensions		ProtocolIE-SingleContainer { {M1ThresholdType-ExtIEs} }
}

M1ThresholdType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

M1PeriodicReporting ::= SEQUENCE {
	reportInterval				ReportIntervalMDT,
	reportAmount				ReportAmountMDT,
	iE-Extensions		ProtocolExtensionContainer { { M1PeriodicReporting-ExtIEs} } OPTIONAL,
	...
}

M1PeriodicReporting-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-ExtendedReportIntervalMDT		CRITICALITY ignore	EXTENSION ExtendedReportIntervalMDT		PRESENCE optional},
	...
}

M4Configuration ::= SEQUENCE {
	m4period			M4period,
	m4-links-to-log		Links-to-log,
	iE-Extensions		ProtocolExtensionContainer { { M4Configuration-ExtIEs} } OPTIONAL,
	...
}

M4Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-M4ReportAmount		CRITICALITY ignore	EXTENSION M4ReportAmountMDT		PRESENCE optional		},
	...
}

M4ReportAmountMDT ::= ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity, ...}

M4period ::= ENUMERATED {ms1024, ms2048, ms5120, ms10240, min1, ... }

M5Configuration ::= SEQUENCE {
	m5period			M5period,
	m5-links-to-log		Links-to-log,
	iE-Extensions		ProtocolExtensionContainer { { M5Configuration-ExtIEs} } OPTIONAL,
	...
}

M5Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-M5ReportAmount		CRITICALITY ignore	EXTENSION M5ReportAmountMDT		PRESENCE optional		},
	...
}

M5ReportAmountMDT ::= ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity, ...}


M5period ::= ENUMERATED {ms1024, ms2048, ms5120, ms10240, min1, ... }

M6Configuration ::= SEQUENCE {
	m6report-Interval	M6report-Interval,
	m6-links-to-log		Links-to-log,
	iE-Extensions		ProtocolExtensionContainer { { M6Configuration-ExtIEs} } OPTIONAL,
	...
}

M6Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-M6ReportAmount		CRITICALITY ignore	EXTENSION M6ReportAmountMDT		PRESENCE optional		}|
	{ ID id-ExcessPacketDelayThresholdConfiguration	CRITICALITY ignore	EXTENSION ExcessPacketDelayThresholdConfiguration		PRESENCE optional		},
	...
}


M6ReportAmountMDT ::= ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity, ...}

M6report-Interval ::= ENUMERATED {
	ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, ms20480, ms40960, min1, min6, min12, min30,
	...
}


M7Configuration ::= SEQUENCE {
	m7period			M7period,
	m7-links-to-log		Links-to-log,
	iE-Extensions		ProtocolExtensionContainer { { M7Configuration-ExtIEs} } OPTIONAL,
	...
}

M7Configuration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-M7ReportAmount		CRITICALITY ignore	EXTENSION M7ReportAmountMDT		PRESENCE optional		},
	...
}

M7ReportAmountMDT ::= ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity, ...}

M7period ::= INTEGER(1..60, ...)

MDT-Location-Info ::= SEQUENCE {
	mDT-Location-Information	MDT-Location-Information,
	iE-Extensions		ProtocolExtensionContainer { { MDT-Location-Info-ExtIEs} } OPTIONAL,
	...
}

MDT-Location-Info-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

MDT-Location-Information::= BIT STRING (SIZE (8))

-- N

N3IWF-ID ::= CHOICE {
	n3IWF-ID				BIT STRING (SIZE(16)),
	choice-Extensions		ProtocolIE-SingleContainer { {N3IWF-ID-ExtIEs} }
}

N3IWF-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NAS-PDU ::= OCTET STRING

NASSecurityParametersFromNGRAN ::= OCTET STRING

NB-IoT-DefaultPagingDRX ::= ENUMERATED {
	rf128, rf256, rf512, rf1024,
	...
}

NB-IoT-PagingDRX ::= ENUMERATED {
	rf32, rf64, rf128, rf256, rf512, rf1024,
	...
}

NB-IoT-Paging-eDRXCycle ::= ENUMERATED {
	hf2, hf4, hf6, hf8, hf10, hf12, hf14, hf16, hf32, hf64, hf128, hf256, hf512, hf1024,
	...
}

NB-IoT-Paging-TimeWindow ::= ENUMERATED {
	s1, s2, s3, s4, s5, s6, s7, s8, s9, s10, s11, s12, s13, s14, s15, s16,
	...
}

NB-IoT-Paging-eDRXInfo ::= SEQUENCE {
	nB-IoT-Paging-eDRXCycle 	NB-IoT-Paging-eDRXCycle,
	nB-IoT-Paging-TimeWindow 	NB-IoT-Paging-TimeWindow 								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { NB-IoT-Paging-eDRXInfo-ExtIEs} } OPTIONAL,
	...
}

NB-IoT-Paging-eDRXInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NB-IoT-UEPriority ::= INTEGER (0..255, ...)

NetworkInstance ::= INTEGER (1..256, ...)

NewSecurityContextInd ::= ENUMERATED {
	true,
	...
}

NextHopChainingCount ::= INTEGER (0..7)

NextPagingAreaScope ::= ENUMERATED {
	same,
	changed,
	...
}

NGAPIESupportInformationRequestList ::= SEQUENCE (SIZE(1.. maxnoofNGAPIESupportInfo)) OF NGAPIESupportInformationRequestItem

NGAPIESupportInformationRequestItem ::= SEQUENCE {
	ngap-ProtocolIE-Id		ProtocolIE-ID,
	iE-Extensions		ProtocolExtensionContainer { { NGAPIESupportInformationRequestItem-ExtIEs} }	OPTIONAL,
	...
}

NGAPIESupportInformationRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGAPIESupportInformationResponseList ::= SEQUENCE (SIZE(1.. maxnoofNGAPIESupportInfo)) OF NGAPIESupportInformationResponseItem

NGAPIESupportInformationResponseItem ::= SEQUENCE {
	ngap-ProtocolIE-Id				ProtocolIE-ID,
	ngap-ProtocolIESupportInfo		ENUMERATED {supported, not-supported, ...},
	ngap-ProtocolIEPresenceInfo		ENUMERATED {present, not-present, ...},
	iE-Extensions		ProtocolExtensionContainer { { NGAPIESupportInformationResponseItem-ExtIEs} }	OPTIONAL,
	...
}

NGAPIESupportInformationResponseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NgENB-ID ::= CHOICE {
	macroNgENB-ID			BIT STRING (SIZE(20)),
	shortMacroNgENB-ID		BIT STRING (SIZE(18)),
	longMacroNgENB-ID		BIT STRING (SIZE(21)),
	choice-Extensions		ProtocolIE-SingleContainer { {NgENB-ID-ExtIEs} }
}

NgENB-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NotifySourceNGRANNode ::= ENUMERATED {
	notifySource,
	...
}

NGRAN-CGI ::= CHOICE {
	nR-CGI			NR-CGI,
	eUTRA-CGI		EUTRA-CGI,
	choice-Extensions		ProtocolIE-SingleContainer { {NGRAN-CGI-ExtIEs} }
}

NGRAN-CGI-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NGRAN-TNLAssociationToRemoveList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF NGRAN-TNLAssociationToRemoveItem

NGRAN-TNLAssociationToRemoveItem::= SEQUENCE {
	tNLAssociationTransportLayerAddress			CPTransportLayerInformation,
	tNLAssociationTransportLayerAddressAMF		CPTransportLayerInformation								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { NGRAN-TNLAssociationToRemoveItem-ExtIEs} } 	OPTIONAL
}

NGRAN-TNLAssociationToRemoveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NGRANTraceID ::= OCTET STRING (SIZE(8))

NID ::= BIT STRING (SIZE(44))

NonDynamic5QIDescriptor ::= SEQUENCE {
	fiveQI						FiveQI,
	priorityLevelQos			PriorityLevelQos										OPTIONAL,
	averagingWindow				AveragingWindow											OPTIONAL,
	maximumDataBurstVolume		MaximumDataBurstVolume									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {NonDynamic5QIDescriptor-ExtIEs} }	OPTIONAL,
	...
}

NonDynamic5QIDescriptor-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CNPacketDelayBudgetDL	CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional		}|
	{ ID id-CNPacketDelayBudgetUL	CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional		},
	...
}

NotAllowedTACs ::= SEQUENCE (SIZE(1..maxnoofAllowedAreas)) OF TAC

NotificationCause ::= ENUMERATED {
	fulfilled,
	not-fulfilled,
	...
}

NotificationControl ::= ENUMERATED {
	notification-requested,
	...
}

NPN-AccessInformation ::= CHOICE {
	pNI-NPN-Access-Information		CellCAGList,
	choice-Extensions				ProtocolIE-SingleContainer { {NPN-AccessInformation-ExtIEs} }
}

NPN-AccessInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NPN-MobilityInformation ::= CHOICE {
	sNPN-MobilityInformation		SNPN-MobilityInformation,
	pNI-NPN-MobilityInformation		PNI-NPN-MobilityInformation,
	choice-Extensions				ProtocolIE-SingleContainer { {NPN-MobilityInformation-ExtIEs} }
}

NPN-MobilityInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}


NPN-PagingAssistanceInformation ::= CHOICE {
	pNI-NPN-PagingAssistance		Allowed-PNI-NPN-List,
	choice-Extensions				ProtocolIE-SingleContainer { {NPN-PagingAssistanceInformation-ExtIEs} }
}

NPN-PagingAssistanceInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NPN-Support ::= CHOICE {
	sNPN					NID,
	choice-Extensions		ProtocolIE-SingleContainer { {NPN-Support-ExtIEs} }
}

NPN-Support-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

NRCellIdentity ::= BIT STRING (SIZE(36))

NR-CGI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	nRCellIdentity		NRCellIdentity,
	iE-Extensions		ProtocolExtensionContainer { {NR-CGI-ExtIEs} } OPTIONAL,
	...
}

NR-CGI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NR-CGIList ::= SEQUENCE (SIZE(1..maxnoofCellsingNB)) OF NR-CGI

NR-CGIListForWarning ::= SEQUENCE (SIZE(1..maxnoofCellIDforWarning)) OF NR-CGI

NR-PagingeDRXInformation ::= SEQUENCE {
	nR-paging-eDRX-Cycle		NR-Paging-eDRX-Cycle,
	nR-paging-Time-Window		NR-Paging-Time-Window					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {NR-PagingeDRXInformation-ExtIEs} }	OPTIONAL,
	...
}

NR-PagingeDRXInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NR-Paging-eDRX-Cycle ::= ENUMERATED {
	hfquarter, hfhalf, hf1, hf2, hf4, hf8, hf16,
	hf32, hf64, hf128, hf256, hf512, hf1024,
	...
}

NR-Paging-Time-Window ::= ENUMERATED {
	s1, s2, s3, s4, s5,
	s6, s7, s8, s9, s10,
	s11, s12, s13, s14, s15, s16,
	...,
	s17, s18, s19, s20, s21, s22, s23, s24,
	s25, s26, s27, s28, s29, s30, s31, s32
}

NRencryptionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRintegrityProtectionAlgorithms ::= BIT STRING (SIZE(16, ...))

NRMobilityHistoryReport ::= OCTET STRING

NRPPa-PDU ::= OCTET STRING

NRUERLFReportContainer ::= OCTET STRING

NRNTNTAIInformation	::= SEQUENCE {
	servingPLMN							PLMNIdentity,
	tACListInNRNTN						TACListInNRNTN,
	uELocationDerivedTACInNRNTN			TAC							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { NRNTNTAIInformation-ExtIEs} } OPTIONAL,
	...
}

NRNTNTAIInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


NumberOfBroadcasts ::= INTEGER (0..65535)

NumberOfBroadcastsRequested ::= INTEGER (0..65535)

NRARFCN	::= INTEGER (0.. maxNRARFCN)

NRFrequencyBand ::= INTEGER (1..1024, ...)

NRFrequencyBand-List ::= SEQUENCE (SIZE(1..maxnoofNRCellBands)) OF NRFrequencyBandItem

NRFrequencyBandItem ::= SEQUENCE {
	nr-frequency-band			NRFrequencyBand,
	iE-Extension		ProtocolExtensionContainer { {NRFrequencyBandItem-ExtIEs} } 	OPTIONAL,
	...
}

NRFrequencyBandItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NRFrequencyInfo ::= SEQUENCE {
	nrARFCN				NRARFCN,
	frequencyBand-List		NRFrequencyBand-List,
	iE-Extension		ProtocolExtensionContainer { {NRFrequencyInfo-ExtIEs} }		OPTIONAL,
	...
}

NRFrequencyInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NR-PCI ::= INTEGER (0..1007, ...)

NRV2XServicesAuthorized ::= SEQUENCE {
	vehicleUE			VehicleUE														OPTIONAL,
	pedestrianUE 		PedestrianUE													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {NRV2XServicesAuthorized-ExtIEs} }	OPTIONAL,
	...
}

NRV2XServicesAuthorized-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

VehicleUE ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

PedestrianUE ::= ENUMERATED {
	authorized,
	not-authorized,
	...
}

NRUESidelinkAggregateMaximumBitrate ::= SEQUENCE {
	uESidelinkAggregateMaximumBitRate		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {NRUESidelinkAggregateMaximumBitrate-ExtIEs} } OPTIONAL,
	...
}

NRUESidelinkAggregateMaximumBitrate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

NSAG-ID ::= INTEGER (0..255, ...)

-- O

OnboardingSupport ::= ENUMERATED {
	true,
	...
}

OverloadAction ::= ENUMERATED {
	reject-non-emergency-mo-dt,
	reject-rrc-cr-signalling,
	permit-emergency-sessions-and-mobile-terminated-services-only,
	permit-high-priority-sessions-and-mobile-terminated-services-only,
	...
}

OverloadResponse ::= CHOICE {
	overloadAction			OverloadAction,
	choice-Extensions		ProtocolIE-SingleContainer { {OverloadResponse-ExtIEs} }
}

OverloadResponse-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

OverloadStartNSSAIList ::= SEQUENCE (SIZE (1..maxnoofSliceItems)) OF OverloadStartNSSAIItem

OverloadStartNSSAIItem ::= SEQUENCE {
	sliceOverloadList						SliceOverloadList,
	sliceOverloadResponse					OverloadResponse								OPTIONAL,
	sliceTrafficLoadReductionIndication		TrafficLoadReductionIndication				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {OverloadStartNSSAIItem-ExtIEs} }	OPTIONAL,
	...
}

OverloadStartNSSAIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- P

PacketDelayBudget ::= INTEGER (0..1023, ...)

PacketErrorRate ::= SEQUENCE {
	pERScalar		INTEGER (0..9, ...),
	pERExponent		INTEGER (0..9, ...),
	iE-Extensions		ProtocolExtensionContainer { {PacketErrorRate-ExtIEs} }	OPTIONAL,
	...
}

PacketErrorRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PacketLossRate ::= INTEGER (0..1000, ...)

PagingAssisDataforCEcapabUE ::= SEQUENCE {
	eUTRA-CGI							EUTRA-CGI,
	coverageEnhancementLevel			CoverageEnhancementLevel,
	iE-Extensions						ProtocolExtensionContainer { { PagingAssisDataforCEcapabUE-ExtIEs} } OPTIONAL,
	...
}

PagingAssisDataforCEcapabUE-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PagingAttemptInformation ::= SEQUENCE {
	pagingAttemptCount					PagingAttemptCount,
	intendedNumberOfPagingAttempts		IntendedNumberOfPagingAttempts,
	nextPagingAreaScope					NextPagingAreaScope									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PagingAttemptInformation-ExtIEs} }	OPTIONAL,
	...
}

PagingAttemptInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PagingAttemptCount ::= INTEGER (1..16, ...)

PagingCause ::= ENUMERATED {
	voice,
	...
}

PagingCauseIndicationForVoiceService ::= ENUMERATED {
	supported,
	...
}

PagingDRX ::= ENUMERATED {
	v32,
	v64,
	v128,
	v256,
	...
}

PagingOrigin ::= ENUMERATED {
	non-3gpp,
	...
}

PagingPriority ::= ENUMERATED {
	priolevel1,
	priolevel2,
	priolevel3,
	priolevel4,
	priolevel5,
	priolevel6,
	priolevel7,
	priolevel8,
	...
}

PagingProbabilityInformation ::= ENUMERATED {
	p00, p05, p10, p15, p20, p25, p30, p35, p40, p45, p50, p55, p60, p65, p70, p75, p80, p85, p90, p95, p100,
	...
}

PathSwitchRequestAcknowledgeTransfer ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation											OPTIONAL,
	securityIndication				SecurityIndication													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestAcknowledgeTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestAcknowledgeTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalNGU-UP-TNLInformation				CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList		PRESENCE optional	}|
	{ ID id-RedundantUL-NGU-UP-TNLInformation			CRITICALITY ignore	EXTENSION UPTransportLayerInformation				PRESENCE optional	}|
	{ ID id-AdditionalRedundantNGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList		PRESENCE optional	}|
	{ ID id-QosFlowParametersList						CRITICALITY ignore	EXTENSION QosFlowParametersList						PRESENCE optional },
	...
}

PathSwitchRequestSetupFailedTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestSetupFailedTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestSetupFailedTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PathSwitchRequestTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation			UPTransportLayerInformation,
	dL-NGU-TNLInformationReused			DL-NGU-TNLInformationReused							OPTIONAL,
	userPlaneSecurityInformation		UserPlaneSecurityInformation						OPTIONAL,
	qosFlowAcceptedList					QosFlowAcceptedList,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalDLQosFlowPerTNLInformation				CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList		PRESENCE optional	}|
	{ ID id-RedundantDL-NGU-UP-TNLInformation					CRITICALITY ignore	EXTENSION UPTransportLayerInformation			PRESENCE optional	}|
	{ ID id-RedundantDL-NGU-TNLInformationReused				CRITICALITY ignore	EXTENSION DL-NGU-TNLInformationReused			PRESENCE optional	}|
	{ ID id-AdditionalRedundantDLQosFlowPerTNLInformation		CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList		PRESENCE optional	}|
	{ ID id-UsedRSNInformation									CRITICALITY ignore	EXTENSION RedundantPDUSessionInformation		PRESENCE optional	}|
	{ ID id-GlobalRANNodeID 										CRITICALITY ignore	EXTENSION GlobalRANNodeID							PRESENCE optional	}|
	{ ID id-MBS-SupportIndicator								CRITICALITY ignore	EXTENSION MBS-SupportIndicator					PRESENCE optional	},
	...
}

PathSwitchRequestUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PathSwitchRequestUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PathSwitchRequestUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PC5QoSParameters ::= SEQUENCE {
	pc5QoSFlowList				PC5QoSFlowList,
	pc5LinkAggregateBitRates	BitRate												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { PC5QoSParameters-ExtIEs} }	OPTIONAL,
	...
}

PC5QoSParameters-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
             ...
}

PC5QoSFlowList ::= SEQUENCE (SIZE(1..maxnoofPC5QoSFlows)) OF PC5QoSFlowItem

PC5QoSFlowItem::= SEQUENCE {
	pQI					FiveQI,
	pc5FlowBitRates		PC5FlowBitRates											OPTIONAL,
	range				Range													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { PC5QoSFlowItem-ExtIEs} }	OPTIONAL,
	...
}

PC5QoSFlowItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
             ...
}

PC5FlowBitRates ::= SEQUENCE {
	guaranteedFlowBitRate		BitRate,
	maximumFlowBitRate			BitRate,
	iE-Extensions		ProtocolExtensionContainer { { PC5FlowBitRates-ExtIEs} }	OPTIONAL,
	...
}

PC5FlowBitRates-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


PCIListForMDT ::= SEQUENCE (SIZE(1.. maxnoofNeighPCIforMDT)) OF NR-PCI

PrivacyIndicator ::= ENUMERATED {
	immediate-MDT,
	logged-MDT,
	...
}

PDUSessionAggregateMaximumBitRate ::= SEQUENCE {
	pDUSessionAggregateMaximumBitRateDL		BitRate,
	pDUSessionAggregateMaximumBitRateUL		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionAggregateMaximumBitRate-ExtIEs} } OPTIONAL,
	...
}

PDUSessionAggregateMaximumBitRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionID ::= INTEGER (0..255)

PDUSessionPairID ::= INTEGER (0..255, ...)

PDUSessionResourceAdmittedList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceAdmittedItem

PDUSessionResourceAdmittedItem ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	handoverRequestAcknowledgeTransfer		OCTET STRING (CONTAINING HandoverRequestAcknowledgeTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceAdmittedItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceAdmittedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToModifyListModCfm ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToModifyItemModCfm

PDUSessionResourceFailedToModifyItemModCfm ::= SEQUENCE {
	pDUSessionID												PDUSessionID,
	pDUSessionResourceModifyIndicationUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyIndicationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToModifyItemModCfm-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToModifyItemModCfm-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToModifyListModRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToModifyItemModRes

PDUSessionResourceFailedToModifyItemModRes ::= SEQUENCE {
	pDUSessionID										PDUSessionID,
	pDUSessionResourceModifyUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToModifyItemModRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToModifyItemModRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToResumeListRESReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToResumeItemRESReq

PDUSessionResourceFailedToResumeItemRESReq ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	cause								Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToResumeItemRESReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToResumeItemRESReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


PDUSessionResourceFailedToResumeListRESRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToResumeItemRESRes

PDUSessionResourceFailedToResumeItemRESRes ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	cause								Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToResumeItemRESRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToResumeItemRESRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListCxtFail ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemCxtFail

PDUSessionResourceFailedToSetupItemCxtFail ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemCxtFail-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemCxtFail-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListCxtRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemCxtRes

PDUSessionResourceFailedToSetupItemCxtRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemCxtRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemCxtRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListHOAck ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemHOAck

PDUSessionResourceFailedToSetupItemHOAck ::= SEQUENCE {
	pDUSessionID										PDUSessionID,
	handoverResourceAllocationUnsuccessfulTransfer		OCTET STRING (CONTAINING HandoverResourceAllocationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemHOAck-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemHOAck-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListPSReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemPSReq

PDUSessionResourceFailedToSetupItemPSReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestSetupFailedTransfer		OCTET STRING (CONTAINING PathSwitchRequestSetupFailedTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemPSReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemPSReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceFailedToSetupListSURes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceFailedToSetupItemSURes

PDUSessionResourceFailedToSetupItemSURes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceSetupUnsuccessfulTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceFailedToSetupItemSURes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceFailedToSetupItemSURes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceHandoverList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceHandoverItem

PDUSessionResourceHandoverItem ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	handoverCommandTransfer				OCTET STRING (CONTAINING HandoverCommandTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceHandoverItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceHandoverItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceInformationList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceInformationItem

PDUSessionResourceInformationItem ::= SEQUENCE {
	pDUSessionID					PDUSessionID,
	qosFlowInformationList			QosFlowInformationList,
	dRBsToQosFlowsMappingList		DRBsToQosFlowsMappingList										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceInformationItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceListCxtRelCpl ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemCxtRelCpl

PDUSessionResourceItemCxtRelCpl ::= SEQUENCE {
	pDUSessionID		PDUSessionID,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemCxtRelCpl-ExtIEs} }	OPTIONAL,
	...
}

-- WS modification: define a dedicated type
PDUSessionResourceReleaseResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING PDUSessionResourceReleaseResponseTransfer)

PDUSessionResourceItemCxtRelCpl-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
-- WS modification: define a dedicated type
--	{ ID id-PDUSessionResourceReleaseResponseTransfer	CRITICALITY ignore	EXTENSION OCTET STRING (CONTAINING PDUSessionResourceReleaseResponseTransfer)	PRESENCE optional	},
	{ ID id-PDUSessionResourceReleaseResponseTransfer	CRITICALITY ignore	EXTENSION PDUSessionResourceReleaseResponseTransfer-OCTET-STRING	PRESENCE optional	},
	...
}

PDUSessionResourceListCxtRelReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemCxtRelReq

PDUSessionResourceItemCxtRelReq ::= SEQUENCE {
	pDUSessionID		PDUSessionID,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemCxtRelReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceItemCxtRelReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceListHORqd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceItemHORqd

PDUSessionResourceItemHORqd ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	handoverRequiredTransfer				OCTET STRING (CONTAINING HandoverRequiredTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceItemHORqd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceItemHORqd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyConfirmTransfer ::= SEQUENCE {
	qosFlowModifyConfirmList			QosFlowModifyConfirmList,
	uLNGU-UP-TNLInformation				UPTransportLayerInformation,
	additionalNG-UUPTNLInformation		UPTransportLayerInformationPairList									OPTIONAL,
	qosFlowFailedToModifyList			QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyConfirmTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyConfirmTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-RedundantUL-NGU-UP-TNLInformation			CRITICALITY ignore	EXTENSION UPTransportLayerInformation				PRESENCE optional	}|
	{ ID id-AdditionalRedundantNGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList		PRESENCE optional	},
	...
}

PDUSessionResourceModifyIndicationUnsuccessfulTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyIndicationUnsuccessfulTransfer-ExtIEs} }		OPTIONAL,
	...
}

PDUSessionResourceModifyIndicationUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyRequestTransferIEs} },
	...
}

PDUSessionResourceModifyRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PDUSessionAggregateMaximumBitRate			CRITICALITY reject	TYPE PDUSessionAggregateMaximumBitRate		PRESENCE	optional		}|
	{ ID id-UL-NGU-UP-TNLModifyList						CRITICALITY reject	TYPE UL-NGU-UP-TNLModifyList					PRESENCE	optional		}|
	{ ID id-NetworkInstance								CRITICALITY reject	TYPE NetworkInstance								PRESENCE optional		}|
	{ ID id-QosFlowAddOrModifyRequestList				CRITICALITY reject	TYPE QosFlowAddOrModifyRequestList			PRESENCE optional		}|
	{ ID id-QosFlowToReleaseList						CRITICALITY reject	TYPE QosFlowListWithCause						PRESENCE optional		}|
	{ ID id-AdditionalUL-NGU-UP-TNLInformation			CRITICALITY reject	TYPE UPTransportLayerInformationList			PRESENCE optional		}|
	{ ID id-CommonNetworkInstance						CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional		}|
	{ ID id-AdditionalRedundantUL-NGU-UP-TNLInformation	CRITICALITY ignore	TYPE UPTransportLayerInformationList			PRESENCE optional		}|
	{ ID id-RedundantCommonNetworkInstance				CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional		}|
	{ ID id-RedundantUL-NGU-UP-TNLInformation			CRITICALITY ignore	TYPE UPTransportLayerInformation				PRESENCE optional	 	}|
	{ ID id-SecurityIndication							CRITICALITY ignore	TYPE SecurityIndication							PRESENCE optional		}|
	{ ID id-MBSSessionSetuporModifyRequestList			CRITICALITY ignore	TYPE MBSSessionSetuporModifyRequestList		PRESENCE optional		}|
	{ ID id-MBSSessionToReleaseList						CRITICALITY ignore	TYPE MBSSessionToReleaseList					PRESENCE optional		},
	...
}

PDUSessionResourceModifyResponseTransfer ::= SEQUENCE {
	dL-NGU-UP-TNLInformation				UPTransportLayerInformation											OPTIONAL,
	uL-NGU-UP-TNLInformation				UPTransportLayerInformation											OPTIONAL,
	qosFlowAddOrModifyResponseList			QosFlowAddOrModifyResponseList										OPTIONAL,
	additionalDLQosFlowPerTNLInformation	QosFlowPerTNLInformationList										OPTIONAL,
	qosFlowFailedToAddOrModifyList			QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-AdditionalNGU-UP-TNLInformation					CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList	PRESENCE optional	}|
	{ ID id-RedundantDL-NGU-UP-TNLInformation				CRITICALITY ignore	EXTENSION UPTransportLayerInformation				PRESENCE optional	}|
	{ ID id-RedundantUL-NGU-UP-TNLInformation				CRITICALITY ignore	EXTENSION UPTransportLayerInformation				PRESENCE optional	}|
	{ ID id-AdditionalRedundantDLQosFlowPerTNLInformation	CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList				PRESENCE optional	}|
	{ ID id-AdditionalRedundantNGU-UP-TNLInformation		CRITICALITY ignore	EXTENSION UPTransportLayerInformationPairList	PRESENCE optional	}|
	{ ID id-SecondaryRATUsageInformation					CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation				PRESENCE optional	}|
	{ ID id-MBS-SupportIndicator							CRITICALITY ignore	EXTENSION MBS-SupportIndicator						PRESENCE optional	}|
	{ ID id-MBSSessionSetuporModifyResponseList				CRITICALITY ignore	EXTENSION MBSSessionSetupResponseList				PRESENCE optional	}|
	{ ID id-MBSSessionFailedtoSetuporModifyList				CRITICALITY ignore	EXTENSION MBSSessionFailedtoSetupList				PRESENCE optional	},
	...
}

PDUSessionResourceModifyIndicationTransfer ::= SEQUENCE {
	dLQosFlowPerTNLInformation					QosFlowPerTNLInformation,
	additionalDLQosFlowPerTNLInformation		QosFlowPerTNLInformationList 									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyIndicationTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyIndicationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation					CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	}|
	{ ID id-SecurityResult									CRITICALITY ignore	EXTENSION SecurityResult						PRESENCE optional	}|
	{ ID id-RedundantDLQosFlowPerTNLInformation				CRITICALITY ignore	EXTENSION QosFlowPerTNLInformation			PRESENCE optional	}|
	{ ID id-AdditionalRedundantDLQosFlowPerTNLInformation	CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList		PRESENCE optional	}|
	{ ID id-GlobalRANNodeID 								CRITICALITY ignore	EXTENSION GlobalRANNodeID						PRESENCE optional	},
	...
}

PDUSessionResourceModifyListModCfm ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModCfm

PDUSessionResourceModifyItemModCfm ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionResourceModifyConfirmTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyConfirmTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModCfm-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModCfm-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyListModInd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModInd

PDUSessionResourceModifyItemModInd ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceModifyIndicationTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyIndicationTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModInd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModInd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyListModReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModReq

PDUSessionResourceModifyItemModReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	nAS-PDU										NAS-PDU													OPTIONAL,
	pDUSessionResourceModifyRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-S-NSSAI											CRITICALITY reject	EXTENSION S-NSSAI						PRESENCE optional	}|
	{ ID id-PduSessionExpectedUEActivityBehaviour			CRITICALITY ignore	EXTENSION ExpectedUEActivityBehaviour	PRESENCE optional	},
	...
}

PDUSessionResourceModifyListModRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceModifyItemModRes

PDUSessionResourceModifyItemModRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceModifyResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceModifyResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyItemModRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyItemModRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceModifyUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceModifyUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceModifyUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceNotifyList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceNotifyItem

PDUSessionResourceNotifyItem ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	pDUSessionResourceNotifyTransfer	OCTET STRING (CONTAINING PDUSessionResourceNotifyTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceNotifyReleasedTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyReleasedTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyReleasedTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	},
	...
}

PDUSessionResourceNotifyTransfer ::= SEQUENCE {
	qosFlowNotifyList		QosFlowNotifyList														OPTIONAL,
	qosFlowReleasedList		QosFlowListWithCause													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceNotifyTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceNotifyTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	}|
	{ ID id-QosFlowFeedbackList					CRITICALITY ignore	EXTENSION QosFlowFeedbackList					PRESENCE optional	},
	...
}

PDUSessionResourceReleaseCommandTransfer ::= SEQUENCE {
	cause				Cause,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleaseCommandTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleaseCommandTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListNot ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemNot

PDUSessionResourceReleasedItemNot ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceNotifyReleasedTransfer		OCTET STRING (CONTAINING PDUSessionResourceNotifyReleasedTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemNot-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemNot-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListPSAck ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemPSAck

PDUSessionResourceReleasedItemPSAck ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestUnsuccessfulTransfer		OCTET STRING (CONTAINING PathSwitchRequestUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemPSAck-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemPSAck-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListPSFail ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemPSFail

PDUSessionResourceReleasedItemPSFail ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestUnsuccessfulTransfer		OCTET STRING (CONTAINING PathSwitchRequestUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemPSFail-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemPSFail-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleasedListRelRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceReleasedItemRelRes

PDUSessionResourceReleasedItemRelRes ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceReleaseResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceReleaseResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleasedItemRelRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleasedItemRelRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceReleaseResponseTransfer ::= SEQUENCE {
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceReleaseResponseTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceReleaseResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SecondaryRATUsageInformation		CRITICALITY ignore	EXTENSION SecondaryRATUsageInformation		PRESENCE optional	},
	...
}

PDUSessionResourceResumeListRESReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceResumeItemRESReq

PDUSessionResourceResumeItemRESReq ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	uEContextResumeRequestTransfer		OCTET STRING (CONTAINING UEContextResumeRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceResumeItemRESReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceResumeItemRESReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceResumeListRESRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceResumeItemRESRes

PDUSessionResourceResumeItemRESRes ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	uEContextResumeResponseTransfer		OCTET STRING (CONTAINING UEContextResumeResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceResumeItemRESRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceResumeItemRESRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSecondaryRATUsageList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSecondaryRATUsageItem

PDUSessionResourceSecondaryRATUsageItem ::= SEQUENCE {
	pDUSessionID							PDUSessionID,
	secondaryRATDataUsageReportTransfer		OCTET STRING (CONTAINING SecondaryRATDataUsageReportTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSecondaryRATUsageItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSecondaryRATUsageItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListCxtReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemCxtReq

PDUSessionResourceSetupItemCxtReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	nAS-PDU										NAS-PDU												OPTIONAL,
	s-NSSAI										S-NSSAI,
	pDUSessionResourceSetupRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemCxtReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemCxtReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PduSessionExpectedUEActivityBehaviour			CRITICALITY ignore	EXTENSION ExpectedUEActivityBehaviour	PRESENCE optional	},
	...
}

PDUSessionResourceSetupListCxtRes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemCxtRes

PDUSessionResourceSetupItemCxtRes ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionResourceSetupResponseTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemCxtRes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemCxtRes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupListHOReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemHOReq

PDUSessionResourceSetupItemHOReq ::= SEQUENCE {
	pDUSessionID				PDUSessionID,
	s-NSSAI						S-NSSAI,
	handoverRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemHOReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemHOReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PduSessionExpectedUEActivityBehaviour			CRITICALITY ignore	EXTENSION ExpectedUEActivityBehaviour	PRESENCE optional	},
	...
}

PDUSessionResourceSetupListSUReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemSUReq

PDUSessionResourceSetupItemSUReq ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pDUSessionNAS-PDU							NAS-PDU												OPTIONAL,
	s-NSSAI										S-NSSAI,
	pDUSessionResourceSetupRequestTransfer		OCTET STRING (CONTAINING PDUSessionResourceSetupRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemSUReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemSUReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PduSessionExpectedUEActivityBehaviour			CRITICALITY ignore	EXTENSION ExpectedUEActivityBehaviour	PRESENCE optional	},
	...
}

PDUSessionResourceSetupListSURes ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSetupItemSURes

PDUSessionResourceSetupItemSURes ::= SEQUENCE {
	pDUSessionID											PDUSessionID,
	pDUSessionResourceSetupResponseTransfer					OCTET STRING (CONTAINING PDUSessionResourceSetupResponseTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupItemSURes-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupItemSURes-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSetupRequestTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupRequestTransferIEs} },
	...
}

PDUSessionResourceSetupRequestTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PDUSessionAggregateMaximumBitRate			CRITICALITY reject	TYPE PDUSessionAggregateMaximumBitRate		PRESENCE optional		}|
	{ ID id-UL-NGU-UP-TNLInformation					CRITICALITY reject	TYPE UPTransportLayerInformation				PRESENCE mandatory	}|
	{ ID id-AdditionalUL-NGU-UP-TNLInformation			CRITICALITY reject	TYPE UPTransportLayerInformationList			PRESENCE optional		}|
	{ ID id-DataForwardingNotPossible					CRITICALITY reject	TYPE DataForwardingNotPossible					PRESENCE optional		}|
	{ ID id-PDUSessionType								CRITICALITY reject	TYPE PDUSessionType									PRESENCE mandatory	}|
	{ ID id-SecurityIndication							CRITICALITY reject	TYPE SecurityIndication							PRESENCE optional		}|
	{ ID id-NetworkInstance								CRITICALITY reject	TYPE NetworkInstance								PRESENCE optional		}|
	{ ID id-QosFlowSetupRequestList						CRITICALITY reject	TYPE QosFlowSetupRequestList					PRESENCE mandatory	}|
	{ ID id-CommonNetworkInstance						CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional		}|
	{ ID id-DirectForwardingPathAvailability			CRITICALITY ignore	TYPE DirectForwardingPathAvailability		PRESENCE optional	 	}|
	{ ID id-RedundantUL-NGU-UP-TNLInformation			CRITICALITY ignore	TYPE UPTransportLayerInformation				PRESENCE optional	 	}|
	{ ID id-AdditionalRedundantUL-NGU-UP-TNLInformation	CRITICALITY ignore	TYPE UPTransportLayerInformationList			PRESENCE optional		}|
	{ ID id-RedundantCommonNetworkInstance				CRITICALITY ignore	TYPE CommonNetworkInstance						PRESENCE optional		}|
	{ ID id-RedundantPDUSessionInformation				CRITICALITY ignore	TYPE RedundantPDUSessionInformation 			PRESENCE optional		}|
	{ ID id-MBSSessionSetupRequestList					CRITICALITY ignore	TYPE MBSSessionSetupRequestList				PRESENCE optional		},
	...
}

PDUSessionResourceSetupResponseTransfer ::= SEQUENCE {
	dLQosFlowPerTNLInformation				QosFlowPerTNLInformation,
	additionalDLQosFlowPerTNLInformation	QosFlowPerTNLInformationList										OPTIONAL,
	securityResult							SecurityResult														OPTIONAL,
	qosFlowFailedToSetupList				QosFlowListWithCause												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupResponseTransfer-ExtIEs} }		OPTIONAL,
	...
}

PDUSessionResourceSetupResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-RedundantDLQosFlowPerTNLInformation				CRITICALITY ignore	EXTENSION QosFlowPerTNLInformation			PRESENCE optional	 	}|
	{ ID id-AdditionalRedundantDLQosFlowPerTNLInformation	CRITICALITY ignore	EXTENSION QosFlowPerTNLInformationList		PRESENCE optional	 	}|
	{ ID id-UsedRSNInformation								CRITICALITY ignore	EXTENSION RedundantPDUSessionInformation	PRESENCE optional		}|
	{ ID id-GlobalRANNodeID 									CRITICALITY ignore	EXTENSION GlobalRANNodeID						PRESENCE optional		}|
	{ ID id-MBS-SupportIndicator							CRITICALITY ignore	EXTENSION MBS-SupportIndicator				PRESENCE optional		}|
	{ ID id-MBSSessionSetupResponseList						CRITICALITY ignore	EXTENSION MBSSessionSetupResponseList		PRESENCE optional		}|
	{ ID id-MBSSessionFailedtoSetupList						CRITICALITY ignore	EXTENSION MBSSessionFailedtoSetupList		PRESENCE optional		},
	...
}

PDUSessionResourceSetupUnsuccessfulTransfer ::= SEQUENCE {
	cause						Cause,
	criticalityDiagnostics		CriticalityDiagnostics																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSetupUnsuccessfulTransfer-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSetupUnsuccessfulTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSuspendListSUSReq ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSuspendItemSUSReq

PDUSessionResourceSuspendItemSUSReq ::= SEQUENCE {
	pDUSessionID						PDUSessionID,
	uEContextSuspendRequestTransfer		OCTET STRING (CONTAINING UEContextSuspendRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceSuspendItemSUSReq-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSuspendItemSUSReq-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceSwitchedList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceSwitchedItem

PDUSessionResourceSwitchedItem ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	pathSwitchRequestAcknowledgeTransfer		OCTET STRING (CONTAINING PathSwitchRequestAcknowledgeTransfer),
	iE-Extensions		ProtocolExtensionContainer { { PDUSessionResourceSwitchedItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceSwitchedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PduSessionExpectedUEActivityBehaviour			CRITICALITY ignore	EXTENSION ExpectedUEActivityBehaviour	PRESENCE optional	},
	...
}

PDUSessionResourceToBeSwitchedDLList ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToBeSwitchedDLItem

PDUSessionResourceToBeSwitchedDLItem ::= SEQUENCE {
	pDUSessionID					PDUSessionID,
	pathSwitchRequestTransfer		OCTET STRING (CONTAINING PathSwitchRequestTransfer),
	iE-Extensions		ProtocolExtensionContainer { { PDUSessionResourceToBeSwitchedDLItem-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToBeSwitchedDLItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceToReleaseListHOCmd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToReleaseItemHOCmd

PDUSessionResourceToReleaseItemHOCmd ::= SEQUENCE {
	pDUSessionID								PDUSessionID,
	handoverPreparationUnsuccessfulTransfer		OCTET STRING (CONTAINING HandoverPreparationUnsuccessfulTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceToReleaseItemHOCmd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToReleaseItemHOCmd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PDUSessionResourceToReleaseListRelCmd ::= SEQUENCE (SIZE(1..maxnoofPDUSessions)) OF PDUSessionResourceToReleaseItemRelCmd

PDUSessionResourceToReleaseItemRelCmd ::= SEQUENCE {
	pDUSessionID									PDUSessionID,
	pDUSessionResourceReleaseCommandTransfer		OCTET STRING (CONTAINING PDUSessionResourceReleaseCommandTransfer),
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionResourceToReleaseItemRelCmd-ExtIEs} }	OPTIONAL,
	...
}

PDUSessionResourceToReleaseItemRelCmd-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}
PDUSessionType ::= ENUMERATED {
	ipv4,
	ipv6,
	ipv4v6,
	ethernet,
	unstructured,
	...
}

PDUSessionUsageReport ::= SEQUENCE {
	rATType								ENUMERATED {nr, eutra, ..., nr-unlicensed, e-utra-unlicensed},
	pDUSessionTimedReportList			VolumeTimedReportList,
	iE-Extensions		ProtocolExtensionContainer { {PDUSessionUsageReport-ExtIEs} } OPTIONAL,
	...
}

PDUSessionUsageReport-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PEIPSassistanceInformation ::= SEQUENCE {
	cNsubgroupID			CNsubgroupID,
	iE-Extensions		ProtocolExtensionContainer { {PEIPSassistanceInformation-ExtIEs} } OPTIONAL,
	...
}

PEIPSassistanceInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

Periodicity ::= INTEGER (0..640000, ...)

PeriodicRegistrationUpdateTimer ::= BIT STRING (SIZE(8))

PLMNIdentity ::= OCTET STRING (SIZE(3))

PLMNAreaBasedQMC ::= SEQUENCE {
	plmnListforQMC		PLMNListforQMC,
	iE-Extensions		ProtocolExtensionContainer { {PLMNAreaBasedQMC-ExtIEs} } OPTIONAL,
	...
}

PLMNAreaBasedQMC-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PLMNListforQMC ::= SEQUENCE (SIZE(1..maxnoofPLMNforQMC)) OF PLMNIdentity

PLMNSupportList ::= SEQUENCE (SIZE(1..maxnoofPLMNs)) OF PLMNSupportItem

PLMNSupportItem ::= SEQUENCE {
	pLMNIdentity			PLMNIdentity,
	sliceSupportList		SliceSupportList,
	iE-Extensions		ProtocolExtensionContainer { {PLMNSupportItem-ExtIEs} } OPTIONAL,
	...
}

PLMNSupportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-NPN-Support						CRITICALITY reject	EXTENSION NPN-Support					PRESENCE optional	}|
	{ ID id-ExtendedSliceSupportList		CRITICALITY reject	EXTENSION ExtendedSliceSupportList 	PRESENCE optional	}|
	{ ID id-OnboardingSupport				CRITICALITY ignore	EXTENSION OnboardingSupport 			PRESENCE optional	},
	...
}

PNI-NPN-MobilityInformation ::= SEQUENCE {
	allowed-PNI-NPI-List		Allowed-PNI-NPN-List,
	iE-Extensions				ProtocolExtensionContainer { {PNI-NPN-MobilityInformation-ExtIEs} }	OPTIONAL,
	...
}

PNI-NPN-MobilityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

PortNumber ::= OCTET STRING (SIZE(2))

Pre-emptionCapability ::= ENUMERATED {
	shall-not-trigger-pre-emption,
	may-trigger-pre-emption,
	...
}

Pre-emptionVulnerability ::= ENUMERATED {
	not-pre-emptable,
	pre-emptable,
	...
}

PriorityLevelARP ::= INTEGER (1..15)

PriorityLevelQos ::= INTEGER (1..127, ...)

PWSFailedCellIDList ::= CHOICE {
	eUTRA-CGI-PWSFailedList		EUTRA-CGIList,
	nR-CGI-PWSFailedList		NR-CGIList,
	choice-Extensions		ProtocolIE-SingleContainer { {PWSFailedCellIDList-ExtIEs} }
}

PWSFailedCellIDList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

-- Q

QMCConfigInfo ::= SEQUENCE {
	uEAppLayerMeasInfoList				UEAppLayerMeasInfoList,
	iE-Extensions		ProtocolExtensionContainer { { QMCConfigInfo-ExtIEs} } OPTIONAL,
	...
}

QMCConfigInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QMCDeactivation ::= SEQUENCE {
	qoEReferenceList				QoEReferenceList,
	iE-Extensions		ProtocolExtensionContainer { { QMCDeactivation-ExtIEs} } OPTIONAL,
	...
}

QMCDeactivation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QoEReferenceList ::= SEQUENCE (SIZE(1..maxnoofUEAppLayerMeas)) OF QoEReference

QoEReference ::= OCTET STRING (SIZE(6))

QosCharacteristics ::= CHOICE {
	nonDynamic5QI		NonDynamic5QIDescriptor,
	dynamic5QI			Dynamic5QIDescriptor,
	choice-Extensions		ProtocolIE-SingleContainer { {QosCharacteristics-ExtIEs} }
}

QosCharacteristics-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

QosFlowAcceptedList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAcceptedItem

QosFlowAcceptedItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAcceptedItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowAcceptedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CurrentQoSParaSetIndex	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetIndex	PRESENCE optional	},
	...
}

QosFlowAddOrModifyRequestList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAddOrModifyRequestItem

QosFlowAddOrModifyRequestItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowLevelQosParameters		QosFlowLevelQosParameters									OPTIONAL,
	e-RAB-ID						E-RAB-ID													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAddOrModifyRequestItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowAddOrModifyRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-TSCTrafficCharacteristics	CRITICALITY ignore	EXTENSION TSCTrafficCharacteristics		PRESENCE optional }|
	{ID id-RedundantQosFlowIndicator	CRITICALITY ignore	EXTENSION RedundantQosFlowIndicator		PRESENCE optional },
	...
}

QosFlowAddOrModifyResponseList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowAddOrModifyResponseItem

QosFlowAddOrModifyResponseItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowAddOrModifyResponseItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowAddOrModifyResponseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CurrentQoSParaSetIndex	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetIndex	PRESENCE optional	},
	...
}

QosFlowFeedbackList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowFeedbackItem

QosFlowFeedbackItem ::= SEQUENCE {
	qosFlowIdentifier			QosFlowIdentifier,
	updateFeedback				UpdateFeedback								OPTIONAL,
	cNpacketDelayBudgetDL		ExtendedPacketDelayBudget					OPTIONAL,
	cNpacketDelayBudgetUL		ExtendedPacketDelayBudget					OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowFeedbackItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowFeedbackItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowIdentifier ::= INTEGER (0..63, ...)

QosFlowInformationList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowInformationItem

QosFlowInformationItem ::= SEQUENCE {
	qosFlowIdentifier	QosFlowIdentifier,
	dLForwarding		DLForwarding													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowInformationItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-ULForwarding				CRITICALITY ignore	EXTENSION ULForwarding			PRESENCE optional}|
	{ID id-SourceTNLAddrInfo		CRITICALITY ignore	EXTENSION TransportLayerAddress	PRESENCE optional}|
	{ID id-SourceNodeTNLAddrInfo	CRITICALITY ignore	EXTENSION TransportLayerAddress	PRESENCE optional},
	...
}

QosFlowLevelQosParameters ::= SEQUENCE {
	qosCharacteristics					QosCharacteristics,
	allocationAndRetentionPriority		AllocationAndRetentionPriority,
	gBR-QosInformation					GBR-QosInformation									OPTIONAL,
	reflectiveQosAttribute				ReflectiveQosAttribute								OPTIONAL,
	additionalQosFlowInformation		AdditionalQosFlowInformation						OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowLevelQosParameters-ExtIEs} }	OPTIONAL,
	...
}

QosFlowLevelQosParameters-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-QosMonitoringRequest	CRITICALITY ignore	EXTENSION QosMonitoringRequest	PRESENCE optional}|
	{ID id-QosMonitoringReportingFrequency	CRITICALITY ignore	EXTENSION QosMonitoringReportingFrequency	PRESENCE optional},
	...
}


QosMonitoringRequest ::= ENUMERATED {ul, dl, both, ..., stop}

QosMonitoringReportingFrequency ::= INTEGER (1..1800, ...)

QoSFlowList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowIdentifier

QosFlowListWithCause ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowWithCauseItem

QosFlowWithCauseItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	cause					Cause,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowWithCauseItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowWithCauseItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowModifyConfirmList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowModifyConfirmItem

QosFlowModifyConfirmItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowModifyConfirmItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowModifyConfirmItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowNotifyList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowNotifyItem

QosFlowNotifyItem ::= SEQUENCE {
	qosFlowIdentifier			QosFlowIdentifier,
	notificationCause			NotificationCause,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowNotifyItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowNotifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CurrentQoSParaSetIndex	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetNotifyIndex	PRESENCE optional	},
	...
}
QosFlowParametersList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowParametersItem

QosFlowParametersItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	alternativeQoSParaSetList		AlternativeQoSParaSetList							OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowParametersItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowParametersItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CNPacketDelayBudgetDL			CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional	}|
	{ ID id-CNPacketDelayBudgetUL			CRITICALITY ignore	EXTENSION ExtendedPacketDelayBudget		PRESENCE optional	}|
	{ ID id-BurstArrivalTimeDownlink		CRITICALITY ignore	EXTENSION BurstArrivalTime					PRESENCE optional	},
	...
}

QosFlowPerTNLInformation ::= SEQUENCE {
	uPTransportLayerInformation		UPTransportLayerInformation,
	associatedQosFlowList			AssociatedQosFlowList,
	iE-Extensions		ProtocolExtensionContainer { { QosFlowPerTNLInformation-ExtIEs} }	OPTIONAL,
	...
}

QosFlowPerTNLInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowPerTNLInformationList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF QosFlowPerTNLInformationItem

QosFlowPerTNLInformationItem ::= SEQUENCE {
	qosFlowPerTNLInformation				QosFlowPerTNLInformation,
	iE-Extensions		ProtocolExtensionContainer { { QosFlowPerTNLInformationItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowPerTNLInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QosFlowSetupRequestList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowSetupRequestItem

QosFlowSetupRequestItem ::= SEQUENCE {
	qosFlowIdentifier				QosFlowIdentifier,
	qosFlowLevelQosParameters		QosFlowLevelQosParameters,
	e-RAB-ID						E-RAB-ID											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowSetupRequestItem-ExtIEs} } OPTIONAL,
	...
}

QosFlowSetupRequestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-TSCTrafficCharacteristics	CRITICALITY ignore	EXTENSION TSCTrafficCharacteristics		PRESENCE optional }|
	{ID id-RedundantQosFlowIndicator	CRITICALITY ignore	EXTENSION RedundantQosFlowIndicator		PRESENCE optional },
	...
}

QosFlowListWithDataForwarding ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowItemWithDataForwarding

QosFlowItemWithDataForwarding ::= SEQUENCE {
	qosFlowIdentifier			QosFlowIdentifier,
	dataForwardingAccepted		DataForwardingAccepted											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowItemWithDataForwarding-ExtIEs} }	OPTIONAL,
	...
}

QosFlowItemWithDataForwarding-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CurrentQoSParaSetIndex	CRITICALITY ignore	EXTENSION AlternativeQoSParaSetIndex	PRESENCE optional	},
	...
}

QosFlowToBeForwardedList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QosFlowToBeForwardedItem

QosFlowToBeForwardedItem ::= SEQUENCE {
	qosFlowIdentifier		QosFlowIdentifier,
	iE-Extensions		ProtocolExtensionContainer { {QosFlowToBeForwardedItem-ExtIEs} }	OPTIONAL,
	...
}

QosFlowToBeForwardedItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

QoSFlowsUsageReportList ::= SEQUENCE (SIZE(1..maxnoofQosFlows)) OF QoSFlowsUsageReport-Item

QoSFlowsUsageReport-Item ::= SEQUENCE {
	qosFlowIdentifier					QosFlowIdentifier,
	rATType								ENUMERATED {nr, eutra, ..., nr-unlicensed, e-utra-unlicensed},
	qoSFlowsTimedReportList				VolumeTimedReportList,
	iE-Extensions		ProtocolExtensionContainer { {QoSFlowsUsageReport-Item-ExtIEs} } OPTIONAL,
	...
}

QoSFlowsUsageReport-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- R

Range ::= ENUMERATED {m50, m80, m180, m200, m350, m400, m500, m700, m1000, ...}

RANNodeName ::= PrintableString (SIZE(1..150, ...))

RANNodeNameVisibleString ::= VisibleString (SIZE(1..150, ...))

RANNodeNameUTF8String ::= UTF8String (SIZE(1..150, ...))

RANPagingPriority ::= INTEGER (1..256)

RANStatusTransfer-TransparentContainer ::= SEQUENCE {
	dRBsSubjectToStatusTransferList		DRBsSubjectToStatusTransferList,
	iE-Extensions		ProtocolExtensionContainer { {RANStatusTransfer-TransparentContainer-ExtIEs} }	OPTIONAL,
	...
}

RANStatusTransfer-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RAN-UE-NGAP-ID ::= INTEGER (0..4294967295)

RAT-Information ::= ENUMERATED {
	unlicensed,
	nb-IoT,
	...,
	nR-LEO,
	nR-MEO,
	nR-GEO,
	nR-OTHERSAT
}

RATRestrictions ::= SEQUENCE (SIZE(1..maxnoofEPLMNsPlusOne)) OF RATRestrictions-Item

RATRestrictions-Item ::= SEQUENCE {
	pLMNIdentity					PLMNIdentity,
	rATRestrictionInformation		RATRestrictionInformation,
	iE-Extensions		ProtocolExtensionContainer { {RATRestrictions-Item-ExtIEs} }		OPTIONAL,
	...
}

RATRestrictions-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-ExtendedRATRestrictionInformation		CRITICALITY ignore	EXTENSION ExtendedRATRestrictionInformation		PRESENCE optional	},
	...
}

RATRestrictionInformation ::= BIT STRING (SIZE(8, ...))

RecommendedCellsForPaging ::= SEQUENCE {
	recommendedCellList			RecommendedCellList,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedCellsForPaging-ExtIEs} }	OPTIONAL,
	...
}

RecommendedCellsForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedCellList ::= SEQUENCE (SIZE(1..maxnoofRecommendedCells)) OF RecommendedCellItem

RecommendedCellItem ::= SEQUENCE {
	nGRAN-CGI				NGRAN-CGI,
	timeStayedInCell		INTEGER (0..4095)		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedCellItem-ExtIEs} }	OPTIONAL,
	...
}

RecommendedCellItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedRANNodesForPaging ::= SEQUENCE {
	recommendedRANNodeList		RecommendedRANNodeList,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedRANNodesForPaging-ExtIEs} }	OPTIONAL,
	...
}

RecommendedRANNodesForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RecommendedRANNodeList::= SEQUENCE (SIZE(1..maxnoofRecommendedRANNodes)) OF RecommendedRANNodeItem

RecommendedRANNodeItem ::= SEQUENCE {
	aMFPagingTarget		AMFPagingTarget,
	iE-Extensions		ProtocolExtensionContainer { {RecommendedRANNodeItem-ExtIEs} }	OPTIONAL,
	...
}

RecommendedRANNodeItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

RedCapIndication ::= ENUMERATED {
	redcap,
	...
}

RedirectionVoiceFallback ::= ENUMERATED {
	possible,
	not-possible,
	...
}

RedundantPDUSessionInformation ::= SEQUENCE {
	rSN					RSN,
	iE-Extensions		ProtocolExtensionContainer { {RedundantPDUSessionInformation-ExtIEs} }	OPTIONAL,
	...
}

RedundantPDUSessionInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PDUSessionPairID	CRITICALITY ignore	EXTENSION PDUSessionPairID	PRESENCE optional	},
	...
}

RedundantQosFlowIndicator ::= ENUMERATED {true, false}

ReflectiveQosAttribute ::= ENUMERATED {
	subject-to,
	...
}

RelativeAMFCapacity ::= INTEGER (0..255)

ReportArea ::= ENUMERATED {
	cell,
	...
}

RepetitionPeriod ::= INTEGER (0..131071)

ResetAll ::= ENUMERATED {
	reset-all,
	...
}

ReportAmountMDT ::= ENUMERATED {
	r1, r2, r4, r8, r16, r32, r64, rinfinity
}

ReportIntervalMDT ::= ENUMERATED {
	ms120, ms240, ms480, ms640, ms1024, ms2048, ms5120, ms10240, min1, min6, min12, min30, min60
}

ExtendedReportIntervalMDT ::= ENUMERATED {
	ms20480, ms40960, ...
}

ResetType ::= CHOICE {
	nG-Interface			ResetAll,
	partOfNG-Interface		UE-associatedLogicalNG-connectionList,
	choice-Extensions		ProtocolIE-SingleContainer { {ResetType-ExtIEs} }
}

ResetType-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

RGLevelWirelineAccessCharacteristics ::= OCTET STRING

RNC-ID ::= INTEGER (0..4095)

RoutingID ::= OCTET STRING

RRCContainer ::= OCTET STRING

RRCEstablishmentCause ::= ENUMERATED {
	emergency,
	highPriorityAccess,
	mt-Access,
	mo-Signalling,
	mo-Data,
	mo-VoiceCall,
	mo-VideoCall,
	mo-SMS,
	mps-PriorityAccess,
	mcs-PriorityAccess,
	...,
	notAvailable,
	mo-ExceptionData
}

RRCInactiveTransitionReportRequest ::= ENUMERATED {
	subsequent-state-transition-report,
	single-rrc-connected-state-report,
	cancel-report,
	...
}

RRCState ::= ENUMERATED {
	inactive,
	connected,
	...
}

RSN ::= ENUMERATED {v1, v2, ...}

RIMInformationTransfer ::= SEQUENCE {
	targetRANNodeID-RIM			TargetRANNodeID-RIM,
	sourceRANNodeID				SourceRANNodeID,
	rIMInformation				RIMInformation,
	iE-Extensions				ProtocolExtensionContainer { {RIMInformationTransfer-ExtIEs} }	OPTIONAL,
	...
}

RIMInformationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


RIMInformation	::= SEQUENCE		{
	targetgNBSetID			GNBSetID,
	rIM-RSDetection			ENUMERATED	{rs-detected, rs-disappeared, ...},
	iE-Extensions			ProtocolExtensionContainer { {RIMInformation-ExtIEs} }	OPTIONAL,
	...
}

RIMInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

GNBSetID ::= BIT STRING (SIZE(22))

-- S

ScheduledCommunicationTime ::= SEQUENCE {
	dayofWeek			BIT STRING (SIZE(7))												OPTIONAL,
	timeofDayStart		INTEGER (0..86399, ...)												OPTIONAL,
	timeofDayEnd		INTEGER (0..86399, ...)												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { ScheduledCommunicationTime-ExtIEs}}	OPTIONAL,
	...
}

ScheduledCommunicationTime-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SCTP-TLAs	::= SEQUENCE (SIZE(1..maxnoofXnTLAs)) OF TransportLayerAddress

SD ::= OCTET STRING (SIZE(3))

SecondaryRATUsageInformation ::= SEQUENCE {
	pDUSessionUsageReport		PDUSessionUsageReport											OPTIONAL,
	qosFlowsUsageReportList		QoSFlowsUsageReportList											OPTIONAL,
	iE-Extension		ProtocolExtensionContainer { {SecondaryRATUsageInformation-ExtIEs} }	OPTIONAL,
	...
}

SecondaryRATUsageInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecondaryRATDataUsageReportTransfer ::= SEQUENCE {
	secondaryRATUsageInformation		SecondaryRATUsageInformation									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SecondaryRATDataUsageReportTransfer-ExtIEs} }	OPTIONAL,
	...
}

SecondaryRATDataUsageReportTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecurityContext ::= SEQUENCE {
	nextHopChainingCount		NextHopChainingCount,
	nextHopNH					SecurityKey,
	iE-Extensions		ProtocolExtensionContainer { {SecurityContext-ExtIEs} }	OPTIONAL,
	...
}

SecurityContext-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SecurityIndication ::= SEQUENCE {
	integrityProtectionIndication				IntegrityProtectionIndication,
	confidentialityProtectionIndication			ConfidentialityProtectionIndication,
	maximumIntegrityProtectedDataRate-UL			MaximumIntegrityProtectedDataRate		OPTIONAL,
-- The above IE shall be present if integrity protection is required or preferred
	iE-Extensions		ProtocolExtensionContainer { {SecurityIndication-ExtIEs} }		OPTIONAL,
	...
}

SecurityIndication-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-MaximumIntegrityProtectedDataRate-DL	CRITICALITY ignore	EXTENSION MaximumIntegrityProtectedDataRate	PRESENCE optional	},
	...
}

SecurityKey	::= BIT STRING (SIZE(256))

SecurityResult ::= SEQUENCE {
	integrityProtectionResult			IntegrityProtectionResult,
	confidentialityProtectionResult		ConfidentialityProtectionResult,
	iE-Extensions		ProtocolExtensionContainer { {SecurityResult-ExtIEs} }	OPTIONAL,
	...
}

SecurityResult-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SensorMeasurementConfiguration ::=	SEQUENCE {
	sensorMeasConfig            SensorMeasConfig,
	sensorMeasConfigNameList	SensorMeasConfigNameList            								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SensorMeasurementConfiguration-ExtIEs} } 	OPTIONAL,
	...
}

SensorMeasurementConfiguration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SensorMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofSensorName)) OF SensorMeasConfigNameItem

SensorMeasConfigNameItem ::= SEQUENCE {
	sensorNameConfig		SensorNameConfig,
	iE-Extensions		ProtocolExtensionContainer { { SensorMeasConfigNameItem-ExtIEs } } 	OPTIONAL,
	...
}

SensorMeasConfigNameItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SensorMeasConfig::= ENUMERATED {setup,...}

SensorNameConfig ::= CHOICE {
	uncompensatedBarometricConfig		ENUMERATED {true, ...},
	ueSpeedConfig						ENUMERATED {true, ...},
	ueOrientationConfig					ENUMERATED {true, ...},
	choice-Extensions		ProtocolIE-SingleContainer { {SensorNameConfig-ExtIEs} }
}

SensorNameConfig-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

SerialNumber ::= BIT STRING (SIZE(16))

ServedGUAMIList ::= SEQUENCE (SIZE(1..maxnoofServedGUAMIs)) OF ServedGUAMIItem

ServedGUAMIItem ::= SEQUENCE {
	gUAMI				GUAMI,
	backupAMFName		AMFName													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ServedGUAMIItem-ExtIEs} }	OPTIONAL,
	...
}

ServedGUAMIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-GUAMIType		CRITICALITY ignore	EXTENSION GUAMIType		PRESENCE optional	},
	...
}

ServiceAreaInformation ::= SEQUENCE (SIZE(1.. maxnoofEPLMNsPlusOne)) OF ServiceAreaInformation-Item

ServiceAreaInformation-Item ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	allowedTACs			AllowedTACs																OPTIONAL,
	notAllowedTACs		NotAllowedTACs															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {ServiceAreaInformation-Item-ExtIEs} }		OPTIONAL,
	...
}

ServiceAreaInformation-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ServiceType ::=  ENUMERATED {streaming, mTSI, vR, ...}

SgNB-UE-X2AP-ID ::= INTEGER (0..4294967295)

SharedNGU-MulticastTNLInformation ::= SEQUENCE {
	iP-MulticastAddress 		TransportLayerAddress,
	iP-SourceAddress			TransportLayerAddress,
	gTP-TEID						GTP-TEID,
	iE-Extensions				ProtocolExtensionContainer { {SharedNGU-MulticastTNLInformation-ExtIEs} } 	OPTIONAL,
	...
}

SharedNGU-MulticastTNLInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SliceOverloadList ::= SEQUENCE (SIZE(1..maxnoofSliceItems)) OF SliceOverloadItem

SliceOverloadItem ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {SliceOverloadItem-ExtIEs} }	OPTIONAL,
	...
}

SliceOverloadItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SliceSupportList ::= SEQUENCE (SIZE(1..maxnoofSliceItems)) OF SliceSupportItem

SliceSupportItem ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {SliceSupportItem-ExtIEs} }	OPTIONAL,
	...
}

SliceSupportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SliceSupportListQMC ::= SEQUENCE (SIZE(1..maxnoofSNSSAIforQMC)) OF SliceSupportQMC-Item

SliceSupportQMC-Item ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {SliceSupportQMC-Item-ExtIEs} }		OPTIONAL,
	...
}

SliceSupportQMC-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SNPN-MobilityInformation ::= SEQUENCE {
	serving-NID			NID,
	iE-Extensions		ProtocolExtensionContainer { {SNPN-MobilityInformation-ExtIEs} }	OPTIONAL,
	...
}

SNPN-MobilityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

S-NSSAI ::= SEQUENCE {
	sST					SST,
	sD					SD													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { S-NSSAI-ExtIEs} }	OPTIONAL,
	...
}

S-NSSAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONConfigurationTransfer ::= SEQUENCE {
	targetRANNodeID-SON			TargetRANNodeID-SON,
	sourceRANNodeID				SourceRANNodeID,
	sONInformation				SONInformation,
	xnTNLConfigurationInfo		XnTNLConfigurationInfo										OPTIONAL,
-- The above IE shall be present if the SON Information IE contains the SON Information Request IE set to “Xn TNL Configuration Info”
	iE-Extensions		ProtocolExtensionContainer { {SONConfigurationTransfer-ExtIEs} }	OPTIONAL,
	...
}

SONConfigurationTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONInformation ::= CHOICE {
	sONInformationRequest		SONInformationRequest,
	sONInformationReply			SONInformationReply,
	choice-Extensions		ProtocolIE-SingleContainer { {SONInformation-ExtIEs} }
}

SONInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SONInformationReport		CRITICALITY ignore	TYPE SONInformationReport		PRESENCE mandatory	},
	...
}

SONInformationReply ::= SEQUENCE {
	xnTNLConfigurationInfo		XnTNLConfigurationInfo									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SONInformationReply-ExtIEs} }		OPTIONAL,
	...
}

SONInformationReply-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONInformationReport::= CHOICE {
	failureIndicationInformation	FailureIndication,
	hOReportInformation				HOReport,
	choice-Extensions		ProtocolIE-SingleContainer { { SONInformationReport-ExtIEs} }
}

SONInformationReport-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SuccessfulHandoverReportList			    CRITICALITY ignore	TYPE SuccessfulHandoverReportList			PRESENCE mandatory },
	...
}

-- --------------------------------------------------------------------
-- SON Information Report
-- --------------------------------------------------------------------

SuccessfulHandoverReportList ::= SEQUENCE (SIZE(1..maxnoofSuccessfulHOReports)) OF SuccessfulHandoverReport-Item

SuccessfulHandoverReport-Item ::= SEQUENCE {
	successfulHOReportContainer			OCTET STRING,
	iE-Extensions		ProtocolExtensionContainer { { SuccessfulHandoverReport-Item-ExtIEs} } OPTIONAL,
	...
}

SuccessfulHandoverReport-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SONInformationRequest ::= ENUMERATED {
	xn-TNL-configuration-info,
	...
}

SourceNGRANNode-ToTargetNGRANNode-TransparentContainer ::= SEQUENCE {
	rRCContainer							RRCContainer,
	pDUSessionResourceInformationList		PDUSessionResourceInformationList													OPTIONAL,
	e-RABInformationList					E-RABInformationList																OPTIONAL,
	targetCell-ID							NGRAN-CGI,
	indexToRFSP								IndexToRFSP																			OPTIONAL,
	uEHistoryInformation					UEHistoryInformation,
	iE-Extensions		ProtocolExtensionContainer { {SourceNGRANNode-ToTargetNGRANNode-TransparentContainer-ExtIEs} }	OPTIONAL,
	...
}

SourceNGRANNode-ToTargetNGRANNode-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SgNB-UE-X2AP-ID								CRITICALITY ignore	EXTENSION SgNB-UE-X2AP-ID 							PRESENCE optional		}|
	{ ID id-UEHistoryInformationFromTheUE				CRITICALITY ignore	EXTENSION UEHistoryInformationFromTheUE			PRESENCE optional		}|
	{ ID id-SourceNodeID								CRITICALITY ignore	EXTENSION SourceNodeID								PRESENCE optional		}|
	{ ID id-UEContextReferenceAtSource 					CRITICALITY ignore	EXTENSION RAN-UE-NGAP-ID								PRESENCE optional		}|
	{ ID id-MBS-ActiveSessionInformation-SourcetoTargetList	CRITICALITY ignore	EXTENSION MBS-ActiveSessionInformation-SourcetoTargetList		PRESENCE optional		}|
	{ ID id-QMCConfigInfo								CRITICALITY ignore	EXTENSION QMCConfigInfo								PRESENCE optional		}|
	{ ID id-NGAPIESupportInformationRequestList			CRITICALITY ignore	EXTENSION NGAPIESupportInformationRequestList	PRESENCE optional		},
	...
}

SourceNodeID ::= CHOICE {
	sourceengNB-ID			GlobalGNB-ID,
	choice-Extensions		ProtocolIE-SingleContainer { { SourceNodeID-ExtIEs} }
}

SourceNodeID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

SourceOfUEActivityBehaviourInformation ::= ENUMERATED {
	subscription-information,
	statistics,
	...
}

SourceRANNodeID ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {SourceRANNodeID-ExtIEs} } OPTIONAL,
	...
}

SourceRANNodeID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

SourceToTarget-TransparentContainer ::= OCTET STRING
-- This IE includes a transparent container from the source RAN node to the target RAN node.
-- The octets of the OCTET STRING are encoded according to the specifications of the target system.

SourceToTarget-AMFInformationReroute ::= SEQUENCE {
	configuredNSSAI					ConfiguredNSSAI														OPTIONAL,
	rejectedNSSAIinPLMN				RejectedNSSAIinPLMN													OPTIONAL,
	rejectedNSSAIinTA				RejectedNSSAIinTA													OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {SourceToTarget-AMFInformationReroute-ExtIEs} }	OPTIONAL,
	...
}

SourceToTarget-AMFInformationReroute-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- This IE includes information from the source Core node to the target Core node for reroute information provide by NSSF.
-- The octets of the OCTET STRING are encoded according to the specifications of the Core network.

SRVCCOperationPossible ::= ENUMERATED {
	possible,
	notPossible,
	...
}

ConfiguredNSSAI  ::=  OCTET STRING (SIZE(128))

RejectedNSSAIinPLMN ::= OCTET STRING (SIZE(32))

RejectedNSSAIinTA ::= OCTET STRING (SIZE(32))

SST ::= OCTET STRING (SIZE(1))

SupportedTAList ::= SEQUENCE (SIZE(1..maxnoofTACs)) OF SupportedTAItem

SupportedTAItem ::= SEQUENCE {
	tAC						TAC,
	broadcastPLMNList		BroadcastPLMNList,
	iE-Extensions		ProtocolExtensionContainer { {SupportedTAItem-ExtIEs} } OPTIONAL,
	...
}

SupportedTAItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-ConfiguredTACIndication		CRITICALITY ignore	EXTENSION ConfiguredTACIndication	PRESENCE optional	}|
	{ID id-RAT-Information				CRITICALITY reject	EXTENSION RAT-Information			PRESENCE optional	},
	...
}

SuspendIndicator ::= ENUMERATED {
	true,
	...
}

Suspend-Request-Indication ::= ENUMERATED {
	suspend-requested,
	...
}

Suspend-Response-Indication ::= ENUMERATED {
	suspend-indicated,
	...
}

SurvivalTime ::= INTEGER (0..1920000, ...)


-- T

TAC ::= OCTET STRING (SIZE(3))

TACListInNRNTN ::= SEQUENCE (SIZE(1..maxnoofTACsinNTN)) OF TAC

TAI ::= SEQUENCE {
	pLMNIdentity		PLMNIdentity,
	tAC					TAC,
	iE-Extensions		ProtocolExtensionContainer { {TAI-ExtIEs} } OPTIONAL,
	...
}

TAI-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIBroadcastEUTRA ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAIBroadcastEUTRA-Item

TAIBroadcastEUTRA-Item ::= SEQUENCE {
	tAI								TAI,
	completedCellsInTAI-EUTRA		CompletedCellsInTAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {TAIBroadcastEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

TAIBroadcastEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIBroadcastNR ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAIBroadcastNR-Item

TAIBroadcastNR-Item ::= SEQUENCE {
	tAI							TAI,
	completedCellsInTAI-NR		CompletedCellsInTAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {TAIBroadcastNR-Item-ExtIEs} } OPTIONAL,
	...
}

TAIBroadcastNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAICancelledEUTRA ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAICancelledEUTRA-Item

TAICancelledEUTRA-Item ::= SEQUENCE {
	tAI								TAI,
	cancelledCellsInTAI-EUTRA		CancelledCellsInTAI-EUTRA,
	iE-Extensions		ProtocolExtensionContainer { {TAICancelledEUTRA-Item-ExtIEs} } OPTIONAL,
	...
}

TAICancelledEUTRA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAICancelledNR ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAICancelledNR-Item

TAICancelledNR-Item ::= SEQUENCE {
	tAI							TAI,
	cancelledCellsInTAI-NR		CancelledCellsInTAI-NR,
	iE-Extensions		ProtocolExtensionContainer { {TAICancelledNR-Item-ExtIEs} } OPTIONAL,
	...
}

TAICancelledNR-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForInactive ::= SEQUENCE (SIZE(1..maxnoofTAIforInactive)) OF TAIListForInactiveItem

TAIListForInactiveItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {TAIListForInactiveItem-ExtIEs} } OPTIONAL,
	...
}

TAIListForInactiveItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForPaging ::= SEQUENCE (SIZE(1..maxnoofTAIforPaging)) OF TAIListForPagingItem

TAIListForPagingItem ::= SEQUENCE {
	tAI					TAI,
	iE-Extensions		ProtocolExtensionContainer { {TAIListForPagingItem-ExtIEs} } OPTIONAL,
	...
}

TAIListForPagingItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListForRestart ::= SEQUENCE (SIZE(1..maxnoofTAIforRestart)) OF TAI

TAIListForWarning ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAI

TAINSAGSupportList ::= SEQUENCE (SIZE(1..maxnoofNSAGs)) OF TAINSAGSupportItem

TAINSAGSupportItem ::= SEQUENCE {
	nSAG-ID						NSAG-ID,
	nSAGSliceSupportList		ExtendedSliceSupportList,
	iE-Extensions		ProtocolExtensionContainer { {TAINSAGSupportItem-ExtIEs} } OPTIONAL,
	...
}

TAINSAGSupportItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargeteNB-ID ::= SEQUENCE {
	globalENB-ID		GlobalNgENB-ID,
	selected-EPS-TAI	EPS-TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargeteNB-ID-ExtIEs} } OPTIONAL,
	...
}

TargeteNB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetHomeENB-ID ::= SEQUENCE {
	pLMNidentity		PLMNIdentity,
	homeENB-ID			BIT STRING (SIZE(28)),
	selected-EPS-TAI	EPS-TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetHomeENB-ID-ExtIEs} } OPTIONAL,
	...
}

TargetHomeENB-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetID ::= CHOICE {
	targetRANNodeID			TargetRANNodeID,
	targeteNB-ID			TargeteNB-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {TargetID-ExtIEs} }
}

TargetID-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ID id-TargetRNC-ID			CRITICALITY reject	TYPE TargetRNC-ID 		PRESENCE mandatory }|
	{ID id-TargetHomeENB-ID		CRITICALITY reject	TYPE TargetHomeENB-ID	PRESENCE mandatory },
	...
}

TargetNGRANNode-ToSourceNGRANNode-TransparentContainer ::= SEQUENCE {
	rRCContainer		RRCContainer,
	iE-Extensions		ProtocolExtensionContainer { {TargetNGRANNode-ToSourceNGRANNode-TransparentContainer-ExtIEs} } OPTIONAL,
	...
}

TargetNGRANNode-ToSourceNGRANNode-TransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-DAPSResponseInfoList						CRITICALITY ignore	EXTENSION DAPSResponseInfoList									PRESENCE optional }|
	{ ID id-DirectForwardingPathAvailability			CRITICALITY ignore	EXTENSION DirectForwardingPathAvailability					PRESENCE optional }|
	{ ID id-MBS-ActiveSessionInformation-TargettoSourceList	CRITICALITY ignore	EXTENSION MBS-ActiveSessionInformation-TargettoSourceList		PRESENCE optional }|
	{ ID id-NGAPIESupportInformationResponseList		CRITICALITY ignore	EXTENSION NGAPIESupportInformationResponseList 			PRESENCE optional },
	...
}

TargetNGRANNode-ToSourceNGRANNode-FailureTransparentContainer ::= SEQUENCE {
	cell-CAGInformation		Cell-CAGInformation			OPTIONAL,
	iE-Extensions			ProtocolExtensionContainer { {TargetNGRANNode-ToSourceNGRANNode-FailureTransparentContainer-ExtIEs} } OPTIONAL,
	...
}

TargetNGRANNode-ToSourceNGRANNode-FailureTransparentContainer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-NGAPIESupportInformationResponseList	CRITICALITY ignore	EXTENSION NGAPIESupportInformationResponseList 		PRESENCE optional },
	...
}

TargetNSSAI ::= SEQUENCE (SIZE(1..maxnoofTargetS-NSSAIs)) OF TargetNSSAI-Item

TargetNSSAI-Item ::= SEQUENCE {
	s-NSSAI				S-NSSAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetNSSAI-Item-ExtIEs} } OPTIONAL,
	...
}

TargetNSSAI-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetNSSAIInformation ::= SEQUENCE {
	targetNSSAI			TargetNSSAI,
	indexToRFSP				IndexToRFSP,
	iE-Extensions		ProtocolExtensionContainer { {TargetNSSAIInformation-Item-ExtIEs} } OPTIONAL,
	...
}

TargetNSSAIInformation-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetRANNodeID ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetRANNodeID-ExtIEs} } OPTIONAL,
	...
}

TargetRANNodeID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetRANNodeID-RIM ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetRANNodeID-RIM-ExtIEs} } OPTIONAL,
	...
}

TargetRANNodeID-RIM-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetRANNodeID-SON ::= SEQUENCE {
	globalRANNodeID		GlobalRANNodeID,
	selectedTAI			TAI,
	iE-Extensions		ProtocolExtensionContainer { {TargetRANNodeID-SON-ExtIEs} } OPTIONAL,
	...
}

TargetRANNodeID-SON-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ID id-NR-CGI	CRITICALITY ignore	EXTENSION NR-CGI PRESENCE optional },
	...
}

TargetRNC-ID ::= SEQUENCE {
	lAI					LAI,
	rNC-ID				RNC-ID,
	extendedRNC-ID		ExtendedRNC-ID											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {TargetRNC-ID-ExtIEs} } 	OPTIONAL,
	...
}

TargetRNC-ID-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TargetToSource-TransparentContainer ::= OCTET STRING
-- This IE includes a transparent container from the target RAN node to the source RAN node.
-- The octets of the OCTET STRING are encoded according to the specifications of the target system.

TargettoSource-Failure-TransparentContainer ::= OCTET STRING
-- This IE includes a transparent container from the target RAN node to the source RAN node.
-- The octets of the OCTET STRING are encoded according to the specifications of the target system (if applicable).

TimerApproachForGUAMIRemoval ::= ENUMERATED {
	apply-timer,
	...
}

TimeStamp ::= OCTET STRING (SIZE(4))

TimeSyncAssistanceInfo ::= SEQUENCE {
	timeDistributionIndication		ENUMERATED {enabled, disabled, ...},
	uUTimeSyncErrorBudget			INTEGER (1..1000000, ...)							OPTIONAL,
	-- The above IE shall be present if the Time Distribution Indication IE is set to the value “enabled”
	iE-Extensions		ProtocolExtensionContainer { {TimeSyncAssistanceInfo-ExtIEs} }	OPTIONAL,
	...
}

TimeSyncAssistanceInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TimeToWait ::= ENUMERATED {v1s, v2s, v5s, v10s, v20s, v60s, ...}

TimeUEStayedInCell ::= INTEGER (0..4095)

TimeUEStayedInCellEnhancedGranularity ::= INTEGER (0..40950)

TMGI ::=  OCTET STRING (SIZE(6))

TNAP-ID ::= OCTET STRING

TNGF-ID ::= CHOICE {
	tNGF-ID				 	BIT STRING (SIZE(32, ...)),
	choice-Extensions		ProtocolIE-SingleContainer { {TNGF-ID-ExtIEs} }
}

TNGF-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

TNLAddressWeightFactor ::= INTEGER (0..255)

TNLAssociationList ::= SEQUENCE (SIZE(1..maxnoofTNLAssociations)) OF TNLAssociationItem

TNLAssociationItem ::= SEQUENCE {
	tNLAssociationAddress		CPTransportLayerInformation,
	cause						Cause,
	iE-Extensions		ProtocolExtensionContainer { {TNLAssociationItem-ExtIEs} } OPTIONAL,
	...
}

TNLAssociationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TNLAssociationUsage ::= ENUMERATED {
	ue,
	non-ue,
	both,
	...
}

TooearlyIntersystemHO::= SEQUENCE {
	sourcecellID			EUTRA-CGI,
	failurecellID			NGRAN-CGI,
	uERLFReportContainer	UERLFReportContainer		OPTIONAL,
	iE-Extensions			ProtocolExtensionContainer { { TooearlyIntersystemHO-ExtIEs} }			OPTIONAL,
	...
}

TooearlyIntersystemHO-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TraceActivation ::= SEQUENCE {
	nGRANTraceID						NGRANTraceID,
	interfacesToTrace					InterfacesToTrace,
traceDepth							TraceDepth,
traceCollectionEntityIPAddress		TransportLayerAddress,
	iE-Extensions		ProtocolExtensionContainer { {TraceActivation-ExtIEs} }	OPTIONAL,
	...
}

TraceActivation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-MDTConfiguration			CRITICALITY ignore	EXTENSION MDT-Configuration		PRESENCE optional 	}|
	{ ID id-TraceCollectionEntityURI	CRITICALITY ignore	EXTENSION URI-address			PRESENCE optional		},
	...
}

TraceDepth ::= ENUMERATED {
	minimum,
	medium,
	maximum,
	minimumWithoutVendorSpecificExtension,
	mediumWithoutVendorSpecificExtension,
	maximumWithoutVendorSpecificExtension,
	...
}

TrafficLoadReductionIndication ::= INTEGER (1..99)

TransportLayerAddress ::= BIT STRING (SIZE(1..160, ...))

TypeOfError ::= ENUMERATED {
	not-understood,
	missing,
	...
}

TAIBasedMDT ::= SEQUENCE {
	tAIListforMDT			TAIListforMDT,
	iE-Extensions			ProtocolExtensionContainer { {TAIBasedMDT-ExtIEs} } OPTIONAL,
	...
}

TAIBasedMDT-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListforMDT ::= SEQUENCE (SIZE(1..maxnoofTAforMDT)) OF TAI

TAIBasedQMC ::= SEQUENCE {
	tAIListforQMC			TAIListforQMC,
	iE-Extensions			ProtocolExtensionContainer { {TAIBasedQMC-ExtIEs} } OPTIONAL,
	...
}

TAIBasedQMC-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAIListforQMC ::= SEQUENCE (SIZE(1..maxnoofTAforQMC)) OF TAI

TABasedQMC ::= SEQUENCE {
	tAListforQMC			TAListforQMC,
	iE-Extensions		ProtocolExtensionContainer { {TABasedQMC-ExtIEs} } OPTIONAL,
	...
}

TABasedQMC-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAListforQMC ::= SEQUENCE (SIZE(1..maxnoofTAforQMC)) OF TAC


TABasedMDT ::= SEQUENCE {
	tAListforMDT		TAListforMDT,
	iE-Extensions		ProtocolExtensionContainer { {TABasedMDT-ExtIEs} } OPTIONAL,
	...
}

TABasedMDT-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

TAListforMDT ::= SEQUENCE (SIZE(1..maxnoofTAforMDT)) OF TAC

Threshold-RSRP ::= INTEGER(0..127)

Threshold-RSRQ ::= INTEGER(0..127)

Threshold-SINR ::= INTEGER(0..127)

TimeToTrigger ::= ENUMERATED {ms0, ms40, ms64, ms80, ms100, ms128, ms160, ms256, ms320, ms480, ms512, ms640, ms1024, ms1280, ms2560, ms5120}


TWAP-ID ::= OCTET STRING

TWIF-ID ::= CHOICE {
	tWIF-ID				 	BIT STRING (SIZE(32, ...)),
	choice-Extensions		ProtocolIE-SingleContainer { {TWIF-ID-ExtIEs} }
}

TWIF-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

TSCAssistanceInformation ::= SEQUENCE {
	periodicity				Periodicity,
	burstArrivalTime		BurstArrivalTime												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {TSCAssistanceInformation-ExtIEs} }	OPTIONAL,
	...
}

TSCAssistanceInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SurvivalTime		CRITICALITY ignore	EXTENSION SurvivalTime			PRESENCE optional},
	...
}

TSCTrafficCharacteristics ::= SEQUENCE {
	tSCAssistanceInformationDL		TSCAssistanceInformation								OPTIONAL,
	tSCAssistanceInformationUL		TSCAssistanceInformation								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {TSCTrafficCharacteristics-ExtIEs} }	OPTIONAL,
	...
}

TSCTrafficCharacteristics-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- U

UEAggregateMaximumBitRate ::= SEQUENCE {
	uEAggregateMaximumBitRateDL		BitRate,
	uEAggregateMaximumBitRateUL		BitRate,
	iE-Extensions		ProtocolExtensionContainer { {UEAggregateMaximumBitRate-ExtIEs} } OPTIONAL,
	...
}

UEAggregateMaximumBitRate-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEAppLayerMeasInfoList ::= SEQUENCE (SIZE(1..maxnoofUEAppLayerMeas)) OF UEAppLayerMeasInfoItem

UEAppLayerMeasInfoItem ::= SEQUENCE {
	uEAppLayerMeasConfigInfo		UEAppLayerMeasConfigInfo,
	iE-Extensions		ProtocolExtensionContainer { { UEAppLayerMeasInfoItem-ExtIEs} } OPTIONAL,
	...
}

UEAppLayerMeasInfoItem-ExtIEs NGAP-PROTOCOL-EXTENSION::= {
	...
}

UEAppLayerMeasConfigInfo ::= SEQUENCE {
	qoEReference								QoEReference,
	serviceType								ServiceType,
	areaScopeOfQMC							AreaScopeOfQMC									OPTIONAL,
	measCollEntityIPAddress					TransportLayerAddress,
	qoEMeasurementStatus						ENUMERATED {ongoing,...}					OPTIONAL,
	containerForAppLayerMeasConfig			OCTET STRING (SIZE(1..8000))				OPTIONAL,
	measConfigAppLayerID						INTEGER (0..15, ...) 					OPTIONAL,
	sliceSupportListQMC						SliceSupportListQMC 						OPTIONAL,
	mDT-AlignmentInfo						MDT-AlignmentInfo						OPTIONAL,
	availableRANVisibleQoEMetrics			AvailableRANVisibleQoEMetrics			OPTIONAL,
	iE-Extensions	ProtocolExtensionContainer { { UEAppLayerMeasConfigInfo-ExtIEs} }		OPTIONAL,
	...
}

UEAppLayerMeasConfigInfo-ExtIEs NGAP-PROTOCOL-EXTENSION::= {
	...
}

UE-associatedLogicalNG-connectionList ::= SEQUENCE (SIZE(1..maxnoofNGConnectionsToReset)) OF UE-associatedLogicalNG-connectionItem

UE-associatedLogicalNG-connectionItem ::= SEQUENCE {
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID																		OPTIONAL,
	rAN-UE-NGAP-ID		RAN-UE-NGAP-ID																		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UE-associatedLogicalNG-connectionItem-ExtIEs} }	OPTIONAL,
	...
}

UE-associatedLogicalNG-connectionItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UECapabilityInfoRequest ::= ENUMERATED {
	requested,
	...
}

UEContextRequest ::= ENUMERATED {requested, ...}


UEContextResumeRequestTransfer ::= SEQUENCE {
	qosFlowFailedToResumeList				QosFlowListWithCause									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UEContextResumeRequestTransfer-ExtIEs} }		OPTIONAL,
	...
}

UEContextResumeRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEContextResumeResponseTransfer ::= SEQUENCE {
	qosFlowFailedToResumeList				QosFlowListWithCause									OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UEContextResumeResponseTransfer-ExtIEs} }		OPTIONAL,
	...
}

UEContextResumeResponseTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEContextSuspendRequestTransfer ::= SEQUENCE {
	suspendIndicator				SuspendIndicator												OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UEContextSuspendRequestTransfer-ExtIEs} }		OPTIONAL,
	...
}

UEContextSuspendRequestTransfer-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UE-DifferentiationInfo ::= SEQUENCE {
	periodicCommunicationIndicator	ENUMERATED {periodically, ondemand, ... }			OPTIONAL,
	periodicTime					INTEGER (1..3600, ...)								OPTIONAL,
	scheduledCommunicationTime		ScheduledCommunicationTime 							OPTIONAL,
	stationaryIndication			ENUMERATED {stationary, mobile, ...}				OPTIONAL,
	trafficProfile					ENUMERATED {single-packet, dual-packets, multiple-packets, ...}	OPTIONAL,
	batteryIndication				ENUMERATED {battery-powered, battery-powered-not-rechargeable-or-replaceable, not-battery-powered, ...}		OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { UE-DifferentiationInfo-ExtIEs} } OPTIONAL,
	...
}

UE-DifferentiationInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEHistoryInformation ::= SEQUENCE (SIZE(1..maxnoofCellsinUEHistoryInfo)) OF LastVisitedCellItem

UEHistoryInformationFromTheUE ::= CHOICE {
	nR						NRMobilityHistoryReport,
	choice-Extensions		ProtocolIE-SingleContainer { {UEHistoryInformationFromTheUE-ExtIEs} }
}

UEHistoryInformationFromTheUE-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UEIdentityIndexValue ::= CHOICE {
	indexLength10			BIT STRING (SIZE(10)),
	choice-Extensions		ProtocolIE-SingleContainer { {UEIdentityIndexValue-ExtIEs} }
}

UEIdentityIndexValue-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UE-NGAP-IDs ::= CHOICE {
	uE-NGAP-ID-pair		UE-NGAP-ID-pair,
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID,
	choice-Extensions		ProtocolIE-SingleContainer { {UE-NGAP-IDs-ExtIEs} }
}

UE-NGAP-IDs-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UE-NGAP-ID-pair ::= SEQUENCE{
	aMF-UE-NGAP-ID		AMF-UE-NGAP-ID,
	rAN-UE-NGAP-ID		RAN-UE-NGAP-ID,
	iE-Extensions		ProtocolExtensionContainer { {UE-NGAP-ID-pair-ExtIEs} } OPTIONAL,
	...
}

UE-NGAP-ID-pair-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UEPagingIdentity ::= CHOICE {
	fiveG-S-TMSI		FiveG-S-TMSI,
	choice-Extensions		ProtocolIE-SingleContainer { {UEPagingIdentity-ExtIEs} }
	}

UEPagingIdentity-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UEPresence ::= ENUMERATED {in, out, unknown, ...}

UEPresenceInAreaOfInterestList ::= SEQUENCE (SIZE(1..maxnoofAoI)) OF UEPresenceInAreaOfInterestItem

UEPresenceInAreaOfInterestItem ::= SEQUENCE {
	locationReportingReferenceID		LocationReportingReferenceID,
	uEPresence							UEPresence,
	iE-Extensions		ProtocolExtensionContainer { {UEPresenceInAreaOfInterestItem-ExtIEs} }	OPTIONAL,
	...
}

UEPresenceInAreaOfInterestItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UERadioCapability ::= OCTET STRING

UERadioCapabilityForPaging ::= SEQUENCE {
	uERadioCapabilityForPagingOfNR		UERadioCapabilityForPagingOfNR					OPTIONAL,
	uERadioCapabilityForPagingOfEUTRA		UERadioCapabilityForPagingOfEUTRA				OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UERadioCapabilityForPaging-ExtIEs} }	OPTIONAL,
	...
}

UERadioCapabilityForPaging-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-UERadioCapabilityForPagingOfNB-IoT		CRITICALITY ignore	EXTENSION UERadioCapabilityForPagingOfNB-IoT		PRESENCE optional	},
	...
}

UERadioCapabilityForPagingOfNB-IoT ::= OCTET STRING

UERadioCapabilityForPagingOfNR ::= OCTET STRING

UERadioCapabilityForPagingOfEUTRA ::= OCTET STRING

UERadioCapabilityID ::= OCTET STRING

UERetentionInformation ::= ENUMERATED {
	ues-retained,
	...
}

UERLFReportContainer ::= CHOICE {
	nR			NRUERLFReportContainer,
	lTE			LTEUERLFReportContainer,
	choice-Extensions		ProtocolIE-SingleContainer { {UERLFReportContainer-ExtIEs} }
}

UERLFReportContainer-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UESecurityCapabilities ::= SEQUENCE {
	nRencryptionAlgorithms					NRencryptionAlgorithms,
	nRintegrityProtectionAlgorithms			NRintegrityProtectionAlgorithms,
	eUTRAencryptionAlgorithms				EUTRAencryptionAlgorithms,
	eUTRAintegrityProtectionAlgorithms		EUTRAintegrityProtectionAlgorithms,
	iE-Extensions		ProtocolExtensionContainer { {UESecurityCapabilities-ExtIEs} }	OPTIONAL,
	...
}

UESecurityCapabilities-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UESliceMaximumBitRateList ::= SEQUENCE (SIZE(1..maxnoofAllowedS-NSSAIs)) OF UESliceMaximumBitRateItem

UESliceMaximumBitRateItem ::= SEQUENCE {
	s-NSSAI						S-NSSAI,
	uESliceMaximumBitRateDL		BitRate,
	uESliceMaximumBitRateUL		BitRate,
	iE-Extensions		ProtocolExtensionContainer { { UESliceMaximumBitRateItem-ExtIEs} } OPTIONAL,
	...
}

UESliceMaximumBitRateItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}


UE-UP-CIoT-Support ::= ENUMERATED {supported, ...}

UL-CP-SecurityInformation ::= SEQUENCE {
	ul-NAS-MAC				UL-NAS-MAC,
	ul-NAS-Count			UL-NAS-Count,
	iE-Extensions			ProtocolExtensionContainer { { UL-CP-SecurityInformation-ExtIEs} }	OPTIONAL,
	...
}

UL-CP-SecurityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

UL-NAS-MAC ::= BIT STRING (SIZE (16))

UL-NAS-Count ::= BIT STRING (SIZE (5))

UL-NGU-UP-TNLModifyList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivity)) OF UL-NGU-UP-TNLModifyItem

UL-NGU-UP-TNLModifyItem ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	dL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UL-NGU-UP-TNLModifyItem-ExtIEs} } OPTIONAL,
	...
}

UL-NGU-UP-TNLModifyItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-RedundantUL-NGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformation		PRESENCE optional	 	}|
	{ ID id-RedundantDL-NGU-UP-TNLInformation	CRITICALITY ignore	EXTENSION UPTransportLayerInformation		PRESENCE optional	 	},
	...
}

UnavailableGUAMIList ::= SEQUENCE (SIZE(1..maxnoofServedGUAMIs)) OF UnavailableGUAMIItem

UnavailableGUAMIItem ::= SEQUENCE {
	gUAMI								GUAMI,
	timerApproachForGUAMIRemoval		TimerApproachForGUAMIRemoval					OPTIONAL,
	backupAMFName						AMFName											OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UnavailableGUAMIItem-ExtIEs} }	OPTIONAL,
	...
}

UnavailableGUAMIItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

ULForwarding ::= ENUMERATED {
	ul-forwarding-proposed,
	...
}

UpdateFeedback ::= BIT STRING (SIZE(8, ...))

UPTransportLayerInformation ::= CHOICE {
	gTPTunnel				GTPTunnel,
	choice-Extensions		ProtocolIE-SingleContainer { {UPTransportLayerInformation-ExtIEs} }
}

UPTransportLayerInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

UPTransportLayerInformationList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF UPTransportLayerInformationItem

UPTransportLayerInformationItem ::= SEQUENCE {
	nGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UPTransportLayerInformationItem-ExtIEs} } OPTIONAL,
	...
}

UPTransportLayerInformationItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-CommonNetworkInstance				CRITICALITY ignore	EXTENSION  CommonNetworkInstance						PRESENCE optional		},
	...
}


UPTransportLayerInformationPairList ::= SEQUENCE (SIZE(1..maxnoofMultiConnectivityMinusOne)) OF UPTransportLayerInformationPairItem

UPTransportLayerInformationPairItem ::= SEQUENCE {
	uL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	dL-NGU-UP-TNLInformation		UPTransportLayerInformation,
	iE-Extensions		ProtocolExtensionContainer { {UPTransportLayerInformationPairItem-ExtIEs} } OPTIONAL,
	...
}

UPTransportLayerInformationPairItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

URI-address ::= VisibleString

UserLocationInformation ::= CHOICE {
	userLocationInformationEUTRA	UserLocationInformationEUTRA,
	userLocationInformationNR		UserLocationInformationNR,
	userLocationInformationN3IWF	UserLocationInformationN3IWF,
	choice-Extensions		ProtocolIE-SingleContainer { {UserLocationInformation-ExtIEs} }
}

UserLocationInformation-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UserLocationInformationTNGF		CRITICALITY ignore	TYPE UserLocationInformationTNGF		PRESENCE mandatory	}|
	{ ID id-UserLocationInformationTWIF		CRITICALITY ignore	TYPE UserLocationInformationTWIF		PRESENCE mandatory	}|
	{ ID id-UserLocationInformationW-AGF	CRITICALITY ignore	TYPE UserLocationInformationW-AGF		PRESENCE mandatory	},
	...
}

UserLocationInformationEUTRA ::= SEQUENCE {
	eUTRA-CGI			EUTRA-CGI,
	tAI					TAI,
	timeStamp			TimeStamp																OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationEUTRA-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationEUTRA-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PSCellInformation	CRITICALITY ignore	EXTENSION NGRAN-CGI				PRESENCE optional},
	...
}

UserLocationInformationN3IWF ::= SEQUENCE {
	iPAddress			TransportLayerAddress,
	portNumber			PortNumber,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationN3IWF-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationN3IWF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-TAI			CRITICALITY ignore	EXTENSION TAI							PRESENCE optional	},
	...
}

UserLocationInformationTNGF ::= SEQUENCE {
	tNAP-ID				TNAP-ID,
	iPAddress			TransportLayerAddress,
	portNumber			PortNumber															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationTNGF-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationTNGF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-TAI			CRITICALITY ignore	EXTENSION TAI							PRESENCE optional	},
	...
}

UserLocationInformationTWIF ::= SEQUENCE {
	tWAP-ID				TWAP-ID,
	iPAddress			TransportLayerAddress,
	portNumber			PortNumber															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationTWIF-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationTWIF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-TAI			CRITICALITY ignore	EXTENSION TAI							PRESENCE optional	},
	...
}

UserLocationInformationW-AGF ::= CHOICE {
	globalLine-ID	GlobalLine-ID,
	hFCNode-ID		HFCNode-ID,
	choice-Extensions		ProtocolIE-SingleContainer { { UserLocationInformationW-AGF-ExtIEs} }
}

UserLocationInformationW-AGF-ExtIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GlobalCable-ID 	CRITICALITY 	ignore 	TYPE 	GlobalCable-ID 		PRESENCE 	mandatory }|
	{ ID id-HFCNode-ID-new 	CRITICALITY 	ignore 	TYPE 	HFCNode-ID-new 		PRESENCE 	mandatory }|
	{ ID id-GlobalCable-ID-new 	CRITICALITY ignore 	TYPE 	GlobalCable-ID-new 	PRESENCE 	mandatory },
	...
}

UserLocationInformationNR ::= SEQUENCE {
	nR-CGI				NR-CGI,
	tAI					TAI,
	timeStamp			TimeStamp															OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {UserLocationInformationNR-ExtIEs} }	OPTIONAL,
	...
}

UserLocationInformationNR-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-PSCellInformation	CRITICALITY ignore	EXTENSION NGRAN-CGI				PRESENCE optional	}|
	{ ID id-NID					CRITICALITY reject	EXTENSION NID					PRESENCE optional	}|
	{ ID id-NRNTNTAIInformation	CRITICALITY ignore	EXTENSION NRNTNTAIInformation 	PRESENCE optional	},
	...
}

UserPlaneSecurityInformation ::= SEQUENCE {
	securityResult			SecurityResult,
	securityIndication		SecurityIndication,
	iE-Extensions		ProtocolExtensionContainer { {UserPlaneSecurityInformation-ExtIEs} }	OPTIONAL,
	...
}

UserPlaneSecurityInformation-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- V

VolumeTimedReportList ::= SEQUENCE (SIZE(1..maxnoofTimePeriods)) OF VolumeTimedReport-Item

VolumeTimedReport-Item ::= SEQUENCE {
	startTimeStamp				OCTET STRING (SIZE(4)),
	endTimeStamp				OCTET STRING (SIZE(4)),
	usageCountUL				INTEGER (0..18446744073709551615),
	usageCountDL				INTEGER (0..18446744073709551615),
	iE-Extensions		ProtocolExtensionContainer { {VolumeTimedReport-Item-ExtIEs} } OPTIONAL,
	...
}

VolumeTimedReport-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- W

W-AGF-ID ::= CHOICE {
	w-AGF-ID				BIT STRING (SIZE(16, ...)),
	choice-Extensions		ProtocolIE-SingleContainer { {W-AGF-ID-ExtIEs} }
}

W-AGF-ID-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

WarningAreaCoordinates ::= OCTET STRING (SIZE(1..1024))

WarningAreaList ::= CHOICE {
	eUTRA-CGIListForWarning			EUTRA-CGIListForWarning,
	nR-CGIListForWarning			NR-CGIListForWarning,
	tAIListForWarning				TAIListForWarning,
	emergencyAreaIDList				EmergencyAreaIDList,
	choice-Extensions		ProtocolIE-SingleContainer { {WarningAreaList-ExtIEs} }
}

WarningAreaList-ExtIEs NGAP-PROTOCOL-IES ::= {
	...
}

WarningMessageContents ::= OCTET STRING (SIZE(1..9600))

WarningSecurityInfo ::= OCTET STRING (SIZE(50))

WarningType ::= OCTET STRING (SIZE(2))

WLANMeasurementConfiguration ::= SEQUENCE {
	wlanMeasConfig             	WLANMeasConfig,
	wlanMeasConfigNameList		WLANMeasConfigNameList            								OPTIONAL,
	wlan-rssi                  	ENUMERATED {true, ...}            								OPTIONAL,
	wlan-rtt                   	ENUMERATED {true, ...}            								OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { { WLANMeasurementConfiguration-ExtIEs } } 	OPTIONAL,
	...
}

WLANMeasurementConfiguration-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

WLANMeasConfigNameList ::= SEQUENCE (SIZE(1..maxnoofWLANName)) OF WLANMeasConfigNameItem

WLANMeasConfigNameItem ::= SEQUENCE {
	wLANName			WLANName,
	iE-Extensions		ProtocolExtensionContainer { { WLANMeasConfigNameItem-ExtIEs } } 	OPTIONAL,
	...
}

WLANMeasConfigNameItem-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

WLANMeasConfig::= ENUMERATED {setup,...}

WLANName ::= OCTET STRING (SIZE (1..32))

WUS-Assistance-Information  ::= SEQUENCE {
	pagingProbabilityInformation             PagingProbabilityInformation,
	iE-Extensions		ProtocolExtensionContainer { { WUS-Assistance-Information-ExtIEs } } OPTIONAL,
	...
}

WUS-Assistance-Information-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- X

XnExtTLAs ::= SEQUENCE (SIZE(1..maxnoofXnExtTLAs)) OF XnExtTLA-Item

XnExtTLA-Item ::= SEQUENCE {
	iPsecTLA					TransportLayerAddress							OPTIONAL,
	gTP-TLAs					XnGTP-TLAs										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {XnExtTLA-Item-ExtIEs} } 	OPTIONAL,
	...
}

XnExtTLA-Item-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	{ ID id-SCTP-TLAs		CRITICALITY ignore	EXTENSION SCTP-TLAs		PRESENCE optional },
	...
}

XnGTP-TLAs ::= SEQUENCE (SIZE(1..maxnoofXnGTP-TLAs)) OF TransportLayerAddress

XnTLAs ::= SEQUENCE (SIZE(1..maxnoofXnTLAs)) OF TransportLayerAddress

XnTNLConfigurationInfo ::= SEQUENCE {
	xnTransportLayerAddresses			XnTLAs,
	xnExtendedTransportLayerAddresses	XnExtTLAs										OPTIONAL,
	iE-Extensions		ProtocolExtensionContainer { {XnTNLConfigurationInfo-ExtIEs} }	OPTIONAL,
	...
}

XnTNLConfigurationInfo-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {
	...
}

-- Y
-- Z

END
