/* Osmocom VTY interface functions in TTCN-3
 * (C) 2017-2018 Harald Welte <laforge@gnumonks.org>
 * contributions by sysmocom - s.f.m.c. GmbH
 * All rights reserved.
 *
 * Released under the terms of GNU General Public License, Version 2 or
 * (at your option) any later version.
 *
 * SPDX-License-Identifier: GPL-2.0-or-later
 */

module Osmocom_VTY_Functions {

import from Misc_Helpers all;
import from TELNETasp_PortType all;
import from Osmocom_Types all;
import from TCCConversion_Functions all;
import from Socket_API_Definitions all;

modulepar {
	charstring mp_prompt_prefix := "OpenBSC";
	float mp_prompt_timeout := 2.0;
}

const charstring VTY_VIEW_SUFFIX := "> ";
const charstring VTY_ENABLE_SUFFIX := "# ";
const charstring VTY_CFG_SUFFIX := "(*)";

template charstring t_vty_unknown := pattern "*% Unknown command.";

/* configure prompts in TELNETasp module */
function f_vty_set_prompts(TELNETasp_PT pt, charstring prompt_prefix := mp_prompt_prefix) {
	var ASP_TelnetDynamicConfig vty_prompt[3] := {
		{
			prompt := {
				id := 1,
				prompt := prompt_prefix & VTY_VIEW_SUFFIX,
				has_wildcards := false
			}
		}, {
			prompt := {
				id := 2,
				prompt := prompt_prefix & VTY_ENABLE_SUFFIX,
				has_wildcards := false
			}
		}, {
			prompt := {
				id := 3,
				prompt := prompt_prefix & VTY_CFG_SUFFIX,
				has_wildcards := true
			}
		}
	};

	/* set some configuration that isn't possible to express
	 * in the config file due to syntactic restrictions (Who invents config
	 * files that don't permit regular expressions? */
	for (var integer i := 0; i < sizeof(vty_prompt); i:= i + 1) {
		pt.send(vty_prompt[i]);
	}
}

/* wait for any of the permitted prompts; buffer + return all intermediate output */
function f_vty_wait_for_prompt(TELNETasp_PT pt, boolean strict := true, charstring log_label := "(?)")
return charstring {
	var charstring rx, buf := "";
	var integer fd;
	timer T;

	T.start(mp_prompt_timeout);
	alt {
	[] pt.receive(pattern "[\w-]+" & VTY_VIEW_SUFFIX) { };
	[] pt.receive(pattern "[\w-]+\# ") { };
	[] pt.receive(pattern "[\w-]+\(*\)\# ") { };
	[] pt.receive(t_vty_unknown) -> value rx {
		if (strict) {
			setverdict(fail, "VTY: Unknown Command: " & log_label);
			mtc.stop;
		} else {
			log("VTY: Unknown Command (ignored): " & log_label);
			buf := buf & rx;
			repeat;
		}
		};
	[] pt.receive(charstring:?) -> value rx { buf := buf & rx; repeat };
	[] pt.receive(integer:?) -> value fd {
		if (fd == -1) {
			setverdict(fail, "VTY Telnet Connection Failure: " & log_label);
			mtc.stop;
		} else {
			repeat; /* telnet connection succeeded */
		}
	}
	[] T.timeout {
		setverdict(fail, "VTY Timeout for prompt: " & log_label);
		mtc.stop;
		};
	}
	T.stop;
	return buf;
}

/* send a VTY command and obtain response until prompt is received */
function f_vty_transceive_ret(TELNETasp_PT pt, charstring tx, boolean strict := true) return charstring {
	pt.send(tx);
	return f_vty_wait_for_prompt(pt, strict, tx);
}

/* send a VTY command and obtain response until prompt is received */
function f_vty_transceive(TELNETasp_PT pt, charstring tx, boolean strict := true) {
	var charstring unused := f_vty_transceive_ret(pt, tx, strict);
}

type integer BtsNr (0..255);
type integer BtsTrxNr (0..255);
type integer BtsTimeslotNr (0..7);
type integer MscNr (0..255);
type integer Cs7Nr (0..255);

type charstring BtsGprsMode ("none", "gprs", "egrps");

/* enter the'confiugration' mode of the VTY */
function f_vty_enter_config(TELNETasp_PT pt) {
	f_vty_transceive(pt, "configure terminal")
}

function f_vty_enter_cfg_network(TELNETasp_PT pt) {
	f_vty_enter_config(pt);
	f_vty_transceive(pt, "network")
}

function f_vty_enter_cfg_bts(TELNETasp_PT pt, BtsNr bts := 0) {
	f_vty_enter_cfg_network(pt);
	f_vty_transceive(pt, "bts " & int2str(bts));
}

function f_vty_enter_cfg_trx(TELNETasp_PT pt, BtsNr bts := 0, BtsTrxNr trx := 0) {
	f_vty_enter_cfg_bts(pt, bts);
	f_vty_transceive(pt, "trx " & int2str(trx));
}

function f_vty_enter_cfg_ts(TELNETasp_PT pt, BtsNr bts := 0, BtsTrxNr trx := 0, BtsTimeslotNr ts) {
	f_vty_enter_cfg_trx(pt, bts, trx);
	f_vty_transceive(pt, "timeslot " & int2str(ts));
}

function f_vty_enter_cfg_msc(TELNETasp_PT pt, MscNr msc := 0) {
	f_vty_enter_config(pt);
	f_vty_transceive(pt, "msc " & int2str(msc));
}

function f_vty_enter_cfg_cs7_inst(TELNETasp_PT pt, Cs7Nr cs7_inst := 0) {
	f_vty_enter_config(pt);
	f_vty_transceive(pt, "cs7 instance " & int2str(cs7_inst));
}

function f_vty_enter_cfg_smlc(TELNETasp_PT pt) {
	f_vty_enter_config(pt);
	f_vty_transceive(pt, "smlc");
}

type record of charstring rof_charstring;
function f_vty_config3(TELNETasp_PT pt, rof_charstring config_nodes, rof_charstring cmds)
{
	/* enter config mode; enter node */
	f_vty_enter_config(pt);
	for (var integer i := 0; i < sizeof(config_nodes); i := i+1) {
		f_vty_transceive(pt, config_nodes[i]);
	}
	/* execute commands */
	for (var integer i := 0; i < sizeof(cmds); i := i+1) {
		f_vty_transceive(pt, cmds[i]);
	}
	/* leave config mode */
	f_vty_transceive(pt, "end");
}

function f_vty_config2(TELNETasp_PT pt, rof_charstring config_nodes, charstring cmd)
{
	f_vty_config3(pt, config_nodes, { cmd });
}

function f_vty_config(TELNETasp_PT pt, charstring config_node, charstring cmd)
{
	f_vty_config2(pt, {config_node}, cmd);
}

function f_vty_cfg_bts(TELNETasp_PT pt, BtsNr bts := 0, rof_charstring cmds) {
	f_vty_config3(pt, {"network", "bts " & int2str(bts)}, cmds);
}

function f_vty_cfg_msc(TELNETasp_PT pt, MscNr msc := 0, rof_charstring cmds) {
	f_vty_config3(pt, {"msc " & int2str(msc)}, cmds);
}

function f_vty_transceive_match(TELNETasp_PT pt, charstring cmd, template charstring exp_ret) {
	var charstring ret := f_vty_transceive_ret(pt, cmd);
	if (not match(ret, exp_ret)) {
		setverdict(fail, "Non-matching VTY response: ", ret);
		mtc.stop;
	}
}

function f_vty_transceive_not_match(TELNETasp_PT pt, charstring cmd, template charstring exp_ret) {
	var charstring ret := f_vty_transceive_ret(pt, cmd);
	if (match(ret, exp_ret)) {
		setverdict(fail, "Unexpected matching VTY response: ", ret);
		mtc.stop;
	}
}

function f_vty_transceive_match_regex(TELNETasp_PT pt, charstring cmd, charstring regex, integer groupno) return charstring
{
	var charstring resp := f_vty_transceive_ret(pt, cmd);
	return regexp(resp, regex, groupno);
}

function f_vty_transceive_match_regexp_retry(TELNETasp_PT pt, charstring cmd, charstring regex,
					     integer groupno, integer num_attempts, float retry_delay) return charstring
{
	 while (num_attempts > 0) {
		var charstring ret := f_vty_transceive_match_regex(pt, cmd, regex, groupno);
		if (ret != "") {
			return ret;
		}
		f_sleep(retry_delay);
		num_attempts := num_attempts - 1;
	}

	Misc_Helpers.f_shutdown(__BFILE__, __LINE__, fail,
				log2str("No matching VTY response for regular expression '",
					regex, "' after ", num_attempts, " attempts." ));
	return "";
}

private type record of charstring StrList;

/* Perform a 'show talloc-context' to get a count of the given object_strs that are still allocated.
 * Retry 'attempts' times until the actual talloc object count matches 'expect_count'.
 * Useful to ensure that no mem leaks remain after running a test. */
function f_verify_talloc_count(TELNETasp_PT pt, StrList object_strs, integer expect_count := 0,
			       integer attempts := 5, float wait_time := 3.0)
{
	var charstring show_cmd := "show talloc-context application full filter ";
	for (var integer i := 0; i < lengthof(object_strs); i := i + 1) {
		var charstring obj_str := object_strs[i];
		/* spaces confuse the VTY command */
		obj_str := f_replaceEveryOccurenceOfSubstring(obj_str, " ", ".");
		/* In the regexp, expect word start and word end to bound the obj name */
		obj_str := "\\<" & obj_str & "\\>";
		if (i > 0) {
			show_cmd := show_cmd & "\\|";
		}
		show_cmd := show_cmd & obj_str;
	}

	while (attempts > 0) {
		attempts := attempts - 1;
		var charstring ret := f_vty_transceive_ret(pt, show_cmd);

		var boolean ok := true;
		for (var integer i := 0; i < lengthof(object_strs); i := i + 1) {
			var charstring object_str := object_strs[i];
			var integer count := f_strstr_count(ret, object_str);
			log("talloc reports ", object_str, " x ", count, ", expecting ", expect_count);
			if (count != expect_count) {
				ok := false;
			}
		}
		if (ok) {
			return;
		}
		if (attempts == 0) {
			break;
		}
		log("count mismatch, retrying in ", wait_time);
		f_sleep(wait_time);
	}
	Misc_Helpers.f_shutdown(__BFILE__, __LINE__, fail, "talloc count mismatch");
}

public function f_verify_talloc_bytes(TELNETasp_PT pt, Misc_Helpers.ro_charstring object_strs, integer expect_bytes := 0,
				       integer attempts := 5, float wait_time := 3.0)
{
	var charstring show_cmd := "show talloc-context application brief";

	while (attempts > 0) {
		attempts := attempts - 1;
		var charstring ret := f_vty_transceive_ret(pt, show_cmd);

		var Misc_Helpers.ro_charstring lines := f_str_split(ret);

		var boolean ok := true;
		for (var integer i := 0; i < lengthof(object_strs); i := i + 1) {
			var charstring object_str := object_strs[i];

			var integer bytes := 0;

			for (var integer j := 0; j < lengthof(lines); j := j + 1) {
				var charstring line := lines[j];
				if (f_strstr(line, object_str) < 0) {
					continue;
				}
				var Misc_Helpers.ro_charstring tokens := f_str_split(line, " ");
				if (lengthof(tokens) < 4) {
					continue;
				}
				if (tokens[3] != "bytes") {
					continue;
				}
				bytes := f_str2int(tokens[2]);
			}

			if (bytes != expect_bytes) {
				ok := false;
				log("ERROR: talloc reports ", object_str, " = ", bytes, " bytes, expecting ", expect_bytes,
				    " from VTY response ", lines);
			} else {
				log("ok: talloc reports ", object_str, " = ", bytes, " bytes");
			}
		}
		if (ok) {
			return;
		}
		if (attempts == 0) {
			break;
		}
		log("bytes count mismatch, retrying in ", wait_time);
		f_sleep(wait_time);
	}
	setverdict(fail, "talloc bytes count mismatch");
	mtc.stop;
}

public function f_logp(TELNETasp_PT pt, charstring log_msg)
{
	// log on TTCN3 log output
	log(log_msg);
	// log in stderr log
	if (pt.checkstate("Mapped")) {
		f_vty_transceive(pt, "logp lglobal notice TTCN3 f_logp(): " & log_msg);
	}
}

}
