<?xml version="1.0" encoding="UTF-8"?>
<vtydoc xmlns="urn:osmocom:xml:libosmocore:vty:doc:1.0">
  <node id="_common_cmds_">
    <name>Common Commands</name>
    <description>These commands are available on all VTY nodes. They are listed here only once, to unclutter the VTY reference.</description>
    <command id="help">
      <params>
        <param name="help" doc="Description of the interactive help system"/>
      </params>
    </command>
    <command id="list [with-flags]">
      <params>
        <param name="list" doc="Print command list"/>
        <param name="[with-flags]" doc="Also print the VTY attribute flags"/>
      </params>
    </command>
    <command id="show vty-attributes">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="vty-attributes" doc="List of VTY attributes"/>
      </params>
    </command>
    <command id="show vty-attributes (application|library|global)">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="vty-attributes" doc="List of VTY attributes"/>
        <param name="application" doc="Application specific attributes only"/>
        <param name="library" doc="Library specific attributes only"/>
        <param name="global" doc="Global attributes only"/>
      </params>
    </command>
    <command id="write terminal">
      <params>
        <param name="write" doc="Write running configuration to memory, network, or terminal"/>
        <param name="terminal" doc="Write to terminal"/>
      </params>
    </command>
    <command id="write file [PATH]">
      <params>
        <param name="write" doc="Write running configuration to memory, network, or terminal"/>
        <param name="file" doc="Write to configuration file"/>
        <param name="[PATH]" doc="Set file path to store the config, or replace if already exists"/>
      </params>
    </command>
    <command id="write memory">
      <params>
        <param name="write" doc="Write running configuration to memory, network, or terminal"/>
        <param name="memory" doc="Write configuration to the file (same as write file)"/>
      </params>
    </command>
    <command id="write">
      <params>
        <param name="write" doc="Write running configuration to memory, network, or terminal"/>
      </params>
    </command>
    <command id="show running-config">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="running-config" doc="running configuration"/>
      </params>
    </command>
    <command id="exit">
      <params>
        <param name="exit" doc="Exit current mode and down to previous mode"/>
      </params>
    </command>
    <command id="end">
      <params>
        <param name="end" doc="End current mode and change to enable mode."/>
      </params>
    </command>
  </node>
  <node id="view">
    <name>view</name>
    <command id="show pid">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="pid" doc="Displays the process ID"/>
      </params>
    </command>
    <command id="show uptime">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="uptime" doc="Displays how long the program has been running"/>
      </params>
    </command>
    <command id="show version">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="version" doc="Displays program version"/>
      </params>
    </command>
    <command id="show online-help">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="online-help" doc="Online help"/>
      </params>
    </command>
    <command id="enable [expert-mode]">
      <params>
        <param name="enable" doc="Turn on privileged mode command"/>
        <param name="[expert-mode]" doc="Enable the expert mode (show hidden commands)"/>
      </params>
    </command>
    <command id="terminal length &lt;0-512&gt;">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="length" doc="Set number of lines on a screen"/>
        <param name="&lt;0-512&gt;" doc="Number of lines on screen (0 for no pausing)"/>
      </params>
    </command>
    <command id="terminal no length">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="length" doc="Set number of lines on a screen"/>
      </params>
    </command>
    <command id="who">
      <params>
        <param name="who" doc="Display who is on vty"/>
      </params>
    </command>
    <command id="show history">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="history" doc="Display the session command history"/>
      </params>
    </command>
    <command id="show runtime">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="runtime" doc="Display runtime information"/>
      </params>
    </command>
    <command id="logging enable">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="enable" doc="Enables logging to this vty"/>
      </params>
    <description>This command is required to make logging commands available
      on the telnet VTY.</description></command>
    <command id="logging disable">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="disable" doc="Disables logging to this vty"/>
      </params>
    </command>
    <command id="logging filter all (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="filter" doc="Filter log messages"/>
        <param name="all" doc="Do you want to log all messages?"/>
        <param name="0" doc="Only print messages matched by other filters"/>
        <param name="1" doc="Bypass filter and print all messages"/>
      </params>
    <description>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </description></command>
    <command id="logging color (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="color" doc="Configure color-printing for log messages"/>
        <param name="0" doc="Don't use color for printing messages"/>
        <param name="1" doc="Use color for printing messages"/>
      </params>
    </command>
    <command id="logging timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp"/>
      </params>
    </command>
    <command id="logging print extended-timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="extended-timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn"/>
      </params>
    </command>
    <command id="logging print thread-id (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="thread-id" doc="Configure log message logging Thread ID"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current Thread ID"/>
      </params>
    </command>
    <command id="logging print category (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem name"/>
      </params>
    </command>
    <command id="logging print category-hex (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category-hex" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')"/>
      </params>
    </command>
    <command id="logging print level (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="level" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the log level name"/>
      </params>
    </command>
    <command id="logging print file (0|1|basename) [last]">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="file" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the source file and line"/>
        <param name="basename" doc="Prefix each log message with the source file's basename (strip leading paths) and line"/>
        <param name="[last]" doc="Log source file info at the end of a log line. If omitted, log source file info just before the log text."/>
      </params>
    </command>
    <command id="logging set-log-mask MASK">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="set-log-mask" doc="Set the logmask of this logging target"/>
        <param name="MASK" doc="List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8"/>
      </params>
    </command>
    <command id="logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="lglobal" doc="Library-internal global log family"/>
        <param name="llapd" doc="LAPD in libosmogsm"/>
        <param name="linp" doc="A-bis Intput Subsystem"/>
        <param name="lmux" doc="A-bis B-Subchannel TRAU Frame Multiplex"/>
        <param name="lmi" doc="A-bis Input Driver for Signalling"/>
        <param name="lmib" doc="A-bis Input Driver for B-Channels (voice)"/>
        <param name="lsms" doc="Layer3 Short Message Service (SMS)"/>
        <param name="lctrl" doc="Control Interface"/>
        <param name="lgtp" doc="GPRS GTP library"/>
        <param name="lstats" doc="Statistics messages and logging"/>
        <param name="lgsup" doc="Generic Subscriber Update Protocol"/>
        <param name="loap" doc="Osmocom Authentication Protocol"/>
        <param name="lss7" doc="libosmo-sigtran Signalling System 7"/>
        <param name="lsccp" doc="libosmo-sigtran SCCP Implementation"/>
        <param name="lsua" doc="libosmo-sigtran SCCP User Adaptation"/>
        <param name="lm3ua" doc="libosmo-sigtran MTP3 User Adaptation"/>
        <param name="lmgcp" doc="libosmo-mgcp Media Gateway Control Protocol"/>
        <param name="ljibuf" doc="libosmo-netif Jitter Buffer"/>
        <param name="lrspro" doc="Remote SIM protocol"/>
        <param name="lns" doc="GPRS NS layer"/>
        <param name="lbssgp" doc="GPRS BSSGP layer"/>
        <param name="lnsdata" doc="GPRS NS layer data PDU"/>
        <param name="lnssignal" doc="GPRS NS layer signal PDU"/>
        <param name="liuup" doc="Iu UP layer"/>
        <param name="lpfcp" doc="libosmo-pfcp Packet Forwarding Control Protocol"/>
        <param name="lcsn1" doc="libosmo-csn1 Concrete Syntax Notation 1 codec"/>
        <param name="lio" doc="libosmocore IO Subsystem"/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level set-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="set-all" doc="Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level force-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="no logging level force-all">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Release any globally forced log level set with 'logging level force-all &lt;level&gt;'"/>
      </params>
    </command>
    <command id="logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal) .LOGMESSAGE">
      <params>
        <param name="logp" doc="Print a message on all log outputs; useful for placing markers in test logs"/>
        <param name="lglobal" doc="Library-internal global log family"/>
        <param name="llapd" doc="LAPD in libosmogsm"/>
        <param name="linp" doc="A-bis Intput Subsystem"/>
        <param name="lmux" doc="A-bis B-Subchannel TRAU Frame Multiplex"/>
        <param name="lmi" doc="A-bis Input Driver for Signalling"/>
        <param name="lmib" doc="A-bis Input Driver for B-Channels (voice)"/>
        <param name="lsms" doc="Layer3 Short Message Service (SMS)"/>
        <param name="lctrl" doc="Control Interface"/>
        <param name="lgtp" doc="GPRS GTP library"/>
        <param name="lstats" doc="Statistics messages and logging"/>
        <param name="lgsup" doc="Generic Subscriber Update Protocol"/>
        <param name="loap" doc="Osmocom Authentication Protocol"/>
        <param name="lss7" doc="libosmo-sigtran Signalling System 7"/>
        <param name="lsccp" doc="libosmo-sigtran SCCP Implementation"/>
        <param name="lsua" doc="libosmo-sigtran SCCP User Adaptation"/>
        <param name="lm3ua" doc="libosmo-sigtran MTP3 User Adaptation"/>
        <param name="lmgcp" doc="libosmo-mgcp Media Gateway Control Protocol"/>
        <param name="ljibuf" doc="libosmo-netif Jitter Buffer"/>
        <param name="lrspro" doc="Remote SIM protocol"/>
        <param name="lns" doc="GPRS NS layer"/>
        <param name="lbssgp" doc="GPRS BSSGP layer"/>
        <param name="lnsdata" doc="GPRS NS layer data PDU"/>
        <param name="lnssignal" doc="GPRS NS layer signal PDU"/>
        <param name="liuup" doc="Iu UP layer"/>
        <param name="lpfcp" doc="libosmo-pfcp Packet Forwarding Control Protocol"/>
        <param name="lcsn1" doc="libosmo-csn1 Concrete Syntax Notation 1 codec"/>
        <param name="lio" doc="libosmocore IO Subsystem"/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
        <param name=".LOGMESSAGE" doc="Arbitrary message to log on given category and log level"/>
      </params>
    </command>
    <command id="show logging vty">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="logging" doc="Show current logging configuration"/>
        <param name="vty" doc="Show current logging configuration for this vty"/>
      </params>
    </command>
    <command id="show alarms">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="alarms" doc="Show current logging configuration"/>
      </params>
    </command>
    <command id="show stats [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="stats" doc="Show statistical values"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="show stats level (global|peer|subscriber) [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="stats" doc="Show statistical values"/>
        <param name="level" doc="Set the maximum group level"/>
        <param name="global" doc="Show global groups only"/>
        <param name="peer" doc="Show global and network peer related groups"/>
        <param name="subscriber" doc="Show global, peer, and subscriber groups"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="show asciidoc counters">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="asciidoc" doc="Asciidoc generation"/>
        <param name="counters" doc="Generate table of all registered counters"/>
      </params>
    </command>
    <command id="show rate-counters [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="rate-counters" doc="Show all rate counters"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; users">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="users" doc="User Table"/>
      </params>
    </command>
    <command id="show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="[&lt;0-65534&gt;]" doc="Local Port Number"/>
      </params>
    </command>
    <command id="show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="sctp" doc="SCTP (Stream Control Transmission Protocol)"/>
        <param name="tcp" doc="TCP (Transmission Control Protocol)"/>
        <param name="[&lt;0-65534&gt;]" doc="Local Port Number"/>
      </params>
    </command>
    <command id="show cs7 config">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="config" doc="Currently running cs7 configuration"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp" doc="Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp" doc="Application Server Process (ASP)"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-remaddr">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-remaddr" doc="Application Server Process (ASP) remote addresses information"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-remaddr" doc="Application Server Process (ASP) remote addresses information"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-assoc-status">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-assoc-status" doc="Application Server Process (ASP) SCTP association status"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-assoc-status" doc="Application Server Process (ASP) SCTP association information"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="active" doc="Display all active ASs"/>
        <param name="all" doc="Display all ASs (default)"/>
        <param name="m3ua" doc="Display all m3ua ASs"/>
        <param name="sua" doc="Display all SUA ASs"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as name AS_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="name" doc="Look up AS with a given name"/>
        <param name="AS_NAME" doc="Name of the Application Server (AS)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="binding-table" doc="Display binding table"/>
        <param name="name" doc="Look up AS with a given name"/>
        <param name="AS_NAME" doc="Name of the Application Server (AS)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route [POINT_CODE]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route" doc="Routing Table"/>
        <param name="[POINT_CODE]" doc="Destination Point Code"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route" doc="Routing Table"/>
        <param name="binding-table" doc="Display binding table"/>
        <param name="[POINT_CODE]" doc="Destination Point Code"/>
        <param name="[all-matches]" doc="Display all matching Combination Links"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route-lookup" doc="Look up route"/>
        <param name="POINT_CODE" doc="Destination PC"/>
        <param name="from" doc="From"/>
        <param name="POINT_CODE" doc="Origin PC"/>
        <param name="sls" doc="SLS"/>
        <param name="&lt;0-15&gt;" doc="SLS value"/>
        <param name="[list-asps]" doc="List ASPs of the AS if route points to an AS"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp addressbook">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="addressbook" doc="List all SCCP addressbook entries"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp users">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="users" doc="Show List of SCCP Users registered"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="ssn" doc="Find an SCCP User registered for the given SSN"/>
        <param name="&lt;0-65535&gt;" doc="Subsystem Number (SSN)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp connections">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="connections" doc="Show List of active SCCP connections"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp timers">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signaling Connection Control Part"/>
        <param name="timers" doc="Show List of SCCP timers"/>
      </params>
    </command>
    <command id="show cpu-sched threads">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cpu-sched" doc="Show Sched section information"/>
        <param name="threads" doc="Show information about running threads)"/>
      </params>
    </command>
    <command id="show fsm NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm" doc="Show information about finite state machines"/>
        <param name="NAME" doc="Display information about a single named finite state machine"/>
      </params>
    </command>
    <command id="show fsm all">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm" doc="Show information about finite state machines"/>
        <param name="all" doc="Display a list of all registered finite state machines"/>
      </params>
    </command>
    <command id="show fsm-state-graph NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-state-graph" doc="Generate a state transition graph (using DOT language)"/>
        <param name="NAME" doc="FSM name"/>
      </params>
    </command>
    <command id="show fsm-instances NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-instances" doc="Show information about finite state machine instances"/>
        <param name="NAME" doc="Display a list of all FSM instances of the named finite state machine"/>
      </params>
    </command>
    <command id="show fsm-instances all">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-instances" doc="Show information about finite state machine instances"/>
        <param name="all" doc="Display a list of all FSM instances of all finite state machine"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH)">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
        <param name="tree" doc="Display only a specific memory chunk"/>
        <param name="ADDRESS" doc="Chunk address (e.g. 0xdeadbeef)"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
        <param name="filter" doc="Filter chunks using regular expression"/>
        <param name="REGEXP" doc="Regular expression"/>
      </params>
    </command>
  <description>The view node is the default node when connecting to the
    VTY interface. This node does not require any additional
    permission and allows to introspect the application.</description></node>
  <node id="enable">
    <name>enable</name>
    <command id="disable">
      <params>
        <param name="disable" doc="Turn off privileged mode command"/>
      </params>
    </command>
    <command id="configure [terminal]">
      <params>
        <param name="configure" doc="Configuration from vty interface"/>
        <param name="[terminal]" doc="Configuration terminal"/>
      </params>
    </command>
    <command id="copy running-config startup-config">
      <params>
        <param name="copy" doc="Copy configuration"/>
        <param name="running-config" doc="Copy running config to... "/>
        <param name="startup-config" doc="Copy running config to startup config (same as write file)"/>
      </params>
    </command>
    <command id="shutdown">
      <params>
        <param name="shutdown" doc="Request a shutdown of the program"/>
      </params>
    </command>
    <command id="show startup-config">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="startup-config" doc="Contentes of startup configuration"/>
      </params>
    </command>
    <command id="show version">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="version" doc="Displays program version"/>
      </params>
    </command>
    <command id="show online-help">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="online-help" doc="Online help"/>
      </params>
    </command>
    <command id="terminal length &lt;0-512&gt;">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="length" doc="Set number of lines on a screen"/>
        <param name="&lt;0-512&gt;" doc="Number of lines on screen (0 for no pausing)"/>
      </params>
    </command>
    <command id="terminal no length">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="length" doc="Set number of lines on a screen"/>
      </params>
    </command>
    <command id="who">
      <params>
        <param name="who" doc="Display who is on vty"/>
      </params>
    </command>
    <command id="show history">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="history" doc="Display the session command history"/>
      </params>
    </command>
    <command id="terminal monitor">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="monitor" doc="Copy debug output to the current terminal line"/>
      </params>
    </command>
    <command id="terminal no monitor">
      <params>
        <param name="terminal" doc="Set terminal line parameters"/>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="monitor" doc="Copy debug output to the current terminal line"/>
      </params>
    </command>
    <command id="show runtime">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="runtime" doc="Display runtime information"/>
      </params>
    </command>
    <command id="logging enable">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="enable" doc="Enables logging to this vty"/>
      </params>
    <description>This command is required to make logging commands available
      on the telnet VTY.</description></command>
    <command id="logging disable">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="disable" doc="Disables logging to this vty"/>
      </params>
    </command>
    <command id="logging filter all (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="filter" doc="Filter log messages"/>
        <param name="all" doc="Do you want to log all messages?"/>
        <param name="0" doc="Only print messages matched by other filters"/>
        <param name="1" doc="Bypass filter and print all messages"/>
      </params>
    <description>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </description></command>
    <command id="logging color (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="color" doc="Configure color-printing for log messages"/>
        <param name="0" doc="Don't use color for printing messages"/>
        <param name="1" doc="Use color for printing messages"/>
      </params>
    </command>
    <command id="logging timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp"/>
      </params>
    </command>
    <command id="logging print extended-timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="extended-timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn"/>
      </params>
    </command>
    <command id="logging print thread-id (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="thread-id" doc="Configure log message logging Thread ID"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current Thread ID"/>
      </params>
    </command>
    <command id="logging print category (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem name"/>
      </params>
    </command>
    <command id="logging print category-hex (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category-hex" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')"/>
      </params>
    </command>
    <command id="logging print level (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="level" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the log level name"/>
      </params>
    </command>
    <command id="logging print file (0|1|basename) [last]">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="file" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the source file and line"/>
        <param name="basename" doc="Prefix each log message with the source file's basename (strip leading paths) and line"/>
        <param name="[last]" doc="Log source file info at the end of a log line. If omitted, log source file info just before the log text."/>
      </params>
    </command>
    <command id="logging set-log-mask MASK">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="set-log-mask" doc="Set the logmask of this logging target"/>
        <param name="MASK" doc="List of logging categories to log, e.g. 'abc:mno:xyz'. Available log categories depend on the specific application, refer to the 'logging level' command. Optionally add individual log levels like 'abc,1:mno,3:xyz,5', where the level numbers are LOGL_DEBUG=1 LOGL_INFO=3 LOGL_NOTICE=5 LOGL_ERROR=7 LOGL_FATAL=8"/>
      </params>
    </command>
    <command id="logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="lglobal" doc="Library-internal global log family"/>
        <param name="llapd" doc="LAPD in libosmogsm"/>
        <param name="linp" doc="A-bis Intput Subsystem"/>
        <param name="lmux" doc="A-bis B-Subchannel TRAU Frame Multiplex"/>
        <param name="lmi" doc="A-bis Input Driver for Signalling"/>
        <param name="lmib" doc="A-bis Input Driver for B-Channels (voice)"/>
        <param name="lsms" doc="Layer3 Short Message Service (SMS)"/>
        <param name="lctrl" doc="Control Interface"/>
        <param name="lgtp" doc="GPRS GTP library"/>
        <param name="lstats" doc="Statistics messages and logging"/>
        <param name="lgsup" doc="Generic Subscriber Update Protocol"/>
        <param name="loap" doc="Osmocom Authentication Protocol"/>
        <param name="lss7" doc="libosmo-sigtran Signalling System 7"/>
        <param name="lsccp" doc="libosmo-sigtran SCCP Implementation"/>
        <param name="lsua" doc="libosmo-sigtran SCCP User Adaptation"/>
        <param name="lm3ua" doc="libosmo-sigtran MTP3 User Adaptation"/>
        <param name="lmgcp" doc="libosmo-mgcp Media Gateway Control Protocol"/>
        <param name="ljibuf" doc="libosmo-netif Jitter Buffer"/>
        <param name="lrspro" doc="Remote SIM protocol"/>
        <param name="lns" doc="GPRS NS layer"/>
        <param name="lbssgp" doc="GPRS BSSGP layer"/>
        <param name="lnsdata" doc="GPRS NS layer data PDU"/>
        <param name="lnssignal" doc="GPRS NS layer signal PDU"/>
        <param name="liuup" doc="Iu UP layer"/>
        <param name="lpfcp" doc="libosmo-pfcp Packet Forwarding Control Protocol"/>
        <param name="lcsn1" doc="libosmo-csn1 Concrete Syntax Notation 1 codec"/>
        <param name="lio" doc="libosmocore IO Subsystem"/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level set-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="set-all" doc="Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level force-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="no logging level force-all">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Release any globally forced log level set with 'logging level force-all &lt;level&gt;'"/>
      </params>
    </command>
    <command id="logp (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal) .LOGMESSAGE">
      <params>
        <param name="logp" doc="Print a message on all log outputs; useful for placing markers in test logs"/>
        <param name="lglobal" doc="Library-internal global log family"/>
        <param name="llapd" doc="LAPD in libosmogsm"/>
        <param name="linp" doc="A-bis Intput Subsystem"/>
        <param name="lmux" doc="A-bis B-Subchannel TRAU Frame Multiplex"/>
        <param name="lmi" doc="A-bis Input Driver for Signalling"/>
        <param name="lmib" doc="A-bis Input Driver for B-Channels (voice)"/>
        <param name="lsms" doc="Layer3 Short Message Service (SMS)"/>
        <param name="lctrl" doc="Control Interface"/>
        <param name="lgtp" doc="GPRS GTP library"/>
        <param name="lstats" doc="Statistics messages and logging"/>
        <param name="lgsup" doc="Generic Subscriber Update Protocol"/>
        <param name="loap" doc="Osmocom Authentication Protocol"/>
        <param name="lss7" doc="libosmo-sigtran Signalling System 7"/>
        <param name="lsccp" doc="libosmo-sigtran SCCP Implementation"/>
        <param name="lsua" doc="libosmo-sigtran SCCP User Adaptation"/>
        <param name="lm3ua" doc="libosmo-sigtran MTP3 User Adaptation"/>
        <param name="lmgcp" doc="libosmo-mgcp Media Gateway Control Protocol"/>
        <param name="ljibuf" doc="libosmo-netif Jitter Buffer"/>
        <param name="lrspro" doc="Remote SIM protocol"/>
        <param name="lns" doc="GPRS NS layer"/>
        <param name="lbssgp" doc="GPRS BSSGP layer"/>
        <param name="lnsdata" doc="GPRS NS layer data PDU"/>
        <param name="lnssignal" doc="GPRS NS layer signal PDU"/>
        <param name="liuup" doc="Iu UP layer"/>
        <param name="lpfcp" doc="libosmo-pfcp Packet Forwarding Control Protocol"/>
        <param name="lcsn1" doc="libosmo-csn1 Concrete Syntax Notation 1 codec"/>
        <param name="lio" doc="libosmocore IO Subsystem"/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
        <param name=".LOGMESSAGE" doc="Arbitrary message to log on given category and log level"/>
      </params>
    </command>
    <command id="show logging vty">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="logging" doc="Show current logging configuration"/>
        <param name="vty" doc="Show current logging configuration for this vty"/>
      </params>
    </command>
    <command id="show alarms">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="alarms" doc="Show current logging configuration"/>
      </params>
    </command>
    <command id="show stats [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="stats" doc="Show statistical values"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="show stats level (global|peer|subscriber) [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="stats" doc="Show statistical values"/>
        <param name="level" doc="Set the maximum group level"/>
        <param name="global" doc="Show global groups only"/>
        <param name="peer" doc="Show global and network peer related groups"/>
        <param name="subscriber" doc="Show global, peer, and subscriber groups"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="show asciidoc counters">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="asciidoc" doc="Asciidoc generation"/>
        <param name="counters" doc="Generate table of all registered counters"/>
      </params>
    </command>
    <command id="show rate-counters [skip-zero]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="rate-counters" doc="Show all rate counters"/>
        <param name="[skip-zero]" doc="Skip items with total count zero"/>
      </params>
    </command>
    <command id="stats report">
      <params>
        <param name="stats" doc="Stats related commands"/>
        <param name="report" doc="Manurally trigger reporting of stats"/>
      </params>
    </command>
    <command id="stats reset">
      <params>
        <param name="stats" doc="Stats related commands"/>
        <param name="reset" doc="Reset all rate counter stats"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; users">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="users" doc="User Table"/>
      </params>
    </command>
    <command id="show cs7 (sua|m3ua|ipa) [&lt;0-65534&gt;]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="[&lt;0-65534&gt;]" doc="Local Port Number"/>
      </params>
    </command>
    <command id="show cs7 (sua|m3ua|ipa) (sctp|tcp) [&lt;0-65534&gt;]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="sctp" doc="SCTP (Stream Control Transmission Protocol)"/>
        <param name="tcp" doc="TCP (Transmission Control Protocol)"/>
        <param name="[&lt;0-65534&gt;]" doc="Local Port Number"/>
      </params>
    </command>
    <command id="show cs7 config">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="config" doc="Currently running cs7 configuration"/>
      </params>
    </command>
    <command id="cs7 instance &lt;0-15&gt; asp NAME disconnect">
      <params>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="Instance related commands"/>
        <param name="&lt;0-15&gt;" doc="SS7 Instance Number"/>
        <param name="asp" doc="ASP related commands"/>
        <param name="NAME" doc="Name of ASP"/>
        <param name="disconnect" doc="Disconnect the ASP (client will reconnect)"/>
      </params>
    </command>
    <command id="cs7 instance &lt;0-15&gt; asp NAME audit point-code POINT_CODE">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="Instance related commands"/>
        <param name="&lt;0-15&gt;" doc="SS7 Instance Number"/>
        <param name="asp" doc="ASP related commands"/>
        <param name="NAME" doc="Name of ASP"/>
        <param name="audit" doc="Audit destination Point Code (xUA DAUD)"/>
        <param name="point-code" doc="Destination Point Code to audit"/>
        <param name="POINT_CODE" doc="Destination Point Code value"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp" doc="Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp" doc="Application Server Process (ASP)"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-remaddr">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-remaddr" doc="Application Server Process (ASP) remote addresses information"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-remaddr name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-remaddr" doc="Application Server Process (ASP) remote addresses information"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-assoc-status">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-assoc-status" doc="Application Server Process (ASP) SCTP association status"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; asp-assoc-status name ASP_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="asp-assoc-status" doc="Application Server Process (ASP) SCTP association information"/>
        <param name="name" doc="Lookup ASP with a given name"/>
        <param name="ASP_NAME" doc="Name of the Application Server Process (ASP)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as (active|all|m3ua|sua)">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="active" doc="Display all active ASs"/>
        <param name="all" doc="Display all ASs (default)"/>
        <param name="m3ua" doc="Display all m3ua ASs"/>
        <param name="sua" doc="Display all SUA ASs"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as name AS_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="name" doc="Look up AS with a given name"/>
        <param name="AS_NAME" doc="Name of the Application Server (AS)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; as binding-table name AS_NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="as" doc="Application Server (AS)"/>
        <param name="binding-table" doc="Display binding table"/>
        <param name="name" doc="Look up AS with a given name"/>
        <param name="AS_NAME" doc="Name of the Application Server (AS)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route [POINT_CODE]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route" doc="Routing Table"/>
        <param name="[POINT_CODE]" doc="Destination Point Code"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route binding-table [POINT_CODE] [all-matches]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route" doc="Routing Table"/>
        <param name="binding-table" doc="Display binding table"/>
        <param name="[POINT_CODE]" doc="Destination Point Code"/>
        <param name="[all-matches]" doc="Display all matching Combination Links"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; route-lookup POINT_CODE from POINT_CODE sls &lt;0-15&gt; [list-asps]">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="route-lookup" doc="Look up route"/>
        <param name="POINT_CODE" doc="Destination PC"/>
        <param name="from" doc="From"/>
        <param name="POINT_CODE" doc="Origin PC"/>
        <param name="sls" doc="SLS"/>
        <param name="&lt;0-15&gt;" doc="SLS value"/>
        <param name="[list-asps]" doc="List ASPs of the AS if route points to an AS"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp addressbook">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="addressbook" doc="List all SCCP addressbook entries"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp users">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="users" doc="Show List of SCCP Users registered"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp ssn &lt;0-65535&gt;">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="ssn" doc="Find an SCCP User registered for the given SSN"/>
        <param name="&lt;0-65535&gt;" doc="Subsystem Number (SSN)"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp connections">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="connections" doc="Show List of active SCCP connections"/>
      </params>
    </command>
    <command id="show cs7 instance &lt;0-15&gt; sccp timers">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="An instance of the SS7 stack"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
        <param name="sccp" doc="Signaling Connection Control Part"/>
        <param name="timers" doc="Show List of SCCP timers"/>
      </params>
    </command>
    <command id="show cpu-sched threads">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="cpu-sched" doc="Show Sched section information"/>
        <param name="threads" doc="Show information about running threads)"/>
      </params>
    </command>
    <command id="show fsm NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm" doc="Show information about finite state machines"/>
        <param name="NAME" doc="Display information about a single named finite state machine"/>
      </params>
    </command>
    <command id="show fsm all">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm" doc="Show information about finite state machines"/>
        <param name="all" doc="Display a list of all registered finite state machines"/>
      </params>
    </command>
    <command id="show fsm-state-graph NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-state-graph" doc="Generate a state transition graph (using DOT language)"/>
        <param name="NAME" doc="FSM name"/>
      </params>
    </command>
    <command id="show fsm-instances NAME">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-instances" doc="Show information about finite state machine instances"/>
        <param name="NAME" doc="Display a list of all FSM instances of the named finite state machine"/>
      </params>
    </command>
    <command id="show fsm-instances all">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="fsm-instances" doc="Show information about finite state machine instances"/>
        <param name="all" doc="Display a list of all FSM instances of all finite state machine"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH)">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH) tree ADDRESS">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
        <param name="tree" doc="Display only a specific memory chunk"/>
        <param name="ADDRESS" doc="Chunk address (e.g. 0xdeadbeef)"/>
      </params>
    </command>
    <command id="show talloc-context (application|global|all) (full|brief|DEPTH) filter REGEXP">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="talloc-context" doc="Show talloc memory hierarchy"/>
        <param name="application" doc="Application's context"/>
        <param name="global" doc="Global context (OTC_GLOBAL)"/>
        <param name="all" doc="All contexts, if NULL-context tracking is enabled"/>
        <param name="full" doc="Display a full talloc memory hierarchy"/>
        <param name="brief" doc="Display a brief talloc memory hierarchy"/>
        <param name="DEPTH" doc="Specify required maximal depth value"/>
        <param name="filter" doc="Filter chunks using regular expression"/>
        <param name="REGEXP" doc="Regular expression"/>
      </params>
    </command>
  <description>The enable node is a privileged node, allowing to make changes
    to the configuration and to access further commands like 'configure'.
    All commands seen on the view node are also available here.</description></node>
  <node id="config">
    <name>config</name>
    <command id="hostname WORD">
      <params>
        <param name="hostname" doc="Set system's network name"/>
        <param name="WORD" doc="This system's network name"/>
      </params>
    </command>
    <command id="no hostname [HOSTNAME]">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="hostname" doc="Reset system's network name"/>
        <param name="[HOSTNAME]" doc="Host name of this router"/>
      </params>
    </command>
    <command id="password (8|) WORD">
      <params>
        <param name="password" doc="Assign the terminal connection password"/>
        <param name="8" doc="Specifies a HIDDEN password will follow"/>
        <param name="" doc="dummy string "/>
        <param name="WORD" doc="The HIDDEN line password string"/>
      </params>
    </command>
    <command id="password LINE">
      <params>
        <param name="password" doc="Assign the terminal connection password"/>
        <param name="LINE" doc="The UNENCRYPTED (cleartext) line password"/>
      </params>
    </command>
    <command id="enable password (8|) WORD">
      <params>
        <param name="enable" doc="Modify enable password parameters"/>
        <param name="password" doc="Assign the privileged level password"/>
        <param name="8" doc="Specifies a HIDDEN password will follow"/>
        <param name="" doc="dummy string "/>
        <param name="WORD" doc="The HIDDEN 'enable' password string"/>
      </params>
    </command>
    <command id="enable password LINE">
      <params>
        <param name="enable" doc="Modify enable password parameters"/>
        <param name="password" doc="Assign the privileged level password"/>
        <param name="LINE" doc="The UNENCRYPTED (cleartext) 'enable' password"/>
      </params>
    </command>
    <command id="no enable password">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="enable" doc="Modify enable password parameters"/>
        <param name="password" doc="Assign the privileged level password"/>
      </params>
    </command>
    <command id="banner motd default">
      <params>
        <param name="banner" doc="Set banner string"/>
        <param name="motd" doc="Strings for motd"/>
        <param name="default" doc="Default string"/>
      </params>
    </command>
    <command id="banner motd file [FILE]">
      <params>
        <param name="banner" doc="Set banner"/>
        <param name="motd" doc="Banner for motd"/>
        <param name="file" doc="Banner from a file"/>
        <param name="[FILE]" doc="Filename"/>
      </params>
    </command>
    <command id="no banner motd">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="banner" doc="Set banner string"/>
        <param name="motd" doc="Strings for motd"/>
      </params>
    </command>
    <command id="service terminal-length &lt;0-512&gt;">
      <params>
        <param name="service" doc="Set up miscellaneous service"/>
        <param name="terminal-length" doc="System wide terminal length configuration"/>
        <param name="&lt;0-512&gt;" doc="Number of lines of VTY (0 means no line control)"/>
      </params>
    </command>
    <command id="no service terminal-length [&lt;0-512&gt;]">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="service" doc="Set up miscellaneous service"/>
        <param name="terminal-length" doc="System wide terminal length configuration"/>
        <param name="[&lt;0-512&gt;]" doc="Number of lines of VTY (0 means no line control)"/>
      </params>
    </command>
    <command id="line vty">
      <params>
        <param name="line" doc="Configure a terminal line"/>
        <param name="vty" doc="Virtual terminal"/>
      </params>
    </command>
    <command id="service advanced-vty">
      <params>
        <param name="service" doc="Set up miscellaneous service"/>
        <param name="advanced-vty" doc="Enable advanced mode vty interface"/>
      </params>
    </command>
    <command id="no service advanced-vty">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="service" doc="Set up miscellaneous service"/>
        <param name="advanced-vty" doc="Enable advanced mode vty interface"/>
      </params>
    </command>
    <command id="show history">
      <params>
        <param name="show" doc="Show running system information"/>
        <param name="history" doc="Display the session command history"/>
      </params>
    </command>
    <command id="log stderr [blocking-io]">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="stderr" doc="Logging via STDERR of the process"/>
        <param name="[blocking-io]" doc="Use blocking, synchronous I/O"/>
      </params>
    </command>
    <command id="no log stderr">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="stderr" doc="Logging via STDERR of the process"/>
      </params>
    </command>
    <command id="log file FILENAME [blocking-io]">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="file" doc="Logging to text file"/>
        <param name="FILENAME" doc="Filename"/>
        <param name="[blocking-io]" doc="Use blocking, synchronous I/O"/>
      </params>
    </command>
    <command id="no log file FILENAME">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="file" doc="Logging to text file"/>
        <param name="FILENAME" doc="Filename"/>
      </params>
    </command>
    <command id="log alarms &lt;2-32700&gt;">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="alarms" doc="Logging alarms to osmo_strrb"/>
        <param name="&lt;2-32700&gt;" doc="Maximum number of messages to log"/>
      </params>
    </command>
    <command id="no log alarms">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="alarms" doc="Logging alarms to osmo_strrb"/>
      </params>
    </command>
    <command id="log syslog (authpriv|cron|daemon|ftp|lpr|mail|news|user|uucp)">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="syslog" doc="Logging via syslog"/>
        <param name="authpriv" doc="Security/authorization messages facility"/>
        <param name="cron" doc="Clock daemon (cron/at) facility"/>
        <param name="daemon" doc="General system daemon facility"/>
        <param name="ftp" doc="Ftp daemon facility"/>
        <param name="lpr" doc="Line printer facility"/>
        <param name="mail" doc="Mail facility"/>
        <param name="news" doc="News facility"/>
        <param name="user" doc="Generic facility"/>
        <param name="uucp" doc="UUCP facility"/>
      </params>
    </command>
    <command id="log syslog local &lt;0-7&gt;">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="syslog" doc="Logging via syslog"/>
        <param name="local" doc="Syslog LOCAL facility"/>
        <param name="&lt;0-7&gt;" doc="Local facility number"/>
      </params>
    </command>
    <command id="no log syslog">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="syslog" doc="Logging via syslog"/>
      </params>
    </command>
    <command id="log systemd-journal [raw]">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="systemd-journal" doc="Logging to systemd-journal"/>
        <param name="[raw]" doc="Offload rendering of the meta information (location, category) to systemd"/>
      </params>
    </command>
    <command id="no log systemd-journal">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="systemd-journal" doc="Logging to systemd-journal"/>
      </params>
    </command>
    <command id="log gsmtap [HOSTNAME]">
      <params>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="gsmtap" doc="Logging via GSMTAP"/>
        <param name="[HOSTNAME]" doc="Host name to send the GSMTAP logging to (UDP port 4729)"/>
      </params>
    </command>
    <command id="no log gsmtap [HOSTNAME]">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="log" doc="Configure logging sub-system"/>
        <param name="gsmtap" doc="Logging via GSMTAP"/>
        <param name="[HOSTNAME]" doc="Host name to send the GSMTAP logging to (UDP port 4729)"/>
      </params>
    </command>
    <command id="stats reporter statsd [NAME]">
      <params>
        <param name="stats" doc="Configure stats sub-system"/>
        <param name="reporter" doc="Configure a stats reporter"/>
        <param name="statsd" doc="Report to a STATSD server"/>
        <param name="[NAME]" doc="Name of the reporter"/>
      </params>
    </command>
    <command id="no stats reporter statsd [NAME]">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="stats" doc="Configure stats sub-system"/>
        <param name="reporter" doc="Configure a stats reporter"/>
        <param name="statsd" doc="Report to a STATSD server"/>
        <param name="[NAME]" doc="Name of the reporter"/>
      </params>
    </command>
    <command id="stats reporter log [NAME]">
      <params>
        <param name="stats" doc="Configure stats sub-system"/>
        <param name="reporter" doc="Configure a stats reporter"/>
        <param name="log" doc="Report to the logger"/>
        <param name="[NAME]" doc="Name of the reporter"/>
      </params>
    </command>
    <command id="no stats reporter log [NAME]">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="stats" doc="Configure stats sub-system"/>
        <param name="reporter" doc="Configure a stats reporter"/>
        <param name="log" doc="Report to the logger"/>
        <param name="[NAME]" doc="Name of the reporter"/>
      </params>
    </command>
    <command id="stats interval &lt;0-65535&gt;">
      <params>
        <param name="stats" doc="Configure stats sub-system"/>
        <param name="interval" doc="Set the reporting interval"/>
        <param name="&lt;0-65535&gt;" doc="Interval in seconds (0 disables the reporting interval)"/>
      </params>
    </command>
    <command id="stats-tcp interval &lt;0-65535&gt;">
      <params>
        <param name="stats-tcp" doc="Configure stats sub-system"/>
        <param name="interval" doc="Set the tcp socket stats polling interval"/>
        <param name="&lt;0-65535&gt;" doc="Interval in seconds (0 disables the polling interval)"/>
      </params>
    </command>
    <command id="stats-tcp batch-size &lt;1-65535&gt;">
      <params>
        <param name="stats-tcp" doc="Configure stats sub-system"/>
        <param name="batch-size" doc="Set the number of tcp sockets that are processed per stats polling interval"/>
        <param name="&lt;1-65535&gt;" doc="Number of sockets per interval"/>
      </params>
    </command>
    <command id="cs7 instance &lt;0-15&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="cs7" doc="ITU-T Signaling System 7"/>
        <param name="instance" doc="Configure a SS7 Instance"/>
        <param name="&lt;0-15&gt;" doc="An instance of the SS7 stack"/>
      </params>
    </command>
    <command id="cpu-sched">
      <params>
        <param name="cpu-sched" doc="Configure CPU Scheduler related settings"/>
      </params>
    </command>
  <description>The config node is the root for all configuration commands,
    which are identical to the config file format. Changes made on the telnet
    VTY can be made persistent with the 'write file' command.</description></node>
  <node id="config-log">
    <name>config-log</name>
    <command id="logging filter all (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="filter" doc="Filter log messages"/>
        <param name="all" doc="Do you want to log all messages?"/>
        <param name="0" doc="Only print messages matched by other filters"/>
        <param name="1" doc="Bypass filter and print all messages"/>
      </params>
    <description>Disable/enable general log output on a given target.
      Typically, 'logging filter all 1' allows to see the usual log output on a
      given target. Setting to '0' can be useful when logging to the telnet VTY
      console: mute all log output to allow typing VTY commands on the telnet
      prompt without interference from log output; 'logging filter all 1' then
      re-enables logging in the same log output configuration as before.

      Some applications provide more specific filters, e.g. to log a given IMSI
      only. To employ such filters, set 'logging filter all 0' to disable
      general logging, and then enable a more specific filter instead.
      </description></command>
    <command id="logging color (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="color" doc="Configure color-printing for log messages"/>
        <param name="0" doc="Don't use color for printing messages"/>
        <param name="1" doc="Use color for printing messages"/>
      </params>
    </command>
    <command id="logging timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp"/>
      </params>
    </command>
    <command id="logging print extended-timestamp (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="extended-timestamp" doc="Configure log message timestamping"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current timestamp with YYYYMMDDhhmmssnnn"/>
      </params>
    </command>
    <command id="logging print thread-id (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="thread-id" doc="Configure log message logging Thread ID"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with current Thread ID"/>
      </params>
    </command>
    <command id="logging print category (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem name"/>
      </params>
    </command>
    <command id="logging print category-hex (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="category-hex" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with category/subsystem nr in hex ('&lt;000b&gt;')"/>
      </params>
    </command>
    <command id="logging print level (0|1)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="level" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the log level name"/>
      </params>
    </command>
    <command id="logging print file (0|1|basename) [last]">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="print" doc="Log output settings"/>
        <param name="file" doc="Configure log message"/>
        <param name="0" doc="Don't prefix each log message"/>
        <param name="1" doc="Prefix each log message with the source file and line"/>
        <param name="basename" doc="Prefix each log message with the source file's basename (strip leading paths) and line"/>
        <param name="[last]" doc="Log source file info at the end of a log line. If omitted, log source file info just before the log text."/>
      </params>
    </command>
    <command id="logging level (lglobal|llapd|linp|lmux|lmi|lmib|lsms|lctrl|lgtp|lstats|lgsup|loap|lss7|lsccp|lsua|lm3ua|lmgcp|ljibuf|lrspro|lns|lbssgp|lnsdata|lnssignal|liuup|lpfcp|lcsn1|lio) (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="lglobal" doc="Library-internal global log family"/>
        <param name="llapd" doc="LAPD in libosmogsm"/>
        <param name="linp" doc="A-bis Intput Subsystem"/>
        <param name="lmux" doc="A-bis B-Subchannel TRAU Frame Multiplex"/>
        <param name="lmi" doc="A-bis Input Driver for Signalling"/>
        <param name="lmib" doc="A-bis Input Driver for B-Channels (voice)"/>
        <param name="lsms" doc="Layer3 Short Message Service (SMS)"/>
        <param name="lctrl" doc="Control Interface"/>
        <param name="lgtp" doc="GPRS GTP library"/>
        <param name="lstats" doc="Statistics messages and logging"/>
        <param name="lgsup" doc="Generic Subscriber Update Protocol"/>
        <param name="loap" doc="Osmocom Authentication Protocol"/>
        <param name="lss7" doc="libosmo-sigtran Signalling System 7"/>
        <param name="lsccp" doc="libosmo-sigtran SCCP Implementation"/>
        <param name="lsua" doc="libosmo-sigtran SCCP User Adaptation"/>
        <param name="lm3ua" doc="libosmo-sigtran MTP3 User Adaptation"/>
        <param name="lmgcp" doc="libosmo-mgcp Media Gateway Control Protocol"/>
        <param name="ljibuf" doc="libosmo-netif Jitter Buffer"/>
        <param name="lrspro" doc="Remote SIM protocol"/>
        <param name="lns" doc="GPRS NS layer"/>
        <param name="lbssgp" doc="GPRS BSSGP layer"/>
        <param name="lnsdata" doc="GPRS NS layer data PDU"/>
        <param name="lnssignal" doc="GPRS NS layer signal PDU"/>
        <param name="liuup" doc="Iu UP layer"/>
        <param name="lpfcp" doc="libosmo-pfcp Packet Forwarding Control Protocol"/>
        <param name="lcsn1" doc="libosmo-csn1 Concrete Syntax Notation 1 codec"/>
        <param name="lio" doc="libosmocore IO Subsystem"/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level set-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="set-all" doc="Once-off set all categories to the given log level. There is no single command to take back these changes -- each category is set to the given level, period."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="logging level force-all (debug|info|notice|error|fatal)">
      <params>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Globally force all logging categories to a specific level. This is released by the 'no logging level force-all' command. Note: any 'logging level &lt;category&gt; &lt;level&gt;' commands will have no visible effect after this, until the forced level is released."/>
        <param name="debug" doc="Log debug messages and higher levels"/>
        <param name="info" doc="Log informational messages and higher levels"/>
        <param name="notice" doc="Log noticeable messages and higher levels"/>
        <param name="error" doc="Log error messages and higher levels"/>
        <param name="fatal" doc="Log only fatal messages"/>
      </params>
    </command>
    <command id="no logging level force-all">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="logging" doc="Configure logging"/>
        <param name="level" doc="Set the log level for a specified category"/>
        <param name="force-all" doc="Release any globally forced log level set with 'logging level force-all &lt;level&gt;'"/>
      </params>
    </command>
  <child_of nodeid="config"/><description>The log node is commonly available in all Osmocom programs and
    allows configuring logging to stderr and/or log files, including logging
    category and level filtering as well as output formatting options.
    Note that the 'logging enable' command is required to make logging commands
    available on the telnet VTY.</description></node>
  <node id="config-stats">
    <name>config-stats</name>
    <command id="local-ip ADDR">
      <params>
        <param name="local-ip" doc="Set the IP address to which we bind locally"/>
        <param name="ADDR" doc="IP Address"/>
      </params>
    </command>
    <command id="no local-ip">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="local-ip" doc="Set the IP address to which we bind locally"/>
      </params>
    </command>
    <command id="remote-ip ADDR">
      <params>
        <param name="remote-ip" doc="Set the remote IP address to which we connect"/>
        <param name="ADDR" doc="IP Address"/>
      </params>
    </command>
    <command id="remote-port &lt;1-65535&gt;">
      <params>
        <param name="remote-port" doc="Set the remote port to which we connect"/>
        <param name="&lt;1-65535&gt;" doc="Remote port number"/>
      </params>
    </command>
    <command id="mtu &lt;100-65535&gt;">
      <params>
        <param name="mtu" doc="Set the maximum packet size"/>
        <param name="&lt;100-65535&gt;" doc="Size in byte"/>
      </params>
    </command>
    <command id="no mtu">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="mtu" doc="Set the maximum packet size"/>
      </params>
    </command>
    <command id="prefix PREFIX">
      <params>
        <param name="prefix" doc="Set the item name prefix"/>
        <param name="PREFIX" doc="The prefix string"/>
      </params>
    </command>
    <command id="no prefix">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="prefix" doc="Set the item name prefix"/>
      </params>
    </command>
    <command id="level (global|peer|subscriber)">
      <params>
        <param name="level" doc="Set the maximum group level"/>
        <param name="global" doc="Report global groups only"/>
        <param name="peer" doc="Report global and network peer related groups"/>
        <param name="subscriber" doc="Report global, peer, and subscriber groups"/>
      </params>
    </command>
    <command id="enable">
      <params>
        <param name="enable" doc="Enable the reporter"/>
      </params>
    </command>
    <command id="disable">
      <params>
        <param name="disable" doc="Disable the reporter"/>
      </params>
    </command>
    <command id="flush-period &lt;0-65535&gt;">
      <params>
        <param name="flush-period" doc="Configure stats sub-system"/>
        <param name="&lt;0-65535&gt;" doc="Send all stats even if they have not changed (i.e. force the flush)every N-th reporting interval. Set to 0 to disable regular flush (default)."/>
      </params>
    </command>
  </node>
  <node id="config-line">
    <name>config-line</name>
    <command id="login">
      <params>
        <param name="login" doc="Enable password checking"/>
      </params>
    </command>
    <command id="no login">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="login" doc="Enable password checking"/>
      </params>
    </command>
    <command id="bind A.B.C.D [&lt;0-65535&gt;]">
      <params>
        <param name="bind" doc="Accept VTY telnet connections on local interface"/>
        <param name="A.B.C.D" doc="Local interface IP address (default: 127.0.0.1)"/>
        <param name="[&lt;0-65535&gt;]" doc="Local TCP port number"/>
      </params>
    </command>
  </node>
  <node id="config-cs7">
    <name>config-cs7</name>
    <command id="description .TEXT">
      <params>
        <param name="description" doc="Save human-readable description of the object"/>
        <param name=".TEXT" doc="Text until the end of the line"/>
      </params>
    </command>
    <command id="network-indicator (international | national | reserved | spare)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="network-indicator" doc="Configure the Network Indicator"/>
        <param name="international" doc="International Network"/>
        <param name="national" doc="National Network"/>
        <param name="reserved" doc="Reserved Network"/>
        <param name="spare" doc="Spare Network"/>
      </params>
    </command>
    <command id="point-code POINT_CODE">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Configure the local Point Code"/>
        <param name="POINT_CODE" doc="Point Code"/>
      </params>
    </command>
    <command id="secondary-pc POINT_CODE">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="secondary-pc" doc="Configure the local Secondary Point Code"/>
        <param name="POINT_CODE" doc="Point Code"/>
      </params>
    </command>
    <command id="point-code format &lt;1-24&gt; [&lt;1-23&gt;] [&lt;1-22&gt;]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Point Code"/>
        <param name="format" doc="Configure Point Code Format"/>
        <param name="&lt;1-24&gt;" doc="Length of first PC component"/>
        <param name="[&lt;1-23&gt;]" doc="Length of second PC component"/>
        <param name="[&lt;1-22&gt;]" doc="Length of third PC component"/>
      </params>
    </command>
    <command id="point-code format default">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Point Code"/>
        <param name="format" doc="Configure Point Code Format"/>
        <param name="default" doc="Default Point Code Format (3.8.3)"/>
      </params>
    </command>
    <command id="point-code delimiter (default|dash)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Point Code"/>
        <param name="delimiter" doc="Configure Point Code Delimiter"/>
        <param name="default" doc="Use dot as delimiter"/>
        <param name="dash" doc="User dash as delimiter"/>
      </params>
    </command>
    <command id="xua rkm routing-key-allocation (static-only|dynamic-permitted)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="xua" doc="SIGTRAN xxxUA related"/>
        <param name="rkm" doc="Routing Key Management"/>
        <param name="routing-key-allocation" doc="Routing Key Management Allocation Policy"/>
        <param name="static-only" doc="Only static (pre-configured) Routing Keys permitted"/>
        <param name="dynamic-permitted" doc="Dynamically allocate Routing Keys for what ASPs request"/>
      </params>
    </command>
    <command id="sls-opc-dpc [opc-shift] [&lt;0-8&gt;] [dpc-shift] [&lt;0-8&gt;]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sls-opc-dpc" doc="Shift OPC and DPC bits used during routing decision"/>
        <param name="[opc-shift]" doc="Shift OPC bits used during routing decision"/>
        <param name="[&lt;0-8&gt;]" doc="How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used"/>
        <param name="[dpc-shift]" doc="Shift DPC bits used during routing decision"/>
        <param name="[&lt;0-8&gt;]" doc="How many bits from ITU DPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used"/>
      </params>
    </command>
    <command id="sls-shift &lt;0-6&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sls-shift" doc="Shift SLS bits used during routing decision"/>
        <param name="&lt;0-6&gt;" doc="How many bits from derivated 7-bit extended-SLS (OPC, DPC, SLS) field (starting from least-significant-bit) to skip"/>
      </params>
    </command>
    <command id="asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="asp" doc="Configure Application Server Process"/>
        <param name="NAME" doc="Name of ASP"/>
        <param name="&lt;0-65535&gt;" doc="Remote port number"/>
        <param name="&lt;0-65535&gt;" doc="Local port number"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
      </params>
    </command>
    <command id="asp NAME &lt;0-65535&gt; &lt;0-65535&gt; (sua|m3ua|ipa) (sctp|tcp)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="asp" doc="Configure Application Server Process"/>
        <param name="NAME" doc="Name of ASP"/>
        <param name="&lt;0-65535&gt;" doc="Remote port number"/>
        <param name="&lt;0-65535&gt;" doc="Local port number"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="sctp" doc="SCTP (Stream Control Transmission Protocol)"/>
        <param name="tcp" doc="TCP (Transmission Control Protocol)"/>
      </params>
    </command>
    <command id="no asp NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="asp" doc="Disable Application Server Process"/>
        <param name="NAME" doc="Name of ASP"/>
      </params>
    </command>
    <command id="as NAME (sua|m3ua|ipa)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="as" doc="Configure an Application Server"/>
        <param name="NAME" doc="Name of the Application Server"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
      </params>
    </command>
    <command id="no as NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="as" doc="Disable Application Server"/>
        <param name="NAME" doc="Name of AS"/>
      </params>
    </command>
    <command id="sccp-address NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sccp-address" doc="Create/Modify an SCCP addressbook entry"/>
        <param name="NAME" doc="Name of the SCCP Address"/>
      </params>
    </command>
    <command id="no sccp-address NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="sccp-address" doc="Delete an SCCP addressbook entry"/>
        <param name="NAME" doc="Name of the SCCP Address"/>
      </params>
    </command>
    <command id="route-table system">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="route-table" doc="Specify the name of the route table"/>
        <param name="system" doc="Name of the route table"/>
      </params>
    </command>
    <command id="listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="listen" doc="Configure/Enable xUA Listener"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="&lt;0-65534&gt;" doc="Port number"/>
        <param name="[sctp]" doc="SCTP (Stream Control Transmission Protocol)"/>
        <param name="[tcp]" doc="TCP (Transmission Control Protocol)"/>
      </params>
    </command>
    <command id="no listen (sua|m3ua|ipa) &lt;0-65534&gt; [(sctp|tcp)]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="listen" doc="Disable xUA Listener on given port"/>
        <param name="sua" doc="SCCP User Adaptation"/>
        <param name="m3ua" doc="MTP3 User Adaptation"/>
        <param name="ipa" doc="IPA Multiplex (SCCP Lite)"/>
        <param name="&lt;0-65534&gt;" doc="Port number"/>
        <param name="[sctp]" doc="SCTP (Stream Control Transmission Protocol)"/>
        <param name="[tcp]" doc="TCP (Transmission Control Protocol)"/>
      </params>
    </command>
    <command id="sccp-timer (conn_est|ias|iar|rel|repeat_rel|int|guard|reset|reassembly) &lt;1-999999&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sccp-timer" doc="Configure SCCP timer values, see ITU-T Q.714"/>
        <param name="conn_est" doc="Waiting for connection confirm message, 1 to 2 minutes (default: 60)"/>
        <param name="ias" doc="Send keep-alive: on an idle connection, delay before sending an Idle Timer message, 5 to 10 minutes (default: 420)"/>
        <param name="iar" doc="Receive keep-alive: on an idle connection, delay until considering a connection as stale, 11 to 21 minutes (default: 900)"/>
        <param name="rel" doc="Waiting for release complete message, 10 to 20 seconds (default: 10)"/>
        <param name="repeat_rel" doc="Waiting for release complete message; or to repeat sending released message after the initial expiry, 10 to 20 seconds (default: 10)"/>
        <param name="int" doc="Waiting for release complete message; or to release connection resources, freeze the LRN and alert a maintenance function after the initial expiry, extending to 1 minute (default: 60)"/>
        <param name="guard" doc="Waiting to resume normal procedure for temporary connection sections during the restart procedure, 23 to 25 minutes (default: 1380)"/>
        <param name="reset" doc="Waiting to release temporary connection section or alert maintenance function after reset request message is sent, 10 to 20 seconds (default: 10)"/>
        <param name="reassembly" doc="Waiting to receive all the segments of the remaining segments, single segmented message after receiving the first segment, 10 to 20 seconds (default: 10)"/>
        <param name="&lt;1-999999&gt;" doc="Timer value, in seconds"/>
      </params>
    </command>
    <command id="sccp max-optional-data (&lt;0-999999&gt;|standard)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sccp" doc="Configure SCCP behavior"/>
        <param name="max-optional-data" doc="Adjust the upper bound for the optional data length (the payload) for CR, CC, CREF and RLSD messages. For any Optional Data part larger than this value in octets, send CR, CC, CREF and RLSD messages without any payload, and send the data payload in a separate Data Form 1 message. ITU-T Q.713 sections 4.2 thru 4.5 define a limit of 128 bytes for the 'Data' parameter. This limit can be adjusted here. May be useful for interop with nonstandard SCCP peers."/>
        <param name="&lt;0-999999&gt;" doc="Set a non-standard maximum allowed number of bytes"/>
        <param name="standard" doc="Use the ITU-T Q.713 4.2 to 4.5 standard value of 128"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-as">
    <name>config-cs7-as</name>
    <command id="description .TEXT">
      <params>
        <param name="description" doc="Save human-readable description of the object"/>
        <param name=".TEXT" doc="Text until the end of the line"/>
      </params>
    </command>
    <command id="asp NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="asp" doc="Specify that a given ASP is part of this AS"/>
        <param name="NAME" doc="Name of ASP to be added to AS"/>
      </params>
    </command>
    <command id="no asp NAME">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="asp" doc="Specify ASP to be removed from this AS"/>
        <param name="NAME" doc="Name of ASP to be removed"/>
      </params>
    </command>
    <command id="traffic-mode (broadcast | roundrobin | override)">
      <params>
        <param name="traffic-mode" doc="Specifies traffic mode of operation of the ASP within the AS"/>
        <param name="broadcast" doc="Broadcast to all ASP within AS"/>
        <param name="roundrobin" doc="Round-Robin between all ASP within AS"/>
        <param name="override" doc="Override"/>
      </params>
    </command>
    <command id="traffic-mode (loadshare|loadshare-tcap) [bindings] [sls] [opc-sls] [opc-shift] [&lt;0-2&gt;]">
      <params>
        <param name="traffic-mode" doc="Specifies traffic mode of operation of the ASP within the AS"/>
        <param name="loadshare" doc="Share Load among all ASP within AS"/>
        <param name="loadshare-tcap" doc="Share Load among all ASP within AS (TCAP)"/>
        <param name="[bindings]" doc="Configure Loadshare parameters"/>
        <param name="[sls]" doc="Configure Loadshare SLS generation parameters"/>
        <param name="[opc-sls]" doc="Generate extended SLS with OPC information"/>
        <param name="[opc-shift]" doc="Shift OPC bits used during routing decision"/>
        <param name="[&lt;0-2&gt;]" doc="How many bits from ITU OPC field (starting from least-significant-bit) to skip (default=0). 6 bits are always used"/>
      </params>
    </command>
    <command id="no traffic-mode">
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="traffic-mode" doc="Remove explicit traffic mode of operation of this AS"/>
      </params>
    </command>
    <command id="sls-shift &lt;0-3&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="sls-shift" doc="Shift SLS bits used during routing decision"/>
        <param name="&lt;0-3&gt;" doc="How many bits from SLS field (starting from least-significant-bit) to skip"/>
      </params>
    </command>
    <command id="binding-table reset">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="binding-table" doc="AS Loadshare binding table operations"/>
        <param name="reset" doc="Reset loadshare binding table"/>
      </params>
    </command>
    <command id="recovery-timeout &lt;1-2000&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="recovery-timeout" doc="Specifies RFC4666 recovery timer T(r) timeout"/>
        <param name="&lt;1-2000&gt;" doc="Recovery Timeout in Milliseconds"/>
      </params>
    </command>
    <command id="qos-class &lt;0-7&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="qos-class" doc="Specity QoS Class of AS"/>
        <param name="&lt;0-7&gt;" doc="QoS Class"/>
      </params>
    </command>
    <command id="routing-key RCONTEXT DPC">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="routing-key" doc="Define a routing key"/>
        <param name="RCONTEXT" doc="Routing context number"/>
        <param name="DPC" doc="Destination Point Code"/>
      </params>
    </command>
    <command id="routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="routing-key" doc="Define a routing key"/>
        <param name="RCONTEXT" doc="Routing context number"/>
        <param name="DPC" doc="Destination Point Code"/>
        <param name="si" doc="Match on Service Indicator"/>
        <param name="aal2" doc="ATM Adaption Layer 2"/>
        <param name="bicc" doc="Bearer Independent Call Control"/>
        <param name="b-isup" doc="Broadband ISDN User Part"/>
        <param name="h248" doc="H.248"/>
        <param name="isup" doc="ISDN User Part"/>
        <param name="sat-isup" doc="Sattelite ISDN User Part"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="tup" doc="Telephony User Part"/>
      </params>
    </command>
    <command id="routing-key RCONTEXT DPC ssn SSN">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="routing-key" doc="Define a routing key"/>
        <param name="RCONTEXT" doc="Routing context number"/>
        <param name="DPC" doc="Destination Point Code"/>
        <param name="ssn" doc="Match on Sub-System Number"/>
        <param name="SSN" doc="Sub-System Number to match on"/>
      </params>
    </command>
    <command id="routing-key RCONTEXT DPC si (aal2|bicc|b-isup|h248|isup|sat-isup|sccp|tup) ssn SSN">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="routing-key" doc="Define a routing key"/>
        <param name="RCONTEXT" doc="Routing context number"/>
        <param name="DPC" doc="Destination Point Code"/>
        <param name="si" doc="Match on Service Indicator"/>
        <param name="aal2" doc="ATM Adaption Layer 2"/>
        <param name="bicc" doc="Bearer Independent Call Control"/>
        <param name="b-isup" doc="Broadband ISDN User Part"/>
        <param name="h248" doc="H.248"/>
        <param name="isup" doc="ISDN User Part"/>
        <param name="sat-isup" doc="Sattelite ISDN User Part"/>
        <param name="sccp" doc="Signalling Connection Control Part"/>
        <param name="tup" doc="Telephony User Part"/>
        <param name="ssn" doc="Match on Sub-System Number"/>
        <param name="SSN" doc="Sub-System Number to match on"/>
      </params>
    </command>
    <command id="point-code override (opc|dpc) PC">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Point Code Specific Features"/>
        <param name="override" doc="Override (force) a point-code of messages received at the AS"/>
        <param name="opc" doc="Override Source Point Code of received messages"/>
        <param name="dpc" doc="Override Destination Point Code of received messages"/>
        <param name="PC" doc="New Point Code"/>
      </params>
    </command>
    <command id="no point-code override (opc|dpc)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="point-code" doc="Point Code Specific Features"/>
        <param name="override" doc="Override (force) a point-code of messages received at the AS"/>
        <param name="opc" doc="Override Source Point Code of received messages"/>
        <param name="dpc" doc="Override Destination Point Code of received messages"/>
      </params>
    </command>
    <command id="point-code override patch-sccp (disabled|both)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Point Code Specific Features"/>
        <param name="override" doc="Override (force) a point-code to hard-coded value"/>
        <param name="patch-sccp" doc="Patch point code values into SCCP called/calling address"/>
        <param name="disabled" doc="Don't patch any point codes into SCCP called/calling address"/>
        <param name="both" doc="Patch both origin and destination point codes into SCCP called/calling address"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-asp">
    <name>config-cs7-asp</name>
    <command id="description .TEXT">
      <params>
        <param name="description" doc="Save human-readable description of the object"/>
        <param name=".TEXT" doc="Text until the end of the line"/>
      </params>
    </command>
    <command id="remote-ip (A.B.C.D|X:X::X:X) [primary]">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="remote-ip" doc="Specify Remote IP Address of ASP"/>
        <param name="A.B.C.D" doc="Remote IPv4 Address of ASP"/>
        <param name="X:X::X:X" doc="Remote IPv6 Address of ASP"/>
        <param name="[primary]" doc="Set remote address as SCTP Primary Address"/>
      </params>
    </command>
    <command id="no remote-ip (A.B.C.D|X:X::X:X)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="remote-ip" doc="Specify Remote IP Address of ASP"/>
        <param name="A.B.C.D" doc="Remote IPv4 Address of ASP"/>
        <param name="X:X::X:X" doc="Remote IPv6 Address of ASP"/>
      </params>
    </command>
    <command id="local-ip (A.B.C.D|X:X::X:X) [primary]">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="local-ip" doc="Specify Local IP Address from which to contact ASP"/>
        <param name="A.B.C.D" doc="Local IPv4 Address from which to contact of ASP"/>
        <param name="X:X::X:X" doc="Local IPv6 Address from which to contact of ASP"/>
        <param name="[primary]" doc="Signal the SCTP peer to use this address as Primary Address"/>
      </params>
    </command>
    <command id="no local-ip (A.B.C.D|X:X::X:X)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="local-ip" doc="Specify Local IP Address from which to contact ASP"/>
        <param name="A.B.C.D" doc="Local IPv4 Address from which to contact of ASP"/>
        <param name="X:X::X:X" doc="Local IPv6 Address from which to contact of ASP"/>
      </params>
    </command>
    <command id="qos-class &lt;0-7&gt;">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="qos-class" doc="Specify QoS Class of ASP"/>
        <param name="&lt;0-7&gt;" doc="QoS Class"/>
      </params>
    </command>
    <command id="role (sg|asp|ipsp)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="role" doc="Specify the xUA role for this ASP"/>
        <param name="sg" doc="SG (Signaling Gateway)"/>
        <param name="asp" doc="ASP (Application Server Process)"/>
        <param name="ipsp" doc="IPSP (IP Signalling Point)"/>
      </params>
    </command>
    <command id="transport-role (client|server)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="transport-role" doc="Specify the transport layer role for this ASP"/>
        <param name="client" doc="Operate as a client; connect to a server"/>
        <param name="server" doc="Operate as a server; wait for client connections"/>
      </params>
    </command>
    <command id="sctp-param init (num-ostreams|max-instreams|max-attempts|timeout) &lt;0-65535&gt;">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="sctp-param" doc="Configure SCTP parameters"/>
        <param name="init" doc="Configure INIT related parameters"/>
        <param name="num-ostreams" doc="Configure INIT Number of Outbound Streams"/>
        <param name="max-instreams" doc="Configure INIT Maximum Inboud Streams"/>
        <param name="max-attempts" doc="Configure INIT Maximum Attempts"/>
        <param name="timeout" doc="Configure INIT Timeout (milliseconds)"/>
        <param name="&lt;0-65535&gt;" doc="Value of the parameter"/>
      </params>
    </command>
    <command id="no sctp-param init (num-ostreams|max-instreams|max-attempts|timeout)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="sctp-param" doc="Configure SCTP parameters"/>
        <param name="init" doc="Configure INIT related parameters"/>
        <param name="num-ostreams" doc="Configure INIT Number of Outbound Streams"/>
        <param name="max-instreams" doc="Configure INIT Maximum Inboud Streams"/>
        <param name="max-attempts" doc="Configure INIT Maximum Attempts"/>
        <param name="timeout" doc="Configure INIT Timeout (milliseconds)"/>
      </params>
    </command>
    <command id="tcp-param keepalive enabled">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="keepalive" doc="Configure TCP keep-alive related parameters"/>
        <param name="enabled" doc="Enable TCP keep-alive"/>
      </params>
    </command>
    <command id="tcp-param keepalive (time|intvl|probes) &lt;0-65535&gt;">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="keepalive" doc="Configure TCP keep-alive related parameters"/>
        <param name="time" doc="Configure number of seconds a connection needs to be idle before beggining to send probes"/>
        <param name="intvl" doc="Configure number of seconds between probes"/>
        <param name="probes" doc="Configure max number of probes to send before giving up if no response is obtained"/>
        <param name="&lt;0-65535&gt;" doc="Value of the parameter"/>
      </params>
    </command>
    <command id="no tcp-param keepalive">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="keepalive" doc="Configure TCP keep-alive related parameters"/>
      </params>
    </command>
    <command id="no tcp-param keepalive (time|intvl|probes)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="keepalive" doc="Configure TCP keep-alive related parameters"/>
        <param name="time" doc="Configure number of seconds a connection needs to be idle before beggining to send probes"/>
        <param name="intvl" doc="Configure number of seconds between probes"/>
        <param name="probes" doc="Configure max number of probes to send before giving up if no response is obtained"/>
      </params>
    </command>
    <command id="tcp-param user-timeout &lt;0-65535&gt;">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="user-timeout" doc="Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)"/>
        <param name="&lt;0-65535&gt;" doc="Value of the parameter"/>
      </params>
    </command>
    <command id="no tcp-param user-timeout">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="tcp-param" doc="Configure TCP parameters"/>
        <param name="user-timeout" doc="Configure TCP User Timeout socket option (TCP_USER_TIMEOUT)"/>
      </params>
    </command>
    <command id="destination-audit asp-active">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="destination-audit" doc="Configure ASP Auditing (xUA DAUD)"/>
        <param name="asp-active" doc="Transmit DAUD after ASP successful activate (for remote PCs in sccp address-book)"/>
      </params>
    </command>
    <command id="no destination-audit asp-active">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="destination-audit" doc="Configure ASP Auditing (xUA DAUD)"/>
        <param name="asp-active" doc="Transmit xUA DAUD after ASP successful activate (for remote PCs in sccp address-book)"/>
      </params>
    </command>
    <command id="quirk (no_notify|daud_in_asp|snm_inactive)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="quirk" doc="Enable quirk to work around interop issues"/>
        <param name="no_notify" doc="Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP"/>
        <param name="daud_in_asp" doc="Allow Rx of DAUD in ASP role"/>
        <param name="snm_inactive" doc="Allow Rx of [S]SNM in AS-INACTIVE state"/>
      </params>
    </command>
    <command id="no quirk (no_notify|daud_in_asp|snm_inactive)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="quirk" doc="Disable quirk to work around interop issues"/>
        <param name="no_notify" doc="Peer SG doesn't send NTFY(AS-INACTIVE) after ASP-UP"/>
        <param name="daud_in_asp" doc="Allow Rx of DAUD in ASP role"/>
        <param name="snm_inactive" doc="Allow Rx of [S]SNM in AS-INACTIVE state"/>
      </params>
    </command>
    <command id="timer xua (ack|beat) &lt;1-999999&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="timer" doc="Configure ASP default timer values"/>
        <param name="xua" doc="Configure ASP default xua timer values"/>
        <param name="ack" doc="Resend ASP Up/Down/Active/Inactive after timeout waiting for ASP Up/Down/Active/Inactive ACK (ASP role)(s) (default: 2)"/>
        <param name="beat" doc="Heartbeat Timer (0 = disabled) (s) (default: 30)"/>
        <param name="&lt;1-999999&gt;" doc="Timer value, in seconds"/>
      </params>
    </command>
    <command id="timer lm (wait_asp_up|wait_notify|wait_notify_rkm|wait_rk_reg_resp) &lt;1-999999&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="timer" doc="Configure ASP default timer values"/>
        <param name="lm" doc="Configure ASP default lm timer values"/>
        <param name="wait_asp_up" doc="Restart ASP after timeout waiting for ASP UP (SG role) / ASP UP ACK (ASP role) (s) (default: 20)"/>
        <param name="wait_notify" doc="Restart ASP after timeout waiting for NOTIFY (s) (default: 2)"/>
        <param name="wait_notify_rkm" doc="Restart ASP after timeout waiting for NOTIFY after RKM registration (s) (default: 20)"/>
        <param name="wait_rk_reg_resp" doc="Restart ASP after timeout waiting for RK_REG_RESP (s) (default: 10)"/>
        <param name="&lt;1-999999&gt;" doc="Timer value, in seconds"/>
      </params>
    </command>
    <command id="block">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="block" doc="Allows a SCTP Association with ASP, but doesn't let it become active"/>
      </params>
    </command>
    <command id="shutdown">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="shutdown" doc="Terminates SCTP association; New associations will be rejected"/>
      </params>
    </command>
    <command id="no shutdown">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="shutdown" doc="Terminates SCTP association; New associations will be rejected"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-listen">
    <name>config-cs7-listen</name>
    <command id="local-ip (A.B.C.D|X:X::X:X)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="local-ip" doc="Configure the Local IP Address for xUA"/>
        <param name="A.B.C.D" doc="IPv4 Address to use for XUA"/>
        <param name="X:X::X:X" doc="IPv6 Address to use for XUA"/>
      </params>
    </command>
    <command id="no local-ip (A.B.C.D|X:X::X:X)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="local-ip" doc="Configure the Local IP Address for xUA"/>
        <param name="A.B.C.D" doc="IPv4 Address to use for XUA"/>
        <param name="X:X::X:X" doc="IPv6 Address to use for XUA"/>
      </params>
    </command>
    <command id="accept-asp-connections (pre-configured|dynamic-permitted)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="accept-asp-connections" doc="Define what kind of ASP connections to accept"/>
        <param name="pre-configured" doc="Accept only pre-configured ASPs (source IP/port)"/>
        <param name="dynamic-permitted" doc="Accept any connection and dynamically create an ASP definition"/>
      </params>
    </command>
    <command id="sctp-param init (num-ostreams|max-instreams) &lt;0-65535&gt;">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="sctp-param" doc="Configure SCTP parameters"/>
        <param name="init" doc="Configure INIT related parameters"/>
        <param name="num-ostreams" doc="Configure INIT Number of Outbound Streams"/>
        <param name="max-instreams" doc="Configure INIT Maximum Inboud Streams"/>
        <param name="&lt;0-65535&gt;" doc="Value of the parameter"/>
      </params>
    </command>
    <command id="no sctp-param init (num-ostreams|max-instreams)">
      <attributes scope="global">
        <attribute doc="This command applies on VTY node exit" flag="@"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="sctp-param" doc="Configure SCTP parameters"/>
        <param name="init" doc="Configure INIT related parameters"/>
        <param name="num-ostreams" doc="Configure INIT Number of Outbound Streams"/>
        <param name="max-instreams" doc="Configure INIT Maximum Inboud Streams"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-rt">
    <name>config-cs7-rt</name>
    <command id="description .TEXT">
      <params>
        <param name="description" doc="Save human-readable description of the object"/>
        <param name=".TEXT" doc="Text until the end of the line"/>
      </params>
    </command>
    <command id="update route POINT_CODE MASK linkset LS_NAME [priority] [(&lt;1-9&gt;|default)] [qos-class] [(&lt;0-7&gt;|default)]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="update" doc="Update the Route"/>
        <param name="route" doc="Update the Route"/>
        <param name="POINT_CODE" doc="Destination Point Code"/>
        <param name="MASK" doc="Point Code Mask"/>
        <param name="linkset" doc="Specify Destination Linkset"/>
        <param name="LS_NAME" doc="Linkset Name"/>
        <param name="[priority]" doc="Specify Priority (lower value means higher priority)"/>
        <param name="[&lt;1-9&gt;]" doc="Priority"/>
        <param name="[default]" doc="Default Priority (5)"/>
        <param name="[qos-class]" doc="Specify QoS Class"/>
        <param name="[&lt;0-7&gt;]" doc="QoS Class"/>
        <param name="[default]" doc="Default QoS Class (0)"/>
      </params>
    </command>
    <command id="remove route POINT_CODE MASK">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="remove" doc="Remove a Route"/>
        <param name="route" doc="Remove a Route"/>
        <param name="POINT_CODE" doc="Destination Point Code"/>
        <param name="MASK" doc="Point Code Mask"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-sccpaddr">
    <name>config-cs7-sccpaddr</name>
    <command id="no point-code">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="point-code" doc="Remove point-code Number"/>
      </params>
    </command>
    <command id="no subsystem-number">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="subsystem-number" doc="Remove Subsystem Number"/>
      </params>
    </command>
    <command id="no global-title">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="no" doc="Negate a command or set its defaults"/>
        <param name="global-title" doc="Remove Global Title"/>
      </params>
    </command>
    <command id="routing-indicator (GT|PC|IP)">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="routing-indicator" doc="Add Routing Indicator"/>
        <param name="GT" doc="by global-title"/>
        <param name="PC" doc="by point-code"/>
        <param name="IP" doc="by ip-address"/>
      </params>
    </command>
    <command id="point-code POINT_CODE">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="point-code" doc="Add point-code Number"/>
        <param name="POINT_CODE" doc="PC"/>
      </params>
    </command>
    <command id="subsystem-number &lt;0-4294967295&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="subsystem-number" doc="Add Subsystem Number"/>
        <param name="&lt;0-4294967295&gt;" doc="SSN"/>
      </params>
    </command>
    <command id="global-title">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="global-title" doc="Add/Modify Global Title"/>
      </params>
    </command>
  </node>
  <node id="config-cs7-sccpaddr-gt">
    <name>config-cs7-sccpaddr-gt</name>
    <command id="global-title-indicator &lt;0-15&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="global-title-indicator" doc="Set Global Title Indicator"/>
        <param name="&lt;0-15&gt;" doc="GTI"/>
      </params>
    </command>
    <command id="translation-type &lt;0-255&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="translation-type" doc="Set Global Title Translation Type"/>
        <param name="&lt;0-255&gt;" doc="TT"/>
      </params>
    </command>
    <command id="numbering-plan-indicator &lt;0-15&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="numbering-plan-indicator" doc="Set Global Title Numbering Plan Indicator"/>
        <param name="&lt;0-15&gt;" doc="NPI"/>
      </params>
    </command>
    <command id="nature-of-address-indicator &lt;0-127&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="nature-of-address-indicator" doc="Set Global Title Nature of Address Indicator"/>
        <param name="&lt;0-127&gt;" doc="NAI"/>
      </params>
    </command>
    <command id="digits DIGITS">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="digits" doc="Set Global Title Digits"/>
        <param name="DIGITS" doc="Number digits"/>
      </params>
    </command>
  </node>
  <node id="config-cpu-sched">
    <name>config-cpu-sched</name>
    <command id="policy rr &lt;1-32&gt;">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="policy" doc="Set the scheduling policy to use for the process"/>
        <param name="rr" doc="Use the SCHED_RR real-time scheduling algorithm"/>
        <param name="&lt;1-32&gt;" doc="Set the SCHED_RR real-time priority"/>
      </params>
    </command>
    <command id="cpu-affinity (self|all|&lt;0-4294967295&gt;|THREADNAME) CPUHEXMASK [delay]">
      <attributes scope="global">
        <attribute doc="This command applies immediately" flag="!"/>
      </attributes>
      <params>
        <param name="cpu-affinity" doc="Set CPU affinity mask on a (group of) thread(s)"/>
        <param name="self" doc="Set CPU affinity mask on thread running the VTY"/>
        <param name="all" doc="Set CPU affinity mask on all process' threads"/>
        <param name="&lt;0-4294967295&gt;" doc="Set CPU affinity mask on a thread with specified PID"/>
        <param name="THREADNAME" doc="Set CPU affinity mask on a thread with specified thread name"/>
        <param name="CPUHEXMASK" doc="CPU affinity mask"/>
        <param name="[delay]" doc="If set, delay applying the affinity mask now and let the app handle it at a later point"/>
      </params>
    </command>
  </node>
</vtydoc>
