(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.532)
  )
  (paper "A4")
  (title_block
    (title "icE1usb RS422 extension")
    (date "2022-08-15")
    (rev "0.1")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.018))
      (layer "dielectric 1" (type "core") (thickness 0.138) (material "FR4") (epsilon_r 4.3) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 1.13) (material "FR4") (epsilon_r 4.3) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.138) (material "FR4") (epsilon_r 4.3) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.018))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "+12VA")
  (net 4 "GNDA")
  (net 5 "+5VA")
  (net 6 "/PPS-")
  (net 7 "Net-(F1-Pad2)")
  (net 8 "Net-(F2-Pad1)")
  (net 9 "/PPS+")
  (net 10 "/RXD-")
  (net 11 "Net-(F3-Pad2)")
  (net 12 "Net-(F4-Pad1)")
  (net 13 "/RXD+")
  (net 14 "/TXD-")
  (net 15 "Net-(F5-Pad2)")
  (net 16 "Net-(F6-Pad1)")
  (net 17 "/TXD+")
  (net 18 "unconnected-(J1-Pad2)")
  (net 19 "/SCL")
  (net 20 "/PPS_IO")
  (net 21 "/SDA")
  (net 22 "/UART_RX")
  (net 23 "/UART_TX")
  (net 24 "/~{PPS_TXEN}")
  (net 25 "Net-(U1-Pad5)")
  (net 26 "Net-(U1-Pad6)")
  (net 27 "/~{PPS_RXEN}")
  (net 28 "/~{RXD_TXEN}")
  (net 29 "Net-(U2-Pad5)")
  (net 30 "Net-(U2-Pad6)")
  (net 31 "/~{RXD_RXEN}")
  (net 32 "/~{TXD_TXEN}")
  (net 33 "Net-(U3-Pad5)")
  (net 34 "Net-(U3-Pad6)")
  (net 35 "/~{TXD_RXEN}")
  (net 36 "/TXD_RO")
  (net 37 "/RXD_RO")
  (net 38 "/PPS_RO")
  (net 39 "/TXD_DI")
  (net 40 "/RXD_DI")
  (net 41 "/PPS_DI")
  (net 42 "unconnected-(U6-Pad13)")
  (net 43 "/~{PPS_RE}")
  (net 44 "/~{RXD_RE}")
  (net 45 "/RXD_DE")
  (net 46 "/~{TXD_RE}")
  (net 47 "/TXD_DE")
  (net 48 "unconnected-(U7-Pad11)")
  (net 49 "unconnected-(U7-Pad12)")
  (net 50 "unconnected-(U7-Pad13)")
  (net 51 "/PPS_DE")
  (net 52 "/SCL_ISO")
  (net 53 "/SDA_ISO")
  (net 54 "unconnected-(U6-Pad7)")
  (net 55 "unconnected-(U6-Pad6)")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.75 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/~{TXD_TXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 109.75 88.75 -90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "4u7" (at 0 1.75 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 114 80 -90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.55 90) (layer "F.SilkS") hide)
    (fp_text value "74LVC2G125" (at 0 2.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/~{PPS_TXEN}") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/PPS_IO") (pintype "input"))
    (pad "3" smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/PPS_IO") (pintype "tri_state"))
    (pad "4" smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(U3-Pad5)") (pintype "input"))
    (pad "6" smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(U3-Pad6)") (pintype "tri_state"))
    (pad "7" smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/~{PPS_RXEN}") (pintype "input"))
    (pad "8" smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 100.5 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/RXD-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(F3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.5 81.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/~{PPS_RE}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.25 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/~{PPS_RXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 103.5 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/PPS-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(F1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 130 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U12" (at 0 -3.4) (layer "F.SilkS") hide)
    (fp_text value "M24C02-FMN" (at 0 3.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E0") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E1") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E2") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "~{WC}") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.75 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/~{PPS_TXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 122.25 102.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U10" (at 0 -3.4 90) (layer "F.SilkS") hide)
    (fp_text value "SP485" (at 0 3.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/TXD_RO") (pinfunction "RO") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/~{TXD_RE}") (pinfunction "~{RE}") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/TXD_DE") (pinfunction "DE") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/TXD_DI") (pinfunction "DI") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/TXD+") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/TXD-") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104 96)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+12VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.25 101.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/RXD-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/RXD+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:TO-252-2" (layer "F.Cu")
    (tedit 5A70A390)
    (at 102.5 91 180)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U11" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "MC78M05_TO252" (at 0 4.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" smd rect (at 3.775 1.525 180) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 -1.525 180) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.425 1.525 180) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.775 -1.525 180) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.2 -2.28 180) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+12VA") (pinfunction "VI") (pintype "power_in"))
    (pad "2" smd rect (at 2.1 0 180) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 4 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -4.2 2.28 180) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5VA") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/RXD_DE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122 85 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.25 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/~{RXD_RXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 97.5 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/TXD-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(F5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 99)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(F6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/TXD+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.5 81.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 110.25 102.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at 0 -3.4 90) (layer "F.SilkS") hide)
    (fp_text value "SP485" (at 0 3.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/PPS_RO") (pinfunction "RO") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/~{PPS_RE}") (pinfunction "~{RE}") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/PPS_DE") (pinfunction "DE") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/PPS_DI") (pinfunction "DI") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/PPS+") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/PPS-") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 116.25 102.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U9" (at 0 -3.4 90) (layer "F.SilkS") hide)
    (fp_text value "SP485" (at 0 3.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/RXD_RO") (pinfunction "RO") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{RXD_RE}") (pinfunction "~{RE}") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/RXD_DE") (pinfunction "DE") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/RXD_DI") (pinfunction "DI") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/RXD+") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "/RXD-") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.25 107 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.25 107 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 105)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(F2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/PPS+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104 102)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(F4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/RXD+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 109.75 93.5 90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.75 90) (layer "F.SilkS") hide)
    (fp_text value "10u" (at 0 1.75 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.35 0 90) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 3 "+12VA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0 90) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.25 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/~{TXD_RXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/~{TXD_RE}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 121 80 -90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.55 90) (layer "F.SilkS") hide)
    (fp_text value "74LVC2G125" (at 0 2.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/~{RXD_TXEN}") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/UART_TX") (pintype "input"))
    (pad "3" smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/UART_RX") (pintype "tri_state"))
    (pad "4" smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(U2-Pad5)") (pintype "input"))
    (pad "6" smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(U2-Pad6)") (pintype "tri_state"))
    (pad "7" smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/~{RXD_RXEN}") (pintype "input"))
    (pad "8" smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm" (layer "F.Cu")
    (tedit 62FA68B4)
    (at 115 90 -90)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
    (tags "SSOP 0.635")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -3.5 90) (layer "F.SilkS") hide)
    (fp_text value "Si8663" (at 0 3.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.6 -2.2225 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "Vcc1") (pintype "power_in"))
    (pad "2" smd rect (at -2.6 -1.5875 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(U1-Pad6)") (pinfunction "INA") (pintype "input"))
    (pad "3" smd rect (at -2.6 -0.9525 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(U2-Pad6)") (pinfunction "INB") (pintype "input"))
    (pad "4" smd rect (at -2.6 -0.3175 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(U3-Pad6)") (pinfunction "INC") (pintype "input"))
    (pad "5" smd rect (at -2.6 0.3175 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(U1-Pad5)") (pinfunction "OUTD") (pintype "output"))
    (pad "6" smd rect (at -2.6 0.9525 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(U2-Pad5)") (pinfunction "OUTE") (pintype "output"))
    (pad "7" smd rect (at -2.6 1.5875 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(U3-Pad5)") (pinfunction "OUTF") (pintype "output"))
    (pad "8" smd rect (at -2.6 2.2225 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND1") (pintype "power_in"))
    (pad "9" smd rect (at 2.6 2.2225 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GNDA") (pinfunction "GND2") (pintype "power_in"))
    (pad "10" smd rect (at 2.6 1.5875 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/PPS_RO") (pinfunction "INF") (pintype "input"))
    (pad "11" smd rect (at 2.6 0.9525 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/RXD_RO") (pinfunction "INE") (pintype "input"))
    (pad "12" smd rect (at 2.6 0.3175 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/TXD_RO") (pinfunction "IND") (pintype "input"))
    (pad "13" smd rect (at 2.6 -0.3175 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/PPS_DI") (pinfunction "OUTC") (pintype "output"))
    (pad "14" smd rect (at 2.6 -0.9525 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/RXD_DI") (pinfunction "OUTB") (pintype "output"))
    (pad "15" smd rect (at 2.6 -1.5875 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/TXD_DI") (pinfunction "OUTA") (pintype "output"))
    (pad "16" smd rect (at 2.6 -2.2225 270) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+5VA") (pinfunction "Vcc2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 128 80 -90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.55 90) (layer "F.SilkS") hide)
    (fp_text value "74LVC2G125" (at 0 2.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/~{TXD_TXEN}") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/UART_TX") (pintype "input"))
    (pad "3" smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/UART_RX") (pintype "tri_state"))
    (pad "4" smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(U1-Pad5)") (pintype "input"))
    (pad "6" smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(U1-Pad6)") (pintype "tri_state"))
    (pad "7" smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/~{TXD_RXEN}") (pintype "input"))
    (pad "8" smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/PPS_DE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 120.75 90 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.4 90) (layer "F.SilkS") hide)
    (fp_text value "Si8400" (at 0 3.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VCC1") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/SDA") (pinfunction "SDA1") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/SCL") (pinfunction "SCL1") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND1") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "GND2") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/SCL_ISO") (pinfunction "SCL2") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/SDA_ISO") (pinfunction "SDA2") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pinfunction "VCC2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.25 85.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107 86.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/TXD_DE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.25 98.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/TXD-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/TXD+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.25 107 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.25 94.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at -0.225 -1.5) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.75 98 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{RXD_RE}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107 96 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+12VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.75 79.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/~{RXD_TXEN}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.25 104.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/PPS-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/PPS+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122 95 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.5 81.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 122.5 78.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.43 90) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 116.25 83 90)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 0 6.1 90) (layer "B.SilkS") hide)
    (fp_text value "TCA9534" (at 0 -6.1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/~{TXD_RXEN}") (pinfunction "P0") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "/~{TXD_TXEN}") (pinfunction "P1") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "unconnected-(U6-Pad6)") (pinfunction "P2") (pintype "bidirectional+no_connect"))
    (pad "7" smd roundrect (at -4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "unconnected-(U6-Pad7)") (pinfunction "P3") (pintype "bidirectional+no_connect"))
    (pad "8" smd roundrect (at -4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "/~{PPS_RXEN}") (pinfunction "P4") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/~{PPS_TXEN}") (pinfunction "P5") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/~{RXD_RXEN}") (pinfunction "P6") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/~{RXD_TXEN}") (pinfunction "P7") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "unconnected-(U6-Pad13)") (pinfunction "~{INT}") (pintype "open_collector+no_connect"))
    (pad "14" smd roundrect (at 4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "15" smd roundrect (at 4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical" locked (layer "B.Cu")
    (tedit 5A19A422)
    (at 131.77 103.8)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.27 2.77) (layer "B.SilkS") hide)
    (fp_text value "EXT_IN" (at -1.27 -10.39) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.27 -3.81 90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/PPS_IO") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/SDA") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "/UART_TX") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3V3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/UART_RX") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 123.25 92.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical" locked (layer "B.Cu")
    (tedit 5A19A422)
    (at 101.29 103.8)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -1.27 2.77) (layer "B.SilkS") hide)
    (fp_text value "EXT_OUT" (at -1.27 -10.39) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.27 -3.81 90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(F2-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(F3-Pad2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(F4-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(F5-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(F6-Pad1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+12VA") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GNDA") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 116.25 97 90)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "icE1usb-rs422.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 6.1 90) (layer "B.SilkS") hide)
    (fp_text value "TCA9534" (at 0 -6.1 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "A1") (pintype "input"))
    (pad "3" smd roundrect (at -4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "A2") (pintype "input"))
    (pad "4" smd roundrect (at -4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/~{TXD_RE}") (pinfunction "P0") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "/TXD_DE") (pinfunction "P1") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "/~{RXD_RE}") (pinfunction "P2") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/RXD_DE") (pinfunction "P3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect (at 4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/PPS_DE") (pinfunction "P4") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/~{PPS_RE}") (pinfunction "P5") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U7-Pad11)") (pinfunction "P6") (pintype "bidirectional+no_connect"))
    (pad "12" smd roundrect (at 4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "unconnected-(U7-Pad12)") (pinfunction "P7") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "unconnected-(U7-Pad13)") (pinfunction "~{INT}") (pintype "open_collector+no_connect"))
    (pad "14" smd roundrect (at 4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/SCL_ISO") (pinfunction "SCL") (pintype "input"))
    (pad "15" smd roundrect (at 4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/SDA_ISO") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "+5VA") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 97.5 108) (end 133 108) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110.75 84.5) (mid 110.457107 85.207107) (end 109.75 85.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 105 86.5) (mid 104.707107 87.207107) (end 104 87.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.75 84.5) (end 110.75 76.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.5 87.5) (end 104 87.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.5 88.5) (mid 96.792893 87.792893) (end 97.5 87.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 133 75.5) (end 111.75 75.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 134 107) (end 134 76.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 106 85.5) (end 109.75 85.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 105 86.5) (mid 105.292893 85.792893) (end 106 85.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110.75 76.5) (mid 111.042893 75.792893) (end 111.75 75.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 134 107) (mid 133.707107 107.707107) (end 133 108) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.5 108) (mid 96.792893 107.707107) (end 96.5 107) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 133 75.5) (mid 133.707107 75.792893) (end 134 76.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.5 88.5) (end 96.5 107) (layer "Edge.Cuts") (width 0.1))
  (zone (net 5) (net_name "+5VA") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.25) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110.5 86.5)
        (xy 110.5 88.25)
        (xy 110.25 88.5)
        (xy 108.5 88.5)
        (xy 108 89)
        (xy 108 89.25)
        (xy 107.75 89.5)
        (xy 105.5 89.5)
        (xy 105.25 89.25)
        (xy 105.25 88.25)
        (xy 105.5 88)
        (xy 107 88)
        (xy 107.25 87.75)
        (xy 107.25 86.25)
        (xy 107.5 86)
        (xy 110 86)
      )
    )
  )
  (zone (net 3) (net_name "+12VA") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 108 92.75)
        (xy 108 93.5)
        (xy 108.5 94)
        (xy 110.25 94)
        (xy 110.75 94.5)
        (xy 110.75 95.25)
        (xy 110.25 95.75)
        (xy 109 95.75)
        (xy 108.25 96.5)
        (xy 107.5 96.5)
        (xy 107.25 96.25)
        (xy 107.25 95.5)
        (xy 107 95.25)
        (xy 104 95.25)
        (xy 103.75 95.5)
        (xy 103.75 96.25)
        (xy 103.5 96.5)
        (xy 102.5 96.5)
        (xy 101.75 97.25)
        (xy 101 97.25)
        (xy 100.25 96.5)
        (xy 100.25 95.75)
        (xy 101.5 94.5)
        (xy 103 94.5)
        (xy 103.75 94.5)
        (xy 105.5 92.75)
        (xy 105.75 92.5)
        (xy 107.75 92.5)
      )
    )
  )
  (zone (net 4) (net_name "GNDA") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.25) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110.25 91.25)
        (xy 124.25 91.25)
        (xy 124.25 95.75)
        (xy 125 96.5)
        (xy 125 108)
        (xy 96.5 108)
        (xy 96.5 87.5)
        (xy 103.5 87.5)
        (xy 105.25 85.75)
        (xy 110.25 85.75)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.25) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 134 108)
        (xy 127.5 108)
        (xy 127.5 94.5)
        (xy 126.5 93.5)
        (xy 126.5 88.75)
        (xy 111.75 88.75)
        (xy 111.75 86.5)
        (xy 111.5 86.25)
        (xy 111.5 85.25)
        (xy 110.75 84.5)
        (xy 110.75 75.5)
        (xy 134 75.5)
      )
    )
  )
  (zone (net 5) (net_name "+5VA") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.25) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 110.25 91.25)
        (xy 124.25 91.25)
        (xy 124.25 95.75)
        (xy 125 96.5)
        (xy 125 108)
        (xy 96.5 108)
        (xy 96.5 87.5)
        (xy 103.5 87.5)
        (xy 105.25 85.75)
        (xy 110.25 85.75)
      )
    )
  )
  (zone (net 1) (net_name "+3V3") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.25) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 134 108)
        (xy 127.5 108)
        (xy 127.5 94.5)
        (xy 126.5 93.5)
        (xy 126.5 88.75)
        (xy 111.75 88.75)
        (xy 111.75 86.5)
        (xy 111.5 86.25)
        (xy 111.5 85.25)
        (xy 110.75 84.5)
        (xy 110.75 75.5)
        (xy 134 75.5)
      )
    )
  )
)
