
// autogenerated by show asciidoc counters
These counters and their description are based on OsmoPCU 0.9.0.244-de96 (OsmoPCU).

=== Rate Counters

// generating tables for rate_ctr_group
// rate_ctr_group table NSVC Peer Statistics
.ns:nsvc - NSVC Peer Statistics
[options="header"]
|===
| Name | Reference | Description
| packets:in | <<ns:nsvc_packets:in>> | Packets at NS Level  ( In)
| packets:out | <<ns:nsvc_packets:out>> | Packets at NS Level  (Out)
| packets:out:drop | <<ns:nsvc_packets:out:drop>> | Dropped Packets      (Out)
| bytes:in | <<ns:nsvc_bytes:in>> | Bytes at NS Level    ( In)
| bytes:out | <<ns:nsvc_bytes:out>> | Bytes at NS Level    (Out)
| bytes:out:drop | <<ns:nsvc_bytes:out:drop>> | Dropped Bytes        (Out)
| blocked | <<ns:nsvc_blocked>> | NS-VC Block count
| unblocked | <<ns:nsvc_unblocked>> | NS-VC Unblock count
| dead | <<ns:nsvc_dead>> | NS-VC gone dead count
| replaced | <<ns:nsvc_replaced>> | NS-VC replaced other count
| nsei-chg | <<ns:nsvc_nsei-chg>> | NS-VC changed NSEI count
| inv-nsvci | <<ns:nsvc_inv-nsvci>> | NS-VCI was invalid count
| inv-nsei | <<ns:nsvc_inv-nsei>> | NSEI was invalid count
| lost:alive | <<ns:nsvc_lost:alive>> | ALIVE ACK missing count
| lost:reset | <<ns:nsvc_lost:reset>> | RESET ACK missing count
|===
// rate_ctr_group table NSE Peer Statistics
.ns:nse - NSE Peer Statistics
[options="header"]
|===
| Name | Reference | Description
| packets:in | <<ns:nse_packets:in>> | Packets at NS Level  ( In)
| packets:out | <<ns:nse_packets:out>> | Packets at NS Level  (Out)
| packets:out:drop | <<ns:nse_packets:out:drop>> | Dropped Packets      (Out)
| bytes:in | <<ns:nse_bytes:in>> | Bytes at NS Level    ( In)
| bytes:out | <<ns:nse_bytes:out>> | Bytes at NS Level    (Out)
| bytes:out:drop | <<ns:nse_bytes:out:drop>> | Dropped Bytes        (Out)
| blocked | <<ns:nse_blocked>> | NS-VC Block count
| unblocked | <<ns:nse_unblocked>> | NS-VC Unblock count
| dead | <<ns:nse_dead>> | NS-VC gone dead count
| replaced | <<ns:nse_replaced>> | NS-VC replaced other count
| nsei-chg | <<ns:nse_nsei-chg>> | NS-VC changed NSEI count
| inv-nsvci | <<ns:nse_inv-nsvci>> | NS-VCI was invalid count
| inv-nsei | <<ns:nse_inv-nsei>> | NSEI was invalid count
| lost:alive | <<ns:nse_lost:alive>> | ALIVE ACK missing count
| lost:reset | <<ns:nse_lost:reset>> | RESET ACK missing count
|===
// rate_ctr_group table SGSN Statistics
.pcu:sgsn - SGSN Statistics
[options="header"]
|===
| Name | Reference | Description
| rx_paging_cs | <<pcu:sgsn_rx_paging_cs>> | Amount of paging CS requests received
| rx_paging_ps | <<pcu:sgsn_rx_paging_ps>> | Amount of paging PS requests received
|===
// rate_ctr_group table BSSGP Peer Statistics
.bssgp:bss_ctx - BSSGP Peer Statistics
[options="header"]
|===
| Name | Reference | Description
| packets:in | <<bssgp:bss_ctx_packets:in>> | Packets at BSSGP Level ( In)
| packets:out | <<bssgp:bss_ctx_packets:out>> | Packets at BSSGP Level (Out)
| bytes:in | <<bssgp:bss_ctx_bytes:in>> | Bytes at BSSGP Level   ( In)
| bytes:out | <<bssgp:bss_ctx_bytes:out>> | Bytes at BSSGP Level   (Out)
| blocked | <<bssgp:bss_ctx_blocked>> | BVC Blocking count
| discarded | <<bssgp:bss_ctx_discarded>> | BVC LLC Discarded count
| status | <<bssgp:bss_ctx_status>> | BVC Status count
|===
// rate_ctr_group table BTS Statistics
.bts - BTS Statistics
[options="header"]
|===
| Name | Reference | Description
| tbf:dl:alloc | <<bts_tbf:dl:alloc>> | TBF DL Allocated
| tbf:dl:freed | <<bts_tbf:dl:freed>> | TBF DL Freed
| tbf:dl:aborted | <<bts_tbf:dl:aborted>> | TBF DL Aborted
| tbf:ul:alloc | <<bts_tbf:ul:alloc>> | TBF UL Allocated
| tbf:ul:freed | <<bts_tbf:ul:freed>> | TBF UL Freed
| tbf:ul:aborted | <<bts_tbf:ul:aborted>> | TBF UL Aborted
| tbf:reused | <<bts_tbf:reused>> | TBF Reused
| tbf:alloc:algo-a | <<bts_tbf:alloc:algo-a>> | TBF Alloc Algo A
| tbf:alloc:algo-b | <<bts_tbf:alloc:algo-b>> | TBF Alloc Algo B
| tbf:alloc:failed | <<bts_tbf:alloc:failed>> | TBF Alloc Failure (any reason)
| tbf:alloc:failed:no_tfi | <<bts_tbf:alloc:failed:no_tfi>> | TBF Alloc Failure (TFIs exhausted)
| tbf:alloc:failed:no_usf | <<bts_tbf:alloc:failed:no_usf>> | TBF Alloc Failure (USFs exhausted)
| tbf:alloc:failed:no_slot_combi | <<bts_tbf:alloc:failed:no_slot_combi>> | TBF Alloc Failure (No valid UL/DL slot combination found)
| tbf:alloc:failed:no_slot_avail | <<bts_tbf:alloc:failed:no_slot_avail>> | TBF Alloc Failure (No slot available)
| rlc:sent | <<bts_rlc:sent>> | RLC Sent
| rlc:resent | <<bts_rlc:resent>> | RLC Resent
| rlc:restarted | <<bts_rlc:restarted>> | RLC Restarted
| rlc:stalled | <<bts_rlc:stalled>> | RLC Stalled
| rlc:nacked | <<bts_rlc:nacked>> | RLC Nacked
| rlc:final_block_resent | <<bts_rlc:final_block_resent>> | RLC Final Blk resent
| rlc:ass:timedout | <<bts_rlc:ass:timedout>> | RLC Assign Timeout
| rlc:ass:failed | <<bts_rlc:ass:failed>> | RLC Assign Failed
| rlc:ack:timedout | <<bts_rlc:ack:timedout>> | RLC Ack Timeout
| rlc:ack:failed | <<bts_rlc:ack:failed>> | RLC Ack Failed
| rlc:rel:timedout | <<bts_rlc:rel:timedout>> | RLC Release Timeout
| rlc:late-block | <<bts_rlc:late-block>> | RLC Late Block
| rlc:sent-dummy | <<bts_rlc:sent-dummy>> | RLC Sent Dummy
| rlc:sent-control | <<bts_rlc:sent-control>> | RLC Sent Control
| rlc:dl_bytes | <<bts_rlc:dl_bytes>> | RLC DL Bytes
| rlc:dl_payload_bytes | <<bts_rlc:dl_payload_bytes>> | RLC DL Payload Bytes
| rlc:ul_bytes | <<bts_rlc:ul_bytes>> | RLC UL Bytes
| rlc:ul_payload_bytes | <<bts_rlc:ul_payload_bytes>> | RLC UL Payload Bytes
| decode:errors | <<bts_decode:errors>> | Decode Errors
| sba:allocated | <<bts_sba:allocated>> | SBA Allocated
| sba:freed | <<bts_sba:freed>> | SBA Freed
| sba:timedout | <<bts_sba:timedout>> | SBA Timeout
| llc:timeout | <<bts_llc:timeout>> | Timedout Frames
| llc:dropped | <<bts_llc:dropped>> | Dropped Frames
| llc:scheduled | <<bts_llc:scheduled>> | Scheduled Frames
| llc:dl_bytes | <<bts_llc:dl_bytes>> | RLC encapsulated PDUs
| llc:ul_bytes | <<bts_llc:ul_bytes>> | full PDUs received
| pch:requests | <<bts_pch:requests>> | PCH requests sent
| pch:requests:timeout | <<bts_pch:requests:timeout>> | PCH requests timeout
| rach:requests | <<bts_rach:requests>> | RACH requests received
| rach:requests:11bit | <<bts_rach:requests:11bit>> | 11BIT_RACH requests received
| rach:requests:one_phase | <<bts_rach:requests:one_phase>> | One phase packet access with request for single TS UL
| rach:requests:two_phase | <<bts_rach:requests:two_phase>> | Single block packet request for two phase packet access
| rach:requests:unexpected | <<bts_rach:requests:unexpected>> | RACH Request with unexpected content received
| spb:uplink_first_segment | <<bts_spb:uplink_first_segment>> | First seg of UL SPB
| spb:uplink_second_segment | <<bts_spb:uplink_second_segment>> | Second seg of UL SPB
| spb:downlink_first_segment | <<bts_spb:downlink_first_segment>> | First seg of DL SPB
| spb:downlink_second_segment | <<bts_spb:downlink_second_segment>> | Second seg of DL SPB
| immediate:assignment_UL | <<bts_immediate:assignment_UL>> | Immediate Assign UL
| immediate:assignment_ul:one_phase | <<bts_immediate:assignment_ul:one_phase>> | Immediate Assign UL (one phase packet access)
| immediate:assignment_ul:two_phase | <<bts_immediate:assignment_ul:two_phase>> | Immediate Assign UL (two phase packet access)
| immediate:assignment_ul:contention_resolution_success | <<bts_immediate:assignment_ul:contention_resolution_success>> | First RLC Block (PDU) on the PDTCH from the MS received
| immediate:assignment_rej | <<bts_immediate:assignment_rej>> | Immediate Assign Rej
| immediate:assignment_DL | <<bts_immediate:assignment_DL>> | Immediate Assign DL
| channel:request_description | <<bts_channel:request_description>> | Channel Request Desc
| pkt:ul_assignment | <<bts_pkt:ul_assignment>> | Packet UL Assignment
| pkt:access_reject | <<bts_pkt:access_reject>> | Packet Access Reject
| pkt:dl_assignment | <<bts_pkt:dl_assignment>> | Packet DL Assignment
| pkt:cell_chg_notification | <<bts_pkt:cell_chg_notification>> | Packet Cell Change Notification
| pkt:cell_chg_continue | <<bts_pkt:cell_chg_continue>> | Packet Cell Change Continue
| pkt:neigh_cell_data | <<bts_pkt:neigh_cell_data>> | Packet Neighbour Cell Data
| ul:control | <<bts_ul:control>> | UL control Block
| ul:assignment_poll_timeout | <<bts_ul:assignment_poll_timeout>> | UL Assign Timeout
| ul:assignment_failed | <<bts_ul:assignment_failed>> | UL Assign Failed
| dl:assignment_timeout | <<bts_dl:assignment_timeout>> | DL Assign Timeout
| dl:assignment_failed | <<bts_dl:assignment_failed>> | DL Assign Failed
| pkt:ul_ack_nack_timeout | <<bts_pkt:ul_ack_nack_timeout>> | PUAN Poll Timeout
| pkt:ul_ack_nack_failed | <<bts_pkt:ul_ack_nack_failed>> | PUAN poll Failed
| pkt:dl_ack_nack_timeout | <<bts_pkt:dl_ack_nack_timeout>> | PDAN poll Timeout
| pkt:dl_ack_nack_failed | <<bts_pkt:dl_ack_nack_failed>> | PDAN poll Failed
| gprs:downlink_cs1 | <<bts_gprs:downlink_cs1>> | CS1 downlink
| gprs:downlink_cs2 | <<bts_gprs:downlink_cs2>> | CS2 downlink
| gprs:downlink_cs3 | <<bts_gprs:downlink_cs3>> | CS3 downlink
| gprs:downlink_cs4 | <<bts_gprs:downlink_cs4>> | CS4 downlink
| egprs:downlink_mcs1 | <<bts_egprs:downlink_mcs1>> | MCS1 downlink
| egprs:downlink_mcs2 | <<bts_egprs:downlink_mcs2>> | MCS2 downlink
| egprs:downlink_mcs3 | <<bts_egprs:downlink_mcs3>> | MCS3 downlink
| egprs:downlink_mcs4 | <<bts_egprs:downlink_mcs4>> | MCS4 downlink
| egprs:downlink_mcs5 | <<bts_egprs:downlink_mcs5>> | MCS5 downlink
| egprs:downlink_mcs6 | <<bts_egprs:downlink_mcs6>> | MCS6 downlink
| egprs:downlink_mcs7 | <<bts_egprs:downlink_mcs7>> | MCS7 downlink
| egprs:downlink_mcs8 | <<bts_egprs:downlink_mcs8>> | MCS8 downlink
| egprs:downlink_mcs9 | <<bts_egprs:downlink_mcs9>> | MCS9 downlink
| gprs:uplink_cs1 | <<bts_gprs:uplink_cs1>> | CS1 Uplink
| gprs:uplink_cs2 | <<bts_gprs:uplink_cs2>> | CS2 Uplink
| gprs:uplink_cs3 | <<bts_gprs:uplink_cs3>> | CS3 Uplink
| gprs:uplink_cs4 | <<bts_gprs:uplink_cs4>> | CS4 Uplink
| egprs:uplink_mcs1 | <<bts_egprs:uplink_mcs1>> | MCS1 Uplink
| egprs:uplink_mcs2 | <<bts_egprs:uplink_mcs2>> | MCS2 Uplink
| egprs:uplink_mcs3 | <<bts_egprs:uplink_mcs3>> | MCS3 Uplink
| egprs:uplink_mcs4 | <<bts_egprs:uplink_mcs4>> | MCS4 Uplink
| egprs:uplink_mcs5 | <<bts_egprs:uplink_mcs5>> | MCS5 Uplink
| egprs:uplink_mcs6 | <<bts_egprs:uplink_mcs6>> | MCS6 Uplink
| egprs:uplink_mcs7 | <<bts_egprs:uplink_mcs7>> | MCS7 Uplink
| egprs:uplink_mcs8 | <<bts_egprs:uplink_mcs8>> | MCS8 Uplink
| egprs:uplink_mcs9 | <<bts_egprs:uplink_mcs9>> | MCS9 Uplink
|===
=== Osmo Stat Items

// generating tables for osmo_stat_items
NSVC Peer Statistics
// osmo_stat_item_group table NSVC Peer Statistics
.ns.nsvc - NSVC Peer Statistics
[options="header"]
|===
| Name | Reference | Description | Unit
| alive.delay | <<ns.nsvc_alive.delay>> | ALIVE response time         | ms
|===
NS Bind Statistics
// osmo_stat_item_group table NS Bind Statistics
.ns.bind - NS Bind Statistics
[options="header"]
|===
| Name | Reference | Description | Unit
| tx_backlog_length | <<ns.bind_tx_backlog_length>> | Transmit backlog length | packets
|===
BTS Statistics
// osmo_stat_item_group table BTS Statistics
.bts - BTS Statistics
[options="header"]
|===
| Name | Reference | Description | Unit
| ms.present | <<bts_ms.present>> | MS Present            |
| pdch.available | <<bts_pdch.available>> | PDCH available        |
| pdch.occupied | <<bts_pdch.occupied>> | PDCH occupied (all)   |
| pdch.occupied.gprs | <<bts_pdch.occupied.gprs>> | PDCH occupied (GPRS)  |
| pdch.occupied.egprs | <<bts_pdch.occupied.egprs>> | PDCH occupied (EGPRS) |
|===
// there are no ungrouped osmo_counters
