(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "SP485" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.096 11.43 0))
    (property "Value" "SP485" (id 1) (at 0.762 11.43 0))
    (property "Footprint" "" (id 2) (at 0 -17.78 0))
    (property "Datasheet" "https://assets.maxlinear.com/web/documents/sp483_sp485.pdf" (id 3) (at 0 1.27 0))
    (property "ki_keywords" "rs485 rs422" (id 4) (at 0 0 0))
    (property "ki_description" "Low Power Half-Duplex RS-485 Transceivers" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0))
    (symbol "SP485_0_1")
    (symbol "SP485_1_1"
      (pin output line (at -10.16 2.54 0) (length 2.54)
        (name "RO")
        (number "1")
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "~{RE}")
        (number "2")
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "DE")
        (number "3")
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "DI")
        (number "4")
      )
      (pin power_in line (at 0 -15.24 90) (length 2.54)
        (name "GND")
        (number "5")
      )
      (pin bidirectional line (at 10.16 -5.08 180) (length 2.54)
        (name "A")
        (number "6")
      )
      (pin bidirectional line (at 10.16 2.54 180) (length 2.54)
        (name "B")
        (number "7")
      )
      (pin power_in line (at 0 12.7 270) (length 2.54)
        (name "VCC")
        (number "8")
      )
    )
  )
  (symbol "Si8400" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -6.35 6.35 0))
    (property "Value" "Si8400" (id 1) (at 3.81 6.35 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 0 -8.89 0))
    (property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/SL/documents/public/data-sheets/Si840x.pdf" (id 3) (at 0 1.27 0))
    (property "ki_keywords" "digital isolator i2c" (id 4) (at 0 0 0))
    (property "ki_description" "I2C Isolator, 2.5 kVrms, Bidirectional clock and data, SOIC-8" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*" (id 6) (at 0 0 0))
    (symbol "Si8400_0_1")
    (symbol "Si8400_1_1"
      (pin power_in line (at -10.16 2.54 0) (length 2.54)
        (name "VCC1")
        (number "1")
      )
      (pin bidirectional line (at -10.16 0 0) (length 2.54)
        (name "SDA1")
        (number "2")
      )
      (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
        (name "SCL1")
        (number "3")
      )
      (pin power_in line (at -10.16 -5.08 0) (length 2.54)
        (name "GND1")
        (number "4")
      )
      (pin power_in line (at 10.16 -5.08 180) (length 2.54)
        (name "GND2")
        (number "5")
      )
      (pin bidirectional line (at 10.16 -2.54 180) (length 2.54)
        (name "SCL2")
        (number "6")
      )
      (pin bidirectional line (at 10.16 0 180) (length 2.54)
        (name "SDA2")
        (number "7")
      )
      (pin power_in line (at 10.16 2.54 180) (length 2.54)
        (name "VCC2")
        (number "8")
      )
    )
  )
  (symbol "Si8663" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 8.255 14.605 0))
    (property "Value" "Si8663" (id 1) (at 8.255 12.065 0))
    (property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm" (id 2) (at 5.715 -13.97 0))
    (property "Datasheet" "https://www.skyworksinc.com/-/media/SkyWorks/SL/documents/public/data-sheets/si866x.pdf" (id 3) (at 10.16 -2.54 0))
    (property "ki_keywords" "6 channel digital isolator" (id 4) (at 0 0 0))
    (property "ki_description" "Low Power Six-Channel Digital Isolator" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*" (id 6) (at 0 0 0))
    (symbol "Si8663_0_1")
    (symbol "Si8663_1_1"
      (pin power_in line (at -5.08 17.78 270) (length 2.54)
        (name "Vcc1")
        (number "1")
      )
      (pin input line (at 10.16 -5.08 180) (length 2.54)
        (name "INF")
        (number "10")
      )
      (pin input line (at 10.16 -2.54 180) (length 2.54)
        (name "INE")
        (number "11")
      )
      (pin input line (at 10.16 0 180) (length 2.54)
        (name "IND")
        (number "12")
      )
      (pin output line (at 10.16 2.54 180) (length 2.54)
        (name "OUTC")
        (number "13")
      )
      (pin output line (at 10.16 5.08 180) (length 2.54)
        (name "OUTB")
        (number "14")
      )
      (pin output line (at 10.16 7.62 180) (length 2.54)
        (name "OUTA")
        (number "15")
      )
      (pin power_in line (at 5.08 17.78 270) (length 2.54)
        (name "Vcc2")
        (number "16")
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "INA")
        (number "2")
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "INB")
        (number "3")
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "INC")
        (number "4")
      )
      (pin output line (at -10.16 0 0) (length 2.54)
        (name "OUTD")
        (number "5")
      )
      (pin output line (at -10.16 -2.54 0) (length 2.54)
        (name "OUTE")
        (number "6")
      )
      (pin output line (at -10.16 -5.08 0) (length 2.54)
        (name "OUTF")
        (number "7")
      )
      (pin power_in line (at -5.08 -15.24 90) (length 2.54)
        (name "GND1")
        (number "8")
      )
      (pin power_in line (at 5.08 -15.24 90) (length 2.54)
        (name "GND2")
        (number "9")
      )
    )
  )
)
