14:38:52.208223 BSC_Tests.ttcn:3234 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_stat_num_msc_connected_2'.
14:38:53.218142 BSC_Tests.ttcn:3234 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-start.sh BSC_Tests.TC_stat_num_msc_connected_2' was executed successfully (exit status: 0).
14:38:53.218338 BSC_Tests.ttcn:3234 Test case TC_stat_num_msc_connected_2 started.
14:38:53.218421 BSC_Tests.ttcn:3234 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_stat_num_msc_connected_2.
14:38:53.218618 BSC_Tests.ttcn:3234 Port IPA_CTRL was started.
14:38:53.218686 BSC_Tests.ttcn:3234 Port RSL_CCHAN[0] was started.
14:38:53.218743 BSC_Tests.ttcn:3234 Port RSL_CCHAN[1] was started.
14:38:53.218796 BSC_Tests.ttcn:3234 Port RSL_CCHAN[2] was started.
14:38:53.218848 BSC_Tests.ttcn:3234 Port IPA_RSL[0][0] was started.
14:38:53.218899 BSC_Tests.ttcn:3234 Port IPA_RSL[0][1] was started.
14:38:53.218951 BSC_Tests.ttcn:3234 Port IPA_RSL[0][2] was started.
14:38:53.219003 BSC_Tests.ttcn:3234 Port IPA_RSL[0][3] was started.
14:38:53.219056 BSC_Tests.ttcn:3234 Port IPA_RSL[1][0] was started.
14:38:53.219108 BSC_Tests.ttcn:3234 Port IPA_RSL[1][1] was started.
14:38:53.219160 BSC_Tests.ttcn:3234 Port IPA_RSL[1][2] was started.
14:38:53.219215 BSC_Tests.ttcn:3234 Port IPA_RSL[1][3] was started.
14:38:53.219272 BSC_Tests.ttcn:3234 Port IPA_RSL[2][0] was started.
14:38:53.219328 BSC_Tests.ttcn:3234 Port IPA_RSL[2][1] was started.
14:38:53.219385 BSC_Tests.ttcn:3234 Port IPA_RSL[2][2] was started.
14:38:53.219440 BSC_Tests.ttcn:3234 Port IPA_RSL[2][3] was started.
14:38:53.219497 BSC_Tests.ttcn:3234 Port IPA was started.
14:38:53.219554 BSC_Tests.ttcn:3234 Port SCCPLITE_IPA_CTRL was started.
14:38:53.219611 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[0][0] was started.
14:38:53.219670 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[0][1] was started.
14:38:53.219728 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[0][2] was started.
14:38:53.219785 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[0][3] was started.
14:38:53.219842 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[1][0] was started.
14:38:53.219987 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[1][1] was started.
14:38:53.220076 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[1][2] was started.
14:38:53.220110 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[1][3] was started.
14:38:53.220142 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[2][0] was started.
14:38:53.220174 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[2][1] was started.
14:38:53.220206 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[2][2] was started.
14:38:53.220258 BSC_Tests.ttcn:3234 Port IPA_CFG_PORT[2][3] was started.
14:38:53.220290 BSC_Tests.ttcn:3234 Port BSCVTY was started.
14:38:53.220323 BSC_Tests.ttcn:3234 Port STPVTY was started.
14:38:53.220355 BSC_Tests.ttcn:3234 Port SCCPLITE_IPA_CFG_PORT[0] was started.
14:38:53.220387 BSC_Tests.ttcn:3234 Port SCCPLITE_IPA_CFG_PORT[1] was started.
14:38:53.220418 BSC_Tests.ttcn:3234 Port SCCPLITE_IPA_CFG_PORT[2] was started.
14:38:53.220449 BSC_Tests.ttcn:3234 Port BSSAP was started.
14:38:53.220480 BSC_Tests.ttcn:3234 Port BSSAP_LE was started.
14:38:53.220512 BSC_Tests.ttcn:3234 Component type BSC_Tests.test_CT was initialized.
14:38:53.220558 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
14:38:53.220603 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
14:38:53.220645 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
14:38:53.221005 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
14:38:53.221061 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
14:38:53.221136 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
14:38:53.221190 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBSC> ", has_wildcards := false } }
14:38:53.221237 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBSC# ", has_wildcards := false } }
14:38:53.221290 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBSC(*)", has_wildcards := true } }
14:38:53.221391 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
14:38:53.221457 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.221507 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:38:53.221546 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:38:53.221583 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:38:53.221619 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:38:53.221656 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
14:38:53.221697 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
14:38:53.221738 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
14:38:53.221780 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
14:38:53.221914 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
14:38:53.222014 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.222097 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.222142 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
14:38:53.222187 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
14:38:53.222234 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.222288 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:53.222350 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.222499 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
14:38:53.222584 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.222661 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.222757 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.222807 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
14:38:53.222854 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
14:38:53.222902 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.222949 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
14:38:53.223006 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.223092 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
14:38:53.223176 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.223253 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.223346 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.223397 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
14:38:53.223454 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
14:38:53.223507 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.223558 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
14:38:53.223617 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.223699 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
14:38:53.223775 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.223847 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.223956 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.224011 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
14:38:53.224058 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
14:38:53.224108 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.224157 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
14:38:53.224216 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.224298 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
14:38:53.224371 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.224442 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.224526 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.224576 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
14:38:53.224622 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
14:38:53.224671 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.224717 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:38:53.224780 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.224854 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
14:38:53.224934 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.225016 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.225071 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
14:38:53.225122 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
14:38:53.225175 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.225230 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:53.225293 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.225379 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
14:38:53.225458 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.225535 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.225637 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.225693 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
14:38:53.225746 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
14:38:53.225802 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.225860 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:38:53.225931 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.226027 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
14:38:53.226116 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.226203 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.226308 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.226368 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
14:38:53.226426 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
14:38:53.226486 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.226542 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:38:53.226611 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.226706 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
14:38:53.226794 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.226880 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.226981 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.227040 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
14:38:53.227097 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
14:38:53.227156 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.227211 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.227279 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.227369 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
14:38:53.227455 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.227539 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.227639 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.227699 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
14:38:53.227755 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
14:38:53.227813 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.227868 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.227953 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.228033 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
14:38:53.228126 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.228215 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.228273 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
14:38:53.228328 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
14:38:53.228385 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.228448 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:38:53.238722 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 31, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
14:38:53.238813 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(31).
14:38:53.238911 StatsD_Checker.ttcnpp:417 Function was started.
14:38:53.238963 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
14:38:53.239041 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.239388 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
14:38:53.239485 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.239566 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.239613 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
14:38:53.239658 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
14:38:53.239703 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.239750 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
14:38:53.239809 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.240005 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 14
14:38:53.240080 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.240148 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.240194 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 14
14:38:53.240240 Osmocom_VTY_Functions.ttcn:73 Message with id 14 was extracted from the queue of BSCVTY.
14:38:53.240287 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.240335 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
14:38:53.240389 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.241934 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
14:38:53.242191 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.242341 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.242422 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
14:38:53.242497 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
14:38:53.242567 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.242757 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:38:53.250927 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 32, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:38:53.251011 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:38:53.257725 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 33, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:38:53.257776 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(33):SCTP_PORT to system:sctp.
14:38:53.259606 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(33):SCTP_PORT to system:sctp finished.
14:38:53.259633 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(33):MTP3_SP_PORT and VirtMSC-SCCP(32):MTP3_SCCP_PORT.
14:38:53.259979 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(33):MTP3_SP_PORT and VirtMSC-SCCP(32):MTP3_SCCP_PORT finished.
14:38:53.260026 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23905, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 1) on component VirtMSC-M3UA(33).
14:38:53.260073 SCCP_Adapter.ttcnpp:127 Function was started.
14:38:53.260103 RAN_Adapter.ttcnpp:57 Creating new alive PTC with component type RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
14:38:53.263885 RAN_Adapter.ttcnpp:57 PTC was created. Component reference: 34, alive: yes, type: RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
14:38:53.263923 RAN_Adapter.ttcnpp:60 Start timer T: 5 s
14:38:53.263948 RAN_Adapter.ttcnpp:72 Connecting BSSAP RAN_Emulation to SCCP_SP_PORT
14:38:53.263974 RAN_Adapter.ttcnpp:73 Connecting ports VirtMSC-RAN(34):BSSAP and VirtMSC-SCCP(32):SCCP_SP_PORT.
14:38:53.266201 RAN_Adapter.ttcnpp:73 Connect operation on VirtMSC-RAN(34):BSSAP and VirtMSC-SCCP(32):SCCP_SP_PORT finished.
14:38:53.266228 RAN_Adapter.ttcnpp:90 Starting RAN_Emulation
14:38:53.266248 RAN_Adapter.ttcnpp:91 Starting function main({ create_cb := refers(RAN_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.UnitdataCallback), decode_dtap := false, role_ms := false, protocol := RAN_PROTOCOL_BSSAP (0), transport := BSSAP_TRANSPORT_AoIP (0), use_osmux := false, bssap_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit } }, "") on component VirtMSC-RAN(34).
14:38:53.266343 RAN_Adapter.ttcnpp:91 Function was started.
14:38:53.266386 BSC_Tests.ttcn:1216 Connecting ports mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(34):CTRL_CLIENT.
14:38:53.266582 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL is waiting for connection from VirtMSC-RAN(34):CTRL_CLIENT on UNIX pathname /tmp/ttcn3-portconn-4b39e002.
14:38:53.269871 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL has accepted the connection from VirtMSC-RAN(34):CTRL_CLIENT.
14:38:53.269893 BSC_Tests.ttcn:1216 Connect operation on mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(34):CTRL_CLIENT finished.
14:38:53.269908 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 185, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(32).
14:38:53.269944 SCCP_Adapter.ttcnpp:165 Function was started.
14:38:53.269988 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:38:53.272776 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 35, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
14:38:53.272792 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:38:53.275340 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 36, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
14:38:53.275391 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(36):SCTP_PORT to system:sctp.
14:38:53.276329 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(36):SCTP_PORT to system:sctp finished.
14:38:53.276368 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(36):MTP3_SP_PORT and VirtMSC-SCCP(35):MTP3_SCCP_PORT.
14:38:53.276696 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(36):MTP3_SP_PORT and VirtMSC-SCCP(35):MTP3_SCCP_PORT finished.
14:38:53.276726 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23906, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 2) on component VirtMSC-M3UA(36).
14:38:53.276773 SCCP_Adapter.ttcnpp:127 Function was started.
14:38:53.276807 RAN_Adapter.ttcnpp:57 Creating new alive PTC with component type RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
14:38:53.279484 RAN_Adapter.ttcnpp:57 PTC was created. Component reference: 37, alive: yes, type: RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
14:38:53.279522 RAN_Adapter.ttcnpp:60 Start timer T: 5 s
14:38:53.279547 RAN_Adapter.ttcnpp:72 Connecting BSSAP RAN_Emulation to SCCP_SP_PORT
14:38:53.279573 RAN_Adapter.ttcnpp:73 Connecting ports VirtMSC-RAN(37):BSSAP and VirtMSC-SCCP(35):SCCP_SP_PORT.
14:38:53.280778 RAN_Adapter.ttcnpp:73 Connect operation on VirtMSC-RAN(37):BSSAP and VirtMSC-SCCP(35):SCCP_SP_PORT finished.
14:38:53.280811 RAN_Adapter.ttcnpp:90 Starting RAN_Emulation
14:38:53.280835 RAN_Adapter.ttcnpp:91 Starting function main({ create_cb := refers(RAN_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.UnitdataCallback), decode_dtap := false, role_ms := false, protocol := RAN_PROTOCOL_BSSAP (0), transport := BSSAP_TRANSPORT_AoIP (0), use_osmux := false, bssap_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000000000010'B, subsystemNumber := 254, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit } }, "") on component VirtMSC-RAN(37).
14:38:53.280924 RAN_Adapter.ttcnpp:91 Function was started.
14:38:53.280954 BSC_Tests.ttcn:1216 Connecting ports mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(37):CTRL_CLIENT.
14:38:53.281163 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL is waiting for connection from VirtMSC-RAN(37):CTRL_CLIENT on UNIX pathname /tmp/ttcn3-portconn-4c39e002.
14:38:53.283335 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL has accepted the connection from VirtMSC-RAN(37):CTRL_CLIENT.
14:38:53.283377 BSC_Tests.ttcn:1216 Connect operation on mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(37):CTRL_CLIENT finished.
14:38:53.283407 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 2, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(35).
14:38:53.283459 SCCP_Adapter.ttcnpp:165 Function was started.
14:38:53.283524 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:38:53.286181 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 38, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
14:38:53.286214 BSSAP_LE_Adapter.ttcn:97 Creating new alive PTC with component type BSSAP_LE_Emulation.BSSAP_LE_Emulation_CT, component name: VirtSMLC-BSSAP_LE.
14:38:53.288730 BSSAP_LE_Adapter.ttcn:97 PTC was created. Component reference: 39, alive: yes, type: BSSAP_LE_Emulation.BSSAP_LE_Emulation_CT, component name: VirtSMLC-BSSAP_LE.
14:38:53.288754 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:38:53.290844 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 40, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
14:38:53.290874 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(40):SCTP_PORT to system:sctp.
14:38:53.291749 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(40):SCTP_PORT to system:sctp finished.
14:38:53.291772 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(40):MTP3_SP_PORT and VirtSMLC-SCCP(38):MTP3_SCCP_PORT.
14:38:53.292022 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(40):MTP3_SP_PORT and VirtSMLC-SCCP(38):MTP3_SCCP_PORT finished.
14:38:53.292045 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({ local_sctp_port := 23908, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 6) on component VirtSMLC-M3UA(40).
14:38:53.292084 BSSAP_LE_Adapter.ttcn:105 Function was started.
14:38:53.292105 BSSAP_LE_Adapter.ttcn:109 Start timer T: 5 s
14:38:53.292125 BSSAP_LE_Adapter.ttcn:112 Connecting BSSAP_LE_Emulation to SCCP_SP_PORT
14:38:53.292146 BSSAP_LE_Adapter.ttcn:113 Connecting ports VirtSMLC-BSSAP_LE(39):BSSAP_LE and VirtSMLC-SCCP(38):SCCP_SP_PORT.
14:38:53.292332 BSSAP_LE_Adapter.ttcn:113 Connect operation on VirtSMLC-BSSAP_LE(39):BSSAP_LE and VirtSMLC-SCCP(38):SCCP_SP_PORT finished.
14:38:53.292353 BSSAP_LE_Adapter.ttcn:114 Starting BSSAP_LE_Emulation
14:38:53.292389 BSSAP_LE_Adapter.ttcn:115 Starting function main({ create_cb := refers(BSSAP_LE_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.BSSAP_LE_UnitdataCallback), decode_dtap := false, role_ms := false, bssap_le_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111110'B, subsystemNumber := 252, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 250, globalTitle := omit } }, "") on component VirtSMLC-BSSAP_LE(39).
14:38:53.292451 BSSAP_LE_Adapter.ttcn:115 Function was started.
14:38:53.292476 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 190, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 252 }) on component VirtSMLC-SCCP(38).
14:38:53.292515 BSSAP_LE_Adapter.ttcn:122 Function was started.
14:38:53.292541 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
14:38:53.292579 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.294300 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
14:38:53.294359 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
14:38:53.295555 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.296677 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.297793 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:38:53.299075 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:38:53.300057 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with ? matched
14:38:53.301141 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
14:38:53.301164 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
14:38:53.301190 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.301213 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.301226 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
14:38:53.301238 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
14:38:53.301251 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.301270 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:53.301296 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.301386 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 18
14:38:53.301407 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.301424 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.301447 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.301459 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 18
14:38:53.301470 Osmocom_VTY_Functions.ttcn:74 Message with id 18 was extracted from the queue of BSCVTY.
14:38:53.301482 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.301494 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
14:38:53.301512 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.301588 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 19
14:38:53.301607 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.301624 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.301646 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.301657 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 19
14:38:53.301668 Osmocom_VTY_Functions.ttcn:74 Message with id 19 was extracted from the queue of BSCVTY.
14:38:53.301681 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.301693 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
14:38:53.301707 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.301783 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 20
14:38:53.301800 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.301816 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.301836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.301847 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 20
14:38:53.301857 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
14:38:53.301869 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.301880 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.301894 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.301959 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 21
14:38:53.301976 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.301992 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302011 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302022 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 21
14:38:53.302033 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
14:38:53.302044 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302055 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.302068 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302089 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
14:38:53.302106 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302122 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.302133 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
14:38:53.302144 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
14:38:53.302155 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302167 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:53.302180 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302209 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
14:38:53.302226 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302243 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302263 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302274 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
14:38:53.302285 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
14:38:53.302297 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302309 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
14:38:53.302322 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302346 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
14:38:53.302362 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302378 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302398 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302409 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
14:38:53.302420 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
14:38:53.302431 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302442 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
14:38:53.302455 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302479 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
14:38:53.302495 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302511 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302529 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302540 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
14:38:53.302551 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
14:38:53.302562 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302573 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.302586 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302607 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
14:38:53.302623 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302638 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302657 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302668 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
14:38:53.302678 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
14:38:53.302689 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302700 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.302714 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302732 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
14:38:53.302747 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302764 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.302774 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
14:38:53.302785 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
14:38:53.302796 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302808 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:53.302821 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302847 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
14:38:53.302863 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.302879 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.302898 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.302909 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
14:38:53.302920 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
14:38:53.302931 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.302943 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
14:38:53.302955 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.302978 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
14:38:53.302994 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.303010 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.303029 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.303040 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
14:38:53.303050 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
14:38:53.303062 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.303073 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
14:38:53.303086 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.303110 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
14:38:53.303126 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.303141 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.303160 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.303171 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
14:38:53.303181 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
14:38:53.303194 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.303205 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.303218 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.303239 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
14:38:53.303255 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.303271 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:53.303289 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:53.303300 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
14:38:53.303311 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
14:38:53.303322 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.303333 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
14:38:53.303346 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:53.303364 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
14:38:53.303379 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:53.303395 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:53.303406 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
14:38:53.303416 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
14:38:53.303427 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:53.303438 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:38:53.305864 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 41, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
14:38:53.305880 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(41):IPA_PORT to system:IPA_CODEC_PT.
14:38:53.306829 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(41):IPA_PORT to system:IPA_CODEC_PT finished.
14:38:53.306842 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT and mtc:IPA_CTRL.
14:38:53.306938 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-d34f21f.
14:38:53.306986 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT.
14:38:53.306998 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
14:38:53.307009 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(41).
14:38:53.307036 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
14:38:53.307047 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
14:38:53.308223 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:38:53.308238 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
14:38:53.308249 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
14:38:53.308262 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
14:38:53.308277 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:38:53.310628 BSC_Tests.ttcn:1073 PTC was created. Component reference: 42, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
14:38:53.310642 BSC_Tests.ttcn:1074 Starting function main({ create_cb := refers(MGCP_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback) }, { callagent_ip := "127.0.0.1", callagent_udp_port := -1, mgw_ip := "127.0.0.1", mgw_udp_port := 2427, multi_conn_mode := false }, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(42).
14:38:53.310681 BSC_Tests.ttcn:1074 Function was started.
14:38:53.310693 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:38:53.310707 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.795168.
14:38:53.310728 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "795167507", variable := "bts.0.oml-connection-state", val := omit } }
14:38:53.310742 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:38:53.312715 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "795167507", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
14:38:53.312730 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:38:53.312743 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "795167507", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
14:38:53.312754 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
14:38:53.312766 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:38:53.312776 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:38:53.469174 BSC_Tests.ttcn:1023 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.0.connection_status", val := "connected" } } id 3
14:38:53.469658 BSC_Tests.ttcn:1023 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc_connection_status", val := "connected" } } id 4
14:38:53.486004 BSC_Tests.ttcn:1023 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.1.connection_status", val := "connected" } } id 5
14:38:54.313094 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:38:54.313532 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:38:54.322406 BSC_Tests.ttcn:951 PTC was created. Component reference: 43, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
14:38:54.322609 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1234, bts_id := 0, trx_id := 0 }
14:38:54.322903 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
14:38:54.323008 BSC_Tests.ttcn:956 Creating new alive PTC with component type RSL_Emulation.RSL_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-RSL.
14:38:54.331975 BSC_Tests.ttcn:956 PTC was created. Component reference: 44, alive: yes, type: RSL_Emulation.RSL_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-RSL.
14:38:54.332079 BSC_Tests.ttcn:957 Connecting ports IPA-BTS0-TRX0-RSL-RSL(44):CCHAN_PT and mtc:RSL_CCHAN[0].
14:38:54.332631 BSC_Tests.ttcn:957 Port RSL_CCHAN[0] is waiting for connection from IPA-BTS0-TRX0-RSL-RSL(44):CCHAN_PT on UNIX pathname /tmp/ttcn3-portconn-545bf91e.
14:38:54.335077 BSC_Tests.ttcn:957 Port RSL_CCHAN[0] has accepted the connection from IPA-BTS0-TRX0-RSL-RSL(44):CCHAN_PT.
14:38:54.335193 BSC_Tests.ttcn:957 Connect operation on IPA-BTS0-TRX0-RSL-RSL(44):CCHAN_PT and mtc:RSL_CCHAN[0] finished.
14:38:54.335245 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(43):IPA_PORT to system:IPA_CODEC_PT.
14:38:54.335473 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(43):IPA_PORT to system:IPA_CODEC_PT finished.
14:38:54.335517 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(43):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
14:38:54.335891 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(43):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-1738b6e.
14:38:54.336066 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(43):CFG_PORT.
14:38:54.336116 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(43):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
14:38:54.336156 BSC_Tests.ttcn:963 Connecting ports IPA-BTS0-TRX0-RSL-IPA(43):IPA_RSL_PORT and IPA-BTS0-TRX0-RSL-RSL(44):IPA_PT.
14:38:54.336792 BSC_Tests.ttcn:963 Connect operation on IPA-BTS0-TRX0-RSL-IPA(43):IPA_RSL_PORT and IPA-BTS0-TRX0-RSL-RSL(44):IPA_PT finished.
14:38:54.336835 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1234/0/0", osmo_rand := "" }, true) on component IPA-BTS0-TRX0-RSL-IPA(43).
14:38:54.336931 BSC_Tests.ttcn:969 Function was started.
14:38:54.336972 BSC_Tests.ttcn:971 Starting function main(true) on component IPA-BTS0-TRX0-RSL-RSL(44).
14:38:54.337048 BSC_Tests.ttcn:971 Function was started.
14:38:54.337093 BSC_Tests.ttcn:1016 Start timer T: 5 s
14:38:54.337146 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.098257.
14:38:54.337224 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "98257198", variable := "bts.0.oml-connection-state", val := omit } }
14:38:54.337283 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:38:54.337347 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL { trap := { variable := "msc.0.connection_status", val := "connected" } } with { resp := { verb := "GET_REPLY", id := "98257198", variable := "bts.0.oml-connection-state", val := ? } } unmatched: First message in the queue does not match the template: 
14:38:54.337399 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
14:38:54.337450 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.0.connection_status", val := "connected" } } id 3
14:38:54.337500 Osmocom_CTRL_Functions.ttcn:43 Message with id 3 was extracted from the queue of IPA_CTRL.
14:38:54.337556 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL { trap := { variable := "msc_connection_status", val := "connected" } } with { resp := { verb := "GET_REPLY", id := "98257198", variable := "bts.0.oml-connection-state", val := ? } } unmatched: First message in the queue does not match the template: 
14:38:54.337602 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
14:38:54.337648 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc_connection_status", val := "connected" } } id 4
14:38:54.337692 Osmocom_CTRL_Functions.ttcn:43 Message with id 4 was extracted from the queue of IPA_CTRL.
14:38:54.337745 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL { trap := { variable := "msc.1.connection_status", val := "connected" } } with { resp := { verb := "GET_REPLY", id := "98257198", variable := "bts.0.oml-connection-state", val := ? } } unmatched: First message in the queue does not match the template: 
14:38:54.337788 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
14:38:54.337840 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.1.connection_status", val := "connected" } } id 5
14:38:54.337882 Osmocom_CTRL_Functions.ttcn:43 Message with id 5 was extracted from the queue of IPA_CTRL.
14:38:54.340997 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "98257198", variable := "bts.0.oml-connection-state", val := "degraded" } } id 6
14:38:54.341064 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:38:54.341119 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "98257198", variable := "bts.0.oml-connection-state", val := "degraded" } } id 6
14:38:54.341170 Osmocom_CTRL_Functions.ttcn:41 Message with id 6 was extracted from the queue of IPA_CTRL.
14:38:54.341228 Osmocom_Types.ttcn:126 Start timer T: 0.1 s
14:38:54.357618 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 1
14:38:54.357988 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 2
14:38:54.358404 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 3
14:38:54.358640 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 4
14:38:54.359009 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 5
14:38:54.359223 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 6
14:38:54.359423 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 7
14:38:54.359635 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 8
14:38:54.359924 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 9
14:38:54.360090 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 10
14:38:54.360323 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 11
14:38:54.360490 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 12
14:38:54.360780 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(44) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 13
14:38:54.441290 Osmocom_Types.ttcn:127 Timeout T: 0.1 s
14:38:54.441725 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.700486.
14:38:54.442126 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "700486496", variable := "bts.0.oml-connection-state", val := omit } }
14:38:54.442522 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:38:54.447977 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "700486496", variable := "bts.0.oml-connection-state", val := "connected" } } id 7
14:38:54.448264 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:38:54.448390 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "700486496", variable := "bts.0.oml-connection-state", val := "connected" } } id 7
14:38:54.448465 Osmocom_CTRL_Functions.ttcn:41 Message with id 7 was extracted from the queue of IPA_CTRL.
14:38:54.448772 BSC_Tests.ttcn:1019 Stop timer T: 5 s
14:38:54.449170 BSC_Tests.ttcn:1022 Start timer T: 1 s
14:38:55.449492 BSC_Tests.ttcn:1023 Timeout T: 1 s
14:38:55.449829 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
14:38:55.450076 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.450503 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
14:38:55.450784 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.451012 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:55.451150 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
14:38:55.451220 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
14:38:55.451289 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
14:38:55.451356 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.451419 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
14:38:55.451502 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.451763 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 34
14:38:55.451864 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.452032 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:55.452344 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
14:38:55.452516 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 34
14:38:55.452614 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
14:38:55.452710 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.452807 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
14:38:55.452951 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.453351 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 35
14:38:55.453529 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.453644 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:55.453777 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:38:55.453842 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 35
14:38:55.453905 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
14:38:55.453968 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.454032 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
14:38:55.454130 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.454549 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 36
14:38:55.454649 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.454742 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:55.454862 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
14:38:55.454925 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 36
14:38:55.454985 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
14:38:55.455045 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.455102 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
14:38:55.455177 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.455576 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
14:38:55.455668 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.455763 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:55.455825 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
14:38:55.455957 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
14:38:55.456043 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.456109 Osmocom_VTY_Functions.ttcn:338 "TC_stat_num_msc_connected_2() start"
14:38:55.456217 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_stat_num_msc_connected_2() start"
14:38:55.456306 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:55.456766 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 38
14:38:55.456896 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:55.457017 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:55.457080 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 38
14:38:55.457139 Osmocom_VTY_Functions.ttcn:73 Message with id 38 was extracted from the queue of BSCVTY.
14:38:55.457197 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:55.457259 Osmocom_Types.ttcn:126 Start timer T: 1 s
14:38:56.457365 Osmocom_Types.ttcn:127 Timeout T: 1 s
14:38:56.457838 BSC_Tests.ttcn:4122 Creating new PTC with component type MSC_ConnectionHandler.MSC_ConnHdlr, component name: TC_stat_num_msc_connected_2.
14:38:56.471356 BSC_Tests.ttcn:4122 PTC was created. Component reference: 45, alive: no, type: MSC_ConnectionHandler.MSC_ConnHdlr, component name: TC_stat_num_msc_connected_2.
14:38:56.471535 BSC_Tests.ttcn:4089 Connecting ports TC_stat_num_msc_connected_2(45):RAN and VirtMSC-RAN(34):PROC.
14:38:56.479495 BSC_Tests.ttcn:4089 Connect operation on TC_stat_num_msc_connected_2(45):RAN and VirtMSC-RAN(34):PROC finished.
14:38:56.479594 BSC_Tests.ttcn:4090 Connecting ports TC_stat_num_msc_connected_2(45):RSL and IPA-BTS0-TRX0-RSL-RSL(44):CLIENT_PT.
14:38:56.480904 BSC_Tests.ttcn:4090 Connect operation on TC_stat_num_msc_connected_2(45):RSL and IPA-BTS0-TRX0-RSL-RSL(44):CLIENT_PT finished.
14:38:56.480960 BSC_Tests.ttcn:4091 Connecting ports TC_stat_num_msc_connected_2(45):RSL_PROC and IPA-BTS0-TRX0-RSL-RSL(44):RSL_PROC.
14:38:56.482061 BSC_Tests.ttcn:4091 Connect operation on TC_stat_num_msc_connected_2(45):RSL_PROC and IPA-BTS0-TRX0-RSL-RSL(44):RSL_PROC finished.
14:38:56.482145 BSC_Tests.ttcn:4100 Connecting ports TC_stat_num_msc_connected_2(45):RAN_CONN and VirtMSC-RAN(34):CLIENT.
14:38:56.483500 BSC_Tests.ttcn:4100 Connect operation on TC_stat_num_msc_connected_2(45):RAN_CONN and VirtMSC-RAN(34):CLIENT finished.
14:38:56.483568 BSC_Tests.ttcn:4102 Connecting ports TC_stat_num_msc_connected_2(45):BSSAP_LE and VirtSMLC-BSSAP_LE(39):CLIENT.
14:38:56.484765 BSC_Tests.ttcn:4102 Connect operation on TC_stat_num_msc_connected_2(45):BSSAP_LE and VirtSMLC-BSSAP_LE(39):CLIENT finished.
14:38:56.484826 BSC_Tests.ttcn:4103 Connecting ports TC_stat_num_msc_connected_2(45):BSSAP_LE_PROC and VirtSMLC-BSSAP_LE(39):PROC.
14:38:56.485571 BSC_Tests.ttcn:4103 Connect operation on TC_stat_num_msc_connected_2(45):BSSAP_LE_PROC and VirtSMLC-BSSAP_LE(39):PROC finished.
14:38:56.485629 BSC_Tests.ttcn:4105 Connecting ports TC_stat_num_msc_connected_2(45):STATSD_PROC and VirtMSC-STATS(31):STATSD_PROC.
14:38:56.486503 BSC_Tests.ttcn:4105 Connect operation on TC_stat_num_msc_connected_2(45):STATSD_PROC and VirtMSC-STATS(31):STATSD_PROC finished.
14:38:56.486562 BSC_Tests.ttcn:4106 Connecting ports TC_stat_num_msc_connected_2(45):MGCP_PROC and VirtMGW-MGCP-0(42):MGCP_PROC.
14:38:56.487326 BSC_Tests.ttcn:4106 Connect operation on TC_stat_num_msc_connected_2(45):MGCP_PROC and VirtMGW-MGCP-0(42):MGCP_PROC finished.
14:38:56.487385 BSC_Tests.ttcn:4107 Connecting ports TC_stat_num_msc_connected_2(45):MGCP and VirtMGW-MGCP-0(42):MGCP_CLIENT.
14:38:56.488184 BSC_Tests.ttcn:4107 Connect operation on TC_stat_num_msc_connected_2(45):MGCP and VirtMGW-MGCP-0(42):MGCP_CLIENT finished.
14:38:56.488245 BSC_Tests.ttcn:4108 Connecting ports TC_stat_num_msc_connected_2(45):MGCP_MULTI and VirtMGW-MGCP-0(42):MGCP_CLIENT_MULTI.
14:38:56.488987 BSC_Tests.ttcn:4108 Connect operation on TC_stat_num_msc_connected_2(45):MGCP_MULTI and VirtMGW-MGCP-0(42):MGCP_CLIENT_MULTI finished.
14:38:56.489048 BSC_Tests.ttcn:4130 Starting function f_handler_init(refers(BSC_Tests.f_tc_stat_num_msc_connected_2), "TC_stat_num_msc_connected_2", omit) on component TC_stat_num_msc_connected_2(45).
14:38:56.489177 BSC_Tests.ttcn:4130 Function was started.
14:38:56.836823 BSC_Tests.ttcn:3213 PTC with component reference 45 is done.
14:38:56.836861 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.036980.
14:38:56.836898 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "36980125", variable := "stat_item.last.bsc.0.num_msc:connected", val := omit } }
14:38:56.836928 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:38:56.837901 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "36980125", variable := "stat_item.last.bsc.0.num_msc:connected", val := "2" } } id 8
14:38:56.837944 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:38:56.837967 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "36980125", variable := "stat_item.last.bsc.0.num_msc:connected", val := "2" } } id 8
14:38:56.838080 Osmocom_CTRL_Functions.ttcn:41 Message with id 8 was extracted from the queue of IPA_CTRL.
14:38:56.838103 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.492303.
14:38:56.838124 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "492302706", variable := "stat_item.last.bsc.0.num_msc:total", val := omit } }
14:38:56.838143 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
14:38:56.838975 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(41) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "492302706", variable := "stat_item.last.bsc.0.num_msc:total", val := "3" } } id 9
14:38:56.838992 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
14:38:56.839006 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(41): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "492302706", variable := "stat_item.last.bsc.0.num_msc:total", val := "3" } } id 9
14:38:56.839020 Osmocom_CTRL_Functions.ttcn:41 Message with id 9 was extracted from the queue of IPA_CTRL.
14:38:56.839045 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
14:38:56.839068 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
14:38:56.839467 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" id 39
14:38:56.839482 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 40
14:38:56.839516 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:56.839539 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
14:38:56.839561 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
14:38:56.839578 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
14:38:56.839592 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" with ? matched
14:38:56.839606 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1466343 bytes in 1341 blocks)" id 39
14:38:56.839619 Osmocom_VTY_Functions.ttcn:85 Message with id 39 was extracted from the queue of BSCVTY.
14:38:56.839641 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
14:38:56.839661 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
14:38:56.839674 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 40
14:38:56.839687 Osmocom_VTY_Functions.ttcn:73 Message with id 40 was extracted from the queue of BSCVTY.
14:38:56.839700 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
14:38:56.839714 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
14:38:56.839733 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
14:38:56.839750 BSC_Tests.ttcn:888 Stopping all components.
14:38:56.840704 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT was closed unexpectedly by the peer.
14:38:56.840719 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(41):IPA_CTRL_PORT.
14:38:56.840848 BSC_Tests.ttcn:888 All components were stopped.
14:38:56.840860 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
14:38:56.840873 BSC_Tests.ttcn:890 Stopping test component execution.
14:38:56.840891 BSC_Tests.ttcn:3235 Test case TC_stat_num_msc_connected_2 was stopped.
14:38:56.840901 BSC_Tests.ttcn:3235 Terminating component type BSC_Tests.test_CT.
14:38:56.840913 BSC_Tests.ttcn:3235 Default with id 1 (altstep as_Tguard) was deactivated.
14:38:56.840924 BSC_Tests.ttcn:3235 Stop timer T_guard: 30 s
14:38:56.840936 BSC_Tests.ttcn:3235 Port IPA_CTRL was stopped.
14:38:56.840946 BSC_Tests.ttcn:3235 Removing unterminated connection between port RSL_CCHAN[0] and IPA-BTS0-TRX0-RSL-RSL(44):CCHAN_PT.
14:38:56.840968 BSC_Tests.ttcn:3235 Message with id 1 was extracted from the queue of RSL_CCHAN[0].
14:38:56.840981 BSC_Tests.ttcn:3235 Message with id 2 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841002 BSC_Tests.ttcn:3235 Message with id 3 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841016 BSC_Tests.ttcn:3235 Message with id 4 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841028 BSC_Tests.ttcn:3235 Message with id 5 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841041 BSC_Tests.ttcn:3235 Message with id 6 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841051 BSC_Tests.ttcn:3235 Message with id 7 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841061 BSC_Tests.ttcn:3235 Message with id 8 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841071 BSC_Tests.ttcn:3235 Message with id 9 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841081 BSC_Tests.ttcn:3235 Message with id 10 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841091 BSC_Tests.ttcn:3235 Message with id 11 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841101 BSC_Tests.ttcn:3235 Message with id 12 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841112 BSC_Tests.ttcn:3235 Message with id 13 was extracted from the queue of RSL_CCHAN[0].
14:38:56.841121 BSC_Tests.ttcn:3235 Port RSL_CCHAN[0] was stopped.
14:38:56.841131 BSC_Tests.ttcn:3235 Port RSL_CCHAN[1] was stopped.
14:38:56.841141 BSC_Tests.ttcn:3235 Port RSL_CCHAN[2] was stopped.
14:38:56.841151 BSC_Tests.ttcn:3235 Port IPA_RSL[0][0] was stopped.
14:38:56.841160 BSC_Tests.ttcn:3235 Port IPA_RSL[0][1] was stopped.
14:38:56.841170 BSC_Tests.ttcn:3235 Port IPA_RSL[0][2] was stopped.
14:38:56.841180 BSC_Tests.ttcn:3235 Port IPA_RSL[0][3] was stopped.
14:38:56.841189 BSC_Tests.ttcn:3235 Port IPA_RSL[1][0] was stopped.
14:38:56.841199 BSC_Tests.ttcn:3235 Port IPA_RSL[1][1] was stopped.
14:38:56.841208 BSC_Tests.ttcn:3235 Port IPA_RSL[1][2] was stopped.
14:38:56.841218 BSC_Tests.ttcn:3235 Port IPA_RSL[1][3] was stopped.
14:38:56.841228 BSC_Tests.ttcn:3235 Port IPA_RSL[2][0] was stopped.
14:38:56.841237 BSC_Tests.ttcn:3235 Port IPA_RSL[2][1] was stopped.
14:38:56.841253 BSC_Tests.ttcn:3235 Port IPA_RSL[2][2] was stopped.
14:38:56.841262 BSC_Tests.ttcn:3235 Port IPA_RSL[2][3] was stopped.
14:38:56.841272 BSC_Tests.ttcn:3235 Port IPA was stopped.
14:38:56.841282 BSC_Tests.ttcn:3235 Removing unterminated connection between port SCCPLITE_IPA_CTRL and VirtMSC-RAN(34):CTRL_CLIENT.
14:38:56.841298 BSC_Tests.ttcn:3235 Removing unterminated connection between port SCCPLITE_IPA_CTRL and VirtMSC-RAN(37):CTRL_CLIENT.
14:38:56.841322 BSC_Tests.ttcn:3235 Port SCCPLITE_IPA_CTRL was stopped.
14:38:56.841341 BSC_Tests.ttcn:3235 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(43):CFG_PORT.
14:38:56.841364 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[0][0] was stopped.
14:38:56.841398 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[0][1] was stopped.
14:38:56.841408 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[0][2] was stopped.
14:38:56.841418 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[0][3] was stopped.
14:38:56.841428 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[1][0] was stopped.
14:38:56.841437 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[1][1] was stopped.
14:38:56.841448 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[1][2] was stopped.
14:38:56.841457 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[1][3] was stopped.
14:38:56.841466 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[2][0] was stopped.
14:38:56.841475 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[2][1] was stopped.
14:38:56.841484 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[2][2] was stopped.
14:38:56.841493 BSC_Tests.ttcn:3235 Port IPA_CFG_PORT[2][3] was stopped.
14:38:56.841502 BSC_Tests.ttcn:3235 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
14:38:56.841523 BSC_Tests.ttcn:3235 Port BSCVTY was unmapped from system:BSCVTY.
14:38:56.841535 BSC_Tests.ttcn:3235 Port BSCVTY was stopped.
14:38:56.841545 BSC_Tests.ttcn:3235 Port STPVTY was stopped.
14:38:56.841554 BSC_Tests.ttcn:3235 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
14:38:56.841564 BSC_Tests.ttcn:3235 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
14:38:56.841573 BSC_Tests.ttcn:3235 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
14:38:56.841582 BSC_Tests.ttcn:3235 Port BSSAP was stopped.
14:38:56.841591 BSC_Tests.ttcn:3235 Port BSSAP_LE was stopped.
14:38:56.841601 BSC_Tests.ttcn:3235 Component type BSC_Tests.test_CT was shut down inside testcase TC_stat_num_msc_connected_2.
14:38:56.841611 BSC_Tests.ttcn:3235 Waiting for PTCs to finish.
14:38:56.851624 BSC_Tests.ttcn:3235 Setting final verdict of the test case.
14:38:56.851680 BSC_Tests.ttcn:3235 Local verdict of MTC: pass
14:38:56.851730 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-STATS(31): none (pass -> pass)
14:38:56.851759 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-SCCP(32): none (pass -> pass)
14:38:56.851807 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-M3UA(33): none (pass -> pass)
14:38:56.851845 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-RAN(34): none (pass -> pass)
14:38:56.851867 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-SCCP(35): none (pass -> pass)
14:38:56.851894 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-M3UA(36): none (pass -> pass)
14:38:56.851909 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMSC-RAN(37): none (pass -> pass)
14:38:56.851926 BSC_Tests.ttcn:3235 Local verdict of PTC VirtSMLC-SCCP(38): none (pass -> pass)
14:38:56.851953 BSC_Tests.ttcn:3235 Local verdict of PTC VirtSMLC-BSSAP_LE(39): none (pass -> pass)
14:38:56.851976 BSC_Tests.ttcn:3235 Local verdict of PTC VirtSMLC-M3UA(40): none (pass -> pass)
14:38:56.852002 BSC_Tests.ttcn:3235 Local verdict of PTC IPA-CTRL-CLI-IPA(41): none (pass -> pass)
14:38:56.852048 BSC_Tests.ttcn:3235 Local verdict of PTC VirtMGW-MGCP-0(42): none (pass -> pass)
14:38:56.852094 BSC_Tests.ttcn:3235 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(43): none (pass -> pass)
14:38:56.852130 BSC_Tests.ttcn:3235 Local verdict of PTC IPA-BTS0-TRX0-RSL-RSL(44): none (pass -> pass)
14:38:56.852160 BSC_Tests.ttcn:3235 Local verdict of PTC TC_stat_num_msc_connected_2(45): none (pass -> pass)
14:38:56.852201 BSC_Tests.ttcn:3235 Test case TC_stat_num_msc_connected_2 finished. Verdict: pass
14:38:56.852242 BSC_Tests.ttcn:3235 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_stat_num_msc_connected_2 pass'.
14:39:02.167645 BSC_Tests.ttcn:3235 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-io_uring/ttcn3-tcpdump-stop.sh BSC_Tests.TC_stat_num_msc_connected_2 pass' was executed successfully (exit status: 0).
14:39:02.167708 BSC_Tests.ttcn:3242 Switching to log file `BSC_Tests-TC_stat_num_msc_connected_3-4ec725da15b5-mtc-9884.log'
